From 8809b176ecde425d13cab8920a66fbfd6fb4c3b7 Mon Sep 17 00:00:00 2001
From: Kurt Mahan <kmahan@freescale.com>
Date: Tue, 24 Jun 2008 23:26:54 -0600
Subject: [PATCH] Make sure interrupt handler calls aren't nested.

LTIBName: m5445x-fecint-nest
Signed-off-by: Kurt Mahan <kmahan@freescale.com>
---
 drivers/net/fec.c |    5 ++++-
 1 files changed, 4 insertions(+), 1 deletions(-)

--- a/drivers/net/fec.c
+++ b/drivers/net/fec.c
@@ -23,6 +23,9 @@
  *
  * Bug fixes and cleanup by Philippe De Muyter (phdm@macqel.be)
  * Copyright (c) 2004-2006 Macq Electronique SA.
+ *
+ * Coldfire bug fixes and cleanup by Kurt Mahan (kmahan@freescale.com)
+ * Copyright 2007-2008 Freescale Semiconductor, Inc. All Rights Reserved.
  */
 
 #include <linux/module.h>
@@ -1865,7 +1868,7 @@ static void __inline__ fec_request_intrs
 
 	/* Setup interrupt handlers. */
 	for (idp = id; idp->name; idp++) {
-		if (request_irq(b+idp->irq, fec_enet_interrupt, 0,
+		if (request_irq(b+idp->irq, fec_enet_interrupt, IRQF_DISABLED,
 		    idp->name, dev) != 0)
 			printk(KERN_ERR "FEC: Could not alloc %s IRQ(%d)!\n",
 				idp->name, b+idp->irq);
