From 2ec88eb0d3d2c877eff811901215390708dd03b9 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Mon, 11 Jan 2010 04:29:39 +0100
Subject: [PATCH] /opt/Projects/openwrt/target/linux/xburst/patches-2.6.31/052-rtc.patch

---
 drivers/rtc/Kconfig  |   11 +++++++++++
 drivers/rtc/Makefile |    1 +
 2 files changed, 12 insertions(+), 0 deletions(-)

--- a/drivers/rtc/Kconfig
+++ b/drivers/rtc/Kconfig
@@ -469,6 +469,17 @@ config RTC_DRV_EFI
 	  This driver can also be built as a module. If so, the module
 	  will be called rtc-efi.
 
+config RTC_DRV_JZ4740
+	tristate "Ingenic JZ4720/JZ4740 SoC"
+	depends on RTC_CLASS
+	depends on SOC_JZ4740
+	help
+	  If you say yes here you get support for the
+	  Ingenic JZ4720/JZ4740 SoC RTC controller.
+
+	  This driver can also be buillt as a module. If so, the module
+	  will be called rtc-jz4740.
+
 config RTC_DRV_STK17TA8
 	tristate "Simtek STK17TA8"
 	depends on RTC_CLASS
--- a/drivers/rtc/Makefile
+++ b/drivers/rtc/Makefile
@@ -44,6 +44,7 @@ obj-$(CONFIG_RTC_DRV_EP93XX)	+= rtc-ep93
 obj-$(CONFIG_RTC_DRV_FM3130)	+= rtc-fm3130.o
 obj-$(CONFIG_RTC_DRV_GENERIC)	+= rtc-generic.o
 obj-$(CONFIG_RTC_DRV_ISL1208)	+= rtc-isl1208.o
+obj-$(CONFIG_RTC_DRV_JZ4740)	+= rtc-jz4740.o
 obj-$(CONFIG_RTC_DRV_M41T80)	+= rtc-m41t80.o
 obj-$(CONFIG_RTC_DRV_M41T94)	+= rtc-m41t94.o
 obj-$(CONFIG_RTC_DRV_M48T35)	+= rtc-m48t35.o
