--- a/arch/powerpc/boot/dts/canyonlands.dts
+++ b/arch/powerpc/boot/dts/canyonlands.dts
@@ -262,28 +262,6 @@
 				interrupts = <0x1 0x4>;
 			};
 
-			UART2: serial@ef600500 {
-				device_type = "serial";
-				compatible = "ns16550";
-				reg = <0xef600500 0x00000008>;
-				virtual-reg = <0xef600500>;
-				clock-frequency = <0>; /* Filled in by U-Boot */
-				current-speed = <0>; /* Filled in by U-Boot */
-				interrupt-parent = <&UIC1>;
-				interrupts = <0x1d 0x4>;
-			};
-
-			UART3: serial@ef600600 {
-				device_type = "serial";
-				compatible = "ns16550";
-				reg = <0xef600600 0x00000008>;
-				virtual-reg = <0xef600600>;
-				clock-frequency = <0>; /* Filled in by U-Boot */
-				current-speed = <0>; /* Filled in by U-Boot */
-				interrupt-parent = <&UIC1>;
-				interrupts = <0x1e 0x4>;
-			};
-
 			IIC0: i2c@ef600700 {
 				compatible = "ibm,iic-460ex", "ibm,iic";
 				reg = <0xef600700 0x00000014>;
