// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	keys {
		compatible = "gpio-keys";

		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&eth0 {
	status = "okay";

	/* default for ar934x, except for 1000M */
	pll-data = <0x06000000 0x00000101 0x00001616>;

	nvmem-cells = <&macaddr_lan>;
	nvmem-cell-names = "mac-address-ascii";

	phy-mode = "rgmii";
	phy-handle = <&phy0>;
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		qca,ar8327-initvals = <
			/* GPL code drop (bsp.h & athrs17_phy.c) */
			0x10 0xc1000000 /* PWS_REG_VALUE */
			0x04 0x07600000 /* PORT0 PAD Mode */
			0x0c 0x01000000 /* PORT6 PAD Mode */
			0x7c 0x0000007e /* PORT0_STATUS */
			0x94 0x0000007e /* PORT6_STATUS */
		>;
	};
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		compatible = "pci168c,0030";
		reg = <0x0000 0 0 0 0>;
		/* "mac-address-ascii" currently does not work for
		   ath9k pci devices. these below are retained for future
		   improvements. */
		/* nvmem-cells = <&macaddr_wan>, <&cal_art_5000>;
		   nvmem-cell-names = "mac-address-ascii", "calibration";
		   mac-address-increment = <1>; */
		qca,no-eeprom; /* remove this when "mac-address-ascii" works  */
		gpio-controller;
		#gpio-cells = <2>;
	};
};

&ref {
	clock-frequency = <40000000>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x000000 0x010000>;
				read-only;
			};

			partition@10000 {
				label = "nvram";
				reg = <0x010000 0x010000>;
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x020000 0xF90000>;
				compatible = "denx,uimage";
			};

			partition@fb0000 {
				label = "lang";
				reg = <0xfb0000 0x030000>;
				read-only;
			};

			mac: partition@fe0000 {
				label = "mac";
				reg = <0xfe0000 0x010000>;
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_lan: macaddr@4 {
					reg = <0x4 0x11>;
				};

				macaddr_wan: macaddr@18 {
					reg = <0x18 0x11>;
				};
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				cal_art_1000: cal@1000 {
					reg = <0x1000 0x440>;
				};

				cal_art_5000: cal@5000 {
					reg = <0x5000 0x440>;
				};
			};
		};
	};
};

&usb {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&wmac {
	status = "okay";
	nvmem-cells = <&macaddr_lan>, <&cal_art_1000>;
	nvmem-cell-names = "mac-address-ascii", "calibration";
};
