From 128dc09b0af36772062142ce9e85b19c84ac789a Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Tue, 28 Feb 2023 17:53:37 +0000
Subject: [PATCH] net: phy: add driver for MediaTek 2.5G PHY

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 drivers/net/phy/Kconfig          |   7 ++
 drivers/net/phy/Makefile         |   1 +
 drivers/net/phy/mediatek-2p5ge.c | 220 +++++++++++++++++++++++++++++++
 3 files changed, 226 insertions(+)
 create mode 100644 drivers/net/phy/mediatek-2p5ge.c

--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -304,6 +304,13 @@ config MEDIATEK_GE_SOC_PHY
 	  present in the SoCs efuse and will dynamically calibrate VCM
 	  (common-mode voltage) during startup.
 
+config MEDIATEK_2P5G_PHY
+	tristate "MediaTek 2.5G Ethernet PHY"
+	depends on (ARCH_MEDIATEK && ARM64) || COMPILE_TEST
+	default NET_MEDIATEK_SOC
+	help
+	  Supports the MediaTek 2.5G Ethernet PHY.
+
 config MICREL_PHY
 	tristate "Micrel PHYs"
 	help
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -80,6 +80,7 @@ obj-$(CONFIG_MARVELL_10G_PHY)	+= marvell
 obj-$(CONFIG_MARVELL_PHY)	+= marvell.o
 obj-$(CONFIG_MARVELL_88X2222_PHY)	+= marvell-88x2222.o
 obj-$(CONFIG_MAXLINEAR_GPHY)	+= mxl-gpy.o
+obj-$(CONFIG_MEDIATEK_2P5G_PHY)	+= mediatek-2p5ge.o
 obj-$(CONFIG_MEDIATEK_GE_PHY)	+= mediatek-ge.o
 obj-$(CONFIG_MEDIATEK_GE_SOC_PHY)	+= mediatek-ge-soc.o
 obj-$(CONFIG_MESON_GXL_PHY)	+= meson-gxl.o
