// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6328.dtsi"

/ {
	model = "Comtrend AR-5387un";
	compatible = "comtrend,ar-5387un", "brcm,bcm6328";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;

		led-dsl = &led_dsl_green;
		led-internet = &led_internet_green;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};

	bcm43225-sprom {
		compatible = "brcm,bcma-sprom";

		pci-bus = <1>;
		pci-dev = <0>;

		nvmem-cells = <&macaddr_cfe_6a0>;
		nvmem-cell-names = "mac-address";
		mac-address-increment = <1>;

		brcm,sprom = "brcm/bcm43225-sprom.bin";
		brcm,sprom-fixups = <2 0x05bb>,
				    <65 0x1204>,
				    <78 0x0303>,
				    <79 0x0202>,
				    <80 0xff02>,
				    <87 0x0315>,
				    <88 0x0315>,
				    <96 0x2048>,
				    <97 0xff11>,
				    <98 0x1567>,
				    <99 0xfb24>,
				    <100 0x3e3c>,
				    <101 0x4038>,
				    <102 0xfe7f>,
				    <103 0x1279>,
				    <112 0x2048>,
				    <113 0xff03>,
				    <114 0x154c>,
				    <115 0xfb27>,
				    <116 0x3e3c>,
				    <117 0x4038>,
				    <118 0xfe87>,
				    <119 0x1233>,
				    <203 0x2226>;
	};
};

&ehci {
	status = "okay";
};

&ethernet {
	status = "okay";

	nvmem-cells = <&macaddr_cfe_6a0>;
	nvmem-cell-names = "mac-address";
};

&hsspi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <16666667>;
		spi-tx-bus-width = <2>;
		spi-rx-bus-width = <2>;
		reg = <0>;

		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			cfe: partition@0 {
				reg = <0x000000 0x010000>;
				label = "cfe";
				read-only;
			};

			partition@10000 {
				compatible = "brcm,bcm963xx-imagetag";
				reg = <0x010000 0xfe0000>;
				label = "firmware";
			};

			partition@ff0000 {
				reg = <0xff0000 0x010000>;
				label = "nvram";
			};
		};
	};
};

&leds {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_leds>;

	led@1 {
		reg = <1>;
		label = "red:internet";
	};

	led_power_red: led@4 {
		reg = <4>;
		label = "red:power";
	};

	led_internet_green: led@7 {
		reg = <7>;
		label = "green:internet";
	};

	led_power_green: led@8 {
		reg = <8>;
		label = "green:power";
	};

	led_dsl_green: led@11 {
		reg = <11>;
		active-low;
		label = "green:dsl";
	};
};

&ohci {
	status = "okay";
};

&pcie {
	status = "okay";
};

&pinctrl {
	pinctrl_leds: leds {
		function = "led";
		pins = "gpio1", "gpio4", "gpio7",
		       "gpio8", "gpio11";
	};
};

&switch0 {
	ports {
		port@0 {
			reg = <0>;
			label = "lan1";

			phy-handle = <&phy1>;
			phy-mode = "mii";
		};

		port@1 {
			reg = <1>;
			label = "lan2";

			phy-handle = <&phy2>;
			phy-mode = "mii";
		};

		port@2 {
			reg = <2>;
			label = "lan3";

			phy-handle = <&phy3>;
			phy-mode = "mii";
		};

		port@3 {
			reg = <3>;
			label = "lan4";

			phy-handle = <&phy4>;
			phy-mode = "mii";
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};

&cfe {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_cfe_6a0: macaddr@6a0 {
		reg = <0x6a0 0x6>;
	};
};
