// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_white;
		led-failsafe = &led_white;
		led-running = &led_blue;
		led-upgrade = &led_blue;
	};

	leds {
		compatible = "gpio-leds";

		led_white: led_white {
			label = "white:dome";
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
		};

		led_blue: led_blue {
			label = "blue:dome";
			gpios = <&gpio 8 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&pcie {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x060000>;
				read-only;
			};

			partition@60000 {
				label = "u-boot-env";
				reg = <0x060000 0x010000>;
				read-only;
			};

			partition@70000 {
				/* Combine kernel0 & kernel1 */
				label = "firmware";
				reg = <0x070000 0xf20000>;
				compatible = "denx,uimage";
			};

			partition@f90000 {
				label = "bs";
				reg = <0xf90000 0x020000>;
			};

			partition@fb0000 {
				label = "cfg";
				reg = <0xfb0000 0x040000>;
				read-only;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
