// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "Arcadyan WE420223-99";
	compatible = "arcadyan,we420223-99", "mediatek,mt7621-soc";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_wps_green;
		led-wifi = &led_wifi_green;
	};

	chosen {
		bootargs = "console=ttyS0,57600 ubi.mtd=5 root=/dev/ubiblock0_0";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 42 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			default-state = "on";
		};

		led_power_red: power_red {
			label = "red:power";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_FAULT;
		};

		led_wifi_blue: wifi_blue {
			label = "blue:wifi";
			gpios = <&gpio 41 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN;
		};

		led_wifi_green: wifi_green {
			label = "green:wifi";
			gpios = <&gpio 43 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
		};

		led_wps_red: wps_red {
			label = "red:wps";
			gpios = <&gpio 45 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WPS;
		};

		led_wps_green: wps_green {
			label = "green:wps";
			gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WPS;
		};

		led_followme_r: followme_red {
			label = "red:followme";
			gpios = <&gpio 47 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
		};

		led_followme_g: followme_green {
			label = "green:followme";
			gpios = <&gpio 48 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";

		reg = <0>;
		spi-max-frequency = <70000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "ALL";
				reg = <0x0 0x2000000>;
				read-only;
			};

			partition@1 {
				label = "Bootloader";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "Config";
				reg = <0x30000 0x10000>;
			};

			factory: partition@40000 {
				label = "Factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "kernel";
				reg = <0x50000 0x1f60000>;
			};

			partition@490000 {
				label = "rootfs";
				reg = <0x490000 0x1b20000>;
			};

			partition@1000000 {
				label = "Kernel2";
				reg = <0x1000000 0xfb0000>;
			};

			partition@1440000 {
				label = "RootFS2";
				reg = <0x1440000 0xb70000>;
			};

			partition@1fb0000 {
				label = "glbcfg";
				reg = <0x1fb0000 0x10000>;
				read-only;
			};

			partition@1fc0000 {
				label = "board_data";
				reg = <0x1fc0000 0x10000>;
				read-only;
			};

			partition@1fd0000 {
				label = "glbcfg2";
				reg = <0x1fd0000 0x10000>;
				read-only;
			};

			partition@1fe0000 {
				label = "board_data2";
				reg = <0x1fe0000 0x10000>;
				read-only;
			};
		};
	};
};

&xhci {
	status = "disabled";
};

&switch0 {
	ports {
		port@1 {
			status = "okay";
			label = "swp1";
		};
	};
};

&gmac1 {
	status = "okay";
	label = "swp0";
	phy-handle = <&ethphy0>;
};

&mdio {
	ethphy0: ethernet-phy@0 {
		reg = <0>;
	};
};

&pcie {
	status = "okay";
};

&pcie1 {
	mt76@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0000>;
	};
};
