From 1a82d7080001d395563ad8266d120d4cf63ad0a5 Mon Sep 17 00:00:00 2001
From: Shawn Guo <shawn.guo@linaro.org>
Date: Wed, 29 Sep 2021 11:42:46 +0800
Subject: [PATCH] arm64: dts: qcom: msm8996: Move '#clock-cells' to QMP PHY
 child node

'#clock-cells' is a required property of QMP PHY child node, not itself.
Move it to fix the dtbs_check warnings.

There are only '#clock-cells' removal from SM8350 QMP PHY nodes, because
child nodes already have the property.

Signed-off-by: Shawn Guo <shawn.guo@linaro.org>
Signed-off-by: Bjorn Andersson <bjorn.andersson@linaro.org>
Link: https://lore.kernel.org/r/20210929034253.24570-4-shawn.guo@linaro.org
---
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/qcom/ipq8074.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq8074.dtsi
@@ -91,7 +91,6 @@
 		ssphy_1: phy@58000 {
 			compatible = "qcom,ipq8074-qmp-usb3-phy";
 			reg = <0x00058000 0x1c4>;
-			#clock-cells = <1>;
 			#address-cells = <1>;
 			#size-cells = <1>;
 			ranges;
@@ -112,6 +111,7 @@
 				      <0x00058800 0x1f8>,     /* PCS  */
 				      <0x00058600 0x044>;     /* PCS misc*/
 				#phy-cells = <0>;
+				#clock-cells = <1>;
 				clocks = <&gcc GCC_USB1_PIPE_CLK>;
 				clock-names = "pipe0";
 				clock-output-names = "usb3phy_1_cc_pipe_clk";
@@ -134,7 +134,6 @@
 		ssphy_0: phy@78000 {
 			compatible = "qcom,ipq8074-qmp-usb3-phy";
 			reg = <0x00078000 0x1c4>;
-			#clock-cells = <1>;
 			#address-cells = <1>;
 			#size-cells = <1>;
 			ranges;
@@ -155,6 +154,7 @@
 				      <0x00078800 0x1f8>,     /* PCS  */
 				      <0x00078600 0x044>;     /* PCS misc*/
 				#phy-cells = <0>;
+				#clock-cells = <1>;
 				clocks = <&gcc GCC_USB0_PIPE_CLK>;
 				clock-names = "pipe0";
 				clock-output-names = "usb3phy_0_cc_pipe_clk";
