// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/* Copyright (c) 2020, Robert Marko <robimarko@gmail.com> */

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	memory {
		device_type = "memory";
		reg = <0x80000000 0x08000000>;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	aliases {
		led-boot = &led_user;
		led-failsafe = &led_user;
		led-running = &led_user;
		led-upgrade = &led_user;
	};

	soc {
		counter@4a1000 {
			compatible = "qcom,qca-gcnt";
			reg = <0x4a1000 0x4>;
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 63 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		power {
			label = "blue:power";
			gpios = <&tlmm 0 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};

		led_user: user {
			label = "green:user";
			gpios = <&tlmm 3 GPIO_ACTIVE_HIGH>;
			panic-indicator;
		};
	};
};

&prng {
	status = "okay";
};

&tlmm {
	serial_pins: serial_pinmux {
		mux {
			pins = "gpio60", "gpio61";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	spi_0_pins: spi_0_pinmux {
		pin {
			function = "blsp_spi0";
			pins = "gpio55", "gpio56", "gpio57";
			drive-strength = <2>;
			bias-disable;
		};
		pin_cs {
			function = "gpio";
			pins = "gpio54";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&blsp1_spi1 {
	status = "okay";

	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	cs-gpios = <&tlmm 54 GPIO_ACTIVE_HIGH>;

	flash@0 {
		reg = <0>;
		compatible = "jedec,spi-nor";
		spi-max-frequency = <40000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "Qualcomm";
				reg = <0x0 0x80000>;
				read-only;
			};

			partition@80000 {
				compatible = "mikrotik,routerboot-partitions";
				#address-cells = <1>;
				#size-cells = <1>;
				label = "RouterBoot";
				reg = <0x80000 0x80000>;

				hard_config {
					read-only;
					size = <0x2000>;
				};

				dtb_config {
					read-only;
				};

				soft_config {
				};
			};

			partition@100000 {
				compatible = "mikrotik,minor";
				label = "firmware";
				reg = <0x100000 0xf00000>;
			};
		};
	};
};

&blsp1_uart1 {
	status = "okay";

	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
};

&cryptobam {
	status = "okay";
};

&crypto {
	status = "okay";
};

&watchdog {
	status = "okay";
};

&mdio {
	status = "okay";
};

&gmac {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport4 {
	status = "okay";
	label = "sw-eth2";
};

&swport5 {
	status = "okay";
	label = "sw-eth1";
};

&wifi0 {
	status = "okay";

	qcom,ath10k-calibration-variant = "MikroTik-wAP-ac";
};

&wifi1 {
	status = "okay";

	qcom,ath10k-calibration-variant = "MikroTik-wAP-ac";
};
