From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Fri, 20 May 2022 20:11:32 +0200
Subject: [PATCH] net: ethernet: mtk_eth_soc: add rxd_size to mtk_soc_data

Similar to tx counterpart, introduce rxd_size in mtk_soc_data data
structure.
This is a preliminary patch to add mt7986 ethernet support.

Tested-by: Sam Shih <sam.shih@mediatek.com>
Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Signed-off-by: David S. Miller <davem@davemloft.net>
---

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -1776,7 +1776,7 @@ static int mtk_rx_alloc(struct mtk_eth *
 	}
 
 	ring->dma = dma_alloc_coherent(eth->dma_dev,
-				       rx_dma_size * sizeof(*ring->dma),
+				       rx_dma_size * eth->soc->txrx.rxd_size,
 				       &ring->phys, GFP_KERNEL);
 	if (!ring->dma)
 		return -ENOMEM;
@@ -1834,9 +1834,8 @@ static void mtk_rx_clean(struct mtk_eth
 
 	if (ring->dma) {
 		dma_free_coherent(eth->dma_dev,
-				  ring->dma_size * sizeof(*ring->dma),
-				  ring->dma,
-				  ring->phys);
+				  ring->dma_size * eth->soc->txrx.rxd_size,
+				  ring->dma, ring->phys);
 		ring->dma = NULL;
 	}
 }
@@ -3406,6 +3405,7 @@ static const struct mtk_soc_data mt2701_
 	.required_pctl = true,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma),
+		.rxd_size = sizeof(struct mtk_rx_dma),
 	},
 };
 
@@ -3417,6 +3417,7 @@ static const struct mtk_soc_data mt7621_
 	.offload_version = 2,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma),
+		.rxd_size = sizeof(struct mtk_rx_dma),
 	},
 };
 
@@ -3429,6 +3430,7 @@ static const struct mtk_soc_data mt7622_
 	.offload_version = 2,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma),
+		.rxd_size = sizeof(struct mtk_rx_dma),
 	},
 };
 
@@ -3440,6 +3442,7 @@ static const struct mtk_soc_data mt7623_
 	.offload_version = 2,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma),
+		.rxd_size = sizeof(struct mtk_rx_dma),
 	},
 };
 
@@ -3451,6 +3454,7 @@ static const struct mtk_soc_data mt7629_
 	.required_pctl = false,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma),
+		.rxd_size = sizeof(struct mtk_rx_dma),
 	},
 };
 
@@ -3461,6 +3465,7 @@ static const struct mtk_soc_data rt5350_
 	.required_pctl = false,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma),
+		.rxd_size = sizeof(struct mtk_rx_dma),
 	},
 };
 
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.h
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.h
@@ -865,6 +865,7 @@ struct mtk_tx_dma_desc_info {
  * @required_pctl		A bool value to show whether the SoC requires
  *				the extra setup for those pins used by GMAC.
  * @txd_size			Tx DMA descriptor size.
+ * @rxd_size			Rx DMA descriptor size.
  */
 struct mtk_soc_data {
 	u32             ana_rgc3;
@@ -875,6 +876,7 @@ struct mtk_soc_data {
 	netdev_features_t hw_features;
 	struct {
 		u32	txd_size;
+		u32	rxd_size;
 	} txrx;
 };
 
