From eab6bb0994b806525fc5e362e8b865f61c4a9e20 Mon Sep 17 00:00:00 2001
From: William Zhang <william.zhang@broadcom.com>
Date: Thu, 9 Jun 2022 17:15:33 -0700
Subject: [PATCH] arm64: dts: Add DTS files for bcmbca SoC BCM6813

Add DTS for ARMv8 based broadband SoC BCM6813. bcm6813.dtsi is the
SoC description DTS header and bcm96813.dts is a simple DTS file for
Broadcom BCM96813 Reference board that only enable the UART port.

Signed-off-by: William Zhang <william.zhang@broadcom.com>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm64/boot/dts/broadcom/bcmbca/Makefile  |   3 +-
 .../boot/dts/broadcom/bcmbca/bcm6813.dtsi     | 128 ++++++++++++++++++
 .../boot/dts/broadcom/bcmbca/bcm96813.dts     |  30 ++++
 3 files changed, 160 insertions(+), 1 deletion(-)
 create mode 100644 arch/arm64/boot/dts/broadcom/bcmbca/bcm6813.dtsi
 create mode 100644 arch/arm64/boot/dts/broadcom/bcmbca/bcm96813.dts

--- a/arch/arm64/boot/dts/broadcom/bcmbca/Makefile
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/Makefile
@@ -9,4 +9,5 @@ dtb-$(CONFIG_ARCH_BCMBCA) += \
 				bcm963158.dtb \
 				bcm96858.dtb \
 				bcm963146.dtb \
-				bcm96856.dtb
+				bcm96856.dtb \
+				bcm96813.dtb
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm6813.dtsi
@@ -0,0 +1,128 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Copyright 2022 Broadcom Ltd.
+ */
+
+#include <dt-bindings/interrupt-controller/irq.h>
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+
+/ {
+	compatible = "brcm,bcm6813", "brcm,bcmbca";
+	#address-cells = <2>;
+	#size-cells = <2>;
+
+	interrupt-parent = <&gic>;
+
+	cpus {
+		#address-cells = <2>;
+		#size-cells = <0>;
+
+		B53_0: cpu@0 {
+			compatible = "brcm,brahma-b53";
+			device_type = "cpu";
+			reg = <0x0 0x0>;
+			next-level-cache = <&L2_0>;
+			enable-method = "psci";
+		};
+
+		B53_1: cpu@1 {
+			compatible = "brcm,brahma-b53";
+			device_type = "cpu";
+			reg = <0x0 0x1>;
+			next-level-cache = <&L2_0>;
+			enable-method = "psci";
+		};
+
+		B53_2: cpu@2 {
+			compatible = "brcm,brahma-b53";
+			device_type = "cpu";
+			reg = <0x0 0x2>;
+			next-level-cache = <&L2_0>;
+			enable-method = "psci";
+		};
+
+		B53_3: cpu@3 {
+			compatible = "brcm,brahma-b53";
+			device_type = "cpu";
+			reg = <0x0 0x3>;
+			next-level-cache = <&L2_0>;
+			enable-method = "psci";
+		};
+
+		L2_0: l2-cache0 {
+			compatible = "cache";
+		};
+	};
+
+	timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			<GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			<GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			<GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
+	};
+
+	pmu: pmu {
+		compatible = "arm,cortex-a53-pmu";
+		interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>,
+			<GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>,
+			<GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>,
+			<GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-affinity = <&B53_0>, <&B53_1>,
+			<&B53_2>, <&B53_3>;
+	};
+
+	clocks: clocks {
+		periph_clk: periph-clk {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <200000000>;
+		};
+		uart_clk: uart-clk {
+			compatible = "fixed-factor-clock";
+			#clock-cells = <0>;
+			clocks = <&periph_clk>;
+			clock-div = <4>;
+			clock-mult = <1>;
+		};
+	};
+
+	psci {
+		compatible = "arm,psci-0.2";
+		method = "smc";
+	};
+
+	axi@81000000 {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges = <0x0 0x0 0x81000000 0x8000>;
+
+		gic: interrupt-controller@1000 {
+			compatible = "arm,gic-400";
+			#interrupt-cells = <3>;
+			interrupt-controller;
+			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
+			reg = <0x1000 0x1000>,
+				<0x2000 0x2000>,
+				<0x4000 0x2000>,
+				<0x6000 0x2000>;
+		};
+	};
+
+	bus@ff800000 {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges = <0x0 0x0 0xff800000 0x800000>;
+
+		uart0: serial@12000 {
+			compatible = "arm,pl011", "arm,primecell";
+			reg = <0x12000 0x1000>;
+			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&uart_clk>, <&uart_clk>;
+			clock-names = "uartclk", "apb_pclk";
+			status = "disabled";
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm96813.dts
@@ -0,0 +1,30 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Copyright 2022 Broadcom Ltd.
+ */
+
+/dts-v1/;
+
+#include "bcm6813.dtsi"
+
+/ {
+	model = "Broadcom BCM96813 Reference Board";
+	compatible = "brcm,bcm96813", "brcm,bcm6813", "brcm,bcmbca";
+
+	aliases {
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	memory@0 {
+		device_type = "memory";
+		reg = <0x0 0x0 0x0 0x08000000>;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
