## 
## This file is part of the coreboot project.
## 
## Copyright (C) 2007 AMD
## (Written by Yinghai Lu <yinghailu@amd.com> for AMD)
## Copyright (C) 2007 Rudolf Marek <r.marek@assembler.cz>
## 
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
## 
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
## 
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
## 

if USE_FALLBACK_IMAGE
  default ROM_SECTION_SIZE   = FALLBACK_SIZE
  default ROM_SECTION_OFFSET = ( ROM_SIZE - FALLBACK_SIZE )
else
  default ROM_SECTION_SIZE   = ( ROM_SIZE - FALLBACK_SIZE )
  default ROM_SECTION_OFFSET = 0
end

default PAYLOAD_SIZE             = ( ROM_SECTION_SIZE - ROM_IMAGE_SIZE )
default CONFIG_ROM_PAYLOAD_START = (0xffffffff - ROM_SIZE + ROM_SECTION_OFFSET + 1)
default CONFIG_ROM_PAYLOAD       = 1
default _ROMBASE     = (CONFIG_ROM_PAYLOAD_START + PAYLOAD_SIZE)
default XIP_ROM_SIZE = 65536
default XIP_ROM_BASE = (_ROMBASE + ROM_IMAGE_SIZE - XIP_ROM_SIZE)

arch i386 end 

driver mainboard.o
if HAVE_ACPI_TABLES
  object acpi_tables.o
  object fadt.o
  makerule dsdt.c
    depends "$(MAINBOARD)/dsdt.asl"
    action  "iasl -p $(PWD)/dsdt -tc $(MAINBOARD)/dsdt.asl"
    action  "mv dsdt.hex dsdt.c"
  end
  object ./dsdt.o
end
if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE object irq_tables.o end
# object reset.o

if USE_DCACHE_RAM
  if CONFIG_USE_INIT
    makerule ./cache_as_ram_auto.o
      depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
      action "$(CC) $(DISTRO_CFLAGS) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -o $@"
    end
  else
    makerule ./cache_as_ram_auto.inc
      depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
      action "$(CC) $(DISTRO_CFLAGS) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -S -o $@"
      action "perl -e 's/.rodata/.rom.data/g' -pi $@"
      action "perl -e 's/.text/.section .rom.text/g' -pi $@"
    end
  end
end

if USE_FALLBACK_IMAGE
  mainboardinit cpu/x86/16bit/entry16.inc
  ldscript /cpu/x86/16bit/entry16.lds
  mainboardinit southbridge/via/k8t890/romstrap.inc
  ldscript /southbridge/via/k8t890/romstrap.lds
end

mainboardinit cpu/x86/32bit/entry32.inc

if USE_DCACHE_RAM
  if CONFIG_USE_INIT
    ldscript /cpu/x86/32bit/entry32.lds
  end
  if CONFIG_USE_INIT
    ldscript /cpu/amd/car/cache_as_ram.lds
  end
end

if USE_FALLBACK_IMAGE
  mainboardinit cpu/x86/16bit/reset16.inc
  ldscript /cpu/x86/16bit/reset16.lds
else
  mainboardinit cpu/x86/32bit/reset32.inc
  ldscript /cpu/x86/32bit/reset32.lds
end

if USE_DCACHE_RAM
  mainboardinit cpu/amd/car/cache_as_ram.inc
end

if USE_FALLBACK_IMAGE
  if USE_DCACHE_RAM
    ldscript /arch/i386/lib/failover.lds
  end
end

if USE_DCACHE_RAM
  if CONFIG_USE_INIT
    initobject cache_as_ram_auto.o
  else
    mainboardinit ./cache_as_ram_auto.inc
  end
end

if CONFIG_CHIP_NAME
  config chip.h
end

chip northbridge/amd/amdk8/root_complex		# Root complex
  device apic_cluster 0 on			# APIC cluster
    chip cpu/amd/socket_939			# CPU
      device apic 0 on end			# APIC
    end
  end
  device pci_domain 0 on			# PCI domain
    chip northbridge/amd/amdk8			# mc0
      device pci 18.0 on			# Northbridge
        # Devices on link 0, link 0 == LDT 0
        chip southbridge/via/vt8237r		# Southbridge
          register "ide0_enable" = "1"		# Enable IDE channel 0
          register "ide1_enable" = "1"		# Enable IDE channel 1
          register "ide0_80pin_cable" = "1"	# 80pin cable on IDE channel 0
          register "ide1_80pin_cable" = "1"	# 80pin cable on IDE channel 1
          register "fn_ctrl_lo" = "0"		# Enable SB functions
          register "fn_ctrl_hi" = "0xad"	# Enable SB functions
          device pci 0.0 on end			# HT
          device pci f.1 on end			# IDE
          device pci 11.0 on			# LPC
            chip drivers/generic/generic	# DIMM 0-0-0
              device i2c 50 on end
            end
            chip drivers/generic/generic	# DIMM 0-0-1
              device i2c 51 on end
            end
            chip drivers/generic/generic	# DIMM 0-1-0
              device i2c 52 on end
            end
            chip drivers/generic/generic	# DIMM 0-1-1
              device i2c 53 on end
            end
            chip superio/winbond/w83627ehg	# Super I/O
              device pnp 2e.0 on		# Floppy
                io 0x60 = 0x3f0
                irq 0x70 = 6
                drq 0x74 = 2
              end
              device pnp 2e.1 on		# Parallel port
                io 0x60 = 0x378
                irq 0x70 = 7
                drq 0x74 = 3
              end
              device pnp 2e.2 on		# Com1
                io 0x60 = 0x3f8
                irq 0x70 = 4
              end
              device pnp 2e.3 off		# Com2 (N/A on this board)
                io 0x60 = 0x2f8
                irq 0x70 = 3
              end
              device pnp 2e.5 off		# PS/2 keyboard (off)
              end
              device pnp 2e.106 off		# Serial flash
                io 0x60 = 0x100
              end
              device pnp 2e.007 off		# GPIO 1
              end
              device pnp 2e.107 on		# Game port
                io 0x60 = 0x201
              end
              device pnp 2e.207 on		# MIDI
                io 0x62 = 0x330
                irq 0x70 = 0xa
              end
              device pnp 2e.307 off		# GPIO 6
              end
              device pnp 2e.8 off		# WDTO_PLED
              end
              device pnp 2e.009 on		# GPIO 2 on LDN 9 is in sio_setup
              end
              device pnp 2e.109 off		# GPIO 3
              end
              device pnp 2e.209 off		# GPIO 4
              end
              device pnp 2e.309 on		# GPIO5
              end
              device pnp 2e.a off		# ACPI
              end
              device pnp 2e.b on		# Hardware monitor
                io 0x60 = 0x290
                irq 0x70 = 0
              end
            end
          end
          device pci 12.0 off end		# VIA LAN (off, other chip used)
        end
        chip southbridge/via/k8t890		# "Southbridge" K8T890
        end
      end
      device pci 18.1 on end
      device pci 18.2 on end
      device pci 18.3 on end
    end
  end
end
