# NOTE: This file must be in UNIX format (not DOS) or build_opt_tbl fails: 
#		"Error - Name  is an invalid identifier in line"

entries

#start-bit length  config config-ID    name
0           512      r       0        reserved_memory1			# We know nothing about the factory BIOS
512         512      r       0        reserved_memory2			# More factory BIOS

# Work in progress.
# This is where we would put the LB RTC_BOOT_BYTE options once the code
# supports finding them there.
#1024         1       e       4        boot_option		
#1025         1       e       4        last_boot
#1026         1       e       1        ECC_memory
#1028         4       r       0        reboot_bits

# Options used by XE7501DevKit
#1032         3       e       5        baud_rate
#1035         1       e       2        hyper_threading
#1036         1       e       1        power_on_after_fail
#1037         1       e       1        nmi

#1040         4       e       6        debug_level

#1048        16       h       0        check_sum



enumerations

#ID value   text
1     0     Disable
1     1     Enable
2     0     Enable
2     1     Disable
4     0     Fallback
4     1     Normal
5     0     115200
5     1     57600
5     2     38400
5     3     19200
5     4     9600
5     5     4800
5     6     2400
5     7     1200
6     6     Notice
6     7     Info
6     8     Debug
6     9     Spew

checksums

# Checksum FROM bit-location TO bit-location STORE AT bit-location
#checksum 1024 1047 1048
