##
## Compute the location and size of where this firmware image
## (coreboot plus bootloader) will live in the boot rom chip.
##
if USE_FALLBACK_IMAGE
	default ROM_SECTION_SIZE   = FALLBACK_SIZE
	default ROM_SECTION_OFFSET = ( ROM_SIZE - FALLBACK_SIZE )
else
	default ROM_SECTION_SIZE   = ( ROM_SIZE - FALLBACK_SIZE )
	default ROM_SECTION_OFFSET = 0
end

##
## Compute the start location and size size of
## The coreboot bootloader.
##
default CONFIG_ROM_PAYLOAD_START = (0xffffffff - ROM_SIZE + ROM_SECTION_OFFSET + 1)
default PAYLOAD_SIZE            = ( ROM_SECTION_SIZE - ROM_IMAGE_SIZE )

##
## Compute where this copy of coreboot will start in the boot rom
##
default _ROMBASE      = ( CONFIG_ROM_PAYLOAD_START + PAYLOAD_SIZE )

##
## Compute a range of ROM that can cached to speed up coreboot,
## execution speed.
##
## XIP_ROM_SIZE must be a power of 2.
## XIP_ROM_BASE must be a multiple of XIP_ROM_SIZE
##
default XIP_ROM_SIZE=65536
default XIP_ROM_BASE = ( _ROMBASE + ROM_IMAGE_SIZE - XIP_ROM_SIZE )

##
## Set all of the defaults for an x86 architecture
##

arch i386 end

##
## Build the objects we have code for in this directory.
##

driver mainboard.o

if HAVE_PIRQ_TABLE object irq_tables.o end
#object reset.o

##
## Romcc output
##
makerule ./failover.E
	depends "$(MAINBOARD)/failover.c ./romcc" 
	action "./romcc -E -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./failover.inc
	depends "$(MAINBOARD)/failover.c ./romcc"
	action "./romcc    -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./auto.E 
	depends	"$(MAINBOARD)/auto.c option_table.h ./romcc" 
	action	"./romcc -E -mcpu=p2 -O -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end
makerule ./auto.inc 
	depends "$(MAINBOARD)/auto.c option_table.h ./romcc"
	action	"./romcc    -mcpu=p2 -O -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end

##
## Build our 16 bit and 32 bit coreboot entry code
##
mainboardinit cpu/x86/16bit/entry16.inc
mainboardinit cpu/x86/32bit/entry32.inc
ldscript /cpu/x86/16bit/entry16.lds
ldscript /cpu/x86/32bit/entry32.lds

##
## Build our reset vector (This is where coreboot is entered)
##
if USE_FALLBACK_IMAGE 
	mainboardinit cpu/x86/16bit/reset16.inc 
	ldscript /cpu/x86/16bit/reset16.lds 
else
	mainboardinit cpu/x86/32bit/reset32.inc 
	ldscript /cpu/x86/32bit/reset32.lds 
end

### Should this be in the northbridge code?
mainboardinit arch/i386/lib/cpu_reset.inc

##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

###
### This is the early phase of coreboot startup 
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
	ldscript /arch/i386/lib/failover.lds 
	mainboardinit ./failover.inc
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
mainboardinit cpu/x86/fpu/enable_fpu.inc
mainboardinit cpu/x86/mmx/enable_mmx.inc
mainboardinit ./auto.inc
mainboardinit cpu/x86/mmx/disable_mmx.inc

##
## Include the secondary Configuration files 
##
dir /pc80
config chip.h

chip northbridge/intel/i82810
	device pci_domain 0 on 
		device pci 0.0 on end # Host bridge
		device pci 1.0 on # Onboard Video
			#chip drivers/pci/onboard
			#	device pci 1.0 on end
			#	register "rom_address" = "0xfff80000"
		        #end
		end
		chip southbridge/intel/i82801xx # Southbridge
			device pci 1e.0 on # PCI Bridge
				#chip drivers/pci/onboard
				#	device pci 1.0 on end
				#	register "rom_address" = "0xfff80000"
			        #end
			end
			device pci 1f.0 on  # ISA/LPC? Bridge
				chip superio/smsc/lpc47b272
					device pnp 2e.0 off # Floppy
						io 0x60 = 0x3f0
						irq 0x70 = 6
						drq 0x74 = 2
					end
					device pnp 2e.3 off # Parallel Port
						io 0x60 = 0x378
						irq 0x70 = 7
					end
					device pnp 2e.4 on # Com1
						io 0x60 = 0x3f8
						irq 0x70 = 4
					end
					device pnp 2e.5 off # Com2
						io 0x60 = 0x2f8
						irq 0x70 = 3
					end
					device pnp 2e.7 on # Keyboard
						io 0x60 = 0x60
						io 0x62 = 0x64
						irq 0x70 = 1 # Keyboard interrupt
						irq 0x72 = 12 # Mouse interrupt
					end
					device pnp 2e.a off end # ACPI
				end
			end
			device pci 1f.1 on end # IDE
			device pci 1f.2 on end # USB
			device pci 1f.3 on end # SMBus
			device pci 1f.5 off end # AC'97, no header on MEW-VM
			device pci 1f.6 off end # AC'97 Modem (MC'97)
		end
	end
	chip cpu/intel/socket_PGA370
	end
end

