##
## Compute the location and size of where this firmware image
## (coreboot plus bootloader) will live in the boot rom chip.
##
if USE_FALLBACK_IMAGE
	default ROM_SECTION_SIZE   = FALLBACK_SIZE
	default ROM_SECTION_OFFSET = ( ROM_SIZE - FALLBACK_SIZE )
else
	default ROM_SECTION_SIZE   = ( ROM_SIZE - FALLBACK_SIZE )
	default ROM_SECTION_OFFSET = 0
end

##
## Compute the start location and size size of
## The coreboot bootloader.
##
default PAYLOAD_SIZE            = ( ROM_SECTION_SIZE - ROM_IMAGE_SIZE )
default CONFIG_ROM_PAYLOAD_START = (0xffffffff - ROM_SIZE + ROM_SECTION_OFFSET + 1)

##
## Compute where this copy of coreboot will start in the boot rom
##
default _ROMBASE      = ( CONFIG_ROM_PAYLOAD_START + PAYLOAD_SIZE )

##
## Compute a range of ROM that can cached to speed up coreboot,
## execution speed.
##
## XIP_ROM_SIZE must be a power of 2.
## XIP_ROM_BASE must be a multiple of XIP_ROM_SIZE
##
default XIP_ROM_SIZE=65536
default XIP_ROM_BASE = ( _ROMBASE + ROM_IMAGE_SIZE - XIP_ROM_SIZE )

arch i386 end 

##
## Build the objects we have code for in this directory.
##

driver mainboard.o

#dir /drivers/si/3114

if HAVE_MP_TABLE object mptable.o end
if HAVE_PIRQ_TABLE object irq_tables.o end

if USE_DCACHE_RAM

if CONFIG_USE_INIT

makerule ./auto.o
        depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
        action "$(CC) $(DISTRO_CFLAGS) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -o auto.o" 
end

else    
                
makerule ./auto.inc
        depends "$(MAINBOARD)/cache_as_ram_auto.c option_table.h"
        action "$(CC) $(DISTRO_CFLAGS) -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/cache_as_ram_auto.c -Os -nostdinc -nostdlib -fno-builtin -Wall -c -S -o $@"         
        action "perl -e 's/.rodata/.rom.data/g' -pi $@"
        action "perl -e 's/.text/.section .rom.text/g' -pi $@"
end

end
else
  
##
## Romcc output
##
makerule ./failover.E
        depends "$(MAINBOARD)/failover.c ./romcc"
        action "./romcc -E -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./failover.inc
        depends "$(MAINBOARD)/failover.c ./romcc"
        action "./romcc    -O --label-prefix=failover -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/failover.c -o $@"
end

makerule ./auto.E
        depends "$(MAINBOARD)/auto.c option_table.h ./romcc"
        action  "./romcc -E -mcpu=k8 -O2 -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end
makerule ./auto.inc
        depends "$(MAINBOARD)/auto.c option_table.h ./romcc"
        action  "./romcc    -mcpu=k8 -O2 -I$(TOP)/src -I. $(CPPFLAGS) $(MAINBOARD)/auto.c -o $@"
end

end
##
## Build our 16 bit and 32 bit coreboot entry code
##
if USE_FALLBACK_IMAGE
        mainboardinit cpu/x86/16bit/entry16.inc
        ldscript /cpu/x86/16bit/entry16.lds
end

mainboardinit cpu/x86/32bit/entry32.inc

if USE_DCACHE_RAM
        if CONFIG_USE_INIT
                ldscript /cpu/x86/32bit/entry32.lds
        end

        if CONFIG_USE_INIT
                ldscript      /cpu/amd/car/cache_as_ram.lds
        end
end

##
## Build our reset vector (This is where coreboot is entered)
##
if USE_FALLBACK_IMAGE 
	mainboardinit cpu/x86/16bit/reset16.inc 
	ldscript /cpu/x86/16bit/reset16.lds 
else
	mainboardinit cpu/x86/32bit/reset32.inc 
	ldscript /cpu/x86/32bit/reset32.lds 
end

if USE_DCACHE_RAM
else
### Should this be in the northbridge code?
mainboardinit arch/i386/lib/cpu_reset.inc
end

##
## Include an id string (For safe flashing)
##
mainboardinit arch/i386/lib/id.inc
ldscript /arch/i386/lib/id.lds

if USE_DCACHE_RAM
##
## Setup Cache-As-Ram
##
mainboardinit cpu/amd/car/cache_as_ram.inc
end

###
### This is the early phase of coreboot startup 
### Things are delicate and we test to see if we should
### failover to another image.
###
if USE_FALLBACK_IMAGE
if USE_DCACHE_RAM
       ldscript /arch/i386/lib/failover.lds
else
       ldscript /arch/i386/lib/failover.lds
        mainboardinit ./failover.inc
end
end

###
### O.k. We aren't just an intermediary anymore!
###

##
## Setup RAM
##
if USE_DCACHE_RAM

if CONFIG_USE_INIT
initobject auto.o
else
mainboardinit ./auto.inc
end

else

##
## Setup RAM
##
mainboardinit cpu/x86/fpu/enable_fpu.inc
mainboardinit cpu/x86/mmx/enable_mmx.inc
mainboardinit cpu/x86/sse/enable_sse.inc
mainboardinit ./auto.inc
mainboardinit cpu/x86/sse/disable_sse.inc
mainboardinit cpu/x86/mmx/disable_mmx.inc

end

##
## Include the secondary Configuration files 
##
if CONFIG_CHIP_NAME
	config chip.h
end

# sample config for tyan/s2875
chip northbridge/amd/amdk8/root_complex
        device apic_cluster 0 on
                chip cpu/amd/socket_940
                        device apic 0 on end
                end
        end
	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on #  northbridge 
				#  devices on link 0, link 0 == LDT 0
				chip southbridge/amd/amd8151
					# the on/off keyword is mandatory
					device pci 0.0 on end
					device pci 1.0 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 off end
						device pci 1.0 off end
                                                chip drivers/pci/onboard
                                                        device pci 5.0 on end
                                                        register "rom_address" = "0xfff80000"
                                                end
					end
					device pci 1.0 on
						chip superio/winbond/w83627hf
							device pnp 2e.0 on #  Floppy
								io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off #  Parallel Port
								io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 on #  Com1
								io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.3 off #  Com2
								io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.5 on #  Keyboard
								io 0x60 = 0x60
								io 0x62 = 0x64
								irq 0x70 = 1
								irq 0x72 = 12
							end
							device pnp 2e.6 off #  CIR
								io 0x60 = 0x100
							end
							device pnp 2e.7 off #  GAME_MIDI_GIPO1
								io 0x60 = 0x220
								io 0x62 = 0x300
								irq 0x70 = 9
							end  
							device pnp 2e.8 off end #  GPIO2
							device pnp 2e.9 off end #  GPIO3
							device pnp 2e.a off end #  ACPI
							device pnp 2e.b on #  HW Monitor
								io 0x60 = 0x290
								irq 0x70 = 5
							end
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.5 on end
					device pci 1.6 off end
                                        register "ide0_enable" = "1"
                                        register "ide1_enable" = "1"
				end
			end #  device pci 18.0 
			
			device pci 18.0 on end
			device pci 18.0 on end
			
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
	end 
end

