##
## This file is part of the coreboot project.
##
## Copyright (C) 2007 Juergen Beisert <juergen@kreuzholzen.de>
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
##

uses HAVE_MP_TABLE
uses HAVE_PIRQ_TABLE
uses USE_FALLBACK_IMAGE
uses HAVE_FALLBACK_BOOT
uses HAVE_HARD_RESET
uses HAVE_OPTION_TABLE
uses USE_OPTION_TABLE
uses CONFIG_ROM_PAYLOAD
uses IRQ_SLOT_COUNT
uses MAINBOARD
uses MAINBOARD_VENDOR
uses MAINBOARD_PART_NUMBER
uses COREBOOT_EXTRA_VERSION
uses ARCH
uses FALLBACK_SIZE
uses STACK_SIZE
uses HEAP_SIZE
uses ROM_SIZE
uses ROM_SECTION_SIZE
uses ROM_IMAGE_SIZE
uses ROM_SECTION_SIZE
uses ROM_SECTION_OFFSET
uses CONFIG_ROM_PAYLOAD_START
uses PAYLOAD_SIZE
uses _ROMBASE
uses _RAMBASE
uses XIP_ROM_SIZE
uses XIP_ROM_BASE
uses CROSS_COMPILE
uses CC
uses HOSTCC
uses OBJCOPY
uses DEFAULT_CONSOLE_LOGLEVEL
uses MAXIMUM_CONSOLE_LOGLEVEL
uses CONFIG_CONSOLE_SERIAL8250
uses TTYS0_BAUD
uses TTYS0_BASE
uses TTYS0_LCS
uses CONFIG_COMPRESSED_PAYLOAD_LZMA
uses CONFIG_UDELAY_TSC
uses CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2
uses CONFIG_VIDEO_MB
uses CONFIG_SPLASH_GRAPHIC
uses CONFIG_GX1_VIDEO
uses CONFIG_GX1_VIDEOMODE
uses PIRQ_ROUTE

## Enable VGA with a splash screen (only 640x480 to run on most monitors).
## We want to support up to 1024x768@16 so we need 2MiB video memory.
## Note: Higher resolutions might need faster SDRAM speed.
default CONFIG_GX1_VIDEO = 1
default CONFIG_GX1_VIDEOMODE = 0
default CONFIG_SPLASH_GRAPHIC = 1
default CONFIG_VIDEO_MB = 2

default ROM_SIZE = 256 * 1024
default MAINBOARD_VENDOR = "BCOM"
default MAINBOARD_PART_NUMBER = "WinNET100"
default HAVE_FALLBACK_BOOT = 1
default HAVE_MP_TABLE = 0
default HAVE_HARD_RESET = 0
default CONFIG_UDELAY_TSC = 1
default CONFIG_TSC_X86RDTSC_CALIBRATE_WITH_TIMER2 = 1
default HAVE_PIRQ_TABLE = 1
default IRQ_SLOT_COUNT = 2	# Soldered NIC, internal USB, no real slots
default PIRQ_ROUTE = 1
default HAVE_OPTION_TABLE = 0
default ROM_IMAGE_SIZE = 64 * 1024
default FALLBACK_SIZE = 128 * 1024
default STACK_SIZE = 8 * 1024
default HEAP_SIZE = 16 * 1024
default USE_OPTION_TABLE = 0
default _RAMBASE = 0x00004000
default CONFIG_ROM_PAYLOAD = 1
default CROSS_COMPILE = ""
default CC = "$(CROSS_COMPILE)gcc "
default HOSTCC = "gcc"
default CONFIG_CONSOLE_SERIAL8250 = 1
default TTYS0_BAUD = 115200
default TTYS0_BASE = 0x3f8
default TTYS0_LCS = 0x3		# 8n1
default DEFAULT_CONSOLE_LOGLEVEL = 6
default MAXIMUM_CONSOLE_LOGLEVEL = 6

end
