00570{"daemon_event_id":1,"daemon_event_name":"init","thread_id":0,"packet_id":0,"source":"cfgs\/default\/pcap\/profinet-io-le.pcap","alias":"nDPId-test","version":"1.6.0","ndpi_version":"4.11.0-4834-92507c0","max-flows-per-thread":2048,"max-idle-flows-per-thread":64,"reader-thread-count":1,"flow-scan-interval":10000000,"generic-max-idle-time":600000000,"icmp-max-idle-time":120000000,"udp-max-idle-time":180000000,"tcp-max-idle-time":7560000000,"max-packets-per-flow-to-send":5,"max-packets-per-flow-to-process":32,"max-packets-per-flow-to-analyse":32,"global_ts_usec":0}
00794{"daemon_event_id":4,"daemon_event_name":"status","thread_id":0,"packet_id":1,"source":"cfgs\/default\/pcap\/profinet-io-le.pcap","alias":"nDPId-test","version":"1.6.0","ndpi_version":"4.11.0-4834-92507c0","packets-captured":1,"packets-processed":0,"pfring_active":false,"pfring_recv":0,"pfring_drop":0,"pfring_shunt":0,"total-skipped-flows":0,"total-l4-payload-len":0,"total-not-detected-flows":0,"total-guessed-flows":0,"total-detected-flows":0,"total-detection-updates":0,"total-updates":0,"current-active-flows":0,"total-active-flows":0,"total-idle-flows":0,"total-compressions":0,"total-compression-diff":0,"current-compression-diff":0,"global-alloc-count":0,"global-free-count":0,"global-alloc-bytes":0,"global-free-bytes":0,"total-events-serialized":2,"global_ts_usec":1287088627587076}
00783{"flow_event_id":1,"flow_event_name":"new","thread_id":0,"packet_id":1,"source":"cfgs\/default\/pcap\/profinet-io-le.pcap","alias":"nDPId-test","flow_id":1,"flow_state":"info","flow_src_packets_processed":1,"flow_dst_packets_processed":0,"flow_first_seen":1287088627587076,"flow_src_last_pkt_time":1287088627587076,"flow_dst_last_pkt_time":1287088627587076,"flow_idle_time":200000000,"flow_src_min_l4_payload_len":164,"flow_dst_min_l4_payload_len":0,"flow_src_max_l4_payload_len":164,"flow_dst_max_l4_payload_len":0,"flow_src_tot_l4_payload_len":164,"flow_dst_tot_l4_payload_len":0,"midstream":0,"thread_ts_usec":1287088627587076,"l3_proto":"ip4","src_ip":"10.10.0.150","dst_ip":"10.10.0.129","src_port":1566,"dst_port":34964,"l4_proto":"udp","flow_datalink":1,"flow_max_packets":5}
00741{"packet_event_id":2,"packet_event_name":"packet-flow","thread_id":0,"packet_id":1,"source":"cfgs\/default\/pcap\/profinet-io-le.pcap","alias":"nDPId-test","flow_id":1,"flow_packet_id":1,"flow_src_last_pkt_time":1287088627587076,"flow_dst_last_pkt_time":1287088627587076,"flow_idle_time":200000000,"pkt_datalink":1,"pkt_caplen":206,"pkt_type":2048,"pkt_l3_offset":14,"pkt_l4_offset":34,"pkt_len":206,"pkt_l4_len":172,"thread_ts_usec":1287088627587076,"pkt":"AAmRRCAXAJAnTuP8CABFAADAsogAAIARcnoKCgCWCgoAgQYeiJQArGiVBAAIABAAAAAAAKDel2zREYJxAAEAAwFaAQCg3pds0RGCcQCgJELffduruuwdAFRDslALAWMKuv0AAAAAAQAAAAAAAAAFAP\/\/\/\/9UAAAAAABAgAAAQAAAAECAAAAAAAAAQAAAAAAJADwBAAAKAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAABAAD4QAAAgAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA="}
01085{"flow_event_id":7,"flow_event_name":"detected","thread_id":0,"packet_id":1,"source":"cfgs\/default\/pcap\/profinet-io-le.pcap","alias":"nDPId-test","flow_id":1,"flow_state":"info","flow_src_packets_processed":1,"flow_dst_packets_processed":0,"flow_first_seen":1287088627587076,"flow_src_last_pkt_time":1287088627587076,"flow_dst_last_pkt_time":1287088627587076,"flow_idle_time":200000000,"flow_src_min_l4_payload_len":164,"flow_dst_min_l4_payload_len":0,"flow_src_max_l4_payload_len":164,"flow_dst_max_l4_payload_len":0,"flow_src_tot_l4_payload_len":164,"flow_dst_tot_l4_payload_len":0,"midstream":0,"thread_ts_usec":1287088627587076,"l3_proto":"ip4","src_ip":"10.10.0.150","dst_ip":"10.10.0.129","src_port":1566,"dst_port":34964,"l4_proto":"udp","ndpi": {"flow_risk": {"5": {"risk":"Known Proto on Non Std Port","severity":"Medium","risk_score": {"total":160,"client":140,"server":20}}},"confidence": {"6":"DPI"},"proto":"DCERPC.PROFINET_IO","proto_id":"370.371","proto_by_ip":"Unknown","proto_by_ip_id":0,"encrypted":0,"breed":"Acceptable","category_id":31,"category":"IoT-Scada"}}
00891{"packet_event_id":2,"packet_event_name":"packet-flow","thread_id":0,"packet_id":2,"source":"cfgs\/default\/pcap\/profinet-io-le.pcap","alias":"nDPId-test","flow_id":1,"flow_packet_id":2,"flow_src_last_pkt_time":1287088627587076,"flow_dst_last_pkt_time":1287088627589136,"flow_idle_time":200000000,"pkt_datalink":1,"pkt_caplen":310,"pkt_type":2048,"pkt_l3_offset":14,"pkt_l4_offset":34,"pkt_len":310,"pkt_l4_len":276,"thread_ts_usec":1287088627589136,"pkt":"AJAnTuP8AAmRRCAXCABFAAEoAAwAAEARZI8KCgCBCgoAloiUBh4BFETGBAIoABAAAAAAAKDel2zREYJxAAEAAwFaAQCg3pds0RGCcQCgJELffduruuwdAFRDslALAWMKuv0BAAAAAQAAAAAAAAAFAP\/\/\/\/+8AAAAAAAAAAAAqAAAAECAAAAAAAAAqAAAAIAJADwBAAAKAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAABAAD4QAAAAGgAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAMAAsAQAAAQAAAAAAAgAAAAAAAQACAAEAAAABAAP\/\/wEKAAH\/\/4FAAAEAAf\/\/gUAAMQAYAQAAAQAAAAAAAQAB\/\/+BQAABAAH\/\/4FAADIAGAEAAAEAAAAAAAEAAAAAAAEAAQABAAAAAQ=="}
01128{"flow_event_id":3,"flow_event_name":"idle","thread_id":0,"packet_id":2,"source":"cfgs\/default\/pcap\/profinet-io-le.pcap","alias":"nDPId-test","flow_id":1,"flow_state":"finished","flow_src_packets_processed":1,"flow_dst_packets_processed":1,"flow_first_seen":1287088627587076,"flow_src_last_pkt_time":1287088627587076,"flow_dst_last_pkt_time":1287088627589136,"flow_idle_time":200000000,"flow_src_min_l4_payload_len":164,"flow_dst_min_l4_payload_len":0,"flow_src_max_l4_payload_len":164,"flow_dst_max_l4_payload_len":268,"flow_src_tot_l4_payload_len":164,"flow_dst_tot_l4_payload_len":268,"midstream":0,"thread_ts_usec":1287088627589136,"l3_proto":"ip4","src_ip":"10.10.0.150","dst_ip":"10.10.0.129","src_port":1566,"dst_port":34964,"l4_proto":"udp","flow_datalink":1,"flow_max_packets":5,"ndpi": {"flow_risk": {"5": {"risk":"Known Proto on Non Std Port","severity":"Medium","risk_score": {"total":160,"client":140,"server":20}}},"confidence": {"6":"DPI"},"proto":"DCERPC.PROFINET_IO","proto_id":"370.371","proto_by_ip":"Unknown","proto_by_ip_id":0,"encrypted":0,"breed":"Acceptable","category_id":31,"category":"IoT-Scada"}}
00798{"daemon_event_id":3,"daemon_event_name":"shutdown","thread_id":0,"packet_id":2,"source":"cfgs\/default\/pcap\/profinet-io-le.pcap","alias":"nDPId-test","version":"1.6.0","ndpi_version":"4.11.0-4834-92507c0","packets-captured":2,"packets-processed":2,"pfring_active":false,"pfring_recv":0,"pfring_drop":0,"pfring_shunt":0,"total-skipped-flows":0,"total-l4-payload-len":432,"total-not-detected-flows":0,"total-guessed-flows":0,"total-detected-flows":1,"total-detection-updates":0,"total-updates":0,"current-active-flows":0,"total-active-flows":1,"total-idle-flows":1,"total-compressions":0,"total-compression-diff":0,"current-compression-diff":0,"global-alloc-count":0,"global-free-count":0,"global-alloc-bytes":0,"global-free-bytes":0,"total-events-serialized":8,"global_ts_usec":1287088627589136}
~~~~~~~~~~~~~~~~~~~~ SUMMARY ~~~~~~~~~~~~~~~~~~~~
~~ packets captured/processed: 2/2
~~ skipped flows.............: 0
~~ total layer4 data length..: 432 bytes
~~ total detected protocols..: 1
~~ total active/idle flows...: 1/1
~~ total timeout flows.......: 0
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
~~ total memory allocated....: 6641357 bytes
~~ total memory freed........: 6641357 bytes
~~ total allocations/frees...: 114021/114021
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
~~ json message min len.......: 575 chars
~~ json message max len.......: 1133 chars
~~ json message avg len.......: 836 chars
