Power mode is set to True
=> it can be modified in eqpt_config.json - Span

There are 6 fiber spans over 500 km between trx_Stockholm and trx_Gothenburg

Now propagating between trx_Stockholm and trx_Gothenburg:
Reference used for design: (Input optical power reference in span = 2.00dBm,
                            spacing = 50.00GHz
                            nb_channels = 96)

Channels propagating: (Input optical power deviation in span = 0.00dB,
                       spacing = 50.00GHz,
                       transceiver output power = 2.00dBm,
                       nb_channels = 96)
Input optical power reference in span = [1;36;40m2.00 dBm[0m:
Transceiver trx_Stockholm
  GSNR (0.1nm, dB):          35.00
  GSNR (signal bw, dB):      30.98
  OSNR ASE (0.1nm, dB):      35.00
  OSNR ASE (signal bw, dB):  30.98
  CD (ps/nm):                0.00
  PMD (ps):                  0.00
  PDL (dB):                  0.00
  Latency (ms):              0.00
  Actual pch out (dBm):      2.00
Roadm roadm_Stockholm
  Type_variety:            default
  Reference loss (dB):     22.00
  Actual loss (dB):        22.00
  Reference pch out (dBm): -20.00
  Actual pch out (dBm):    -20.00
Edfa Edfa_booster_roadm_Stockholm_to_fiber (Stockholm → Norrköping)_(1/2)
  type_variety:           openroadm_mw_mw_booster
  effective gain(dB):     22.00
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      -inf
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        21.82
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.00
  output VOA (dB):        0.00
Fiber          fiber (Stockholm → Norrköping)_(1/2)
  type_variety:                SSMF
  length (km):                 81.63
  pad att_in (dB):             0.00
  total loss (dB):             16.33
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -14.33
  actual pch out (dBm):        -14.31
Edfa Edfa_fiber (Stockholm → Norrköping)_(1/2)
  type_variety:           openroadm_ila_low_noise
  effective gain(dB):     16.33
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      8.01
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         5.51
  Power Out (dBm):        21.84
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.01
  output VOA (dB):        0.00
Fiber          fiber (Stockholm → Norrköping)_(2/2)
  type_variety:                SSMF
  length (km):                 81.63
  pad att_in (dB):             0.00
  total loss (dB):             16.33
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -14.33
  actual pch out (dBm):        -14.30
Edfa Edfa_preamp_roadm_Norrköping_from_fiber (Stockholm → Norrköping)_(2/2)
  type_variety:           openroadm_mw_mw_preamp
  effective gain(dB):     16.33
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      12.59
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         5.52
  Power Out (dBm):        21.86
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.03
  output VOA (dB):        0.00
Roadm roadm_Norrköping
  Type_variety:            default
  Reference loss (dB):     22.00
  Actual loss (dB):        22.03
  Reference pch out (dBm): -20.00
  Actual pch out (dBm):    -20.00
Edfa Edfa_booster_roadm_Norrköping_to_fiber (Norrköping → Linköping)
  type_variety:           openroadm_mw_mw_booster
  effective gain(dB):     22.00
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      -inf
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        21.82
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.00
  output VOA (dB):        0.00
Fiber          fiber (Norrköping → Linköping)
  type_variety:                SSMF
  length (km):                 45.99
  pad att_in (dB):             1.80
  total loss (dB):             11.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -9.00
  actual pch out (dBm):        -9.00
Edfa Edfa_preamp_roadm_Linköping_from_fiber (Norrköping → Linköping)
  type_variety:           openroadm_mw_mw_preamp
  effective gain(dB):     11.00
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      16.00
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         10.83
  Power Out (dBm):        21.83
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.01
  output VOA (dB):        0.00
Roadm roadm_Linköping
  Type_variety:            default
  Reference loss (dB):     22.00
  Actual loss (dB):        22.01
  Reference pch out (dBm): -20.00
  Actual pch out (dBm):    -20.00
Edfa Edfa_booster_roadm_Linköping_to_fiber (Linköping → Jönköping)
  type_variety:           openroadm_mw_mw_booster
  effective gain(dB):     22.00
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      -inf
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        21.82
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.00
  output VOA (dB):        0.00
Fiber          fiber (Linköping → Jönköping)
  type_variety:                SSMF
  length (km):                 134.02
  pad att_in (dB):             0.00
  total loss (dB):             26.80
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -24.80
  actual pch out (dBm):        -24.79
Edfa Edfa_preamp_roadm_Jönköping_from_fiber (Linköping → Jönköping)
  type_variety:           openroadm_mw_mw_preamp
  effective gain(dB):     26.80
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      8.09
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -4.97
  Power Out (dBm):        21.87
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.05
  output VOA (dB):        0.00
Roadm roadm_Jönköping
  Type_variety:            default
  Reference loss (dB):     22.00
  Actual loss (dB):        22.05
  Reference pch out (dBm): -20.00
  Actual pch out (dBm):    -20.00
Edfa Edfa_booster_roadm_Jönköping_to_fiber (Jönköping → Borås)
  type_variety:           openroadm_mw_mw_booster
  effective gain(dB):     22.00
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      -inf
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        21.82
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.00
  output VOA (dB):        0.00
Fiber          fiber (Jönköping → Borås)
  type_variety:                SSMF
  length (km):                 89.12
  pad att_in (dB):             0.00
  total loss (dB):             17.82
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -15.82
  actual pch out (dBm):        -15.81
Edfa Edfa_preamp_roadm_Borås_from_fiber (Jönköping → Borås)
  type_variety:           openroadm_mw_mw_preamp
  effective gain(dB):     17.82
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      11.94
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         4.01
  Power Out (dBm):        21.84
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.02
  output VOA (dB):        0.00
Roadm roadm_Borås
  Type_variety:            default
  Reference loss (dB):     22.00
  Actual loss (dB):        22.02
  Reference pch out (dBm): -20.00
  Actual pch out (dBm):    -20.00
Edfa Edfa_booster_roadm_Borås_to_fiber (Borås → Gothenburg)
  type_variety:           openroadm_mw_mw_booster
  effective gain(dB):     22.00
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      -inf
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        21.82
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.00
  output VOA (dB):        0.00
Fiber          fiber (Borås → Gothenburg)
  type_variety:                SSMF
  length (km):                 67.64
  pad att_in (dB):             0.00
  total loss (dB):             13.53
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -11.53
  actual pch out (dBm):        -11.52
Edfa Edfa_preamp_roadm_Gothenburg_from_fiber (Borås → Gothenburg)
  type_variety:           openroadm_mw_mw_preamp
  effective gain(dB):     13.53
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      13.78
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         8.30
  Power Out (dBm):        21.84
  Delta_P (dB):           0.00
  target pch (dBm):       2.00
  actual pch out (dBm):   2.02
  output VOA (dB):        0.00
Roadm roadm_Gothenburg
  Type_variety:            default
  Reference loss (dB):     22.00
  Actual loss (dB):        22.02
  Reference pch out (dBm): -20.00
  Actual pch out (dBm):    -20.00
Transceiver trx_Gothenburg
  GSNR (0.1nm, dB):          18.89
  GSNR (signal bw, dB):      14.86
  OSNR ASE (0.1nm, dB):      21.20
  OSNR ASE (signal bw, dB):  17.18
  CD (ps/nm):                8350.42
  PMD (ps):                  7.99
  PDL (dB):                  3.74
  Latency (ms):              2.45
  Actual pch out (dBm):      2.00

Transmission result for input optical power reference in span = 2.00 dBm:
  Final GSNR (0.1 nm): [1;36;40m18.89 dB[0m

(No source node specified: picked trx_Stockholm)

(No destination node specified: picked trx_Gothenburg)
