Power mode is set to True
=> it can be modified in eqpt_config.json - Span

There are 3 fiber spans over 130 km between trx Lannion_CAS and trx Lorient_KMA

Now propagating between trx Lannion_CAS and trx Lorient_KMA:
Reference used for design: (Input optical power reference in span = 3.00dBm,
                            spacing = 50.00GHz
                            nb_channels = 96)

Channels propagating: (Input optical power deviation in span = 0.00dB,
                       spacing = 50.00GHz,
                       transceiver output power = 3.00dBm,
                       nb_channels = 96)
Input optical power reference in span = [1;36;40m3.00 dBm[0m:
Transceiver trx Lannion_CAS
  GSNR (0.1nm, dB):          100.00
  GSNR (signal bw, dB):      95.92
  OSNR ASE (0.1nm, dB):      100.00
  OSNR ASE (signal bw, dB):  95.92
  CD (ps/nm):                0.00
  PMD (ps):                  0.00
  PDL (dB):                  0.00
  Latency (ms):              0.00
  Actual pch out (dBm):      3.00
Roadm roadm Lannion_CAS
  Type_variety:            default
  Reference loss (dB):     23.00
  Actual loss (dB):        23.00
  Reference pch out (dBm): -20.00
  Actual pch out (dBm):    -20.00
Edfa east edfa in Lannion_CAS to Corlay
  type_variety:           test
  effective gain(dB):     21.18
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      6.13
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        21.01
  Delta_P (dB):           -1.82
  target pch (dBm):       1.18
  actual pch out (dBm):   1.18
  output VOA (dB):        0.00
Fiber          fiber (Lannion_CAS → Corlay)-F061
  type_variety:                SSMF
  length (km):                 20.00
  pad att_in (dB):             0.00
  total loss (dB):             4.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -2.82
  actual pch out (dBm):        -2.81
Fused west fused spans in Corlay
  loss (dB): 1.00
Fiber          fiber (Corlay → Loudeac)-F010
  type_variety:                SSMF
  length (km):                 50.00
  pad att_in (dB):             0.00
  total loss (dB):             10.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -13.82
  actual pch out (dBm):        -13.81
Fused west fused spans in Loudeac
  loss (dB): 1.00
Fiber          fiber (Loudeac → Lorient_KMA)-F054
  type_variety:                SSMF
  length (km):                 60.00
  pad att_in (dB):             0.00
  total loss (dB):             12.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -26.82
  actual pch out (dBm):        -26.81
Edfa west edfa in Lorient_KMA to Loudeac
  type_variety:           std_medium_gain
  effective gain(dB):     27.99
  (before att_in and before output VOA)
  tilt-target(dB)         0.00
  noise figure (dB):      5.98
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -6.99
  Power Out (dBm):        21.03
  Delta_P (dB):           -1.82
  target pch (dBm):       1.18
  actual pch out (dBm):   1.21
  output VOA (dB):        0.00
Roadm roadm Lorient_KMA
  Type_variety:            default
  Reference loss (dB):     21.18
  Actual loss (dB):        21.21
  Reference pch out (dBm): -20.00
  Actual pch out (dBm):    -20.00
Transceiver trx Lorient_KMA
  GSNR (0.1nm, dB):          23.77
  GSNR (signal bw, dB):      19.69
  OSNR ASE (0.1nm, dB):      24.11
  OSNR ASE (signal bw, dB):  20.03
  CD (ps/nm):                2171.00
  PMD (ps):                  0.46
  PDL (dB):                  0.00
  Latency (ms):              0.64
  Actual pch out (dBm):      3.00

Transmission result for input optical power reference in span = 3.00 dBm:
  Final GSNR (0.1 nm): [1;36;40m23.77 dB[0m

(Invalid source node 'lannion' replaced with trx Lannion_CAS)

(Invalid destination node 'lorient' replaced with trx Lorient_KMA)
