INFO     gnpy.tools.cli_examples:cli_examples.py Computing path requests service_pluggable.json into JSON format
WARNING  gnpy.tools.json_io:json_io.py 
	WARNING missing type_variety attribute in eqpt_config.json[Roadm]
	default value is type_variety = default

WARNING  gnpy.tools.json_io:json_io.py 
	Equipment file extra_eqpt_config.json: duplicate equipment entry found: Transceiver-ZR400G

INFO     gnpy.tools.worker_utils:worker_utils.py List of disjunctions:
[]
INFO     gnpy.tools.worker_utils:worker_utils.py Aggregating similar requests
INFO     gnpy.tools.worker_utils:worker_utils.py The following services have been requested:
[PathRequest 0
	source: 	trx Brest_KLA
	destination:	trx Lannion_CAS
	trx type:	ZR400G
	trx mode:	SFF-ID:70
	baud_rate:	60.13854679800001 Gbaud
	bit_rate:	400.0 Gb/s
	spacing:	100.0 GHz
	power:  	0.0 dBm
	tx_power_dbm:  	1.76 dBm
	nb channels: 	48
	path_bandwidth: 	400.0 Gbit/s
	nodes-list:	[]
	loose-list:	[]
]
INFO     gnpy.tools.worker_utils:worker_utils.py Propagating on selected path
INFO     gnpy.topology.request:request.py 
	request 0
	Computing path from trx Brest_KLA to trx Lannion_CAS
	with path constraint: ['trx Brest_KLA', 'trx Lannion_CAS']
	Computed path (roadms):['roadm Brest_KLA', 'roadm Lannion_CAS']
