[1;34;40mList of disjunctions[0m
[Disjunction 3
	relaxable:    false
	link-diverse: True
	node-diverse: True
	request-id-numbers: ['3', '1']
, Disjunction 4
	relaxable:    false
	link-diverse: True
	node-diverse: True
	request-id-numbers: ['4', '5']
]
[1;34;40mAggregating similar requests[0m
[1;34;40mThe following services have been requested:[0m
[PathRequest 0
	source: 	trx Lorient_KMA
	destination:	trx Vannes_KBE
	trx type:	Voyager
	trx mode:	None
	baud_rate:	None Gbaud
	bit_rate:	None Gb/s
	spacing:	50.0 GHz
	power:  	1.0 dBm
	nb channels: 	80
	path_bandwidth: 	100.0 Gbit/s
	nodes-list:	[]
	loose-list:	[]
, PathRequest 1
	source: 	trx Brest_KLA
	destination:	trx Vannes_KBE
	trx type:	Voyager
	trx mode:	mode 1
	baud_rate:	32.0 Gbaud
	bit_rate:	100.0 Gb/s
	spacing:	50.0 GHz
	power:  	1.0 dBm
	nb channels: 	95
	path_bandwidth: 	200.0 Gbit/s
	nodes-list:	['roadm Brest_KLA', 'roadm Lannion_CAS', 'roadm Lorient_KMA', 'roadm Vannes_KBE']
	loose-list:	['LOOSE', 'LOOSE', 'LOOSE', 'LOOSE']
, PathRequest 3
	source: 	trx Lannion_CAS
	destination:	trx Rennes_STA
	trx type:	vendorA_trx-type1
	trx mode:	mode 1
	baud_rate:	32.0 Gbaud
	bit_rate:	100.0 Gb/s
	spacing:	50.0 GHz
	power:  	0.0 dBm
	nb channels: 	95
	path_bandwidth: 	60.0 Gbit/s
	nodes-list:	[]
	loose-list:	[]
, PathRequest 4
	source: 	trx Rennes_STA
	destination:	trx Lannion_CAS
	trx type:	vendorA_trx-type1
	trx mode:	None
	baud_rate:	None Gbaud
	bit_rate:	None Gb/s
	spacing:	75.0 GHz
	power:  	3.0 dBm
	nb channels: 	63
	path_bandwidth: 	150.0 Gbit/s
	nodes-list:	[]
	loose-list:	[]
, PathRequest 5
	source: 	trx Rennes_STA
	destination:	trx Lannion_CAS
	trx type:	vendorA_trx-type1
	trx mode:	mode 2
	baud_rate:	66.0 Gbaud
	bit_rate:	200.0 Gb/s
	spacing:	75.0 GHz
	power:  	3.0 dBm
	nb channels: 	63
	path_bandwidth: 	20.0 Gbit/s
	nodes-list:	[]
	loose-list:	[]
, PathRequest 7 | 6
	source: 	trx Lannion_CAS
	destination:	trx Lorient_KMA
	trx type:	Voyager
	trx mode:	mode 1
	baud_rate:	32.0 Gbaud
	bit_rate:	100.0 Gb/s
	spacing:	50.0 GHz
	power:  	0.0 dBm
	nb channels: 	76
	path_bandwidth: 	700.0 Gbit/s
	nodes-list:	[]
	loose-list:	[]
, PathRequest 7b
	source: 	trx Lannion_CAS
	destination:	trx Lorient_KMA
	trx type:	Voyager
	trx mode:	mode 1
	baud_rate:	32.0 Gbaud
	bit_rate:	100.0 Gb/s
	spacing:	75.0 GHz
	power:  	0.0 dBm
	nb channels: 	50
	path_bandwidth: 	400.0 Gbit/s
	nodes-list:	[]
	loose-list:	[]
]
[1;34;40mComputing all paths with constraints[0m
[1;34;40mPropagating on selected path[0m
[1;34;40mResult summary[0m
req id   demand                                GSNR@bandwidth A-Z (Z-A)   GSNR@0.1nm A-Z (Z-A)        Receiver minOSNR               mode                    Gbit/s              nb of tsp pairs      N,M or blocking reason 
0       trx Lorient_KMA to trx Vannes_KBE :             24.83                    28.92                      14                     mode 1                   100.0                      1                   ([-284],[4])      
1       trx Brest_KLA to trx Vannes_KBE :               17.74                    21.82                      14                     mode 1                   200.0                      2                   ([-272],[8])      
3       trx Lannion_CAS to trx Rennes_STA :             22.19                    26.28                      13                     mode 1                    60.0                      1                   ([-284],[4])      
4       trx Rennes_STA to trx Lannion_CAS :             16.06                    23.29                      17                     mode 2                   150.0                      1                   ([-258],[6])      
5       trx Rennes_STA to trx Lannion_CAS :              20.3                    27.53                      17                     mode 2                    20.0                      1                   ([-274],[6])      
7 | 6   trx Lannion_CAS to trx Lorient_KMA :            19.52                    23.61                      14                     mode 1                   700.0                      7                  ([-224],[28])      
7b      trx Lannion_CAS to trx Lorient_KMA :            19.61                    23.69                      14                     mode 1                   400.0                      4                  ([-172],[24])      
[1;33;40mResult summary shows mean GSNR and OSNR (average over all channels)[0m
