There are 96 channels propagating
Power mode is set to True
=> it can be modified in eqpt_config.json - Span

There are 15 fiber spans over 1200 km between Site_A and Site_B

Now propagating between Site_A and Site_B:

Propagating with input power = [1;36;40m0.00 dBm[0m:
Transceiver Site_A
  GSNR (0.1nm, dB):          100.00
  GSNR (signal bw, dB):      95.92
  OSNR ASE (0.1nm, dB):      100.00
  OSNR ASE (signal bw, dB):  95.92
  CD (ps/nm):                0.00
  PMD (ps):                  0.00
  PDL (dB):                  0.00
  Latency (ms):              0.00
Roadm roadm Site A
  effective loss (dB):     20.00
  reference pch out (dBm): -20.00
  actual pch out (dBm):    -20.00
Edfa booster A
  type_variety:           std_medium_gain
  effective gain(dB):     20.00
  (before att_in and before output VOA)
  noise figure (dB):      6.58
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        19.83
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.01
  output VOA (dB):        0.00
Fiber          Span1
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.99
Edfa Edfa1
  type_variety:           test
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      8.86
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         3.84
  Power Out (dBm):        19.84
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.02
  output VOA (dB):        0.00
Fiber          Span2
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.98
Edfa Edfa2
  type_variety:           test_fixed_gain
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      9.00
  (including att_in)
  pad att_in (dB):        4.00
  Power In (dBm):         3.84
  Power Out (dBm):        19.85
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.03
  output VOA (dB):        0.00
Fiber          Span3
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.97
Edfa Edfa3
  type_variety:           test
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      8.86
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         3.85
  Power Out (dBm):        19.86
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.04
  output VOA (dB):        0.00
Fiber          Span4
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.96
Edfa Edfa4
  type_variety:           test_fixed_gain
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      9.00
  (including att_in)
  pad att_in (dB):        4.00
  Power In (dBm):         3.86
  Power Out (dBm):        19.87
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.05
  output VOA (dB):        0.00
Fiber          Span5
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.95
Edfa Edfa5
  type_variety:           test
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      8.86
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         3.87
  Power Out (dBm):        19.88
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.06
  output VOA (dB):        0.00
Roadm roadm Site C
  effective loss (dB):     20.00
  reference pch out (dBm): -20.00
  actual pch out (dBm):    -20.00
Edfa booster C
  type_variety:           std_medium_gain
  effective gain(dB):     20.00
  (before att_in and before output VOA)
  noise figure (dB):      6.58
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        19.83
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.01
  output VOA (dB):        0.00
Fiber          Span6
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.99
Edfa Edfa6
  type_variety:           test_fixed_gain
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      9.00
  (including att_in)
  pad att_in (dB):        4.00
  Power In (dBm):         3.84
  Power Out (dBm):        19.84
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.02
  output VOA (dB):        0.00
Fiber          Span7
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.98
Edfa Edfa7
  type_variety:           test
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      8.86
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         3.84
  Power Out (dBm):        19.85
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.03
  output VOA (dB):        0.00
Fiber          Span8
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.97
Edfa Edfa8
  type_variety:           test_fixed_gain
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      9.00
  (including att_in)
  pad att_in (dB):        4.00
  Power In (dBm):         3.85
  Power Out (dBm):        19.86
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.04
  output VOA (dB):        0.00
Fiber          Span9
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.96
Edfa Edfa9
  type_variety:           test
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      8.86
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         3.86
  Power Out (dBm):        19.87
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.05
  output VOA (dB):        0.00
Fiber          Span10
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.95
Edfa Edfa10
  type_variety:           test_fixed_gain
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      9.00
  (including att_in)
  pad att_in (dB):        4.00
  Power In (dBm):         3.87
  Power Out (dBm):        19.88
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.06
  output VOA (dB):        0.00
Roadm roadm Site D
  effective loss (dB):     20.00
  reference pch out (dBm): -20.00
  actual pch out (dBm):    -20.00
Edfa booster D
  type_variety:           std_medium_gain
  effective gain(dB):     20.00
  (before att_in and before output VOA)
  noise figure (dB):      6.58
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        19.83
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.01
  output VOA (dB):        0.00
Fiber          Span11
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.99
Edfa Edfa11
  type_variety:           test
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      8.86
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         3.83
  Power Out (dBm):        19.84
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.02
  output VOA (dB):        0.00
Fiber          Span12
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.98
Edfa Edfa12
  type_variety:           test_fixed_gain
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      9.00
  (including att_in)
  pad att_in (dB):        4.00
  Power In (dBm):         3.84
  Power Out (dBm):        19.85
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.03
  output VOA (dB):        0.00
Roadm roadm Site E
  effective loss (dB):     20.00
  reference pch out (dBm): -20.00
  actual pch out (dBm):    -20.00
Edfa booster E
  type_variety:           std_medium_gain
  effective gain(dB):     20.00
  (before att_in and before output VOA)
  noise figure (dB):      6.58
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         -0.18
  Power Out (dBm):        19.83
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.01
  output VOA (dB):        0.00
Fiber          Span13
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.99
Edfa Edfa13
  type_variety:           test
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      8.86
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         3.83
  Power Out (dBm):        19.84
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.02
  output VOA (dB):        0.00
Fiber          Span14
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.98
Edfa Edfa14
  type_variety:           test_fixed_gain
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      9.00
  (including att_in)
  pad att_in (dB):        4.00
  Power In (dBm):         3.84
  Power Out (dBm):        19.85
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.03
  output VOA (dB):        0.00
Fiber          Span15
  type_variety:                SSMF
  length (km):                 80.00
  pad att_in (dB):             0.00
  total loss (dB):             16.00
  (includes conn loss (dB) in: 0.00 out: 0.00)
  (conn loss out includes EOL margin defined in eqpt_config.json)
  reference pch out (dBm):     -16.00
  actual pch out (dBm):        -15.97
Edfa Edfa15
  type_variety:           test
  effective gain(dB):     16.00
  (before att_in and before output VOA)
  noise figure (dB):      8.86
  (including att_in)
  pad att_in (dB):        0.00
  Power In (dBm):         3.85
  Power Out (dBm):        19.86
  Delta_P (dB):           0.00
  target pch (dBm):       0.00
  actual pch out (dBm):   0.04
  output VOA (dB):        0.00
Roadm roadm Site B
  effective loss (dB):     20.00
  reference pch out (dBm): -20.00
  actual pch out (dBm):    -20.00
Transceiver Site_B
  GSNR (0.1nm, dB):          17.84
  GSNR (signal bw, dB):      13.76
  OSNR ASE (0.1nm, dB):      19.70
  OSNR ASE (signal bw, dB):  15.62
  CD (ps/nm):                20040.00
  PMD (ps):                  1.39
  PDL (dB):                  0.00
  Latency (ms):              5.88

Transmission result for input power = 0.00 dBm:
  Final GSNR (0.1 nm): [1;36;40m17.84 dB[0m

(No source node specified: picked Site_A)

(No destination node specified: picked Site_B)
