There are 95 channels propagating
Power mode is set to True
=> it can be modified in eqpt_config.json - Span

There are 4 fiber spans over 200 km between trx Brest_KLA and trx Rennes_STA

Now propagating between trx Brest_KLA and trx Rennes_STA:

Propagating with input power = [1;36;40m-3.00 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          23.73
  GSNR (signal bw, dB):      19.65
  OSNR ASE (0.1nm, dB):      23.99
  OSNR ASE (signal bw, dB):  19.91
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m-2.50 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.01
  GSNR (signal bw, dB):      19.93
  OSNR ASE (0.1nm, dB):      24.37
  OSNR ASE (signal bw, dB):  20.29
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m-2.00 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.25
  GSNR (signal bw, dB):      20.17
  OSNR ASE (0.1nm, dB):      24.74
  OSNR ASE (signal bw, dB):  20.66
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m-1.50 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.44
  GSNR (signal bw, dB):      20.36
  OSNR ASE (0.1nm, dB):      25.10
  OSNR ASE (signal bw, dB):  21.01
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m-1.00 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.57
  GSNR (signal bw, dB):      20.49
  OSNR ASE (0.1nm, dB):      25.44
  OSNR ASE (signal bw, dB):  21.36
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m-0.50 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.63
  GSNR (signal bw, dB):      20.55
  OSNR ASE (0.1nm, dB):      25.77
  OSNR ASE (signal bw, dB):  21.69
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m-0.00 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.60
  GSNR (signal bw, dB):      20.52
  OSNR ASE (0.1nm, dB):      26.09
  OSNR ASE (signal bw, dB):  22.00
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m0.50 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.42
  GSNR (signal bw, dB):      20.34
  OSNR ASE (0.1nm, dB):      26.29
  OSNR ASE (signal bw, dB):  22.20
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m1.00 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.16
  GSNR (signal bw, dB):      20.08
  OSNR ASE (0.1nm, dB):      26.47
  OSNR ASE (signal bw, dB):  22.39
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m1.50 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.02
  GSNR (signal bw, dB):      19.93
  OSNR ASE (0.1nm, dB):      26.55
  OSNR ASE (signal bw, dB):  22.47
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m2.00 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.02
  GSNR (signal bw, dB):      19.93
  OSNR ASE (0.1nm, dB):      26.55
  OSNR ASE (signal bw, dB):  22.47
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m2.50 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.02
  GSNR (signal bw, dB):      19.93
  OSNR ASE (0.1nm, dB):      26.55
  OSNR ASE (signal bw, dB):  22.47
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

Propagating with input power = [1;36;40m3.00 dBm[0m:
Transceiver trx Rennes_STA
  GSNR (0.1nm, dB):          24.02
  GSNR (signal bw, dB):      19.93
  OSNR ASE (0.1nm, dB):      26.55
  OSNR ASE (signal bw, dB):  22.47
  CD (ps/nm):                3340.00
  PMD (ps):                  0.57
  PDL (dB):                  0.00
  Latency (ms):              0.98

(Invalid source node 'brest' replaced with trx Brest_KLA)

(Invalid destination node 'rennes' replaced with trx Rennes_STA)
