From f1acfc2f397e86548ae1b479c198d4bef57050f6 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Sun, 29 Sep 2013 18:10:34 +0200
Subject: [PATCH] rt2x00: rt2800lib: use high memory for beacons on RT3883

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c |    3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -97,7 +97,8 @@ static inline void rt2800_shared_mem_sel
 
 static inline bool rt2800_beacon_uses_high_mem(struct rt2x00_dev *rt2x00dev)
 {
-	if (rt2x00_rt(rt2x00dev, RT3593))
+	if (rt2x00_rt(rt2x00dev, RT3593) ||
+	    rt2x00_rt(rt2x00dev, RT3883))
 		return true;
 
 	return false;
