From: Sven Eckelmann <sven@narfation.org>
Date: Tue, 26 Feb 2019 08:06:35 +0100
Subject: ath10k-ct: apply mac80211 rates to ath10k-ct rate state

The rates from mac80211 have to be copied to the state of ath10k-ct or
otherwise the ath10k_check_apply_special_rates function overwrites
them again with some default values. This breaks for example the
mcast_rate set for a wifi-iface.

Signed-off-by: Sven Eckelmann <sven@narfation.org>

--- a/ath10k-5.4/mac.c
+++ b/ath10k-5.4/mac.c
@@ -6793,6 +6793,7 @@ static void ath10k_bss_info_changed(stru
 			   "mac vdev %d mcast_rate %x\n",
 			   arvif->vdev_id, rate);
 
+		arvif->mcast_rate[band] = rate;
 		vdev_param = ar->wmi.vdev_param->mcast_data_rate;
 		ret = ath10k_wmi_vdev_set_param(ar, arvif->vdev_id,
 						vdev_param, rate);
@@ -6801,6 +6802,7 @@ static void ath10k_bss_info_changed(stru
 				    "failed to set mcast rate on vdev %i: %d\n",
 				    arvif->vdev_id,  ret);
 
+		arvif->bcast_rate[band] = rate;
 		vdev_param = ar->wmi.vdev_param->bcast_data_rate;
 		ret = ath10k_wmi_vdev_set_param(ar, arvif->vdev_id,
 						vdev_param, rate);
@@ -6827,6 +6829,7 @@ static void ath10k_bss_info_changed(stru
 			return;
 		}
 
+		arvif->mgt_rate[def.chan->band] = hw_rate_code;
 		vdev_param = ar->wmi.vdev_param->mgmt_rate;
 		ret = ath10k_wmi_vdev_set_param(ar, arvif->vdev_id, vdev_param,
 						hw_rate_code);
