config usteer
	# The network interface for inter-AP communication
	option 'network' 'lan'

	# Log messages to syslog (0/1)
	option 'syslog' '1'

	# Minimum level of logged messages
	# 0 = fatal
	# 1 = info
	# 2 = verbose
	# 3 = some debug messages
	# 4 = network packet information
	# 5 = all debug messages
	option 'debug_level' '2'

	# Maximum amount of time (ms) a station may be blocked due to policy decisions
	#option sta_block_timeout 30000

	# Maximum amount of time (ms) a local unconnected station is tracked
	#option local_sta_timeout 120000

	# Local station information update interval (ms)
	#option local_sta_update 1000

	# Maximum number of consecutive times a station may be blocked by policy
	#option max_retry_band 5

	# Maximum idle time of a station entry (ms) to be considered for policy decisions
	#option seen_policy_timeout 30000

	# Minimum number of stations delta between APs before load balancing policy is active
	#option load_balancing_threshold 5

	# Minimum number of stations delta between bands before band steering policy is active
	#option band_steering_threshold 5

	# Interval (ms) between sending state updates to other APs
	#option remote_update_interval 1000

	# Allow rejecting assoc requests for steering purposes (0/1)
	#option assoc_steering 0

	# Minimum signal-to-noise ratio or signal level (dBm) to allow connections
	#option min_connect_snr 0

	# Minimum signal-to-noise ratio or signal level (dBm) to remain connected
	#option min_snr 0

	# Minimum signal-to-noise ratio or signal level (dBm) before attempting to trigger
	# client scans for roaming
	#option roam_scan_snr 0

	# Maximum number of client roaming scan trigger attempts
	#option roam_scan_tries 3

	# Minimum time (ms) between client roaming scan trigger attempts
	#option roam_scan_interval 10000

	# Minimum signal-to-noise ratio or signal level (dBm) before attempting to trigger
	# forced client roaming
	#option roam_trigger_snr 0

	# Minimum time (ms) between client roaming trigger attempts
	#option roam_trigger_interval 60000

	# Timeout (in 100ms beacon intervals) for client roam requests
	#option roam_kick_delay 100

	# Minimum signal strength difference until AP steering policy is active
	#option signal_diff_threshold 0

	# Initial delay (ms) before responding to probe requests (to allow other APs to see packets as well)
	#option initial_connect_delay 0

	# Enable kicking client on excessive channel load (0/1)
	#option load_kick_enabled 0

	# Minimum channel load (%) before kicking clients
	#option load_kick_threshold 75

	# Minimum amount of time (ms) that channel load is above threshold before starting to kick clients
	#option load_kick_delay 10000

	# Minimum number of connected clients before kicking based on channel load
	#option load_kick_min_clients 10

	# Reason code on client kick based on channel load (default: WLAN_REASON_DISASSOC_AP_BUSY)
	#option load_kick_reason_code 5

	# Script to run after bringing up a node
	#option node_up_script ''

	# Message types to include in log
	# Available types:
	# - probe_req_accept
	# - probe_req_deny
	# - auth_req_accept
	# - auth_req_deny
	# - assoc_req_accept
	# - assoc_req_deny
	# - load_kick_trigger
	# - load_kick_reset
	# - load_kick_min_clients
	# - load_kick_no_client
	# - load_kick_client
	# - signal_kick
	#list event_log_types ''

	# List of SSIDs to enable steering on
	#list ssid_list ''
