From 1616650aea676541d4dc8adc6f4219856d193c8b Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Tue, 1 Oct 2013 17:27:57 +0200
Subject: [PATCH] rt2x00: rt2800lib: fix EEPROM LNA validation for RT3883

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c |    9 ++++++---
 1 file changed, 6 insertions(+), 3 deletions(-)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -7607,7 +7607,8 @@ static int rt2800_validate_eeprom(struct
 	rt2800_eeprom_read(rt2x00dev, EEPROM_RSSI_BG2, &word);
 	if (abs(rt2x00_get_field16(word, EEPROM_RSSI_BG2_OFFSET2)) > 10)
 		rt2x00_set_field16(&word, EEPROM_RSSI_BG2_OFFSET2, 0);
-	if (!rt2x00_rt(rt2x00dev, RT3593)) {
+	if (!rt2x00_rt(rt2x00dev, RT3593) &&
+	    !rt2x00_rt(rt2x00dev, RT3883)) {
 		if (rt2x00_get_field16(word, EEPROM_RSSI_BG2_LNA_A1) == 0x00 ||
 		    rt2x00_get_field16(word, EEPROM_RSSI_BG2_LNA_A1) == 0xff)
 			rt2x00_set_field16(&word, EEPROM_RSSI_BG2_LNA_A1,
@@ -7627,7 +7628,8 @@ static int rt2800_validate_eeprom(struct
 	rt2800_eeprom_read(rt2x00dev, EEPROM_RSSI_A2, &word);
 	if (abs(rt2x00_get_field16(word, EEPROM_RSSI_A2_OFFSET2)) > 10)
 		rt2x00_set_field16(&word, EEPROM_RSSI_A2_OFFSET2, 0);
-	if (!rt2x00_rt(rt2x00dev, RT3593)) {
+	if (!rt2x00_rt(rt2x00dev, RT3593) &&
+	    !rt2x00_rt(rt2x00dev, RT3883)) {
 		if (rt2x00_get_field16(word, EEPROM_RSSI_A2_LNA_A2) == 0x00 ||
 		    rt2x00_get_field16(word, EEPROM_RSSI_A2_LNA_A2) == 0xff)
 			rt2x00_set_field16(&word, EEPROM_RSSI_A2_LNA_A2,
@@ -7635,7 +7637,8 @@ static int rt2800_validate_eeprom(struct
 	}
 	rt2800_eeprom_write(rt2x00dev, EEPROM_RSSI_A2, word);
 
-	if (rt2x00_rt(rt2x00dev, RT3593)) {
+	if (rt2x00_rt(rt2x00dev, RT3593) ||
+	    rt2x00_rt(rt2x00dev, RT3883)) {
 		rt2800_eeprom_read(rt2x00dev, EEPROM_EXT_LNA2, &word);
 		if (rt2x00_get_field16(word, EEPROM_EXT_LNA2_A1) == 0x00 ||
 		    rt2x00_get_field16(word, EEPROM_EXT_LNA2_A1) == 0xff)
