From bd7e19e3cc30bda8d0b0ae6f3d0c44425c6b7541 Mon Sep 17 00:00:00 2001
From: Rohan Nathi <rohan.nathi@indionetworks.com>
Date: Thu, 24 Jun 2021 13:48:45 +0000
Subject: [PATCH 01/22] ath79: add Support for Indio 305AC

Signed-off-by: Rohan Nathi <rohan.nathi@indionetworks.com>
---
 .../ath79/dts/qca9531_indio_um-305ac.dts      | 121 ++++++++++++++++++
 .../etc/hotplug.d/firmware/11-ath10k-caldata  |   1 +
 target/linux/ath79/image/generic.mk           |  11 ++
 3 files changed, 133 insertions(+)
 create mode 100755 target/linux/ath79/dts/qca9531_indio_um-305ac.dts

diff --git a/target/linux/ath79/dts/qca9531_indio_um-305ac.dts b/target/linux/ath79/dts/qca9531_indio_um-305ac.dts
new file mode 100755
index 0000000000..3952c4ad2c
--- /dev/null
+++ b/target/linux/ath79/dts/qca9531_indio_um-305ac.dts
@@ -0,0 +1,121 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+
+#include "qca953x.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+
+/ {
+	model = "Indio UM-305AC";
+	compatible = "indio,um-305ac", "qca,qca9531";
+
+	aliases {
+		led-boot = &led_status;
+		led-failsafe = &led_status;
+		led-running = &led_status;
+		led-upgrade = &led_status;
+	};
+
+	keys {
+		compatible = "gpio-keys";
+
+		reset {
+			label = "reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
+			debounce-interval = <60>;
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		lan {
+			label = "green:lan";
+			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
+		};
+
+		led_status: status {
+			label = "green:status";
+			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
+			default-state = "keep";
+		};
+
+		wan {
+			label = "green:wan";
+			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
+		};
+
+		wlan2g {
+			label = "red:wlan2g";
+			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "phy1tpt";
+		};
+	};
+};
+
+&spi {
+	status = "okay";
+
+	flash@0 {
+		compatible = "jedec,spi-nor";
+		reg = <0>;
+		spi-max-frequency = <25000000>;
+
+		partitions {
+			compatible = "fixed-partitions";
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			partition@0 {
+				label = "u-boot";
+				reg = <0x000000 0x040000>;
+				read-only;
+			};
+
+			partition@40000 {
+				label = "u-boot-env";
+				reg = <0x040000 0x010000>;
+			};
+
+			partition@50000 {
+				compatible = "denx,uimage";
+				label = "firmware";
+				reg = <0x050000 0xf90000>;
+			};
+
+			partition@fe0000 {
+				label = "certificates";
+				reg = <0xfe0000 0x010000>;
+			};
+
+			art: partition@ff0000 {
+				label = "art";
+				reg = <0xff0000 0x010000>;
+				read-only;
+			};
+		};
+	};
+};
+
+&eth0 {
+	status = "okay";
+
+	phy-handle = <&swphy4>;
+
+	mtd-mac-address = <&art 0x0>;
+};
+
+&eth1 {
+	mtd-mac-address = <&art 0x6>;
+};
+
+&pcie0 {
+	status = "okay";
+};
+
+&wmac {
+	status = "okay";
+
+	mtd-cal-data = <&art 0x1000>;
+};
diff --git a/target/linux/ath79/generic/base-files/etc/hotplug.d/firmware/11-ath10k-caldata b/target/linux/ath79/generic/base-files/etc/hotplug.d/firmware/11-ath10k-caldata
index 783895525b..80f755b343 100644
--- a/target/linux/ath79/generic/base-files/etc/hotplug.d/firmware/11-ath10k-caldata
+++ b/target/linux/ath79/generic/base-files/etc/hotplug.d/firmware/11-ath10k-caldata
@@ -44,6 +44,7 @@ case "$FIRMWARE" in
 	ubnt,powerbeam-5ac-500|\
 	ubnt,powerbeam-5ac-gen2|\
 	ubnt,unifiac-pro|\
+	indio,um-305ac|\
 	yuncore,a770)
 		caldata_extract "art" 0x5000 0x844
 		;;
diff --git a/target/linux/ath79/image/generic.mk b/target/linux/ath79/image/generic.mk
index ce4e462a40..24778e8f1c 100644
--- a/target/linux/ath79/image/generic.mk
+++ b/target/linux/ath79/image/generic.mk
@@ -2209,6 +2209,17 @@ define Device/yuncore_a770
 endef
 TARGET_DEVICES += yuncore_a770
 
+define Device/indio_um-305ac
+  SOC := qca9531
+  DEVICE_VENDOR := Indio Network
+  DEVICE_MODEL := UM-305AC
+  DEVICE_PACKAGES := kmod-ath10k ath10k-firmware-qca9887
+  IMAGE_SIZE := 16000k
+  IMAGES += tftp.bin
+  IMAGE/tftp.bin := $$(IMAGE/sysupgrade.bin) | yuncore-tftp-header-16m
+endef
+TARGET_DEVICES += indio_um-305ac
+
 define Device/yuncore_a782
   SOC := qca9563
   DEVICE_VENDOR := YunCore
-- 
2.25.1

