From patchwork Thu May 28 06:16:48 2020
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
X-Patchwork-Submitter: Chuanjia Liu <chuanjia.liu@mediatek.com>
X-Patchwork-Id: 11574797
Return-Path: 
 <SRS0=ftSA=7K=lists.infradead.org=linux-mediatek-bounces+patchwork-linux-mediatek=patchwork.kernel.org@kernel.org>
Received: from mail.kernel.org (pdx-korg-mail-1.web.codeaurora.org
 [172.30.200.123])
	by pdx-korg-patchwork-2.web.codeaurora.org (Postfix) with ESMTP id 30A5E1392
	for <patchwork-linux-mediatek@patchwork.kernel.org>;
 Thu, 28 May 2020 06:29:05 +0000 (UTC)
Received: from bombadil.infradead.org (bombadil.infradead.org
 [198.137.202.133])
	(using TLSv1.2 with cipher ECDHE-RSA-AES256-GCM-SHA384 (256/256 bits))
	(No client certificate requested)
	by mail.kernel.org (Postfix) with ESMTPS id 08B6320721
	for <patchwork-linux-mediatek@patchwork.kernel.org>;
 Thu, 28 May 2020 06:29:05 +0000 (UTC)
Authentication-Results: mail.kernel.org;
	dkim=pass (2048-bit key) header.d=lists.infradead.org
 header.i=@lists.infradead.org header.b="auhxDafY";
	dkim=fail reason="signature verification failed" (1024-bit key)
 header.d=mediatek.com header.i=@mediatek.com header.b="Kj09Arxb"
DMARC-Filter: OpenDMARC Filter v1.3.2 mail.kernel.org 08B6320721
Authentication-Results: mail.kernel.org;
 dmarc=fail (p=none dis=none) header.from=mediatek.com
Authentication-Results: mail.kernel.org;
 spf=none
 smtp.mailfrom=linux-mediatek-bounces+patchwork-linux-mediatek=patchwork.kernel.org@lists.infradead.org
DKIM-Signature: v=1; a=rsa-sha256; q=dns/txt; c=relaxed/relaxed;
	d=lists.infradead.org; s=bombadil.20170209; h=Sender:
	Content-Transfer-Encoding:Content-Type:Cc:List-Subscribe:List-Help:List-Post:
	List-Archive:List-Unsubscribe:List-Id:MIME-Version:References:In-Reply-To:
	Message-ID:Date:Subject:To:From:Reply-To:Content-ID:Content-Description:
	Resent-Date:Resent-From:Resent-Sender:Resent-To:Resent-Cc:Resent-Message-ID:
	List-Owner; bh=+QPxF1vlOH7StIZYuXJa3V40x8QVDxCLF9AFXHblB9M=; b=auhxDafYBeaUZO
	aYp2KVO8Aie0v4tYtRwBon7hF+x55JwD78SAxQR2RsSvrlOo9cMYYby+ToUWflVUWQ60FapAl+w+l
	nkEjIOrLBErHwxNOcsD8T5kjyCBMqlz4OMAQYUDNJ3fSugRlGhOtxkjCGd9ebB8N2Rvu6/U8P1A9n
	P15mEQoc+RLonR1+9mBgwTEXErjsraxkimTD4Txsp4IvMs3UdsMkP+r3OT5S/p+Uj6O9ES0h7xIon
	aL79KaVqRLHrfZxnrVwuGiecAiTp8qLy9clHuJU32NA6ZcXH1OnWipKApgp8Ck7ys80WPKaMrat9B
	XuskJ63w13DZAbCVvuGQ==;
Received: from localhost ([127.0.0.1] helo=bombadil.infradead.org)
	by bombadil.infradead.org with esmtp (Exim 4.92.3 #3 (Red Hat Linux))
	id 1jeC2J-00014n-M9; Thu, 28 May 2020 06:29:03 +0000
Received: from mailgw02.mediatek.com ([216.200.240.185])
 by bombadil.infradead.org with esmtps (Exim 4.92.3 #3 (Red Hat Linux))
 id 1jeC2H-00013t-Li; Thu, 28 May 2020 06:29:03 +0000
X-UUID: a4877c1586e64afeb2d6172e10605d2b-20200527
DKIM-Signature: v=1; a=rsa-sha256; q=dns/txt; c=relaxed/relaxed;
 d=mediatek.com;
 s=dk;
 h=Content-Transfer-Encoding:Content-Type:MIME-Version:References:In-Reply-To:Message-ID:Date:Subject:CC:To:From;
 bh=CIwcBFK1x0LbOjDt1BG6/knHFxDHRiqj8ov/jWEZDBY=;
 b=Kj09ArxbnLVTc9bpaVPT3jQrIVjhL87sSYyVF9dFypS976k78Ce9gZd0f4K3zAZbYZHYoQtuyOQ9TOeufQfgD+Cr+j5VR7pTdO2E1iXHFs/eQAz5gAjvjlK01z1JiunrLnn9dvIr6c1gEkjQHny0VpuZ1duxx79jwYusg/Nw6Wc=;
X-UUID: a4877c1586e64afeb2d6172e10605d2b-20200527
Received: from mtkcas66.mediatek.inc [(172.29.193.44)] by
 mailgw02.mediatek.com
 (envelope-from <chuanjia.liu@mediatek.com>)
 (musrelay.mediatek.com ESMTP with TLS)
 with ESMTP id 899663677; Wed, 27 May 2020 22:29:21 -0800
Received: from MTKMBS07N2.mediatek.inc (172.21.101.141) by
 MTKMBS62DR.mediatek.inc (172.29.94.18) with Microsoft SMTP Server (TLS) id
 15.0.1497.2; Wed, 27 May 2020 23:18:50 -0700
Received: from mtkcas07.mediatek.inc (172.21.101.84) by
 mtkmbs07n2.mediatek.inc (172.21.101.141) with Microsoft SMTP Server (TLS) id
 15.0.1497.2; Thu, 28 May 2020 14:18:54 +0800
Received: from localhost.localdomain (10.17.3.153) by mtkcas07.mediatek.inc
 (172.21.101.73) with Microsoft SMTP Server id 15.0.1497.2 via Frontend
 Transport; Thu, 28 May 2020 14:18:52 +0800
From: <chuanjia.liu@mediatek.com>
To: <robh+dt@kernel.org>, <ryder.lee@mediatek.com>, <matthias.bgg@gmail.com>
Subject: [PATCH v2 4/4] ARM: dts: mediatek: Update mt7629 PCIe node
Date: Thu, 28 May 2020 14:16:48 +0800
Message-ID: <20200528061648.32078-5-chuanjia.liu@mediatek.com>
X-Mailer: git-send-email 2.18.0
In-Reply-To: <20200528061648.32078-1-chuanjia.liu@mediatek.com>
References: <20200528061648.32078-1-chuanjia.liu@mediatek.com>
MIME-Version: 1.0
X-MTK: N
X-CRM114-Version: 20100106-BlameMichelson ( TRE 0.8.0 (BSD) ) MR-646709E3 
X-CRM114-CacheID: sfid-20200527_232901_719172_E5A99C62 
X-CRM114-Status: GOOD (  11.61  )
X-Spam-Score: -0.2 (/)
X-Spam-Report: SpamAssassin version 3.4.4 on bombadil.infradead.org summary:
 Content analysis details:   (-0.2 points)
 pts rule name              description
 ---- ----------------------
 --------------------------------------------------
 -0.0 SPF_PASS               SPF: sender matches SPF record
 0.0 SPF_HELO_NONE          SPF: HELO does not publish an SPF Record
 0.0 MIME_BASE64_TEXT       RAW: Message text disguised using base64
 encoding
 -0.1 DKIM_VALID_AU          Message has a valid DKIM or DK signature from
 author's domain
 0.1 DKIM_SIGNED            Message has a DKIM or DK signature,
 not necessarily
 valid
 -0.1 DKIM_VALID Message has at least one valid DKIM or DK signature
 -0.1 DKIM_VALID_EF          Message has a valid DKIM or DK signature from
 envelope-from domain
 0.0 UNPARSEABLE_RELAY      Informational: message has unparseable relay
 lines
X-BeenThere: linux-mediatek@lists.infradead.org
X-Mailman-Version: 2.1.29
Precedence: list
List-Id: <linux-mediatek.lists.infradead.org>
List-Unsubscribe: <http://lists.infradead.org/mailman/options/linux-mediatek>,
 <mailto:linux-mediatek-request@lists.infradead.org?subject=unsubscribe>
List-Archive: <http://lists.infradead.org/pipermail/linux-mediatek/>
List-Post: <mailto:linux-mediatek@lists.infradead.org>
List-Help: <mailto:linux-mediatek-request@lists.infradead.org?subject=help>
List-Subscribe: <http://lists.infradead.org/mailman/listinfo/linux-mediatek>,
 <mailto:linux-mediatek-request@lists.infradead.org?subject=subscribe>
Cc: devicetree@vger.kernel.org, lorenzo.pieralisi@arm.com,
 srv_heupstream@mediatek.com, "chuanjia.liu" <Chuanjia.Liu@mediatek.com>,
 linux-pci@vger.kernel.org, linux-kernel@vger.kernel.org,
 jianjun.wang@mediatek.com, linux-mediatek@lists.infradead.org,
 yong.wu@mediatek.com, bhelgaas@google.com,
 linux-arm-kernel@lists.infradead.org, amurray@thegoodpenguin.co.uk
Sender: "Linux-mediatek" <linux-mediatek-bounces@lists.infradead.org>
Errors-To: 
 linux-mediatek-bounces+patchwork-linux-mediatek=patchwork.kernel.org@lists.infradead.org

From: "chuanjia.liu" <Chuanjia.Liu@mediatek.com>

Remove unused property and add pciecfg node.

Signed-off-by: chuanjia.liu <Chuanjia.Liu@mediatek.com>
---
 arch/arm/boot/dts/mt7629-rfb.dts |  3 ++-
 arch/arm/boot/dts/mt7629.dtsi    | 23 +++++++++++++----------
 2 files changed, 15 insertions(+), 11 deletions(-)

--- a/arch/arm/boot/dts/mt7629-rfb.dts
+++ b/arch/arm/boot/dts/mt7629-rfb.dts
@@ -171,9 +171,10 @@
 	};
 };
 
-&pcie {
+&pcie1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&pcie_pins>;
+	status = "okay";
 };
 
 &pciephy1 {
--- a/arch/arm/boot/dts/mt7629.dtsi
+++ b/arch/arm/boot/dts/mt7629.dtsi
@@ -368,16 +368,21 @@
 			#reset-cells = <1>;
 		};
 
-		pcie: pcie@1a140000 {
+		pciecfg: pciecfg@1a140000 {
+			compatible = "mediatek,mt7629-pciecfg", "syscon";
+			reg = <0x1a140000 0x1000>;
+		};
+
+		pcie1: pcie@1a145000 {
 			compatible = "mediatek,mt7629-pcie";
 			device_type = "pci";
-			reg = <0x1a140000 0x1000>,
-			      <0x1a145000 0x1000>;
-			reg-names = "subsys","port1";
+			reg = <0x1a145000 0x1000>;
+			reg-names = "port1";
+			mediatek,pcie-cfg = <&pciecfg>;
 			#address-cells = <3>;
 			#size-cells = <2>;
-			interrupts = <GIC_SPI 176 IRQ_TYPE_LEVEL_LOW>,
-				     <GIC_SPI 229 IRQ_TYPE_LEVEL_LOW>;
+			interrupts = <GIC_SPI 229 IRQ_TYPE_LEVEL_LOW>;
+			interrupt-names = "pcie_irq";
 			clocks = <&pciesys CLK_PCIE_P1_MAC_EN>,
 				 <&pciesys CLK_PCIE_P0_AHB_EN>,
 				 <&pciesys CLK_PCIE_P1_AUX_EN>,
@@ -398,21 +403,19 @@
 			power-domains = <&scpsys MT7622_POWER_DOMAIN_HIF0>;
 			bus-range = <0x00 0xff>;
 			ranges = <0x82000000 0 0x20000000 0x20000000 0 0x10000000>;
+			status = "disabled";
 
-			pcie1: pcie@1,0 {
-				device_type = "pci";
+			slot1: pcie@1,0 {
 				reg = <0x0800 0 0 0 0>;
 				#address-cells = <3>;
 				#size-cells = <2>;
 				#interrupt-cells = <1>;
 				ranges;
-				num-lanes = <1>;
 				interrupt-map-mask = <0 0 0 7>;
 				interrupt-map = <0 0 0 1 &pcie_intc1 0>,
 						<0 0 0 2 &pcie_intc1 1>,
 						<0 0 0 3 &pcie_intc1 2>,
 						<0 0 0 4 &pcie_intc1 3>;
-
 				pcie_intc1: interrupt-controller {
 					interrupt-controller;
 					#address-cells = <0>;
