/*
 * Copyright (c) 2018 MediaTek Inc.
 * Author: Wenzhen.Yu <Wenzhen.Yu@mediatek.com>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 *
 * This program is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 */

&clkitg {
	bring-up {
		compatible = "mediatek,clk-bring-up";
		clocks =
			<&apmixedsys CK_APMIXED_ARMPLL>,
			<&apmixedsys  CK_APMIXED_NET2PLL>,
			<&apmixedsys  CK_APMIXED_MMPLL>,
			<&apmixedsys  CK_APMIXED_SGMPLL>,
			<&apmixedsys  CK_APMIXED_WEDMCUPLL>,
			<&apmixedsys  CK_APMIXED_NET1PLL>,
			<&apmixedsys  CK_APMIXED_MPLL>,
			<&apmixedsys  CK_APMIXED_APLL2>,
			<&infracfg CK_INFRA_CK_F26M>,
			<&infracfg CK_INFRA_UART>,
			<&infracfg CK_INFRA_ISPI0>,
			<&infracfg CK_INFRA_I2C>,
			<&infracfg CK_INFRA_ISPI1>,
			<&infracfg CK_INFRA_PWM>,
			<&infracfg CK_INFRA_66M_MCK>,
			<&infracfg CK_INFRA_CK_F32K>,
			<&infracfg CK_INFRA_PCIE_CK>,
			<&infracfg CK_INFRA_PWM_BCK>,
			<&infracfg CK_INFRA_PWM_CK1>,
			<&infracfg CK_INFRA_PWM_CK2>,
			<&infracfg CK_INFRA_133M_HCK>,
			<&infracfg CK_INFRA_66M_PHCK>,
			<&infracfg CK_INFRA_FAUD_L_CK	>,
			<&infracfg CK_INFRA_FAUD_AUD_CK>,
			<&infracfg CK_INFRA_FAUD_EG2_CK>,
			<&infracfg CK_INFRA_I2CS_CK>,
			<&infracfg CK_INFRA_MUX_UART0>,
			<&infracfg CK_INFRA_MUX_UART1>,
			<&infracfg CK_INFRA_MUX_UART2>,
			<&clk40m>,
			<&clk40m>,
			<&infracfg CK_INFRA_MUX_SPI0>,
			<&infracfg CK_INFRA_MUX_SPI1>,
			<&infracfg CK_INFRA_RTC_32K>,
			<&infracfg CK_INFRA_FMSDC_CK>,
			<&infracfg CK_INFRA_FMSDC_HCK_CK>,
			<&infracfg CK_INFRA_PERI_133M>,
			<&infracfg CK_INFRA_133M_PHCK>,
			<&infracfg CK_INFRA_USB_SYS_CK>,
			<&infracfg CK_INFRA_USB_CK>,
			<&infracfg CK_INFRA_USB_XHCI_CK>,
			<&infracfg CK_INFRA_PCIE_GFMUX_TL_O_PRE>,
			<&infracfg CK_INFRA_F26M_CK0>,
			<&infracfg_ao CK_INFRA_UART0_SEL>,
			<&infracfg_ao CK_INFRA_UART1_SEL>,	
			<&infracfg_ao CK_INFRA_UART2_SEL>,
			<&infracfg_ao CK_INFRA_SPI0_SEL>,
			<&infracfg_ao CK_INFRA_SPI1_SEL>,
			<&infracfg_ao CK_INFRA_PWM1_SEL>,
			<&infracfg_ao CK_INFRA_PWM2_SEL>,
			<&infracfg_ao CK_INFRA_PWM_BSEL>,
			<&infracfg_ao CK_INFRA_PCIE_SEL>,
			<&infracfg_ao CK_INFRA_GPT_STA>,
			<&infracfg_ao CK_INFRA_PWM_HCK>,
			<&infracfg_ao CK_INFRA_PWM_STA>,
			<&infracfg_ao CK_INFRA_PWM1_CK>,
			<&infracfg_ao CK_INFRA_PWM2_CK>,
			<&infracfg_ao CK_INFRA_CQ_DMA_CK>,
			<&clk40m>,
			<&clk40m>,
			<&clk40m>,
			<&clk40m>,
			<&clk40m>,
			<&infracfg_ao CK_INFRA_DRAMC_26M_CK>,
			<&clk40m>,
			<&infracfg_ao CK_INFRA_AP_DMA_CK>,
			<&infracfg_ao CK_INFRA_SEJ_CK>,
			<&infracfg_ao CK_INFRA_SEJ_13M_CK>,
			<&infracfg_ao CK_INFRA_THERM_CK>,
			<&infracfg_ao CK_INFRA_I2CO_CK>,
			<&infracfg_ao CK_INFRA_UART0_CK>,
			<&infracfg_ao CK_INFRA_UART1_CK>,
			<&infracfg_ao CK_INFRA_UART2_CK>,
			<&infracfg_ao CK_INFRA_SPI2_CK>,
			<&infracfg_ao CK_INFRA_SPI2_HCK_CK>,
			<&clk40m>,
			<&clk40m>,
			<&clk40m>,
			<&infracfg_ao CK_INFRA_SPI0_CK>,
			<&infracfg_ao CK_INFRA_SPI1_CK>,
			<&infracfg_ao CK_INFRA_SPI0_HCK_CK>,
			<&infracfg_ao CK_INFRA_SPI1_HCK_CK>,
			<&infracfg_ao CK_INFRA_FRTC_CK>,
			<&infracfg_ao CK_INFRA_MSDC_CK>,
			<&infracfg_ao CK_INFRA_MSDC_HCK_CK>,
			<&infracfg_ao CK_INFRA_MSDC_133M_CK>,
			<&infracfg_ao CK_INFRA_MSDC_66M_CK>,
			<&clk40m>,
			<&clk40m>,
			<&infracfg_ao CK_INFRA_FBIST2FPC_CK>,
			<&infracfg_ao CK_INFRA_I2C_MCK_CK>,
			<&infracfg_ao CK_INFRA_I2C_PCK_CK>,
			<&infracfg_ao CK_INFRA_IUSB_133_CK>,
			<&infracfg_ao CK_INFRA_IUSB_66M_CK>,
			<&infracfg_ao CK_INFRA_IUSB_SYS_CK>,
			<&infracfg_ao CK_INFRA_IUSB_CK>,
			<&infracfg_ao CK_INFRA_IPCIE_CK>,
			<&infracfg_ao CK_INFRA_IPCIER_CK>,
			<&infracfg_ao CK_INFRA_IPCIEB_CK>,
			<&topckgen CK_TOP_CB_M_416M>,
			<&topckgen CK_TOP_CB_M_D2>,
			<&topckgen CK_TOP_CB_M_D4>,
			<&topckgen CK_TOP_CB_M_D8>,
			<&topckgen CK_TOP_M_D8_D2>,
			<&topckgen CK_TOP_M_D3_D2>,
			<&topckgen CK_TOP_CB_MM_D2>,
			<&topckgen CK_TOP_CB_MM_D4>,
			<&topckgen CK_TOP_CB_MM_D8>,
			<&topckgen CK_TOP_CB_APLL2_196M>,
			<&topckgen CK_TOP_APLL2_D4>,
			<&topckgen CK_TOP_CB_NET1_D4>,
			<&topckgen CK_TOP_CB_NET1_D5>,
			<&topckgen CK_TOP_NET1_D5_D2>,
			<&topckgen CK_TOP_NET1_D5_D4>,
			<&topckgen CK_TOP_NET1_D8_D2>,
			<&topckgen CK_TOP_NET1_D8_D4>,
			<&clk40m>,
			<&topckgen CK_TOP_CB_NET2_D4>,
			<&topckgen CK_TOP_NET2_D4_D2>,
			<&topckgen CK_TOP_CB_WEDMCU_208M>,
			<&clk40m>,
			<&topckgen CK_TOP_CB_RTC_32K>,
			<&topckgen CK_TOP_CB_RTC_32P7K>,
			<&clk40m>,
			<&topckgen CK_TOP_USB_EQ_RX250M>,
			<&topckgen CK_TOP_USB_TX250M>,
			<&topckgen CK_TOP_USB_LN0_CK>,
			<&topckgen CK_TOP_USB_CDR_CK>,
			<&clk40m>,
			<&topckgen CK_TOP_I2C_BCK>,
			<&topckgen CK_TOP_PEXTP_TL>,
			<&topckgen CK_TOP_EMMC_208M>,
			<&topckgen CK_TOP_EMMC_400M>,
			<&topckgen CK_TOP_F26M_SEL>,
			<&topckgen CK_TOP_SYSAXI>,
			<&topckgen CK_TOP_NETSYS_WED_MCU>,
			<&topckgen CK_TOP_NETSYS_2X>,
			<&topckgen CK_TOP_SGM_325M>,
			<&topckgen CK_TOP_A1SYS>,
			<&topckgen CK_TOP_F26M>,
			<&topckgen CK_TOP_AUD_L>,
			<&topckgen CK_TOP_A_TUNER>,
			<&topckgen CK_TOP_U2U3_REF>,
			<&topckgen CK_TOP_U2U3_SYS>,
			<&topckgen CK_TOP_U2U3_XHCI>,
			<&topckgen CK_TOP_AP2CNN_HOST>,
			<&clk40m>,
			<&clk40m>,
			<&topckgen CK_TOP_UART_SEL>,
			<&topckgen CK_TOP_PWM_SEL>,
			<&topckgen CK_TOP_I2C_SEL>,
			<&topckgen CK_TOP_PEXTP_TL_SEL>,
			<&topckgen CK_TOP_EMMC_208M_SEL	>,
			<&topckgen CK_TOP_EMMC_400M_SEL	>,
			<&topckgen CK_TOP_F26M_SEL>,
			<&topckgen CK_TOP_DRAMC_SEL>,
			<&topckgen CK_TOP_DRAMC_MD32_SEL>,
			<&topckgen CK_TOP_SYSAXI_SEL>,
			<&topckgen CK_TOP_SYSAPB_SEL>,
			<&topckgen CK_TOP_ARM_DB_MAIN_SEL>,
			<&topckgen CK_TOP_AP2CNN_HOST_SEL>,
			<&topckgen CK_TOP_NETSYS_SEL>,
			<&topckgen CK_TOP_NETSYS_500M_SEL>,
			<&topckgen CK_TOP_NETSYS_MCU_SEL>,
			<&clk40m>,
			<&clk40m>,
			<&topckgen CK_TOP_SGM_REG_SEL>,
			<&topckgen CK_TOP_NETSYS_500M_SEL>,
			<&clk40m>,
			<&topckgen CK_TOP_USB3_PHY_SEL>,
			<&topckgen CK_TOP_F26M_SEL>,
			<&topckgen CK_TOP_U2U3_SEL>,
			<&topckgen CK_TOP_U2U3_SYS_SEL>,
			<&topckgen CK_TOP_U2U3_XHCI_SEL>,
			<&topckgen CK_TOP_USB_FRMCNT_SEL>;


		clock-names = "0", "1", "2", "3", "4", "5", "6", "7", "8", "9", "10", "11",
		"12", "13", "14", "15", "16", "17", "18", "19", "20", "21", "22", "23",
		"24", "25", "26", "27", "28", "29", "30", "31", "32", "33", "34", "35",
		"36", "37", "38", "39", "40", "41", "42", "43", "44", "45", "46", "47",
		"48", "49", "50", "51", "52", "53", "54", "55", "56", "57", "58", "59",
		"60", "61", "62", "63", "64", "65", "66", "67", "68", "69", "70", "71",
		"72", "73", "74", "75", "76", "77", "78", "79", "80", "81", "82", "83",
		"84", "85", "86", "87", "88", "89", "90", "91", "92", "93", "94", "95",
		"96", "97", "98", "99", "100", "101", "102", "103", "104", "105", "106", "107",
		"108", "109", "110", "111", "112", "113", "114", "115", "116", "117",
		"118", "119", "120", "121", "122", "123",
		"124", "125", "126", "127", "128", "129", "130", "131", "132", "133", "134", "135",
		"136", "137", "138", "139", "140", "141", "142", "143", "144", "145", "146", "147",
		"148", "149", "150", "151", "152", "153", "154", "155", "156", "157", "158", "159",
		"160", "161", "162", "163", "164", "165", "166", "167", "168", "169", "170", "171",
		"172", "173", "174", "175", "176", "177", "178", "179", "180", "181", "182", "183";
	};
};
