From: Russell King <rmk+kernel@armlinux.org.uk>
Date: Wed, 26 Feb 2020 10:23:41 +0000
Subject: [PATCH] net: phylink: propagate resolved link config via
 mac_link_up()

Propagate the resolved link parameters via the mac_link_up() call for
MACs that do not automatically track their PCS state. We propagate the
link parameters via function arguments so that inappropriate members
of struct phylink_link_state can't be accessed, and creating a new
structure just for this adds needless complexity to the API.

Tested-by: Andre Przywara <andre.przywara@arm.com>
Tested-by: Alexandre Belloni <alexandre.belloni@bootlin.com>
Tested-by: Vladimir Oltean <vladimir.oltean@nxp.com>
Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
Signed-off-by: David S. Miller <davem@davemloft.net>
---

--- a/Documentation/networking/sfp-phylink.rst
+++ b/Documentation/networking/sfp-phylink.rst
@@ -74,10 +74,13 @@ phylib to the sfp/phylink support.  Plea
 this documentation.
 
 1. Optionally split the network driver's phylib update function into
-   three parts dealing with link-down, link-up and reconfiguring the
-   MAC settings. This can be done as a separate preparation commit.
+   two parts dealing with link-down and link-up. This can be done as
+   a separate preparation commit.
 
-   An example of this preparation can be found in git commit fc548b991fb0.
+   An older example of this preparation can be found in git commit
+   fc548b991fb0, although this was splitting into three parts; the
+   link-up part now includes configuring the MAC for the link settings.
+   Please see :c:func:`mac_link_up` for more information on this.
 
 2. Replace::
 
@@ -207,6 +210,14 @@ this documentation.
    using. This is particularly important for in-band negotiation
    methods such as 1000base-X and SGMII.
 
+   The :c:func:`mac_link_up` method is used to inform the MAC that the
+   link has come up. The call includes the negotiation mode and interface
+   for reference only. The finalised link parameters are also supplied
+   (speed, duplex and flow control/pause enablement settings) which
+   should be used to configure the MAC when the MAC and PCS are not
+   tightly integrated, or when the settings are not coming from in-band
+   negotiation.
+
    The :c:func:`mac_config` method is used to update the MAC with the
    requested state, and must avoid unnecessarily taking the link down
    when making changes to the MAC configuration.  This means the
--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -3655,9 +3655,11 @@ static void mvneta_mac_link_down(struct
 	mvneta_set_eee(pp, false);
 }
 
-static void mvneta_mac_link_up(struct phylink_config *config, unsigned int mode,
-			       phy_interface_t interface,
-			       struct phy_device *phy)
+static void mvneta_mac_link_up(struct phylink_config *config,
+			       struct phy_device *phy,
+			       unsigned int mode, phy_interface_t interface,
+			       int speed, int duplex,
+			       bool tx_pause, bool rx_pause)
 {
 	struct net_device *ndev = to_net_dev(config->dev);
 	struct mvneta_port *pp = netdev_priv(ndev);
--- a/drivers/net/ethernet/marvell/mvpp2/mvpp2_main.c
+++ b/drivers/net/ethernet/marvell/mvpp2/mvpp2_main.c
@@ -58,8 +58,11 @@ static struct {
  */
 static void mvpp2_mac_config(struct phylink_config *config, unsigned int mode,
 			     const struct phylink_link_state *state);
-static void mvpp2_mac_link_up(struct phylink_config *config, unsigned int mode,
-			      phy_interface_t interface, struct phy_device *phy);
+static void mvpp2_mac_link_up(struct phylink_config *config,
+			      struct phy_device *phy,
+			      unsigned int mode, phy_interface_t interface,
+			      int speed, int duplex,
+			      bool tx_pause, bool rx_pause);
 
 /* Queue modes */
 #define MVPP2_QDIST_SINGLE_MODE	0
@@ -3468,8 +3471,9 @@ static void mvpp2_start_dev(struct mvpp2
 			.interface = port->phy_interface,
 		};
 		mvpp2_mac_config(&port->phylink_config, MLO_AN_INBAND, &state);
-		mvpp2_mac_link_up(&port->phylink_config, MLO_AN_INBAND,
-				  port->phy_interface, NULL);
+		mvpp2_mac_link_up(&port->phylink_config, NULL,
+				  MLO_AN_INBAND, port->phy_interface,
+				  SPEED_UNKNOWN, DUPLEX_UNKNOWN, false, false);
 	}
 
 	netif_tx_start_all_queues(port->dev);
@@ -5137,8 +5141,11 @@ static void mvpp2_mac_config(struct phyl
 	mvpp2_port_enable(port);
 }
 
-static void mvpp2_mac_link_up(struct phylink_config *config, unsigned int mode,
-			      phy_interface_t interface, struct phy_device *phy)
+static void mvpp2_mac_link_up(struct phylink_config *config,
+			      struct phy_device *phy,
+			      unsigned int mode, phy_interface_t interface,
+			      int speed, int duplex,
+			      bool tx_pause, bool rx_pause)
 {
 	struct mvpp2_port *port = mvpp2_phylink_to_port(config);
 	u32 val;
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -449,9 +449,10 @@ static void mtk_mac_link_down(struct phy
 	mtk_w32(mac->hw, mcr, MTK_MAC_MCR(mac->id));
 }
 
-static void mtk_mac_link_up(struct phylink_config *config, unsigned int mode,
-			    phy_interface_t interface,
-			    struct phy_device *phy)
+static void mtk_mac_link_up(struct phylink_config *config,
+			    struct phy_device *phy,
+			    unsigned int mode, phy_interface_t interface,
+			    int speed, int duplex, bool tx_pause, bool rx_pause)
 {
 	struct mtk_mac *mac = container_of(config, struct mtk_mac,
 					   phylink_config);
--- a/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
+++ b/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
@@ -925,8 +925,10 @@ static void stmmac_mac_link_down(struct
 }
 
 static void stmmac_mac_link_up(struct phylink_config *config,
+			       struct phy_device *phy,
 			       unsigned int mode, phy_interface_t interface,
-			       struct phy_device *phy)
+			       int speed, int duplex,
+			       bool tx_pause, bool rx_pause)
 {
 	struct stmmac_priv *priv = netdev_priv(to_net_dev(config->dev));
 
--- a/drivers/net/ethernet/xilinx/xilinx_axienet_main.c
+++ b/drivers/net/ethernet/xilinx/xilinx_axienet_main.c
@@ -1499,9 +1499,10 @@ static void axienet_mac_link_down(struct
 }
 
 static void axienet_mac_link_up(struct phylink_config *config,
-				unsigned int mode,
-				phy_interface_t interface,
-				struct phy_device *phy)
+				struct phy_device *phy,
+				unsigned int mode, phy_interface_t interface,
+				int speed, int duplex,
+				bool tx_pause, bool rx_pause)
 {
 	/* nothing meaningful to do */
 }
--- a/drivers/net/phy/phylink.c
+++ b/drivers/net/phy/phylink.c
@@ -447,8 +447,11 @@ static void phylink_mac_link_up(struct p
 	struct net_device *ndev = pl->netdev;
 
 	pl->cur_interface = link_state.interface;
-	pl->ops->mac_link_up(pl->config, pl->cur_link_an_mode,
-			     pl->cur_interface, pl->phydev);
+	pl->ops->mac_link_up(pl->config, pl->phydev,
+			     pl->cur_link_an_mode, pl->cur_interface,
+			     link_state.speed, link_state.duplex,
+			     !!(link_state.pause & MLO_PAUSE_TX),
+			     !!(link_state.pause & MLO_PAUSE_RX));
 
 	if (ndev)
 		netif_carrier_on(ndev);
--- a/include/linux/phylink.h
+++ b/include/linux/phylink.h
@@ -91,9 +91,10 @@ struct phylink_mac_ops {
 	void (*mac_an_restart)(struct phylink_config *config);
 	void (*mac_link_down)(struct phylink_config *config, unsigned int mode,
 			      phy_interface_t interface);
-	void (*mac_link_up)(struct phylink_config *config, unsigned int mode,
-			    phy_interface_t interface,
-			    struct phy_device *phy);
+	void (*mac_link_up)(struct phylink_config *config,
+			    struct phy_device *phy, unsigned int mode,
+			    phy_interface_t interface, int speed, int duplex,
+			    bool tx_pause, bool rx_pause);
 };
 
 #if 0 /* For kernel-doc purposes only. */
@@ -217,19 +218,34 @@ void mac_link_down(struct phylink_config
 /**
  * mac_link_up() - allow the link to come up
  * @config: a pointer to a &struct phylink_config.
+ * @phy: any attached phy
  * @mode: link autonegotiation mode
  * @interface: link &typedef phy_interface_t mode
- * @phy: any attached phy
+ * @speed: link speed
+ * @duplex: link duplex
+ * @tx_pause: link transmit pause enablement status
+ * @rx_pause: link receive pause enablement status
+ *
+ * Configure the MAC for an established link.
+ *
+ * @speed, @duplex, @tx_pause and @rx_pause indicate the finalised link
+ * settings, and should be used to configure the MAC block appropriately
+ * where these settings are not automatically conveyed from the PCS block,
+ * or if in-band negotiation (as defined by phylink_autoneg_inband(@mode))
+ * is disabled.
+ *
+ * Note that when 802.3z in-band negotiation is in use, it is possible
+ * that the user wishes to override the pause settings, and this should
+ * be allowed when considering the implementation of this method.
  *
- * If @mode is not an in-band negotiation mode (as defined by
- * phylink_autoneg_inband()), allow the link to come up. If @phy
- * is non-%NULL, configure Energy Efficient Ethernet by calling
+ * If in-band negotiation mode is disabled, allow the link to come up. If
+ * @phy is non-%NULL, configure Energy Efficient Ethernet by calling
  * phy_init_eee() and perform appropriate MAC configuration for EEE.
  * Interface type selection must be done in mac_config().
  */
-void mac_link_up(struct phylink_config *config, unsigned int mode,
-		 phy_interface_t interface,
-		 struct phy_device *phy);
+void mac_link_up(struct phylink_config *config, struct phy_device *phy,
+		 unsigned int mode, phy_interface_t interface,
+		 int speed, int duplex, bool tx_pause, bool rx_pause);
 #endif
 
 struct phylink *phylink_create(struct phylink_config *, struct fwnode_handle *,
--- a/net/dsa/port.c
+++ b/net/dsa/port.c
@@ -529,9 +529,11 @@ void dsa_port_phylink_mac_link_down(stru
 EXPORT_SYMBOL_GPL(dsa_port_phylink_mac_link_down);
 
 void dsa_port_phylink_mac_link_up(struct phylink_config *config,
+				  struct phy_device *phydev,
 				  unsigned int mode,
 				  phy_interface_t interface,
-				  struct phy_device *phydev)
+				  int speed, int duplex,
+				  bool tx_pause, bool rx_pause)
 {
 	struct dsa_port *dp = container_of(config, struct dsa_port, pl_config);
 	struct dsa_switch *ds = dp->ds;
