From: Joe Stefek <jstefek@datto.com>
Date: Tue, 15 Sep 2020 08:44:21 -0700
Subject: Drop regd patch which prevents changing reg domain on system with vdevs.

diff --git a/drivers/net/wireless/ath/ath11k/reg.c b/drivers/net/wireless/ath/ath11k/reg.c
index 03e2a5ca60dcde2173f1abf10d10d1648f0ba29d..b83d89c1af33073c25e2877557d947895ef9537d 100644
--- a/drivers/net/wireless/ath/ath11k/reg.c
+++ b/drivers/net/wireless/ath/ath11k/reg.c
@@ -41,37 +41,6 @@ static bool ath11k_regdom_changes(struct ath11k *ar, char *alpha2)
 	return memcmp(regd->alpha2, alpha2, 2) != 0;
 }
 
-static bool ath11k_reg_validate_pdev_state(struct ath11k* ar)
-{
-	struct ath11k_base *ab = ar->ab;
-	struct ath11k_pdev *pdev;
-	struct ath11k* tmp_ar;
-	int i;
-
-	rcu_read_lock();
-	for (i = 0; i < ab->num_radios; i++) {
-		pdev = rcu_dereference(ab->pdevs_active[i]);
-		if (!pdev)
-			continue;
-
-		tmp_ar = pdev->ar;
-		if (tmp_ar) {
-			mutex_lock(&tmp_ar->conf_mutex);
-			if (tmp_ar->num_started_vdevs) {
-				if (tmp_ar == ar)
-					ath11k_warn(ab, "%s has active interface, please bring down to set country code",
-						    wiphy_name(ar->hw->wiphy));
-				mutex_unlock(&tmp_ar->conf_mutex);
-				rcu_read_unlock();
-				return false;
-			}
-			mutex_unlock(&tmp_ar->conf_mutex);
-		}
-	}
-	rcu_read_unlock();
-	return true;
-}
-
 static void
 ath11k_reg_notifier(struct wiphy *wiphy, struct regulatory_request *request)
 {
@@ -105,13 +74,6 @@ ath11k_reg_notifier(struct wiphy *wiphy, struct regulatory_request *request)
 		return;
 	}
 
-	/* The SET_INIT_COUNTRY command should not be sent to firmware while any vdev is active.
-	 * Also it does not make sense to give the command for certain pdev's alone.
-	 * Hence check all the pdev's if any have an active vdev before sending the command.
-	 */
-	if (!ath11k_reg_validate_pdev_state(ar))
-		return;
-
 	/* Set the country code to the firmware and wait for
 	 * the WMI_REG_CHAN_LIST_CC EVENT for updating the
 	 * reg info
