From 6d4a858d6f7db2a86f6513a543feb8f7b8a8b4c1 Mon Sep 17 00:00:00 2001
From: "Mingming.Su" <Mingming.Su@mediatek.com>
Date: Wed, 30 Jun 2021 16:59:32 +0800
Subject: [PATCH] mt7986: trng: add rng support

1. Add trng compatible name for MT7986
2. Fix mtk_rng_wait_ready() function

Signed-off-by: Mingming.Su <Mingming.Su@mediatek.com>
---
 drivers/char/hw_random/mtk-rng.c | 5 +++--
 1 file changed, 3 insertions(+), 2 deletions(-)

diff --git a/drivers/char/hw_random/mtk-rng.c b/drivers/char/hw_random/mtk-rng.c
index e649be5a5..496adb0a0 100644
--- a/drivers/char/hw_random/mtk-rng.c
+++ b/drivers/char/hw_random/mtk-rng.c
@@ -22,7 +22,7 @@
 #define RNG_AUTOSUSPEND_TIMEOUT		100
 
 #define USEC_POLL			2
-#define TIMEOUT_POLL			20
+#define TIMEOUT_POLL			60
 
 #define RNG_CTRL			0x00
 #define RNG_EN				BIT(0)
@@ -77,7 +77,7 @@ static bool mtk_rng_wait_ready(struct hwrng *rng, bool wait)
 		readl_poll_timeout_atomic(priv->base + RNG_CTRL, ready,
 					  ready & RNG_READY, USEC_POLL,
 					  TIMEOUT_POLL);
-	return !!ready;
+	return !!(ready & RNG_READY);
 }
 
 static int mtk_rng_read(struct hwrng *rng, void *buf, size_t max, bool wait)
@@ -181,6 +181,7 @@ static UNIVERSAL_DEV_PM_OPS(mtk_rng_pm_ops, mtk_rng_runtime_suspend,
 #endif	/* CONFIG_PM */
 
 static const struct of_device_id mtk_rng_match[] = {
+	{ .compatible = "mediatek,mt7986-rng" },
 	{ .compatible = "mediatek,mt7623-rng" },
 	{},
 };
-- 
2.18.0

