--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -824,6 +824,16 @@ config LEDS_LM36274
 	  Say Y to enable the LM36274 LED driver for TI LMU devices.
 	  This supports the LED device LM36274.
 
+config LEDS_UBNT_LEDBAR
+	tristate "LED support for Ubiquiti UniFi 6 LR"
+	depends on LEDS_CLASS && I2C && OF
+	help
+	  This option enables support for the Ubiquiti LEDBAR
+	  LED driver.
+
+	  To compile this driver as a module, choose M here: the module
+	  will be called leds-ubnt-ledbar.
+
 comment "LED Triggers"
 source "drivers/leds/trigger/Kconfig"
 
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -85,6 +85,7 @@ obj-$(CONFIG_LEDS_LM3601X)		+= leds-lm36
 obj-$(CONFIG_LEDS_TI_LMU_COMMON)	+= leds-ti-lmu-common.o
 obj-$(CONFIG_LEDS_LM3697)		+= leds-lm3697.o
 obj-$(CONFIG_LEDS_LM36274)		+= leds-lm36274.o
+obj-$(CONFIG_LEDS_UBNT_LEDBAR)	+= leds-ubnt-ledbar.o
 
 # LED SPI Drivers
 obj-$(CONFIG_LEDS_CR0014114)		+= leds-cr0014114.o
