From b341f120cfc9ca1dfd48364b7f36ac2c1fbdea43 Mon Sep 17 00:00:00 2001
From: Xiangsheng Hou <xiangsheng.hou@mediatek.com>
Date: Wed, 3 Apr 2019 16:30:01 +0800
Subject: [PATCH 3/6] mtd: spinand: disable on-die ECC

Change-Id: I9745adaed5295202fabbe8ab8947885c57a5b847
Signed-off-by: Xiangsheng Hou <xiangsheng.hou@mediatek.com>
---
 drivers/mtd/nand/spi/core.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/mtd/nand/spi/core.c
+++ b/drivers/mtd/nand/spi/core.c
@@ -491,7 +491,7 @@ static int spinand_mtd_read(struct mtd_i
 	int ret = 0;
 
 	if (ops->mode != MTD_OPS_RAW && spinand->eccinfo.ooblayout)
-		enable_ecc = true;
+		enable_ecc = false;
 
 	mutex_lock(&spinand->lock);
 
@@ -539,7 +539,7 @@ static int spinand_mtd_write(struct mtd_
 	int ret = 0;
 
 	if (ops->mode != MTD_OPS_RAW && mtd->ooblayout)
-		enable_ecc = true;
+		enable_ecc = false;
 
 	mutex_lock(&spinand->lock);
 
