VERSION:621184076

8,i,[ wlan_swbmiss_offload.c : 492 ] wlan_bmiss_update_hwbmiss = %d 
7,iiiiiiii,[ wlan_swbmiss_offload.c : 639 ] SWBMISS_NULL_SEND_CMPLT: vdev_id=%d, isQosNullSuccess=%d, isFinalBmiss=%d, first_bmiss_detected=%d, final_bmiss_detected=%d, fbmiss_evnt_posted=%d, vbmiss->connected = %d, cons_bmiss_count = %d  
6,ii,[ wlan_swbmiss_offload.c : 510 ] SWBMISS_BCON_RECVED: vdev_id=%d, IS_HWBMISS=%d 
5,iiiiiii,[ wlan_swbmiss_offload.c : 947 ] SWBMISS_TIMER_FN: vdev_id=%d, curr_bmiss_bcnt=%d, pre_bmiss_detected=%d, first_bmiss_detected=%d, final_bmiss_detected=%d, b_timeout=%d, cons_bmiss_count = %d  
4,iIii,[ wlan_swbmiss_offload.c : 1132 ] SWBMISS_DELIVER_EVT: vdev_id=%d, evt_type=0x%x, bcn_rssi_avg=%d, bcn_rssi_last=%d 
3,iiIIiI,[ wlan_swbmiss_offload.c : 460 ] SWBMISS_DISABLED: vdev_id=%d, module_id=%d, bmiss_disable_bitmap_63_32=0x%x, bmiss_disable_bitmap_31_0=0x%x, curr_bmiss_bcnt=%d, cur_disable_bitmask=0x%x 
2,iiIIii,[ wlan_swbmiss_offload.c : 417 ] SWBMISS_ENABLED: vdev_id=%d, module_id=%d, bmiss_disable_bitmap_63_32=0x%x, bmiss_disable_bitmap_31_0=0x%x, curr_bmiss_bcnt=%d, final_bmiss_detected=%d 
1,ii,[ wlan_swbmiss_offload.c : 569 ] SWBMISS_TIMER_SET: vdev_id=%d, timeout_val=%d 
0,iiii,[ wlan_swbmiss_offload.c : 1198 ] SWBMISS_VDEV_EVT: vdev_id=%d, mac id %d notif=%d , HBMISS %d  
74,,[ wlan_dev.c : 7637 ] WMI_PDEV_SET_WMM_PARAMS_CMDID DEPRECATED - use VDEV level command instead 
73,,[ wlan_dev.c : 7840 ] wlan_pdev_resume_cmd: NOT expected to receive during wifi on 
72,i,[ wlan_dev.c : 7853 ] wlan_pdev_resume_cmd: NOT expected to receive during wifi on, mac id=%d 
71,,[ wlan_dev.c : 8073 ] WMI_REQUEST_LINK_STATS_CMDID, ftm mode 
70,iII,[ wlan_dev.c : 8203 ] WMI_LRO_CONFIG_CMDID 1 mac=%d en=%x flags=%x 
69,i,[ wlan_dev.c : 8409 ] WMI_PDEV_SMART_ANT_ENABLE_CMDID  gpio_handler_num : %d 
68,i,[ wlan_dev.c : 8439 ] WMI_PDEV_SMART_ANT_ENABLE_CMDID loop number : %d 
67,i,[ wlan_dev.c : 8650 ] BSS_CHAN_INFO_CMD_RCVD mac_id:%d 
66,IIII,[ wlan_dev.c : 8831 ] WMI_GPIO_CONFIG_CMDID: %x %x %x %x 
65,II,[ wlan_dev.c : 8901 ] WMI_GPIO_OUTPUT_CMDID: %x %x 
64,II,[ wlan_dev.c : 7247 ] smart_ant_gpio_handler smart_gpio_cfg.gpio_num :%x, smart_gpio_cfg.func: %x 
63,iiii,[ wlan_dev.c : 2745 ] To serve %d peers %d TIDs is enough (TQM TIDs = %d, TQM BYPASS TIDs = %d) 
62,iiii,[ wlan_dev.c : 2752 ] To serve %d peers %d TIDs required (TQM TIDs = %d, TQM BYPASS TIDs = %d) 
61,ii,[ wlan_dev.c : 6443 ] wlan_dev_set_pcl not match pcl_cnt=%d,supp_chan_cnt=%d 
60,iii,[ wlan_dev.c : 6469 ] wlan_dev_set_pcl: cur_category %d: num_chans_in_category %d -> cur_idx %d 
59,i,[ wlan_dev.c : 6477 ] wlan_dev_set_pcl: num_chans=%d 
58,i,[ wlan_dev.c : 9279 ] unit_test: sleep for %d ms 
57,I,[ wlan_dev.c : 9301 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_TX_CHAIN_MASK, value=0x%x 
56,I,[ wlan_dev.c : 9310 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_RX_CHAIN_MASK, value=0x%x 
55,I,[ wlan_dev.c : 9320 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_TX_CHAIN_MASK_2G, value=0x%x 
54,I,[ wlan_dev.c : 9330 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_RX_CHAIN_MASK_2G, value=0x%x 
53,I,[ wlan_dev.c : 9340 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_TX_CHAIN_MASK_5G, value=0x%x 
52,I,[ wlan_dev.c : 9350 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_RX_CHAIN_MASK_5G, value=0x%x 
51,ii,[ wlan_dev.c : 9360 ] wlan_dev_unit_test: cca_busy_detector_config time_diff_threshold = %d us, cca_busy_percent_threshold = %d 
50,I,[ wlan_dev.c : 9288 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_ABG_MODE_TX_CHAIN_NUM, value = 0x%x 
49,iiii,[ wlan_dev.c : 411 ] GreenAP Curr Chainmask: %d/%d, Phy_mode: %d, bw[20/40/80/160]: %d 
48,iiiii,[ wlan_dev.c : 413 ] GreenAP saved tx/rx chainmask: %d/%d, phymode: %d, freq1: %d, valid flag: %d 
47,iii,[ wlan_dev.c : 415 ] GreenAP cur_channel mhz: %d, freq1: %d, freq2: %d 
46,,[ wlan_dev.c : 3272 ] phymode_param Received multi-vdev command 
45,iii,[ wlan_dev.c : 3352 ] Update Stream: vdev_id=%d preferred_tx_stream = %d preferred_rx_stream = %d 
44,ii,[ wlan_dev.c : 3360 ] phymode_param: applying phymode=%d for vdev at index %d 
43,IIi,[ wlan_dev.c : 9797 ] wlan_pdev_get_hw_mode_transition_event: old_hw_idx=0x%x, new_hw_idx=0x%x, vdev_num=%d 
42,ii,[ wlan_dev.c : 10362 ] wlan_pdev_handle_get_channel_ani_cmd max_channel_limit %d, received_count %d 
41,i,[ wlan_dev.c : 10374 ] wlan_pdev_handle_get_channel_ani_cmd memory allocation failed, %d 
40,iii,[ wlan_dev.c : 10406 ] wlan_pdev_handle_get_channel_ani_cmd freq:%d, mac_id:%d, ani:%d 
39,i,[ wlan_dev.c : 10410 ] wlan_pdev_handle_get_channel_ani_cmd unsupported freq:%d 
38,iiiI,[ wlan_dev.c : 6857 ] pdev_id = %d: DMA %d push config status %d event %p 
37,i,[ wlan_dev.c : 2362 ] BSS_CHAN_INFO_EVENT_SENT mac_id:%d 
36,ii,[ wlan_dev.c : 431 ] GreenAP wlan_pdev_set_greenap_cmd enable: %d, zero_client:%d 
35,I,[ wlan_dev.c : 6525 ] wlan_pdev_set_hw_mode: HW_Mode_Idx = 0x%x 
34,I,[ wlan_dev.c : 6550 ] wlan_pdev_set_hw_mode: DBSMGR_Ret_Status = 0x%x 
33,,[ wlan_dev.c : 6695 ] wlan_pdev_set_hw_mode_resp_event: WMI Event Alloc Failed!!! 
32,II,[ wlan_dev.c : 6735 ] wlan_pdev_set_hw_mode_resp_event: status=0x%x, cfg_hw_mode_idx=0x%x 
31,,[ wlan_dev.c : 6604 ] WMI_PDEV_SET_MAC_CONFIG_RESP_EVENT: WMI Event Alloc Failed!!! 
30,I,[ wlan_dev.c : 6621 ] WMI_PDEV_SET_MAC_CONFIG_RESP_EVENT: status=0x%x 
29,I,[ wlan_dev.c : 3698 ] wlan_pdev_set_param: WMI_PDEV_PARAM_TX_CHAIN_MASK 0x%x 
28,I,[ wlan_dev.c : 3727 ] wlan_pdev_set_param: WMI_PDEV_PARAM_TX_CHAIN_MASK 0x%x not valid 
27,I,[ wlan_dev.c : 3760 ] wlan_pdev_set_param: WMI_PDEV_PARAM_RX_CHAIN_MASK 0x%x 
26,I,[ wlan_dev.c : 3783 ] wlan_pdev_set_param: WMI_PDEV_PARAM_RX_CHAIN_MASK 0x%x not valid 
25,,[ wlan_dev.c : 4670 ] PDEV_PARAM_RX_FILTER not supported 
24,I,[ wlan_dev.c : 4847 ] PDEV_PARAM_IOT_PATTERN=%08x 
23,,[ wlan_dev.c : 4962 ] PDEV_PARAM_GCMP_SUPPORT_ENABLE not handled in FW 
22,,[ wlan_dev.c : 7068 ] WMI_PDEV_UPDATE_PKT_ROUTING_CMDID SOC level command not valid
 
21,ii,[ wlan_dev.c : 3174 ] wlan_resync_imps: IMPS_ENABLED=%d, VDEV_UP_COUNT=%d 
20,,[ wlan_dev.c : 10180 ] DISPLAY_TPC_STATS:  Alloc tpc_configs_reg_event_buf failed
 
19,,[ wlan_dev.c : 10204 ] DISPLAY_TPC_STATS:  Alloc tgt_pwrs_event_buf failed
 
18,,[ wlan_dev.c : 10232 ] DISPLAY_TPC_STATS:  Alloc tgt_pwrs_set2_event_buf failed
 
17,,[ wlan_dev.c : 10261 ] DISPLAY_TPC_STATS:  Alloc ctl_event_buf failed
 
16,,[ wlan_dev.c : 10270 ] DISPLAY_TPC_STATS:  Allocation complete! 
15,,[ wlan_dev.c : 10720 ] ANI - Memory Allocation fail 
14,,[ wlan_dev.c : 10742 ] ANI - Invalid PDEV_ID 
13,i,[ wlan_dev.c : 10744 ] ANI - CCK_level=%d 
12,,[ wlan_dev.c : 10679 ] ANI - Memory Allocation fail 
11,,[ wlan_dev.c : 10701 ] ANI - Invalid PDEV_ID 
10,i,[ wlan_dev.c : 10703 ] ANI - OFDM_level=%d 
9,II,[ wlan_dev.c : 6194 ] WMI: WMI_PDEV_GET_DPD_STATUS_EVENTID pdev_id %ld ev->dpd_status %ld 
148,,[ wlan_peer.c : 5765 ] Invalid sta_fixed_rate: Found CCK rate in 5G
 
147,,[ wlan_peer.c : 5782 ] Invalid sta_fixed_rate: Found CCK rate in 5G
 
146,IIIIIIII,[ wlan_peer.c : 5877 ] WMI_PEER_PARAM_DISABLE_AGGRESSIVE_TX:peer %x value %x mac_address %x:%x:%x:%x:%x:%x 
145,,[ wlan_peer.c : 6324 ] PEER_CHAN_WIDTH null vdev 
144,IIi,[ wlan_peer.c : 6349 ] Invalid CHAN_WIDTH_SWITCH: mac_addr31to0 = 0x%x, mac_addr47to32 = 0x%x, phy_mode %d 
143,iIiiI,[ wlan_peer.c : 6361 ] Invalid CHAN_WIDTH_SWITCH:peer_id = %d  chan_width =0x%X, new_phy_mode= %d old_phy_mode = %d he_mcs_nss_160=0x%x 
142,iIiiI,[ wlan_peer.c : 6367 ] Invalid CHAN_WIDTH_SWITCH:peer_id = %d  chan_width =0x%X, new_phy_mode= %d old_phy_mode = %d he_mcs_nss_80_80=0x%x 
141,iiIIiiII,[ wlan_peer.c : 5062 ] WLAN_PEER_ASSOC_REQ peer %d peer_assoc_evt %d, ni_flags 0x%x, valid_tx_chainmask 0x%x, peer_nss %d, phymode %d, ni_vht_mcs_set 0x%x, ni_legacy_rate_set 0x%x, 
140,ii,[ wlan_peer.c : 5082 ] WLAN_PEER_CHANGE_BW peerid %d  bw %d 
139,iii,[ wlan_peer.c : 5116 ] WLAN_PEER_CHANGE_NSS peer %d  peer_nss %d ul_nss %d 
138,ii,[ wlan_peer.c : 5149 ] WLAN_PEER_CHANGE_PHY_MODE peer %d  bw %d 
137,iIIiiII,[ wlan_peer.c : 5177 ] WLAN_PEER_CHANGE_CHAN_WIDTH peer %d ni_flags 0x%x, valid_tx_chainmask 0x%x, peer_nss %d, phymode %d, ni_vht_mcs_set 0x%x, ni_legacy_rate_set 0x%x, 
136,iIIiiI,[ wlan_peer.c : 555 ] RESOURCE_PEER_ALLOC duplicate PEER_TYPE_BSS vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x mac_id = %d/%d peer=0x%x 
135,iIIIi,[ wlan_peer.c : 645 ] wal peer allocaton status = %d vdev_id_8/mac_id_8 = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x peer_type = %d 
134,iIIIi,[ wlan_peer.c : 668 ] wal peer allocaton status = %d vdev_id_8/mac_id_8 = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x peer_type = %d 
133,,[ wlan_peer.c : 261 ] wlan_find_peer: NULL vdev 
132,iIIi,[ wlan_peer.c : 871 ] VDEV EVT:RESOURCE_PEER_FREE vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d 
131,iI,[ wlan_peer.c : 956 ] VDEV EVT PEER: wlan_free_peer del_resp=%d, wal_peer:0x%x 
130,iI,[ wlan_peer.c : 2580 ] HE160NSS : 160_mcs_nss_set %d, 160_mcs_nss_map %x 
129,II,[ wlan_peer.c : 6834 ] Deauth frame is not sent because of different RT thread addr1 0x%x addr2 = 0x%x 
128,I,[ wlan_peer.c : 5010 ] wlan_peer_mask_cck_rates_internal:wlan_peer 0x%x 
127,,[ wlan_peer.c : 2855 ] rc_node_update: ABORT 
126,III,[ wlan_peer.c : 2497 ] Assoc OMI: NSS=0x%x BW=0x%x er_su_disable=0x%x 
125,iiIIii,[ wlan_peer.c : 1703 ] peer_update status=%d,vdevid=%d,macaddr=0x%8x0x%4x peer_type=%d,req_peer_type=%d
 
124,IIII,[ wlan_peer.c : 4684 ] wal_vdev non_data_rc:0x%x bcast_data_rc:0x%x mcast_data_rc:0x%x beacon_rc:0x%x 
 
123,II,[ wlan_peer.c : 4758 ] update rts_rix, peer:0x%x, rts_rix:0x%x 
122,I,[ wlan_peer.c : 4706 ] wal_peer: %x, wlan_peer_vdev_restart_done: tearing down tx_ba and rx_ba 
121,II,[ wlan_peer.c : 4721 ] update non data1, peer:0x%x, rc:0x%x 
120,i,[ wlan_peer.c : 5243 ] WMI_PEER_UNMAP_RESPONSE_CMDID: %d 
119,ii,[ wlan_peer.c : 5250 ] peer_id[%d]: %d 
118,I,[ wlan_peer.c : 2257 ] wlan_set_peer_he_txbf_cap:ax_txbf_caps.suax_max_nc=%x 
117,I,[ wlan_peer.c : 1424 ] wlan_set_peer_vht_txbf_cap vht_caps: %x 
116,III,[ wlan_peer.c : 1455 ] Nr=%x Nrx=%x, Nc=%x
 
115,IIII,[ wlan_peer.c : 1529 ] Nr=%x Nc=%x peer_nss=%x Ntx=%x 
114,iIIiii,[ wlan_peer.c : 470 ] RESOURCE_PEER_ALLOC error vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d, peer_type = %d, delete_in_process:%d 
113,Iii,[ wlan_peer.c : 6620 ] wlan_vdev_delete_all_peer_conf_msg_hdlr: wal_vdev=%p, delete_all_peer_in_progress=%d, WLAN_FW_THREAD_IS_RT=%d 
 
112,i,[ wlan_peer.c : 6625 ] wlan_vdev_delete_all_peer_conf_msg_hdlr: vdev_id=%d 
 
111,ii,[ wlan_peer.c : 6686 ] veriware wlan_vdev_delete_all_peer_conf_msg_hdlr: vdev_id=%d dbg_conf_del_all_peer_num = %d 
 
110,i,[ wlan_peer.c : 2076 ] delete_all_peer: WMI_VDEV_DELETE_ALL_PEER_CMDID command for vdev_id %d 
 
109,,[ wlan_peer.c : 2079 ] DELETE_ALL_PEER max vdev 
108,,[ wlan_peer.c : 2086 ] DELETE_ALL_PEER null vdev 
107,,[ wlan_peer.c : 2100 ] DELETE_ALL_PEER alredy in progress 
106,,[ wlan_peer.c : 2143 ] DELETE_ALL_PEER No active peer 
105,,[ wlan_peer.c : 3002 ] PEER_ASSOC null vdev 
104,,[ wlan_peer.c : 3014 ] PEER_ASSOC null peer 
103,,[ wlan_peer.c : 3016 ] PEER_ASSOC null wal_peer 
102,iiIIi,[ wlan_peer.c : 3132 ] PEER_ASSOC Overridding phymode. Orig phy %d, new phy %d. Orig flag 0x%x, new flag 0x%x. Error:%d 
101,IIiIIIii,[ wlan_peer.c : 3278 ] PEER_ASSOC cmd for mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x, num_peer_ht_rates=%d, ni_flags=0x%x phymode=0x%x nss=0x%x mpdudensity=%d max_mpdu=%d 
100,IIIII,[ wlan_peer.c : 3304 ] PEER_ASSOC ni_legacy_rate_set= 0x%x ht_caps=0x%x vht_caps=0x%x vht_mcs_set=0x%x ht_mcs_set= 0x%x 
99,I,[ wlan_peer.c : 3483 ] Peer_assoc:peer_he_cap_phy = 0x%x 
98,II,[ wlan_peer.c : 3489 ] Peer_assoc: he_ops=0x%x he_cap_info_internal=0x%x 
97,,[ wlan_peer.c : 3688 ] PEER_ASSOC Sending KO for STA as invalid phymode config 
96,IIIII,[ wlan_peer.c : 4248 ] wlan_vdev_dispatch_peer_change_bw:prev_ni_flags=%x new_ni_flags=%x new_bw = %x ht_caps = %x vht_caps = %x 
95,iII,[ wlan_peer.c : 1743 ] peer create cmd ingored vdev_id =%d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
 
94,II,[ wlan_peer.c : 1840 ]  DFS nol protection peer create cmd ingored mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x  
 
93,II,[ wlan_peer.c : 1851 ] peer create command for mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
 
92,iII,[ wlan_peer.c : 1994 ] peer delete command for vdev_id %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
91,,[ wlan_peer.c : 2007 ] PEER_DELETE null vdev 
90,,[ wlan_peer.c : 2014 ] PEER_DELETE parent vdev delete_all_peer_in_progress 
89,,[ wlan_peer.c : 2039 ] PEER_DELETE peer not exist, still generating PEER_DELETE_RESP_EVENTID 
88,IIII,[ wlan_peer.c : 4652 ] wlan_vdev_dispatch_peer_mask_cck_rates is-2g:0x%x rc_node:0x%x legacy_rate:0x%x  is_cck_rate_mask 0x%x 
87,i,[ wlan_peer.c : 3954 ] RATE_DBG wlan_vdev_migrate_rate_reset peer_params NULL: peer_id %d 
86,i,[ wlan_peer.c : 3959 ] RATE_DBG wlan_vdev_migrate_rate_reset: peer_id %d 
85,I,[ wlan_peer.c : 3919 ] wlan_vdev_peer_autorate_reset: user_start_rate 0x=%x 
84,I,[ wlan_peer.c : 4114 ] wlan_vdev_peer_change_bw_internal: new_bw = %x 
83,iI,[ wlan_peer.c : 4054 ] wlan_vdev_peer_change_phymode_internal: peerid %d phymode = %x 
82,I,[ wlan_peer.c : 4990 ] wlan_vdev_peer_mimo_ps_internal: valid_tx_chainmask 0x=%x 
81,II,[ wlan_peer.c : 4319 ] TXBF_UPDATE_PEER_PARAMS peer_nss = %u, nc_idx = %u. 
80,II,[ wlan_peer.c : 4328 ] TXBF_UPDATE_PEER_PARAMS peer_nss_160 = %u, nc_idx_160 = %u. 
79,iii,[ wlan_peer.c : 831 ] delete_all_peer: VDEV EVT:WMI_VDEV_DELETE_ALL_PEER_RESP_EVENTID vdevId=%d status=%d time=%d 
78,,[ wlan_peer.c : 783 ] WMI_EVENT_ALLOC_FAILURE: WMI_PEER_DELETE_RESP_EVENTID buffer failure 
77,iiII,[ wlan_peer.c : 799 ] VDEV EVT:WMI_PEER_DELETE_RESP_EVENTID send vdevId=%d time=%d peer_macaddr31to0 =0x%x peer_macaddr47to32 =0x%x 
76,,[ wlan_peer.c : 5275 ] WMI_PEER_TX_PN_REQUEST :  Invalid Peer 
75,ii,[ wlan_peer.c : 5284 ] WMI_PEER_TX_PN_REQUEST : vdev_id = %d, key_type = %d   
171,IIIII,[ wlan_mgmt_local_txrx.c : 2206 ] _wlan_local_send_peer_change_omi()invalid rx=0x%x bw=0x%x ulmu=0x%x tx=0x%x ulmu_data=0x%x
 
170,I,[ wlan_mgmt_local_txrx.c : 2221 ] _wlan_local_send_peer_change_omi()newOMI=0x%x 
169,III,[ wlan_mgmt_local_txrx.c : 1590 ] mac id mismatch:rx:%x vdev:%x, frame: %x
 
168,III,[ wlan_mgmt_local_txrx.c : 1734 ] mac id mismatch:rx:%x vdev:%x, frame: %x
 
167,,[ wlan_mgmt_local_txrx.c : 1797 ] IEEE80211_FC0_SUBTYPE_NDPA 
166,,[ wlan_mgmt_local_txrx.c : 408 ] SCAN_RADIO_SUPPORT_DBUG _wlan_mgmt_local_send cur_channel NULL 
165,ii,[ wlan_mgmt_local_txrx.c : 627 ] MGMT_TXRX_SENT_FROM_LOCAL: send failure:%d, flags:%d 
164,i,[ wlan_mgmt_local_txrx.c : 417 ] SCAN_RADIO_SUPPORT_DBUG: _wlan_mgmt_local_send DFS channel = %d Detected Skipping...
 
163,IIIIIiII,[ wlan_mgmt_local_txrx.c : 520 ] MGMT_TXRX_SENT_FROM_LOCAL: macidh8/tid8/ptype16:0x%08x, cbflags=0x%08x, peerflag=0x%x,addr=0x%08x 0x%04x cur_chan=%d ppdu_H32=0x%x ppdu_L32=0x%x 
162,I,[ wlan_mgmt_local_txrx.c : 2062 ] LOCAL MGMT DEAUTH-DISASSOC tx compl. status 0x%x 
161,IiI,[ wlan_mgmt_local_txrx.c : 898 ] _wlan_mgmt_local_send_nullfunc() get nullfunc failed: peer = %p peer_type = %d cb_flags: 0x%x 
160,IIIII,[ wlan_mgmt_local_txrx.c : 661 ] OMI: wlan_mgmt_txrx_send_omi rx_nss: 0x%lx, bw: 0x%lx, ulmu_disable: 0x%lx, ulmu_data_disable: 0x%lx, tx_nss: 0x%lx
 
159,IIIIIIiii,[ wlan_mgmt_local_txrx.c : 1391 ] MGMT_TXRX_FORWARD_TO_HOST: mgmt pkt, Ch_VdevActCnt_ToHost=0x%08x MacId_Type_Subtype=0x%06x Seq=%04d(0x%03x) Addr2=0x%04x 0x%08x RssiComb=%d Chain0=%d Chain1=%d 
158,i,[ wlan_mgmt_local_txrx.c : 1394 ] MGMT_TXRX_FORWARD_TO_HOST: mgmt pkt,sta_mon_mode=%d 
157,IIiIiii,[ wlan_mgmt_local_txrx.c : 1422 ] MGMT_TXRX_FORWARD_TO_HOST: not mgmt pkt, Ch_VdevActCnt_ToHost=0x%08x MacId_Type_Subtype=0x%06x Seq=%d(0x%x) RssiComb=%d Chain0=%d Chain1=%d 
156,i,[ wlan_mgmt_local_txrx.c : 1425 ] MGMT_TXRX_FORWARD_TO_HOST: mgmt pkt,sta_mon_mode=%d 
155,i,[ wlan_mgmt_local_txrx.c : 649 ] wlan_mgmt_txrx_omi_req_completion: set mu  as %d
 
154,II,[ wlan_mgmt_local_txrx.c : 707 ] setUnitTestCmd 13 9 1 %x %x - couldn't find peer! 
153,IIIIiI,[ wlan_mgmt_local_txrx.c : 718 ] OMI: Unit test with rx_nss = 0x%lx, bw = 0x%lx, ulmu disable = 0x%lx, tx_nss = 0x%lx, er_su disable %d, ulmu_data_disable = 0x%lx
 
152,,[ wlan_mgmt_local_txrx.c : 722 ] Invalid input for OMI unit test.
 
151,,[ wlan_mgmt_local_txrx.c : 776 ] Invalid input for muedca unit test to set mu wmm params.
 
150,,[ wlan_mgmt_local_txrx.c : 808 ] Invalid input for muedca unit test to emulate trigger frm.
 
149,I,[ wlan_mgmt_local_txrx.c : 818 ] Unit test: mu edca enable = %lu
 
201,I,[ wlan_mgmt_txrx.c : 1435 ] QOS_NULL_TX_WMI_FROM_HOST: Host is not expected to use this command other than QoS null, frame subtype = 0x%X  
200,IIIi,[ wlan_mgmt_txrx.c : 1484 ] QOS_NULL_TX_WMI_FROM_HOST subtype=0x%02x addr=0x%04x%08x chanfreq=%d  
199,iiIiI,[ wlan_mgmt_txrx.c : 1489 ] QOS_NULL_TX_WMI_FROM_HOST tx_param_valid=%d  frame_len=%d  desc_id=0x%x tid_num=%d ppdu_info=0x%x 
198,iIiI,[ wlan_mgmt_txrx.c : 1539 ] QOS_NULL_TX_WMI_FROM_HOST FAIL invalid input param vdev_id=%d, vdev_opmode=%x, desc_id=%d peer =0x%X   
197,I,[ wlan_mgmt_txrx.c : 1443 ] QOS_NULL_TX_WMI_FROM_HOST: Command is expected only for AP VDEV wlan_vdev->ic_opmode= 0x%X  
196,I,[ wlan_mgmt_txrx.c : 1452 ] QOS_NULL_TX_WMI_FROM_HOST: Expected wlan peer value = 0x%X  
195,IIi,[ wlan_mgmt_txrx.c : 400 ] _wlan_mgmt_rx_frame_handler Droping frame from non associated Peer type=0x%x subtype=0x%x bNull=%d 
194,,[ wlan_mgmt_txrx.c : 2351 ] SCAN_RADIO_SUPPORT_DBUG WMI_SCAN_EVENT_FOREIGN_CHANNEL_ENTRY pmac NULL 
193,,[ wlan_mgmt_txrx.c : 2357 ] SCAN_RADIO_SUPPORT_DBUG WMI_SCAN_EVENT_FOREIGN_CHANNEL_ENTRY cur_channel NULL 
192,ii,[ wlan_mgmt_txrx.c : 2384 ] SCAN_RADIO_SUPPORT_DBUG WMI_SCAN_EVENT_FOREIGN_CHANNEL_ENTRY DFS_Flag = %d channel = %d 
191,IIii,[ wlan_mgmt_txrx.c : 1661 ] MGMT_TX_WMI_FROM_HOST is_home_8/is_curr_8=0x%x mode_8/submode_8=0x%x pmac->mac_id=%d e_mac_id=%d 
190,IIIi,[ wlan_mgmt_txrx.c : 1742 ] MGMT_TX_WMI_FROM_HOST subtype=0x%02x addr=0x%04x%08x chanfreq=%d 
189,iiIiIIiI,[ wlan_mgmt_txrx.c : 1747 ] MGMT_TX_WMI_FROM_HOST check_tag=%d tx_param_valid=%d cmd_ch=0x%x frame_len=%d tx_flags=0x%x desc_id=0x%x tid_num=%d ppdu_info=0x%x 
188,,[ wlan_mgmt_txrx.c : 1819 ] Dropping CFR capture 
187,ii,[ wlan_mgmt_txrx.c : 2501 ] MGMT_TX_WMI_FROM_HOST register %d %d 
186,ii,[ wlan_mgmt_txrx.c : 2506 ] MGMT_TX_WMI_FROM_HOST register %d %d 
185,ii,[ wlan_mgmt_txrx.c : 2512 ] MGMT_TX_WMI_FROM_HOST register %d %d 
184,iii,[ wlan_mgmt_txrx.c : 2228 ] WMI TX comp hold,idx:%d, desc id=%d,comp=%d 
183,I,[ wlan_mgmt_txrx.c : 1886 ] WMI TX comp send bundle: bundle_evt_size:0x%x 
182,iii,[ wlan_mgmt_txrx.c : 1951 ] WMI TX comp send bundle, num:%d, desc id=%d comp=%d 
181,,[ wlan_mgmt_txrx.c : 2057 ] MGMT_TX_WMI_TXCOMP_SEND_EVT PKT NULL 
180,,[ wlan_mgmt_txrx.c : 2063 ] MGMT_TX_WMI_TXCOMP_SEND_EVT PKT NULL 
179,IIii,[ wlan_mgmt_txrx.c : 2107 ] MGMT_TX_WMI_FROM_HOST_COMP desc_id=0x%x tx_status=0x%x ppdu_id:%d ack_rssi=%d 
178,I,[ wlan_mgmt_txrx.c : 996 ] WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x 
177,I,[ wlan_mgmt_txrx.c : 909 ] WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x 
176,,[ wlan_mgmt_txrx.c : 1966 ] OFFCHAN_DATA_TX_WMI_TXCOMP_SEND_EVT PKT NULL 
175,II,[ wlan_mgmt_txrx.c : 1982 ] MGMT_TX_WMI_FROM_HOST_COMP desc_id=0x%x tx_status=0x%x 
174,,[ wlan_mgmt_txrx.c : 2001 ]  QOS_NULL_TX_WMI_FROM_HOST PKT NULL 
173,IIIII,[ wlan_mgmt_txrx.c : 2020 ] QOS_NULL_TX_WMI_FROM_HOST Send Evt: desc_id = 0x%x comp_type=0x%x,pdev_id =0x%X, ppdu_id=0x%X ack_rssi =0x%X 
172,IIIII,[ wlan_mgmt_txrx.c : 1349 ] MGMT_TX_WMI_FROM_HOST: dword0=0x%x dword1=0x%x, subtype:%x, ppdu_info:0x%x multiplier:0x%x 
243,iii,[ offload_mgr.c : 1954 ] OFLD drop wmi evt, id=%d, len:%d status:%d 
242,ii,[ offload_mgr.c : 342 ] OFLD dereg data name=%d vdev id=%d, vdev mask 
241,ii,[ offload_mgr.c : 384 ] OFLD dereg htt name=%d ref_cnt=%d 
240,ii,[ offload_mgr.c : 322 ] OFLD dereg nondata name=%d ref_cnt=%d 
239,ii,[ offload_mgr.c : 363 ] OFLD dereg wmi name=%d ref_cnt=%d 
238,,[ offload_mgr.c : 1245 ] drop data in wow awake 
237,I,[ offload_mgr.c : 1264 ] OFLD remote data hdlr dropping frame as L2_valid :%x 
236,II,[ offload_mgr.c : 1280 ] OFLD remote data hdlr ds2ds, id:%x, mode:%x 
235,II,[ offload_mgr.c : 1287 ] OFLD remote data hdlr nonds, id:%x, mode:%x 
234,iiii,[ offload_mgr.c : 1296 ] OFLD remote data hdlr pktlen=%d, dataT=%d addrT=%d vdevId=%d 
233,iii,[ offload_mgr.c : 1359 ] OFLD enhanced data hdlr ofld id=%d status=%d, wow data state:%d 
232,I,[ offload_mgr.c : 2006 ] evt store:%x 
231,III,[ offload_mgr.c : 1667 ] offldmgr_non_data_handler: Received rx buf as null for peer = 0x%x  mac_id =0x%X rxbuf =0x%X 
230,III,[ offload_mgr.c : 1741 ] _offldmgr_non_data_handler: peer = 0x%x addr1 0x%x addr2 = 0x%x 
229,IIII,[ offload_mgr.c : 1837 ] _offldmgr_non_data_handler: status= 0x%x, sub_status = 0x%x offld_id 0x%x frametype = 0x%x 
228,II,[ offload_mgr.c : 1924 ] offldmgr_non_data_handler: status = 0x%x frametype = 0x%x 
227,ii,[ offload_mgr.c : 1409 ] OFLD proto data hdlr ret_Status=%d curr_wow=%d 
226,III,[ offload_mgr.c : 211 ] OFLD reg data name=0x%x, vdevid:0x%x, vdev_bitmap:0x%x 
225,ii,[ offload_mgr.c : 230 ] OFLD reg data vdev id=%d, max_len =%d 
224,II,[ offload_mgr.c : 286 ] OFLD reg HTT name=0x%x, refcnt:0x%x 
223,II,[ offload_mgr.c : 170 ] OFLD reg nondata name=0x%x, refcnt:0x%x 
222,II,[ offload_mgr.c : 248 ] OFLD reg wmi name=0x%x, refcnt:0x%x 
221,II,[ offload_mgr.c : 972 ] OFLD status hdlr ds2ds, id:%x, mode:%x 
220,II,[ offload_mgr.c : 980 ] OFLD status hdlr nonds, id:%x, mode:%x 
219,I,[ offload_mgr.c : 988 ] OFLD status hdlr invalid eth type,l2 present:%x 
218,,[ offload_mgr.c : 1079 ] OFLD status hdlr: unable to handle this in status buf! HIF CPY 
217,iiii,[ offload_mgr.c : 1084 ] OFLD status hdlr pktlen=%d, dataT=%d addrT=%d vdevId=%d 
216,iiiI,[ offload_mgr.c : 1197 ] OFLD status hdlr ofld id=%d status=%d, route_type=%d, status_buf_flags:0x%x 
215,ii,[ offload_mgr.c : 2127 ] OFLD wmi evt flush evt_id=%d, evt_len=%d 
214,ii,[ offload_mgr.c : 2096 ] OFLD wmi evt store evt_id=%d, evt_len=%d 
213,,[ offload_mgr.c : 2101 ] ofld wmi evt store failure - no memory 
212,Iiiii,[ offload_mgr.c : 646 ] OFLD data parse 11c_snap_hdr_t exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d,dsDir:%d 
211,Iiii,[ offload_mgr.c : 693 ] OFLD data parse llc_snap_hdr_t exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
210,i,[ offload_mgr.c : 709 ] Unknown RX Decap mode %d 
209,IIIIII,[ offload_mgr.c : 735 ] OFLD data parse DA %x %x %x %x %x %x 
208,iiI,[ offload_mgr.c : 738 ] OFLD data parse rx_mode:%d, L3 offset=%d, L2 ethType=%x 
207,Iiii,[ offload_mgr.c : 763 ] OFLD data parse IP_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
206,Iiii,[ offload_mgr.c : 779 ] OFLD data parse IP6_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
205,Iiii,[ offload_mgr.c : 811 ] OFLD data parse TCP_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
204,Iiii,[ offload_mgr.c : 824 ] OFLD data parse UDP_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
203,Iiii,[ offload_mgr.c : 836 ] OFLD data parse ICMPV6_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
202,Iiii,[ offload_mgr.c : 676 ] OFLD data parse ether_header exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
252,iII,[ channel_mgr.c : 58 ] CHAN_MGR_PAUSE_COMPLETE: curr_chan = %d link = 0x%x link_flgs = 0x%x 
251,,[ channel_mgr.c : 100 ] chan mgr pause complete timeout 
250,ii,[ channel_mgr.c : 115 ] CHAN_MANAGER_SM_EVENT: %d < %d
 
249,II,[ channel_mgr.c : 294 ] CHAN_MGR_CTS2S_TX_COMP: status = 0x%x ch_handle = 0x%x 
248,II,[ channel_mgr.c : 261 ] CHAN_MGR_PAUSE_CMPL_CB: status = 0x%x curr_time = 0x%x 
247,iIIiI,[ channel_mgr.c : 198 ] CHAN_MGR_VDEV_PAUSE: chan = %d link = 0x%x flg = 0x%x max_sw_time = %d curr_time = 0x%x 
246,III,[ channel_mgr.c : 165 ] CHAN_MANAGER_SM_EVENT_DATA: chan = 0x%x sec_chan = 0x%x sw_time = 0x%x 
245,iiIIIIi,[ channel_mgr.c : 468 ] CHAN_MGR_TRIGGER_CHANNEL_CHANGE: pri_ch = %d, chan_change_dur = %d,is_chm_valid = 0x%x tx_chm = 0x%x, rx_chm = 0x%x, selfgen_chm = 0x%x, pf_cnt = %d 
244,iII,[ channel_mgr.c : 232 ] CHAN_MGR_VDEV_UNPAUSE:chan =%d link =0x%x curr_time = 0x%x 
256,ii,[ channel_mgr_sm.c : 134 ] CHAN_MANAGER_SM: %d => %d 
255,III,[ channel_mgr_sm.c : 132 ] RESMGR_CHMGR_SEND_CTS2SELF: cur_vc = 0x%x link = 0x%x status = 0x%x 
254,ii,[ channel_mgr_sm.c : 115 ] CHAN_MANAGER_SM_EVENT: %d < %d
 
253,ii,[ channel_mgr_sm.c : 261 ] CHAN_MGR_UNPAUSE: PF %d, time %d 
266,II,[ resmgr.c : 100 ] RESMGR_OCS_INVALID_QUOTA Different MAC: chan0 = 0x%x chan1 = 0x%x 
265,II,[ resmgr.c : 153 ] RESMGR_OCS_INVALID_LATENCY Different MAC: chan0 = 0x%x chan1 = 0x%x 
264,II,[ resmgr.c : 559 ] RESMGR_DEREG_EVT_HDLR:  handler = 0x%x arg = 0x%x not found!!! 
263,II,[ resmgr.c : 565 ] RESMGR_DEREG_EVT_HDLR:  handler = 0x%x arg = 0x%x deregistered 
262,II,[ resmgr.c : 523 ] RESMGR_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x exists!!! 
261,II,[ resmgr.c : 531 ] RESMGR_REG_EVT_HDLR: handler = 0x%x arg = 0x%x no memory!!! 
260,II,[ resmgr.c : 541 ] RESMGR_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x registered 
259,III,[ resmgr.c : 361 ] RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x 
258,III,[ resmgr.c : 383 ] RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x 
257,III,[ resmgr.c : 369 ] RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x 
271,i,[ resmgr_ocm.c : 351 ] RESMGR_OCS_ALLOCRAM_SIZE  size_in_bytes = %d 
270,I,[ resmgr_ocm.c : 511 ] OCM_Migrate: migrate_mode = 0x%x 
269,II,[ resmgr_ocm.c : 568 ] OCM_Resume: ocs_cfg = 0x%x, Pause_OCS = 0x%x 
268,II,[ resmgr_ocm.c : 440 ] OCM_Suspend: Pause_Pending = 0x%x, Pause_OCS = 0x%x 
267,,[ resmgr_ocm.c : 283 ] RESMGR_OCS_CHAN_CHANGE_PROGRESS FAILURE 
280,iIII,[ resmgr_dyn_sch.c : 163 ] RESMGR_DYN_SCH_CH_SX_STATS  chan_mhz = %d accu_tx_rx_dur_us = 0x%x accu_free_dur_us = 0x%x accu_sampling_dur_us = 0x%x 
279,iiii,[ resmgr_dyn_sch.c : 250 ] RESMGR_DYN_SCH_HOME_CH_QUOTA  chan0_mhz = %d ch0_new_quota = %d chan1_mhz = %d ch1_new_quota = %d 
278,iIII,[ resmgr_dyn_sch.c : 170 ] RESMGR_DYN_SCH_CH_SX_STATS  chan_mhz = %d accu_tx_rx_dur_us = 0x%x accu_free_dur_us = 0x%x accu_sampling_dur_us = 0x%x 
277,iiii,[ resmgr_dyn_sch.c : 184 ] RESMGR_DYN_SCH_TOT_UTIL_PER  chan0_mhz = %d chan0_util_percentage = %d chan1_mhz = %d chan1_util_percentage = %d 
276,iiiii,[ resmgr_dyn_sch.c : 477 ] RESMGR_DYN_SCH_CH_STATS_END  chan_mhz = %d rx_clear_cnt = %d tx_frame_cnt = %d rx_frame_cnt_us = %d sampling_dur_us = %d 
275,iiiii,[ resmgr_dyn_sch.c : 547 ] RESMGR_DYN_SCH_CH_STATS_START  chan_mhz = %d start_rx_clear_cnt = %d start_tx_frame_cnt = %d start_rx_frame_cnt_us = %d start_time_us = %d 
274,i,[ resmgr_dyn_sch.c : 296 ] RESMGR_DYN_SCH_ALLOCRAM_SIZE  size = %d 
273,II,[ resmgr_dyn_sch.c : 357 ] RESMGR_DYN_SCH_ENABLE  enable = 0x%x fw_disable_bmap = 0x%x 
272,i,[ resmgr_dyn_sch.c : 88 ] RESMGR_DYN_SCH_ACTIVE  is_active = %d 
345,IIiii,[ resmgr_ocs.c : 4652 ] RESMGR_OCS_CHREQ_CREATE: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d, sec_chan_mhz = %d prioirty = %d  
344,IiiIiI,[ resmgr_ocs.c : 4658 ] RESMGR_OCS_CHREQ_CREATE: start_tsf = 0x%x duration_usec = %d interval = %d dtim_start_tsf = 0x%x dtim_period = %d end_tsf = 0x%x 
343,IIiii,[ resmgr_ocs.c : 4684 ] RESMGR_OCS_CHREQ_DELETE: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d sec_chan_mhz = %d state = %d 
342,IIiiii,[ resmgr_ocs.c : 5053 ] RESMGR_OCS_CHREQ_START: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d sec_chan_mhz = %d band_center_freq2 = %d prioirty = %d  
341,IiiIiI,[ resmgr_ocs.c : 5058 ] RESMGR_OCS_CHREQ_START: start_tsf = 0x%x duration_usec = %d interval = %d dtim_start_tsf = 0x%x dtim_period=%d end_tsf = 0x%x 
340,IIiii,[ resmgr_ocs.c : 5121 ] RESMGR_OCS_CHREQ_STOP: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d sec_chan_mhz = %d state = %d 
339,I,[ resmgr_ocs.c : 4736 ] RESMGR_OCS_CHREQ_UPDATE: start_tsf/req_id = 0x%x 
338,IIiii,[ resmgr_ocs.c : 4861 ] RESMGR_OCS_CHREQ_UPDATE: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d sec_chan_mhz = %d prioirty = %d  
337,IIiIiI,[ resmgr_ocs.c : 4866 ] RESMGR_OCS_CHREQ_UPDATE: start_tsf = 0x%x duration_usec = 0x%x interval = %d dtim_start_tsf = 0x%x dtim_period=%d end_tsf = 0x%x 
336,i,[ resmgr_ocs.c : 4495 ] RESMGR_OCS_ALLOCRAM_SIZE  size_in_bytes = %d 
335,i,[ resmgr_ocs.c : 2928 ] RESMGR_OCS_WIN_CAT_DUR  duration = %d 
334,IIiII,[ resmgr_ocs.c : 574 ] RESMGR_OCS_CHREQ_UPDATE  start_tsf = 0x%x duration_usec = 0x%x interval=%d prioirty = 0x%x chan_req_addr = 0x%x 
333,IIIi,[ resmgr_ocs.c : 666 ] RESMGR_OCS_CHREQ_RESTART  start_tsf = 0x%x stop_tsf = 0x%x dtim_start_tsf = 0x%x dtim_period = %d 
332,IIiII,[ resmgr_ocs.c : 583 ] RESMGR_OCS_CHREQ_UPDATE req_id = 0x%x dtim_start_tsf = 0x%x dtim_period=%d purge_flag = 0x%x end_tsf = 0x%x 
331,ii,[ resmgr_ocs.c : 586 ] RESMGR_OCS_CHREQ_UPDATE chan_mhz = %d sec_chan_mhz = %d 
330,,[ resmgr_ocs.c : 4427 ] RESMGR_OCS_CH_SWITCH_REQ 
329,II,[ resmgr_ocs.c : 1957 ] RESMGR_OCS_LATENCY_STRICT_TIME_SLOT  slot1_start_tsf = 0x%x slot2_start_tsf = 0x%x 
328,I,[ resmgr_ocs.c : 1976 ] RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
327,I,[ resmgr_ocs.c : 2147 ] RESMGR_OCS_CURR_TSF  current_tsf = 0x%x 
326,II,[ resmgr_ocs.c : 2149 ] RESMGR_OCS_QUOTA_REM  cat1_quota_remain = 0x%x cat2_quota_remain = 0x%x 
325,I,[ resmgr_ocs.c : 2194 ] RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
324,I,[ resmgr_ocs.c : 2198 ] RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
323,I,[ resmgr_ocs.c : 2222 ] RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
322,I,[ resmgr_ocs.c : 2272 ] RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
321,I,[ resmgr_ocs.c : 2276 ] RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
320,I,[ resmgr_ocs.c : 2291 ] RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
319,I,[ resmgr_ocs.c : 2320 ] RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
318,I,[ resmgr_ocs.c : 3534 ] RESMGR_OCS_CLEANUP_CH_ALLOCATORS  cur_ch_alloc_addr = 0x%x 
317,I,[ resmgr_ocs.c : 3553 ] RESMGR_OCS_CH_ALLOCATOR_FREE  cur_ch_alloc_addr = 0x%x 
316,I,[ resmgr_ocs.c : 3604 ] RESMGR_OCS_CLEANUP_STALE_REQS  cur_ch_alloc_addr = 0x%x 
315,IIi,[ resmgr_ocs.c : 3684 ] RESMGR_OCS_CHREQ_TERMINATE: req_id = 0x%x cur_ch_req = 0x%x state = %d 
314,II,[ resmgr_ocs.c : 3625 ] RESMGR_OCS_CHREQ_COMPLETE  curr_time = 0x%x ch_req_addr = 0x%x 
313,II,[ resmgr_ocs.c : 3649 ] RESMGR_OCS_CHREQ_COMPLETE  curr_time = 0x%x ch_req_addr = 0x%x 
312,Iii,[ resmgr_ocs.c : 1520 ] RESMGR_OCS_CONSTRUCT_CAT_WIN  chan_alloc_addr=0x%x chan_mhz=%d sec_ch_mhz=%d 
311,Ii,[ resmgr_ocs.c : 1559 ] RESMGR_OCS_NEW_CAT_WINDOW_REQ  ch_req_addr = 0x%x state = %d 
310,II,[ resmgr_ocs.c : 1562 ] RESMGR_OCS_NEW_CAT_WINDOW_TIMESLOT  start_tsf = 0x%x stop_tsf = 0x%x 
309,IIIII,[ resmgr_ocs.c : 4339 ] RESMGR_OCS_RESOURCES  req_id = 0x%x ch_req_addr = 0x%x ch_alloc_addr = 0x%x state = 0x%x priority = 0x%x 
308,iii,[ resmgr_ocs.c : 4342 ] RESMGR_OCS_RESOURCES chan_mhz = %d sec_chan_mhz = %d, band_center_freq2 = %d 
307,II,[ resmgr_ocs.c : 135 ] RESMGR_OCS_CHREQ_GRANT  curr_time = 0x%x ch_req_addr = 0x%x 
306,II,[ resmgr_ocs.c : 733 ] RESMGR_OCS_CHREQ_COMPLETE  curr_time = 0x%x ch_req_addr = 0x%x 
305,i,[ resmgr_ocs.c : 5157 ] RESMGR_OCS_CHANNEL_SWITCHED  status = %d 
304,II,[ resmgr_ocs.c : 1872 ] RESMGR_OCS_MISS_TOLERANCE  miss_tolerance_cnt_timeslot1 = 0x%x miss_tolerance_cnt_timeslot2 = 0x%x 
303,i,[ resmgr_ocs.c : 5292 ] RESMGR_OCS_NEXT_SCH_INTERVAL = %d 
302,Ii,[ resmgr_ocs.c : 3421 ] RESMGR_OCS_PURGE_CHREQ  cur_ch_alloc_addr = 0x%x chan_mhz = %d 
301,I,[ resmgr_ocs.c : 3472 ] RESMGR_OCS_PURGE_CHREQ  cur_ch_req_addr = 0x%x 
300,ii,[ resmgr_ocs.c : 4959 ] RESMGR_OCS_RECAL_QUOTAS  num_home_chans = %d tracking_interval = %d 
299,ii,[ resmgr_ocs.c : 5006 ] RESMGR_OCS_RECAL_QUOTAS  chan_mhz = %d latency = %d 
298,iii,[ resmgr_ocs.c : 5013 ] RESMGR_OCS_ALLOCATED_QUOTA_STATS  chan_mhz = %d req_chan_time_percentage = %d chan_time_quota = %d 
297,i,[ resmgr_ocs.c : 3046 ] RESMGR_OCS_RECOMPUTE_SCHEDULE: ocs_ins = %d 
296,i,[ resmgr_ocs.c : 3052 ] RESMGR_OCS %d has been paused 
295,,[ resmgr_ocs.c : 349 ] RESMGR_OCS_CURR_CAT_WINDOW 
294,IIi,[ resmgr_ocs.c : 367 ] RESMGR_OCS_CURR_CAT_WINDOW_REQ  req_id = 0x%x ch_req_addr = 0x%x state = %d 
293,II,[ resmgr_ocs.c : 370 ] RESMGR_OCS_CURR_CAT_WINDOW_TIMESLOT  start_tsf = 0x%x stop_tsf = 0x%x 
292,I,[ resmgr_ocs.c : 385 ] RESMGR_OCS_CURR_CAT_WINDOW: Channel change pending, flags = 0x%x 
291,Iii,[ resmgr_ocs.c : 2998 ] RESMGR_OCS_CUR_CH_ALLOC  curr_chan_alloc_addr = 0x%x chan_mhz = %d sec_ch_mhz = %d 
290,Iii,[ resmgr_ocs.c : 3008 ] RESMGR_OCS_WINNING_CH_ALLOC  curr_chan_alloc_addr = 0x%x chan_mhz = %d sec_ch_mhz = %d 
289,iII,[ resmgr_ocs.c : 3824 ] RESMGR_OCS_INVOKED: ocs_ins = %d last_ocs_entry_time = 0x%x current_time = 0x%x 
288,III,[ resmgr_ocs.c : 3828 ] RESMGR_OCS_INVOKED: Cur_Ch_Alloc = 0x%x Flags = 0x%x Resched_Req = 0x%x 
287,I,[ resmgr_ocs.c : 3961 ] RESMGR_OCS_TSF_TIMEOUT_US defer_sch_time = %x 
286,i,[ resmgr_ocs.c : 3977 ] RESMGR_OCS_SCHED_CH_CHANGE: ocs_ins = %d 
285,I,[ resmgr_ocs.c : 4029 ] RESMGR_OCS_TSF_TIMEOUT_US next_tsftime = %x 
284,I,[ resmgr_ocs.c : 4041 ] RESMGR_OCS_NEXT_TSFTIME  next_tsf_time = 0x%x 
283,iii,[ resmgr_ocs.c : 4066 ] RESMGR_OCS_TSF_TIMEOUT_US wake up latency = %d, wlan_chan_num = %d, wlan_cb_num = %d 
282,i,[ resmgr_ocs.c : 4073 ] RESMGR_OCS_TSF_TIMEOUT_US  timeout_us = %d 
281,iII,[ resmgr_ocs.c : 4146 ] RESMGR_OCS_INVOKED: ocs_ins = %d ocs_entry_time = 0x%x ocs_exit_time = 0x%x 
350,,[ resmgr_vcm.c : 48 ] RESMGR_CREATE_LINK failed due to invalid channel param 
349,IIiiii,[ resmgr_vcm.c : 137 ] RESMGR_LINK_CREATE link_pointer = 0x%x link_flags = 0x%x ch_mhz = %d phy_mode = %d band_center_freq1 = %d band_center_freq2 = %d 
348,I,[ resmgr_vcm.c : 150 ] RESMGR_LINK_DELETE  Link Pointer = 0x%x 
347,,[ resmgr_vcm.c : 265 ] RESMGR_UPDATE_LINK failed due to invalid channel param 
346,I,[ resmgr_vcm.c : 816 ] VCM_Init:  VC Pool Size = 0x%x 
362,iII,[ virtual_channel.c : 397 ] RESMGR_VC_UPDATE_HOME_CHAN_INFO: mac_id = %d virtual_chan_count = 0x%x home_chan_count = 0x%x 
361,iiIIiiII,[ virtual_channel.c : 474 ] RESMGR_ADD_LINK ch_mhz = %d phy_mode = %d link_flags = 0x%x link_valid_attr = 0x%x no_160_link_cnt = %d 160_link_cnt = %d vc = 0x%x link = 0x%x 
360,iIIIIi,[ virtual_channel.c : 276 ] RESMGR_VC_INIT_VIR_CHAN: chan_mhz = %d, mac_id = 0x%x, band = 0x%x, tx_chm = 0x%x, rx_chm = 0x%x, rx_nss = %d 
359,IIIIIII,[ virtual_channel.c : 286 ] RESMGR_VC_INIT_VIR_CHAN: nss1_tx_chm = 0x%x, nss2_tx_chm = 0x%x, selfgen_chm = 0x%x, nss_tx_11b_chainmask = 0x%x, selfgen_11b_chainmask = 0x%x, nss_tx_ofdm_chainmask = 0x%x, selfgen_ofdm_chainmask = 0x%x 
358,i,[ virtual_channel.c : 314 ] RESMGR_VC_INIT_HOME_CHAN: chan_mhz = %d 
357,iI,[ virtual_channel.c : 610 ] RESMGR_OCS_REQ_QUOTA_STATS chan_mhz = %d req_chan_time/latency = 0x%x 
356,II,[ virtual_channel.c : 616 ] RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x req_chan_time/latency = 0x%x 
355,iiiiII,[ virtual_channel.c : 793 ] RESMGR_VC_REGISTER_LINK: chan_mhz = %d link_count = %d ephemeral_link_count = %d is_home_chan = %d link_flags = 0x%x link_valid_attr = 0x%x 
354,iiIIii,[ virtual_channel.c : 511 ] RESMGR_RMV_LINK ch_mhz = %d phy_mode = %d link_flags = 0x%x link_valid_attr = 0x%x no_160_link_cnt = %d 160_link_cnt = %d 
353,III,[ virtual_channel.c : 990 ] !cts2s_sent: 0x%x 0x%x 0x%x 
352,iiii,[ virtual_channel.c : 815 ] RESMGR_VC_UNREGISTER_LINK: chan_mhz = %d link_count = %d ephemeral_link_count = %d is_home_chan = %d 
351,i,[ virtual_channel.c : 671 ] RESMGR_VC_UPDATE_CUR_VC  chan_mhz = %d 
370,iii,[ virtual_channel_arbiter.c : 908 ] wlan_virtual_chan_apply_chan_num  rx = %d tx = %d org = %d 
369,Ii,[ virtual_channel_arbiter.c : 953 ] RESMGR_VC_ARBITRATE_ATTRIBUTES link_var = 0x%x link_count = %d 
368,iiiII,[ virtual_channel_arbiter.c : 1093 ] RESMGR_VC_ARBITRATE_ATTRIBUTES  chan_mhz = %d phy_mode/vc_prog_latency = %d band_center_freq = %d virtual_chan_ctxt = 0x%x virtual_chan = 0x%x 
367,ii,[ virtual_channel_arbiter.c : 1120 ] RESMGR_VC_ARBITRATE_ATTRIBUTES  chan_mhz = %d phy_mode/vc_prog_latency = %d 
366,iiii,[ virtual_channel_arbiter.c : 1141 ] RESMGR_VC_ARBITRATE_ATTRIBUTES  chan_mhz = %d current_chan_mhz = %d per link tx_chainmask = %d, rx_chainmask = %d 
365,iii,[ virtual_channel_arbiter.c : 1035 ] RESMGR_VC_ARBITRATE_ATTRIBUTES  link_count = %d chain_number = %d per_link_chain_num = %d 
364,iII,[ virtual_channel_arbiter.c : 1049 ] RESMGR_VC_ARBITRATE_ATTRIBUTES  num = %d, tx_mask = %x rx_mask = %x 
363,iii,[ virtual_channel_arbiter.c : 1192 ] VC_ARB_SMPS: mhz = %d, smps_supp = %d, dyn_smps = %d 
371,iiIi,[ resmgr_chainmask_mgr.c : 3209 ] RESMGR_CHMMGR_RESOLVE_BANDWIDTH: band = %d, mac = %d, max_bw_supported = 0x%x, hw_mode = %d 
377,II,[ resmgr_concurrency_mgr.c : 161 ] RESMGR_CONCURRENCY_DEREG_EVT_HDLR:  handler = 0x%x arg = 0x%x deregistered 
376,IIIi,[ resmgr_concurrency_mgr.c : 259 ] _resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  active_sta_vdev_num = 0x%x, active_vdev_num = 0x%x, resmgr_nan_discovery_enable = 0x%x, result = %d 
375,I,[ resmgr_concurrency_mgr.c : 338 ] resmgr_concurrency_mgr_notify:  module = 0x%x 
374,II,[ resmgr_concurrency_mgr.c : 105 ] RESMGR_CONCURRENCY_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x exists!!! 
373,II,[ resmgr_concurrency_mgr.c : 113 ] RESMGR_CONCURRENCY_REG_EVT_HDLR: handler = 0x%x arg = 0x%x no memory!!! 
372,II,[ resmgr_concurrency_mgr.c : 123 ] RESMGR_CONCURRENCY_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x registered 
394,iiiiii,[ wlan_scan.c : 1412 ] SCAN_ENG_CALC_CHAN num_2g = %d num_5g_active = %d num_5g_passive = %d double_passive_chan_scan = %d num_6g_ch = %d num_extra_6g_ch = %d 
393,IIII,[ wlan_scan.c : 1440 ] SCAN_ENG_SPOOFED_MAC_ADDR full_mac_addr = %08x%04x partial_mac_addr = %08x%04x 
392,IIIIIiii,[ wlan_scan.c : 766 ] SCAN_ENG_START scan_id = 0x%x eng_id(3)|req_type(3) = %06d num_chans_[req(3)|granted_2g(3)|granted_5g(3)] = %09d num_[ssid(3)|bssid(3)] = %06d flags = 0x%x vdev_freq = %d cur_ch_idx_2g|5g = %d %d 
391,iiiiii,[ wlan_scan.c : 778 ] SCAN_ENG_PARAM_1 dwell_time_active = %d dwell_time_active_2g = %d msec dwell_time_passive = %d msec min_rest_time = %d msec max_rest_time = %d msec max_scan_time = %d msec 
390,iiiiiii,[ wlan_scan.c : 789 ] SCAN_ENG_PARAM_2 idle_time = %d msec repeat_probe_time = %d msec probe_spacing_time = %d msec probe_delay = %d msec burst_duration = %d msec max_num_probes(2g|5g) = %d cancel_probe_req_defer = %d 
389,iiii,[ wlan_scan.c : 1569 ] SCAN_ADJUST_PARAM active=%d active_2g=%d passive=%d rest=%d 
388,IIIIIii,[ wlan_scan.c : 200 ] CHANNEL_CONGESTION_PRINTS cycle_cnt = %10d, busy = %10d, tx = %10d, rx = %10d, mr_rx = %10d, chan_freq= %d send_stats:%d 
387,iiiiiiii,[ wlan_scan.c : 985 ] SCAN_ENG_CALC_CHAN num_6g_active = %d num_6g_passive = %d num_items_in_cache = %d scan_all_psc_chan = %d scan_all_non_psc_chan = %d match_hint = %d skip_non_rnr_chan = %d client_priority = %d 
386,iIIiii,[ wlan_scan.c : 1780 ] SCAN_ENG_CANCEL scanhandler_id = %d scan_id = 0x%x requestor= 0x%x stop_mode = %d scan_in_progress = %d cancel_in_progress = %d 
385,iiiII,[ wlan_scan.c : 80 ] AUTO_CHAN_EVT_HDNLR CURR_CHAN_STATS_ERROR error_code = %d (1:scan_handle NULL, 2:chan_freq 0) scan_id = %d evt_mac_id = %d type = 0x%x freq = 0x%x 
384,iIii,[ wlan_scan.c : 2086 ] SCAN_BCN_RECVD mhz=%d at %08x is_scan_in_progress=%d (0 ignored) send_probe_req_on_DFS_ch=%d (1 ignored) 
383,ii,[ wlan_scan.c : 1838 ] SCAN_SET_CHANLIST_FAILED support_chan %d num_scan_chans %d 
382,iiiIIii,[ wlan_scan.c : 1946 ] SCAN_SET_CHAN_LIST idx = %d, mhz = %d, is_passive = %d ch_info = 0x%x reg_info_1 = 0x%x max_bd = %d  is_nan_disabled = %d 
381,,[ wlan_scan.c : 2212 ] ath11k passive scan
 
380,IIIi,[ wlan_scan.c : 1608 ] SCAN_ENG_START_IN_PROGRESS = 1 scan_id = 0x%x requestor = 0x%x req_sub_id = 0x%x priority = %d -> return EBUSY 
379,I,[ wlan_scan.c : 1731 ] SCAN_SM_START_COMMAND_FAILED cur_sch_scan_req = NULL handle = 0x%x 
378,iI,[ wlan_scan.c : 642 ] SCAN_ENG_MAX_SCAN_TIMEOUT scanhandle_id = %d scan_id = 0x%x 
406,I,[ wlan_dcs.c : 526 ] WLAN_DCS_DBGID_TIMER  0x%x 
405,I,[ wlan_dcs.c : 724 ] Init = 0x%x 
404,I,[ wlan_dcs.c : 55 ] WMI_EVENT_ALLOC_FAILURE EventId = 0x%x 
403,iiiII,[ wlan_dcs.c : 87 ] AWGN_INT_DBG ATH_CAP_DCS_AGWNIM sent chan_freq = %d center_freq0 = %d center_freq1 = %d channel_width = 0x%x bitmap = 0x%x
 
402,I,[ wlan_dcs.c : 161 ] WMI_EVENT_ALLOC_FAILURE EventId = 0x%x 
401,I,[ wlan_dcs.c : 191 ] WLAN_DCS_DBGID_WMI_CWINT  0x%x 
400,I,[ wlan_dcs.c : 250 ] WMI_EVENT_ALLOC_FAILURE EventId = 0x%x 
399,I,[ wlan_dcs.c : 278 ] WLAN_DCS_DBGID_WMI_WLAN_INT  0x%x 
398,I,[ wlan_dcs.c : 507 ] WLAN_DCS_DBGID_TIMER  0x%x 
397,iiiii,[ wlan_dcs.c : 124 ] AWGN_INT_DBG unit_test command invoked num_args = %d vdev_id = %d e_mac_id = %d pmac_id = %d g_chan_bw_interference_bitmap = %d
 
396,ii,[ wlan_dcs.c : 130 ] AWGN_INT_DBG unit_test wrong param  num_args = %d args[0] = %d
 
395,iIii,[ wlan_dcs.c : 100 ] AWGN_INT_DBG pdev_id = %d seg = 0x%x bw_drop = %d pkt_drop = %d 
 
438,I,[ wlan_scan_sch.c : 2653 ] SCAN_SCH_CSA_FAILED status = 0x%x 
437,III,[ wlan_scan_sch.c : 2920 ] SCAN_SCH_RESUME requestor_id = 0x%x suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
436,iIIi,[ wlan_scan_sch.c : 181 ] SCAN_SCH_SUPPRESS_REQ req_mod_id=%d sch_class = 0x%x id = 0x%x is_disable_scan = %d 
435,III,[ wlan_scan_sch.c : 2894 ] SCAN_SCH_SUSPEND requestor_id = 0x%x suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
434,IIiiIIii,[ wlan_scan_sch.c : 1215 ] SCAN_INTERN_EVT evt_type=%x(1:start 2:compl 4:bss 8:frn_ch 10:deq 20:preempt 40:start_fail 80:restart 100:frn_ch_exit 200:susp 400:resume) scan_id=0x%x vdev_id=%d freq=%d req_sub_id=0x%x to_host(8b)|reason(8b)=0x%x abs_pri=%d dwell=%d 
433,Iiiii,[ wlan_scan_sch.c : 1265 ] SCAN_INTERN_EVT (FOREIGN_CHANNEL) scan_id = 0x%x ch_freq = %d bss_ch_freq = %d passive/active = %d dwell_time = %d 
432,IIi,[ wlan_scan_sch.c : 1278 ] SCAN_INTERN_EVT (PREEMPTED) scan_id = 0x%x preempted_by (scan_id) = 0x%x reason = %d 
431,I,[ wlan_scan_sch.c : 1840 ] SCAN_SCH_WMI_START_SCAN vdev_id = 0x%x is FREE  
430,Iiiii,[ wlan_scan_sch.c : 1942 ] SCAN_SCH_WMI_START s_ssid_bssid_cache = 0x%x num_hint_freq_short_ssid_list = %d num_hint_freq_bssid_list = %d dtime_act = %d dtime_pas = %d 
429,iiiii,[ wlan_scan_sch.c : 1994 ] CheckNOL status = %d, p_cmd->num_chan = %d, numOfChans = %d, scan_id = %d, req_id = %d 
428,iI,[ wlan_scan_sch.c : 2025 ] SCAN_START_COMMAND_FAILED err_ret_code = %d(1:normal 2:NOL) status = 0x%x 
427,iiiiii,[ wlan_scan_sch.c : 1892 ] SCAN_SCH_WMI_START_SCAN num_ssid from %d to %d, num_bssid from %d to %d, num_chan = %d ie_len = %d 
426,I,[ wlan_scan_sch.c : 2050 ] SCAN_SCH_STOP_COMMAND_FAILED status = 0x%x 
425,II,[ wlan_scan_sch.c : 630 ] SCAN_SCH_SUSPENDED suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
424,i,[ wlan_scan_sch.c : 657 ] SCAN_SCH_START_NEW_REQ_FAILED error_code=%d 
423,,[ wlan_scan_sch.c : 660 ] SCAN_DETERM_HIGH_PRI cur scan not completed 
422,I,[ wlan_scan_sch.c : 1672 ] %s: Invalid params 
421,I,[ wlan_scan_sch.c : 1649 ] %s: Invalid params 
420,iI,[ wlan_scan_sch.c : 849 ] SCAN_SCH_START_PARAM_INVALID scan_id=0x%d param=0x%x 
419,IIIiiiii,[ wlan_scan_sch.c : 1015 ] SCAN_SCH_START scan_id = 0x%x requestor_id = 0x%x req_sub_id = 0x%x requested_priority = %d absolute_priority = %d actv_time_5g = %d actv_time_2g = %d pass_time = %d 
418,iiIii,[ wlan_scan_sch.c : 1045 ] SCAN_SCH_START_INFO monitoring_interval = %d ie_len = %d ie_chunk_bitmap = 0x%x opmode = %d subopmode = %d 
417,iiIIii,[ wlan_scan_sch.c : 1062 ] SCAN_SCH_START_FAIL err_code = %d(1:misc 2:vdev_invalid 3:no_mem_new_req 4:chunk_copy_fail) scan_id = 0x%d requestor_id = 0x%x req_sub_id = 0x%x requested_priority = %d ie_len = %d 
416,I,[ wlan_scan_sch.c : 1620 ] SCAN_EVENT_SEND_FAILED 0x%x 
415,IiiIi,[ wlan_scan_sch.c : 1360 ] SCAN_EVENT_SEND_FAILED scan_id = 0x%x vdev_id = %d ch_freq = %d req_sub_id = 0x%x reason = %d 
414,IIii,[ wlan_scan_sch.c : 303 ] SCAN_SCH_CANCEL scan_id = 0x%x requestor_id = 0x%x vdev_id = %d req_type = %d 
413,,[ wlan_scan_sch.c : 355 ] SCAN_SCH_CANCEL already in progress 
412,,[ wlan_scan_sch.c : 361 ] SCAN_SCH_CANCEL no match found 
411,II,[ wlan_scan_sch.c : 556 ] SCAN_SCH_SUSPEND_NEXT_SCAN suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
410,IIIIIII,[ wlan_scan_sch.c : 589 ] SCAN_SCH_SUPPRESS_MATCH scan_id = 0x%x, requestor = 0x%x, vdev_id = 0x%x, suppress_vdev_id_bitmap = 0x%x suppress_mod_bitmap[0:2] 0x%x 0x%x 0x%x 
409,II,[ wlan_scan_sch.c : 1108 ] SCAN_SCH_ENGINE_STOP_DUE_TO_TIMEOUT  evt_scan_id = 0x%x evt_reason = 0x%x 
408,i,[ wlan_scan_sch.c : 1469 ] SCAN_SCH_NEXT_SCAN_FAILED error_code=%d 
407,i,[ wlan_scan_sch.c : 1172 ] SCAN_EVENT_COMPLETED really cancelled scan_id %d 
458,iii,[ wlan_scan_sm.c : 109 ] SCAN_SM_TRANSITIONS_MAC_%d %d => %d 
457,iii,[ wlan_scan_sm.c : 94 ] SCAN_SM_DISPATCH_MAC_%d %d < %d 
456,Iiii,[ wlan_scan_sm.c : 6687 ] SCAN_SM_OCS_TIMEOUT scan_id 0x%x, requestor = %d, curr_index = %d, curr_policy = %d 
455,iiIIiiii,[ wlan_scan_sm.c : 826 ] SCAN_SM_REQ_NEXT_CHAN cur_policy=%d hdl_id=%d 2g_idx(16)|tot(16)=0x%x 5g_idx(8)|tot(E8_H8_L8)=0x%x dwell=%dms dur=%dus freq_pri=%d freq_sec=%d 
454,IiiiiiiIi,[ wlan_scan_sm.c : 4735 ] SCAN_SEND_PROBE_REQ scan_id = 0x%x mac_id = %d freq = %d cur_index = %d max_num_probe = %d probe_timer_count = %d chainmask = %d ppdu_info = 0x%x max_tx_power = %d 
453,Ii,[ wlan_scan_sm.c : 6787 ] SCAN_SM_CANCEL scan_stop = 0x%x scan_timeout = %d 
452,i,[ wlan_scan_sm.c : 3249 ] SCAN_SM_REQ_NEXT_CHAN !error! not implemented scan policy: %d 
451,ii,[ wlan_scan_sm.c : 4821 ] SCAN_SM_PROBE_REQ_FRAME_GEN_FAILED scanhandler_id = %d 6g_freq = %d 
450,iIiIIII,[ wlan_scan_sm.c : 4860 ] SEND_PROBE_ON_6GHZ_CH freq = %d short_ssid = 0x%x (cur_20TU_idx = %d add_flags_save = 0x%x add_flags = 0x%x chainmask = 0x%x ppdu_info = 0x%x) 
449,iIIiIIII,[ wlan_scan_sm.c : 4870 ] SEND_PROBE_ON_6GHZ_CH freq = %d bssid = %08x%04x (cur_20TU_idx = %d add_flags_save = 0x%x add_flags = 0x%x chainmask = 0x%x ppdu_info = 0x%x) 
448,i,[ wlan_scan_sm.c : 4962 ] SCAN_SEND_PROBE_REQ_6G_MGR err_ret = %d 
447,IiiI,[ wlan_scan_sm.c : 5839 ] SCAN_SEND_PROBE_REQ_2G_RET scan_id = 0x%x freq = %d cur_index = %d flags = 0x%02x 
446,IiiI,[ wlan_scan_sm.c : 5852 ] SCAN_SEND_PROBE_REQ_5G_RET scan_id = 0x%x freq = %d cur_index = %d flags = 0x%02x 
445,IIIiiiii,[ wlan_scan_sm.c : 5998 ] SCAN_SEND_PROBE_REQ_INFO scan_id = 0x%x band_2G_info = 0x%x band_5G_info = 0x%x probe_time = %d last_ssid_idx = %d last_bssid_idx = %d last_sent_probes = %d increase_probe_cnt:%d 
444,iI,[ wlan_scan_sm.c : 6004 ] SCAN_SEND_PROBE_REQ_RET err_ret = %d scan_id = 0x%x 
443,i,[ wlan_scan_sm.c : 5511 ] SCAN_SM_PROBE_REQ_FRAME_GEN_FAILED scanhandler_id = %d 
442,iii,[ wlan_scan_sm.c : 5177 ] SCAN_SM_PROBE_REQ_FRAME_GEN_FAILED scanhandler_id = %d 5g_freq = %d 2g_freq = %d 
441,iii,[ wlan_scan_sm.c : 4249 ] SCAN_SM_FOREIGN_CH actual_probe_delay = %d, scan_sch_handle->cancel_probe_req_defer = %d, params.cancel_probe_req_defer = %d 
440,iiii,[ wlan_scan_sm.c : 4272 ] SCAN_SM_LEGACY_MAC_CHANGE scanhandler_id = %d, last_legacy_macid = %d req_mac_id = %d, index = %d 
439,i,[ wlan_scan_sm.c : 6387 ] SCAN_SM_FOREIGN_CHAN_EVENT !error! not implemented scan policy: %d 
480,iiii,[ wlan_scan_mgr.c : 439 ] SCAN_MGR_PDEV_SUSPEND_RESUME_CHANGE_EVT pdev_id = %d requestor = %d reason %d state = %d 
479,IIII,[ wlan_scan_mgr.c : 410 ] SCAN_POLICY_EVENT current_allowed_policy = 0x%x new_allowed_policy = 0x%x current_scan_req = 0x%x suppress_mode_bitmap = 0x%x 
478,Iiiii,[ wlan_scan_mgr.c : 90 ] SCAN_MGR_STATE_CHANGE scan_id = 0x%x num_ssid = %d num_bssid = %d num_chan = %d new_scan_state = %d (0:completed 1:legacy 2:sync_DBS 3:async_DBS 4:agile 5:agile_DFS_2g 6:agile_DFS_5g) 
477,iii,[ wlan_scan_mgr.c : 1207 ] SCAN_MGR_BCN_RECV_WRONG_CH mac_id = %d freq (%d != %d) 
476,ii,[ wlan_scan_mgr.c : 1264 ] SCAN_MGR_BCN_RECV_FAIL err_code = %d(1:macid_invalid 2:cur_sch_scan_req_null) mac_id = %d 
475,iii,[ wlan_scan_mgr.c : 1214 ] SCAN_MGR_BCN_RECV_WRONG_CH mac_id = %d cur_freq (%d != %d) 
474,,[ wlan_scan_mgr.c : 1417 ] SCAN_MGR_CH_MODE_CHANGE scan cancelled 
473,iiiii,[ wlan_scan_mgr.c : 1484 ] SCAN_MGR_CHECK_PARAMS_CHANNELS params->num_chan=%d params->chan_list[0]=%d has_2g_chan=%d has_5g_chan_active=%d has_5g_chan_passive=%d 
472,iii,[ wlan_scan_mgr.c : 1283 ] SCAN_MGR_DS_PARAM mac_id = %d, chan = %d len = %d 
471,iI,[ wlan_scan_mgr.c : 154 ] SCAN_MGR_EVENT_FAIL: Invalid input - scan_handler_id = %d, current_scan_sch_req = 0x%x 
470,IIiiiiiIi,[ wlan_scan_mgr.c : 296 ] SCAN_MGR_EVENT_PREEMPTED scan_id = 0x%x cur_chan_index = 0x%x  mac_id = %d 2g_next_idx = %d 2g_curr = %d 5g_next_idx = %d 5g_curr = %dreason = 0x%x cur_scan_policy = %d 
469,IIIi,[ wlan_scan_mgr.c : 302 ] SCAN_MGR_EVENT_SUSPENDED scan_id = 0x%x cur_chan_index = 0x%x reason = 0x%x cur_scan_policy = %d 
468,i,[ wlan_scan_mgr.c : 308 ] SCAN_MGR_EVENT_PREEMPTED or SCAN_MGR_EVENT_SUSPENDED drop_event = %d 
467,Iiiii,[ wlan_scan_mgr.c : 366 ] SCAN_MGR_EVENT_COMPLETED scan_id = 0x%x num_ssid = %d num_bssid = %d num_chan = %d is_drop = %d 
466,I,[ wlan_scan_mgr.c : 1574 ] SCAN_MGR_SCAN_POLICY_RECOMPUTE_START suppress mode bitmap = 0x%x 
465,iiii,[ wlan_scan_mgr.c : 1628 ] SCAN_MGR_SCAN_POLICY_RECOMPUTE invalid chan index vdev_index=%d has_2g_chan=%d passive_5g=%d has_5g_chan_active=%d 
464,iiiiiI,[ wlan_scan_mgr.c : 1678 ] SCAN_MGR_SCAN_POLICY_RECOMPUTE_END vdev_index = %d, chan_index = %d, new_scan_policy = %d, scan_mgr_handle->cur_scan_policy = %d, scan_policy_max = %d, suppress mode bitmap = 0x%x 
463,IIii,[ wlan_scan_mgr.c : 960 ] SCAN_MGR_CANCEL scan_id = 0x%x requstor = 0x%x stop_mode = %d scan_eng_start_pending = %d 
462,II,[ wlan_scan_mgr.c : 1056 ] SCAN_MGR_CANCEL comp_pending=0x%x cancel_pending=0x%x 
461,Ii,[ wlan_scan_mgr.c : 925 ] SCAN_MGR_SCAN_START_NON_DBS scan_id = 0x%x  cur_scan_policy = %d  
460,i,[ wlan_scan_mgr.c : 1119 ] SCAN_SCH_NEXT_SCAN_FAILED after setting new channel lists, error_code=%d 
459,iiiiiiii,[ wlan_scan_mgr.c : 620 ] SCAN_MGR_RESUME_EVENT 2g cur_chan = %d, 2g next_chan = %d, 5g cur_chan = %d, 5g next_chan = %d, band_5g_low(high)_num_chan_indices = %d(%d), band_5g_low(high)_num_chan_indices = %d(%d) 
481,i,[ wlan_scan_unit_test.c : 53 ] SCAN_NUM_SUPP_CHAN_LIST %d 
483,i,[ wlan_scan_6g_discv.c : 669 ] SCAN_FILSD_HANDLER_ERROR err_code = %d 
482,iiI,[ wlan_scan_6g_discv.c : 707 ] SCAN_FILSD_PARSER_ERROR rx_freq = %d len = %d ret = 0x%x 
491,iii,[ wlan_thermal_unit_test.c : 86 ] WLAN_THERMAL_TSENS_TEMP_1 temp_req = %d, sensor_id = %d, temp = %d 
490,iiiiiiii,[ wlan_thermal_unit_test.c : 96 ] WLAN_THERMAL_TSENS_TEMP_2 sensor[1-8] %d %d %d %d %d %d %d %d 
489,ii,[ wlan_thermal_unit_test.c : 369 ] wlan_thermal_unit_test %d %d 
488,ii,[ wlan_thermal_unit_test.c : 48 ] WLAN_THERMAL_TSENS_INVALID_CONFIG vdev_id = %d, num_args = %d 
487,iiiiii,[ wlan_thermal_unit_test.c : 52 ] WLAN_THERMAL_TSENS_RECONFIG num_args = %d, Temp1|2 degC = %d %d, kp|ki|kd = %d %d %d 
486,iiiii,[ wlan_thermal_unit_test.c : 299 ] tt enabled. pdev_id(%d) dc:%d, dc_per_event:%d, hwm:%d, throt_levels:%d 
485,i,[ wlan_thermal_unit_test.c : 314 ] tt disabled for pdev_id: (%d)  
484,iiii,[ wlan_thermal_unit_test.c : 358 ] level configured. level:%d, lwm:%d, hwm:%d, dcoff:%d 
583,,[ wlan_vdev.c : 469 ] vdev connecting client is registered in non wow mode 
582,I,[ wlan_vdev.c : 493 ] allow during connecting, subtype:%x 
581,iiI,[ wlan_vdev.c : 567 ] set_restore_mac_addr status = %d, freq = %d, evh = 0x%x 
580,ii,[ wlan_vdev.c : 6633 ] VDEV_MGR_STA_PS_EVENT: vdev_id=%d, event_type=%d 
579,ii,[ wlan_vdev.c : 1515 ] VDEV EVT:RT thread handle vdev_stop_down_del cmd:%d, vdev_id:%d 
578,iii,[ wlan_vdev.c : 1445 ] VDEV EVT:DATA offload thread handle vdev_stop_down_del msg cmd = %d, vdev_id = %d, vdev_mode = %d 
577,iii,[ wlan_vdev.c : 1351 ] VDEV EVT:RT thread handle vdev_stop_down_del msg cmd = %d, vdev_id = %d, vdev_mode = %d 
576,i,[ wlan_vdev.c : 11123 ] wmi vdev send event %d 
575,II,[ wlan_vdev.c : 7205 ] VDEV_STOP_ABORT_TX try_to_abort, hwq=0x%x, swq=0x%x 
574,II,[ wlan_vdev.c : 7212 ] VDEV_STOP_ABORT_TX abort_fails, hwq=0x%x, swq=0x%x 
573,II,[ wlan_vdev.c : 7216 ] VDEV_STOP_ABORT_TX abort_succeeds, hwq=0x%x, swq=0x%x 
572,II,[ wlan_vdev.c : 7223 ] VDEV_STOP_ABORT_TX after_abort, hwq=0x%x, swq=0x%x 
571,iii,[ wlan_vdev.c : 7243 ] VDEV_STOP_EVT VDEV ID = %d HW Q depth= %d, SW Q depth = %d 
570,ii,[ wlan_vdev.c : 7335 ] WMI_CMD_PARAMS VdevId/AC/Arg1 = %d Cmd/Med-Time/Action/Arg2 = %d 
569,iii,[ wlan_vdev.c : 1006 ] VDEV EVT: vdev create id=%d, mode=%d submode=%d 
568,ii,[ wlan_vdev.c : 1969 ] VDEV EVT: vdev delete id=%d, mode=%d 
567,i,[ wlan_vdev.c : 1557 ] wlan_beacon_tx: vdev id = %d vdev delete return becasue bcn ctxt is not free yet 
566,iii,[ wlan_vdev.c : 1628 ] VDEV EVT: WMI_VDEV_DELETE_RESP_EVENTID vdevId=%d vdev_type: %d vdev_subtype: %d 
565,iiIIi,[ wlan_vdev.c : 1588 ] VDEV EVT peer not cleared idx=%d vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d 
564,,[ wlan_vdev.c : 9462 ] Failed to allocate memory for DISA event!!! 
563,i,[ wlan_vdev.c : 9492 ] DISA event sent to HOST: frame_len=%d 
562,iiiii,[ wlan_vdev.c : 9996 ] Error: vdev id %d, aggregation type %d, ac %d, max num frames %d, enable_bitmap %d 
 
561,iiiiii,[ wlan_vdev.c : 10003 ] vdev id %d, aggregation type %d, ac %d, max num frames %d, enable_bitmap %d rx_size %d
 
560,iiiiii,[ wlan_vdev.c : 10080 ] vdev id %d, ac %d, software retry type %d, software retry threshold %d, pdev->agg_retry_th %d, pdev->non_agg_retry_th %d 
559,i,[ wlan_vdev.c : 9514 ] WMI_VDEV_ENCRYPT_DECRYPT_DATA_REQ_CMDID invalid vdev_id %d 
558,i,[ wlan_vdev.c : 9523 ] WMI_VDEV_ENCRYPT_DECRYPT_DATA_REQ_CMDID invalid data_len %d 
557,i,[ wlan_vdev.c : 9543 ] VDEV_DISPATCH_DISA_FRAME_TX failed status=%d 
556,i,[ wlan_vdev.c : 8814 ] WMI_VDEV_GET_ARP_STAT_CMDID: vdev_id = %d event alloc failed 
555,,[ wlan_vdev.c : 8529 ] wlan_vdev_dispatch_get_big_data Err vdev || vdev not free  
554,i,[ wlan_vdev.c : 8676 ] WMI_VDEV_GET_KEEPALIVE_CMDID: vdev_id = %d event alloc failed 
553,iiiii,[ wlan_vdev.c : 7909 ] 11w PMF vdevId=%d key_ix=%d cipher=%d is_group_key_valid %d group_key_ix %d 
552,,[ wlan_vdev.c : 7992 ] key cache POOL ALLOC FAILURE 
551,iIIi,[ wlan_vdev.c : 8030 ] VDEV_INSTALL_KEY_FAIL vdev_id %d mac_addr %04x:%08x status %d 
550,iIIi,[ wlan_vdev.c : 8078 ] VDEV_INSTALL_KEY_FAIL_MESH vdev_id %d mac_addr %04x:%08x status %d 
549,iI,[ wlan_vdev.c : 8116 ] WAL_DBGID_SET_M4_SENT_MANUALLY  VDEV ID = %d, peer = 0x%x 
548,i,[ wlan_vdev.c : 9725 ] LIMIT_OFFCHAN_ERROR client_id=%d 
547,i,[ wlan_vdev.c : 9735 ] LIMIT_OFFCHAN_ERROR vdev_id=%d 
546,Iiii,[ wlan_vdev.c : 9388 ] dispatch_set_ie_cmd: ie_id = 0x%x, id_len = %d, source=%d, band=%d 
545,Iii,[ wlan_vdev.c : 9406 ] vdev_set_scan_default_ie status = 0x%x vdev_id=%d prunned_ie_len=%d 
544,iII,[ wlan_vdev.c : 8634 ] KA: cmd handler() -> start timer vdev_id = %d keepalive_interval = 0x%x keepalive_method = 0x%x 
543,i,[ wlan_vdev.c : 7737 ] Invalid VDEV in WMI_VDEV_SET_WMM_PARAMS_CMDID, VDEV ID = %d 
542,i,[ wlan_vdev.c : 7760 ] WMI_VDEV_SET_WMM_PARAMS_CMDID type=%d 
541,IIII,[ wlan_vdev.c : 7773 ] WMI_VDEV_SET_WMM_PARAMS_CMDID ac[31-16]/acm[15-0] = 0x%x cw_min = 0x%x cw_max = 0x%x txop_limit[31-16]/aifs[15-0] = 0x%x 
540,i,[ wlan_vdev.c : 7744 ] Invalid WAL VDEV in WMI_VDEV_SET_WMM_PARAMS_CMDID, VDEV ID = %d 
539,Iiii,[ wlan_vdev.c : 7534 ] Rejecting vdev_start Invalid Regdomain  vdev_id= 0x%x, host_regdomain = %d regdomain = %d isDFSSTA=%d 
538,I,[ wlan_vdev.c : 7546 ] Rejecting vdev_start Roaming in progress  vdev_id= 0x%x  
537,I,[ wlan_vdev.c : 7555 ] Rejecting vdev_start BSS Peer not created  vdev_id= 0x%x  
536,I,[ wlan_vdev.c : 7563 ] Rejecting vdev_start Home channel not in supported band vdev_id= 0x%x  
535,III,[ wlan_vdev.c : 7584 ] Rejecting vdev_start request from requestor_id = 0x%x. start_delay_us = 0x%x, max_start_delay_us=0x%x 
534,iI,[ wlan_vdev.c : 7597 ] Rejecting vdev_start request for vdev_id = %d from requestor_id = 0x%x. STA + STA not supported 
533,i,[ wlan_vdev.c : 7652 ] STA-DFS flag SET in wmi_channel for vdev %d 
532,IIIIIii,[ wlan_vdev.c : 8410 ] WLAN_DISPATCH_VDEV_UP vdev_flags:0x%x vdev_bssid:%x_%x trans_bssid:%x_%x profile_idx:%d profile_num:%d 
531,,[ wlan_vdev.c : 8446 ] WLAN_DISPATCH_VDEV_UP !!!host sends wrong MBSSID param!!! 
530,iii,[ wlan_vdev.c : 8187 ] WMI_CMD_PARAMS AC = %d Med-Time usec = %d DwnGrd_Type = %d 
529,ii,[ wlan_vdev.c : 8879 ] dispatch_wmm_delts_cmd: ac = %d vdev id = %d 
528,,[ wlan_vdev.c : 8899 ] dispatch_wmm_delts_cmd: end 
527,ii,[ wlan_vdev.c : 4614 ] VDEV EVT: vdev down id=%d, mode=%d 
526,ii,[ wlan_vdev.c : 9348 ] vdev_extract_mandatory_ies: id=%d, len=%d 
525,Ii,[ wlan_vdev.c : 9262 ] vdev_extract_optional_vendor_ies: oui=0x%x, len=%d 
524,I,[ wlan_vdev.c : 6906 ] VDEV free error, peer addr:0x%x, mac:0x8x 0x8x 
523,ii,[ wlan_vdev.c : 10584 ] SET TPC POWER CMD num_pwr_levels limit exceeded vdev_id %d num_pwr_levels %d 
522,iii,[ wlan_vdev.c : 10601 ] VDEV_SET_PARAM_TPC_POWER psd_power=%d, eirp_power=%d, num_pwr_levels=%d 
521,iiiii,[ wlan_vdev.c : 10569 ] wlan_vdev_handle_wfa_config_cmd override_rsnxe=%d, ignore_csa=%d, deauth_on_saquery_timeout=%d override_oci_chan frame_types=%d, override_oci_chan=%d 
520,iIii,[ wlan_vdev.c : 9686 ] LIMIT_OFFCHAN_ARBITER client=%d flag=0x%x max_offchan_time=%d rest_time=%d 
519,Iii,[ wlan_vdev.c : 9708 ] LIMIT_OFFCHAN_ARBITER_RESULT flag=0x%x max_offchan_time=%d rest_time=%d 
518,II,[ wlan_vdev.c : 2417 ] wlan_vdev_migrate vdev_id[31-16]/from_mac[15-8]/to_mac[7-0] 0x%x, is_up[24]/is_active[16]/mode[15-8]/submode[7-0] 0x%x 
517,,[ wlan_vdev.c : 7430 ] WMI_EVENT_ALLOC_FAILURE: VDEV_REJECT_VDEV_START_REQ_RESP_EVENTID buffer failure 
516,ii,[ wlan_vdev.c : 9102 ] vdev_set_mandatory_ie: ie_id=%d, id_len=%d 
515,i,[ wlan_vdev.c : 9213 ] vdev_set_mandatory_ie: not handled ie_id=%d 
514,iii,[ wlan_vdev.c : 8998 ] vdev_set_mandatory_ie_by_band: ie_id=%d, band=%d, id_len=%d 
513,ii,[ wlan_vdev.c : 5482 ] WMI_CMD_PARAMS VdevId/AC/Arg1 = %d Cmd/Med-Time/Action/Arg2 = %d 
512,iII,[ wlan_vdev.c : 5487 ] vdev_id: %d vdev_set_param: id: 0x%x param_value: 0x%x 
511,iII,[ wlan_vdev.c : 6008 ] WLAN_VDEV_SET_PARAM_FAIL3 paramid:%d vdevp:0x%x vdevp->bss:0x%x 
510,iii,[ wlan_vdev.c : 6231 ] WMI_VDEV_PARAM_DISABLE_NOA_P2P_GO ic_mode:%d ic_subopmode:%d param:%d  
509,ii,[ wlan_vdev.c : 6250 ] WMI_VDEV_PARAM_SMPS_INTOLERANT: vdev_id:%d, param:%d 
508,I,[ wlan_vdev.c : 6449 ] Setting CABQ to %x 
507,,[ wlan_vdev.c : 6497 ] Err: WMI_VDEV_PARAM_NTH_BEACON_TO_HOST command came for non STA vdev 
506,IiiiiiI,[ wlan_vdev.c : 3314 ] VDEV_START: vdev_id[31-24]/mode[23-16]/mode[15-8]/mac_id[7-0] = 0x%x chan_mhz = %d  phy_mode=%d band_center_freq1=%d band_center_freq2=%d ldpc_rx_enabled=%d vdev_flags:0x%x 
505,IiI,[ wlan_vdev.c : 3507 ] VDEV_MGR_HP_START_TIME  vdev_id = 0x%x chan_mhz = %d start_tsf = 0x%x 
504,Ii,[ wlan_vdev.c : 599 ] resmgr link already exist: 0x%X vdev_id = %d 
503,iIIII,[ wlan_vdev.c : 8228 ] wlan_vdev_tsf_report: vdev_id = %d, tsf_low = 0x%x, tsf_high = 0x%x, qtimer_low=0x%x, qtimer_high=0x%x 
502,iI,[ wlan_vdev.c : 8249 ] wlan_vdev_tsf_tstamp_action:vdev_id = %d, action = 0x%x 
501,ii,[ wlan_vdev.c : 8257 ] wlan_vdev_tsf_tstamp_action: vdev_id = %d, vdev_ifUp = %d 
500,iI,[ wlan_vdev.c : 11146 ] wlan_vdev_unit_test: vdev_id = %d, cmd = WMI_VDEV_PARAM_ABG_MODE_TX_CHAIN_NUM, value = 0x%x 
499,ii,[ wlan_vdev.c : 4159 ] VDEV_MGR_VDEV_UP id=%d, mode=%d 
498,i,[ wlan_vdev.c : 4377 ] VDEV RESMGR_LINK_ATTR_SMPS_VALID Peer_flags:%d 
497,i,[ wlan_vdev.c : 4419 ] VDEV RESMGR_LINK_ATTR_SMPS_VALID VHT mode:%d 
496,iII,[ wlan_vdev.c : 4486 ] KA: wlan_vdev_up() -> start timer vdev_id = %d keepalive_interval = 0x%x keepalive_method = 0x%x 
495,i,[ wlan_vdev.c : 2723 ] wlan_vdevs_migrate, vdevs_migrate_duration = %d us 
494,iiii,[ wlan_vdev.c : 780 ] WMI NRP Config : addr1=%d, idx=%d, type=%d, action=%d 
493,iii,[ wlan_vdev.c : 6940 ] WAL Peer event vdevp %d is_free %d, is_vdev_stopping %d 
492,iii,[ wlan_vdev.c : 6948 ] WAL Peer event Vdev ID = %d HW Q depth= %d, SW Q depth = %d 
602,iii,[ wlan_vdev_misc.c : 1138 ] VDEV_MGR_MY_BEACON_PARSED malformed id = %d len=%d remain_len=%d 
601,iiI,[ wlan_vdev_misc.c : 1170 ] VDEV_MGR_MY_BEACON_BAD_IE id=%d,len=%d,status=0x%x 
600,IIIII,[ wlan_vdev_misc.c : 1061 ] wlan_vdev_256BA_support_check :: VENDOR SPECIFIC IE :%u, %u, %02x, %02x, %02x 
599,IIIIII,[ wlan_vdev_misc.c : 970 ] VENDOR SPECIFIC IE :%u, %u, %02x, %02x, %02x, %02x 
598,ii,[ wlan_vdev_misc.c : 3267 ] User configured fils discovery period (%d) is more than max supported value (%d). Capping fd period to max supported 
597,ii,[ wlan_vdev_misc.c : 2835 ] wlan_vdev_fill_vdev_mac_entry: vdev_id=%d, pdev_id=%d 
596,,[ wlan_vdev_misc.c : 3208 ] FD_TMPL_CMD: buf_len is greater than max len 
595,,[ wlan_vdev_misc.c : 3216 ] FD_TMPL_CMD: invalid vdev_id 
594,,[ wlan_vdev_misc.c : 3225 ] failed to allocate buffer for FD TMPL CMD 
593,I,[ wlan_vdev_misc.c : 2985 ] wlan_vdev_get_migrate_active_vdev_list  vdev_id_list=0x%x 
592,I,[ wlan_vdev_misc.c : 1701 ] Received IBSS Beacon peer = 0x%x send_to_host =  
591,iIIIiii,[ wlan_vdev_misc.c : 1435 ] VDEV_MGR_MY_BEACON_RECEIVED: vdev_id = %d curr_time = 0x%x  curr_vdev_tsf = 0x%x seq = 0x%x rssi = %d bss_ch = %d recv_ch = %d 
590,iii,[ wlan_vdev_misc.c : 1529 ] VDEV_MGR_HANDLE_OWN_BEACON fail freq:%d len:%d err_code:%d(1:NULL_wal_peer 2:ch_0 3:NULL_wlan_peer 4:short_len) 
589,i,[ wlan_vdev_misc.c : 3770 ] wlan_vdev_is_mcc_vdev_connect_in_progress result %d 
588,IIIIi,[ wlan_vdev_misc.c : 2075 ] OMI: Error peernss = 0x%lx OMI nss = 0x%lx bssBw= %1x OMI Bw= %1x peerMaxBw = %d
 
587,IIIII,[ wlan_vdev_misc.c : 1086 ] set_ignore_check_for_OUI :: VENDOR SPECIFIC IE :%u, %u, %02x, %02x, %02x 
586,IIII,[ wlan_vdev_misc.c : 1325 ] MU EDCA BEACON UPDATE FROM AP                     ac = 0x%x cw_min = 0x%x cw_max = 0x%x                     mu_edca_timer[31-16]/aifs[15-0] = 0x%x 
585,iiii,[ wlan_vdev_misc.c : 1345 ] MU EDCA BEACON: ignoring edca update qos_present=%d                 mu_edca_present=%d bcn_update_cnt=%d vdev_update_cnt=%d 
584,i,[ wlan_vdev_misc.c : 325 ] STA_KICKOUT: Reason=%d 
612,iIIII,[ wlan_vdev_keepalive.c : 770 ] KA: VDEV_MGR_AP_KEEPALIVE_INACTIVE  vdev_id = %d cur_txrx_ref_time = 0x%x last_txrx_time = 0x%xlast_tx_time = 0x%x last_rx_time = 0x%x 
611,IIi,[ wlan_vdev_keepalive.c : 781 ] KA: wlan_vdev_keepalive_ready_to_send cur_txrx_ref_time = 0x%x last_txrx_time = 0x%x inactive_time_ms = %d 
610,iIII,[ wlan_vdev_keepalive.c : 374 ] VDEV_MGR_AP_KEEPALIVE_IDLE  vdev_id = %d assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x 
609,iiIIIIIi,[ wlan_vdev_keepalive.c : 449 ] VDEV_MGR_AP_KEEPALIVE KICKOUT: vdevid:%d, aid:%d, max_inactivity:0x%x last_txrx_activity:0x%x curr_time:0x%x, data_act:0x%x, mgmt_ctrl_act:0x%x, IdleOption:%d 
608,III,[ wlan_vdev_keepalive.c : 492 ] IBSS Keep Alive  rx_last_activity = 0x%x ibss_max_bcn_lost_uses = 0x%x current time = 0x%x 
607,IIII,[ wlan_vdev_keepalive.c : 380 ] VDEV_MGR_AP_KEEPALIVE_INACTIVE  vdev_id = 0x%x assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x 
606,iIII,[ wlan_vdev_keepalive.c : 386 ] VDEV_MGR_AP_KEEPALIVE_UNRESPONSIVE  vdev_id = %d assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x 
605,i,[ wlan_vdev_keepalive.c : 838 ] VDEV_MGR_FIRST_BMISS_DETECTED: vdev_id = %d 
604,i,[ wlan_vdev_keepalive.c : 848 ] VDEV_MGR_FINAL_BMISS_DETECTED: vdev_id = %d 
603,i,[ wlan_vdev_keepalive.c : 880 ] VDEV_MGR_BCN_IN_SYNC: vdev_id = %d  
640,iIIII,[ wlan_vdev_schedule.c : 618 ] VDEV_MGR_AP_TBTT_CONFIG: vdev_id =%d, chan_mhz = 0x%x, tbtt_link_type = 0x%x, ni_intval = 0x%x, tbtt_offset = 0x%x 
639,iII,[ wlan_vdev_schedule.c : 690 ] Corr_sta_tbtt_drift: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x 
638,iIIi,[ wlan_vdev_schedule.c : 3139 ] VDEV_MGR AP Connection protection critical channel request: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x, duration = %d 
637,iIIi,[ wlan_vdev_schedule.c : 3074 ] VDEV_MGR SWBA  protection critical channel request: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x, duration = %d 
636,,[ wlan_vdev_schedule.c : 1800 ] vdev_bmiss_crit_ch_req_cb: ch_req granted 
635,,[ wlan_vdev_schedule.c : 1840 ] vdev_bmiss_crit_ch_req_cb: ch_req completed without receiving beacon 
634,i,[ wlan_vdev_schedule.c : 2483 ] VDEV_MGR_VDEV_START_OCS_HP_REQ_STOP: vdev_id = %d 
633,i,[ wlan_vdev_schedule.c : 2518 ] VDEV_MGR_FIRST_BCN_RECEIVED: vdev_id = %d 
632,i,[ wlan_vdev_schedule.c : 2523 ] VDEV_MGR_PEER_AUTHORIZED: vdev_id = %d 
631,i,[ wlan_vdev_schedule.c : 2545 ] VDEV_MGR_VDEV_START_OCS_HP_REQ_STOP: vdev_id = %d 
630,i,[ wlan_vdev_schedule.c : 2557 ] WLAN_VDEV_DPD_CAL_START vdev_id:%d 
629,iI,[ wlan_vdev_schedule.c : 2385 ] VDEV_MGR_VDEV_START_OCS_HP_REQ_COMPLETE without VDEV UP: vdev_id = %d, ch_req_flag = 0x%x 
628,i,[ wlan_vdev_schedule.c : 2424 ] VDEV_MGR_VDEV_START_OCS_HP_REQ_COMPLETE: vdev_id = %d 
627,ii,[ wlan_vdev_schedule.c : 2116 ] WLAN_VDEV_DPD_CAL_DONE vdev_id:%d ch:%d 
626,iiI,[ wlan_vdev_schedule.c : 2244 ] multi_vdev response: vdev_id=%d, num_multi_vdev_restart_compl=%d, multi_vdev_restart_bitmap=0x%x 
625,ii,[ wlan_vdev_schedule.c : 2065 ] WMI_EVENT_ALLOC_FAILURE: vdev_id = %d, opmode = %d, evt_id = WMI_PDEV_MULTIPLE_VDEV_RESTART_RESP_EVENTID 
624,i,[ wlan_vdev_schedule.c : 2090 ] multi_vdev WMI_EVENT_SEND: pdev_id = %d, event = WMI_PDEV_MULTIPLE_VDEV_RESTART_RESP_EVENTID 
623,ii,[ wlan_vdev_schedule.c : 1985 ] WMI_EVENT_ALLOC_FAILURE: vdev_id = %d, opmode = %d, evt_id = WMI_VDEV_START_RESP_EVENTID 
622,ii,[ wlan_vdev_schedule.c : 2039 ] WMI_EVENT_SEND: vdev_id = %d, opmode = %d, event = WMI_VDEV_START_RESP_EVENTID 
621,iII,[ wlan_vdev_schedule.c : 3370 ] wlan_vdev_sta_concurrency_event_handler: vdev_id = %d, next_state  = 0x%x, cur_state = 0x%x 
620,Ii,[ wlan_vdev_schedule.c : 1965 ] SCAN_RADIO_SUPPORT_DBUG scan_radio_lpri_req setup lp_ch_req created = %p channel = %d
 
619,,[ wlan_vdev_schedule.c : 3006 ] VDEV_MGR_FIRST_BMISS_DETECTED: Post Critical ch_req 
618,iIII,[ wlan_vdev_schedule.c : 1425 ] VDEV_MGR_AP_TBTT_CONFIG: vdev_id = %d, chan_mhz = 0x%x, tbtt_link_type = 0x%x, ap_tbtt_offset = 0x%x 
617,iI,[ wlan_vdev_schedule.c : 2789 ] VDEV_MGR_LOWPOWER_HP_CHREQ_ENABLED: vdev_id = %d, chan_mhz  = 0x%x 
616,iII,[ wlan_vdev_schedule.c : 2872 ] VDEV_MGR_HP_START_TIME: vdev_id = %d, chan_mhz  = 0x%x, start_tsf = 0x%x 
615,iI,[ wlan_vdev_schedule.c : 2907 ] VDEV_MGR_LOWPOWER_LP_CHREQ_ENABLED: vdev_id = %d, factor = 0x%x 
614,iI,[ wlan_vdev_schedule.c : 2913 ] VDEV_MGR_LOWPOWER_LP_CHREQ_ENABLED: vdev_id = %d, factor = 0x%x 
613,iII,[ wlan_vdev_schedule.c : 2931 ] VDEV_MGR_OCS_HP_LP_REQ_POSTED: vdev_id = %d, hp_ch_req = 0x%x, lp_ch_req = 0x%x 
654,iI,[ wlan_vdev_pause.c : 475 ] VDEV Unpause Failure: VDEV ID = %d pause_bitmap = 0x%x in Unpause complete 
653,ii,[ wlan_vdev_pause.c : 1251 ] Disable leaky AP CTS2S: vdev_id = %d pause_delay_us = %d  
652,I,[ wlan_vdev_pause.c : 1254 ] enable_null_leaky_ap_pause=0x%x 
651,I,[ wlan_vdev_pause.c : 585 ] vdev->bcn_tx_paused_wlan_vdev_pause_1=0x%x 
650,,[ wlan_vdev_pause.c : 603 ] VDEV_PAUSE_FAIL ifPaused set with pause_bitmap = 0 in _wlan_vdev_pause 
649,IiiiI,[ wlan_vdev_pause.c : 669 ] VDEV_MGR_VDEV_PAUSE: enable_null_leaky_ap_pause=0x%x no_null_to_ap_for_roaming=%d leakyAp_cts2s_enable=%d pause_delay_us=%d req from mod_id = %x 
648,iiiii,[ wlan_vdev_pause.c : 249 ] VDEV_MGR_VDEV_PAUSE_COMP: vdev_id = %d pause_status = LEAKY AP DETECTED data_null_tx_delay = %d actual_leak_window = %d pause_delay_us = %d consec_detect_leaky_ap_cnt = %d 
647,iiiii,[ wlan_vdev_pause.c : 383 ] VDEV_MGR_VDEV_PAUSE_DELAY_UPDATE: vdev_id = %d avg_data_null_tx_delay = %d avg_rx_leak_window = %d pause_delay_us = %d is_bt_connected = %d 
646,iiiii,[ wlan_vdev_pause.c : 304 ] VDEV_MGR_VDEV_PAUSE_COMP: vdev_id = %d pause_status = FAILURE data_null_tx_delay = %d avg_data_null_tx_delay = %d actual_leak_window = %d avg_rx_leak_window = %d 
645,iiiii,[ wlan_vdev_pause.c : 327 ] VDEV_MGR_VDEV_PAUSE_COMP: vdev_id = %d pause_status = SUCCESS data_null_tx_delay = %d avg_data_null_tx_delay = %d actual_leak_window = %d avg_rx_leak_window = %d 
644,i,[ wlan_vdev_pause.c : 1262 ] no_null_to_ap_for_roaming=%d 
643,I,[ wlan_vdev_pause.c : 853 ] VDEV_UNPAUSE_FAIL: ifPaused not set with pause_bitmap = 0x%x in _wlan_vdev_unpause 
642,,[ wlan_vdev_pause.c : 894 ] VDEV_MGR_VDEV_PAUSE unpause non_protocol_unpaused 
641,,[ wlan_vdev_pause.c : 960 ] VDEV_MGR_VDEV_PAUSE csa_roaming_ongoing and no host unpause 
659,,[ wlan_vdev_unit_test.c : 86 ] wlan_vdev_config_test: vdev is NULL 
658,iiii,[ wlan_vdev_unit_test.c : 157 ] wlan_vdev_unit_test: vdev_id = %d, custom_sw_retry_th_cmd, ac %d sw_retry_type = %d sw_retry_th = %d 
657,I,[ wlan_vdev_unit_test.c : 232 ] wlan_vdev_unit_test: g_wmi_cmd_enable_pf_log = 0x%x 
656,iiiii,[ wlan_vdev_unit_test.c : 100 ] wlan_vdev_config_test: vdev_id = %d, test_cmd = %d, args[1] = %d, args[2] = %d, num_args = %d  
655,iii,[ wlan_vdev_unit_test.c : 135 ] wlan_vdev_unit_test: vdev_id = %d, custom_aggr_size_cmd, subfram %d ac = %d 
686,,[ wlan_pmf_offload.c : 1141 ] 11w PMF: PN Replay attack detected 
685,ii,[ wlan_pmf_offload.c : 1035 ] 11w PMF KEY ID MISMATCH MMIE key_id = %d, igtk_key_id = %d 
684,i,[ wlan_pmf_offload.c : 723 ] 11w PMF: can not handle frame size: %d 
683,,[ wlan_pmf_offload.c : 742 ] 11w PMF: IE is not Mgmt MIC IE or Invalid length 
682,,[ wlan_pmf_offload.c : 764 ] 11w PMF: BC/MC/Beacon MGMT IPN check Failed 
681,,[ wlan_pmf_offload.c : 836 ] 11w PMF: BC/MC/Beacon CMAC MGMT frame MMIE MIC check Failed 
680,,[ wlan_pmf_offload.c : 913 ] 11w PMF: BC/MC/Beacon GMAC MGMT frame MMIE MIC check Failed 
679,,[ wlan_pmf_offload.c : 970 ] 11W PMF: MMIE valid 
678,iiIII,[ wlan_pmf_offload.c : 1207 ] 11W PMF mgmt hdlr subtype=%d len=%d wal_peer: %p vdev: %p wlan_peer:%p 
677,,[ wlan_pmf_offload.c : 1217 ] 11W PMF mgmt hdlr pmf not enabled 
676,,[ wlan_pmf_offload.c : 1242 ] 11W PMF mgmt hdlr pmf not enabled 
675,,[ wlan_pmf_offload.c : 1251 ] 11W PMF mgmt hdlr frame not from Associated AP  
674,,[ wlan_pmf_offload.c : 1284 ] 11w PMF BIP check failed  
673,I,[ wlan_pmf_offload.c : 1299 ] 11w PMF decrypt error, rx status 0x%x 
672,,[ wlan_pmf_offload.c : 1322 ] 11w PMF drop unenryp robust action category 
671,IIII,[ wlan_pmf_offload.c : 1331 ] 11w PMF action frm %x %x %x %x 
670,ii,[ wlan_pmf_offload.c : 1374 ] 11w PMF current transId=%d startTransId=%d 
669,,[ wlan_pmf_offload.c : 1379 ] 11w PMF SA query rsp with valid transId rcvd 
668,Ii,[ wlan_pmf_offload.c : 1396 ] 11w PMF deauth/disassoc reason_code %x frmType=%d 
667,i,[ wlan_pmf_offload.c : 1399 ] 11w PMF send SA query state=%d 
666,ii,[ wlan_pmf_offload.c : 565 ] 11W PMF: SA query timeout hdlr vdevId=%d, query_state=%d  
665,ii,[ wlan_pmf_offload.c : 570 ] 11W PMF: SA query timeout hdlr cur retry cnt=%d, max retry cnt=%d  
664,iiii,[ wlan_pmf_offload.c : 1078 ] 11W PMF: Send SA query vdevId=%d, transId=%d query_type=%d tx_status=%d 
663,iii,[ wlan_pmf_offload.c : 658 ] 11W PMF: Update iGTK vdevId=%d, keyIdx=%d, KeyLen=%d 
662,,[ wlan_pmf_offload.c : 675 ] igtk: Same key reinstalled 
661,iii,[ wlan_pmf_offload.c : 618 ] 11W PMF Offload CMD hdlr: WMI_PMF_OFFLOAD_SET_SA_QUERY_CMDID vdevId=%d, interval=%d, retry_count=%d 
660,,[ wlan_pmf_offload.c : 1458 ] 11w PMF is not enabled 
694,iii,[ wlan_roam_host.c : 126 ] ROAM_LOW_RSSI_INTERRUPT  bcn_rssi_avg =  -%d dBm bcn_rssi_last = -%d dBm hi_thresh = -%d dBm 
693,iii,[ wlan_roam_host.c : 139 ] ROAM_LOW_RSSI_INTERRUPT  bcn_rssi_avg =  -%d dBm bcn_rssi_last = -%d dBm hi_thresh = -%d dBm  
692,i,[ wlan_roam_host.c : 324 ] ROAM_VDEV_EVT_NOT_INUSE type=%d 
691,,[ wlan_roam_host.c : 202 ] ROAM_FREE_NOT_IN_USE 
690,i,[ wlan_roam_host.c : 232 ] ROAM_CONFIG_RSSI_CHANGE  chagne_val = %d 
689,i,[ wlan_roam_host.c : 242 ] ROAM_CONFIG_RSSI_CHANGE  chagne_val = %d dBm  
688,,[ wlan_roam_host.c : 260 ] ROAM_START_FAIL_NOT_INUSE 
687,,[ wlan_roam_host.c : 288 ] ROAM_STOP_FAIL_NOT_INUSE 
695,iiiii,[ wlan_roam_wmi.c : 399 ] ROAM_EVENT_TO_HOST reason=%d, notif=%d, notif_params=%d, ret=%d ev_size=%d 
699,iII,[ wlan_dsm_filter.c : 213 ] DSM_LIST_UPDATE bssid_type = %d bssid removed is %08x%04x 
698,iIIiiiii,[ wlan_dsm_filter.c : 104 ] i | bssid_type = %d, bssid_disallow_ap = %08x%04x retry_delay = %d msec, rssi = %d dbm source|reason = %d original_timestamp = %d original_timeout = %d 
697,iIIiiiii,[ wlan_dsm_filter.c : 196 ] FW added:  i | bssid_type = %d, bssid_disallow_ap = %08x%04x retry_delay = %d msec, rssi = %d dbm source|reason = %d original_timestamp = %d original_timeout = %d 
696,iIIii,[ wlan_dsm_filter.c : 346 ] AP Blacklisted: bssid_type = %d, bssid %08x%04x exp_delay = %d msec, exp_rssi = %ddBm 
709,I,[ wlan_framegen.c : 2180 ] WLAN_FRMGEN_GET_ACTION_SMPS incorrect sm_power_control:0x%x 
708,iIiIiIiI,[ wlan_framegen.c : 1858 ] WLAN_FRMGEN_GET_ACTION_TM lci_ie_len:%d lci_ie:0x%x civ_ie_len:%d civ_ie:0x%x ftm_ie_len:%d ftm_ie:0x%x vendor_ie_len:%d vendor_ie:0x%x 
707,iIiIiIiI,[ wlan_framegen.c : 1685 ] WLAN_FRMGEN_GET_ACTION_TMR lci_ie_len:%d lci_ie:0x%x civ_ie_len:%d civ_ie:0x%x ftm_ie_len:%d ftm_ie:0x%x vendor_ie_len:%d vendor_ie:0x%x 
706,iiii,[ wlan_framegen.c : 5472 ] bss color gen evt rpt ie_len=%d evt_token=%d evt_type=%d evt_status=%d 
705,iIi,[ wlan_framegen.c : 5873 ] frmgen_get_default_ie vdev_id=%d fc_type=0x%x length=%d 
704,III,[ wlan_framegen.c : 263 ] WLAN_FRMGEN_GET_NULLFUNC_WITH_HTCTRL FAIL! peer:0x%x addr1:0x%x addr3:0x%x 
703,i,[ wlan_framegen.c : 1514 ] SKIPPED inserting some IE's error_code:%d 
702,iIIi,[ wlan_framegen.c : 5839 ] frmgen_insert_default_ie vdev_id=%d frm_type=0x%x sub_type=0x%x ies_len=%d 
701,IIIi,[ wlan_framegen.c : 5970 ] frmgen_set_default_ie: vdev=0x%x,frm_type=0x%x,buf=0x%x,len=%d 
700,iIiii,[ wlan_framegen.c : 6017 ] frmgen_set_default_ie vdev_id=%d frm_type=0x%x ies_len=%d status=%d i=%d 
775,ii,[ wlan_frameparse.c : 5323 ] FRAME_PARSER frm_len=%d fils_d_size=%d 
774,iiii,[ wlan_frameparse.c : 4991 ] bss color parse evt rpt ie_len=%d evt_token=%d evt_type=%d evt_status=%d 
773,iii,[ wlan_frameparse.c : 581 ] FRMPARSE_WARN ie->ie_len %d (exp %d) remaining_len %d. ignore this IE 
772,ii,[ wlan_frameparse.c : 3885 ] MLME_FRMPARSE_WARN_EXT_CAP ie->ie_len %d (remaining %d) ignore this IE 
771,i,[ wlan_frameparse.c : 3891 ] MLME_FRMPARSE_WARN_EXT_CAP ie->ie_len %d ignore this IE 
770,ii,[ wlan_frameparse.c : 1366 ] MLME_FRMPARSE_WARN_EXT_SUPP_RATE ie->ie_len %d remaining_len %d. ignore this IE 
769,iii,[ wlan_frameparse.c : 1375 ] MLME_FRMPARSE_WARN_EXT_SUPP_RATE rate_index %d (> %d)-> trimmed to %d 
768,I,[ wlan_frameparse.c : 1386 ] MLME_FRMPARSE_WARN_EXT_SUPP_RATE skipped unknown rate 0x%x 
767,,[ wlan_frameparse.c : 1393 ] MLME_FRMPARSE_WARN_EXT_SUPP_RATE no known rate value 
766,iiiI,[ wlan_frameparse.c : 5097 ] wlan_frmparse_get_mgmt_payload frm_len=%d iv_len=%d ivmic_len=%d htctrl_len=%u 
765,ii,[ wlan_frameparse.c : 733 ] MLME_FRMPARSE_WARN_HE_6GHZ_BAND_CAP ie->ie_len %d (exp %d) ignore this IE 
764,ii,[ wlan_frameparse.c : 740 ] MLME_FRMPARSE_WARN_HE_6GHZ_BAND_CAP remaining_len %d (exp %d) ignore this IE 
763,ii,[ wlan_frameparse.c : 638 ] MLME_FRMPARSE_HE_CAP remaining_len %d (exp %d) ignore this IE 
762,ii,[ wlan_frameparse.c : 645 ] MLME_FRMPARSE_HE_CAP remaining_len %d (exp %d) ignore this IE 
761,ii,[ wlan_frameparse.c : 678 ] MLME_FRMPARSE_HE_CAP_MSC remaining_len %d (exp %d) ignore this IE 
760,ii,[ wlan_frameparse.c : 708 ] MLME_FRMPARSE_HE_PPET remaining_len %d (exp %d) ignore this IE 
759,iiii,[ wlan_frameparse.c : 557 ] FRMPARSE he op ie heop_present=%d vht_op_present=%d 6ghz_op=%d max_co_loc_bssid_present=%d. 
758,ii,[ wlan_frameparse.c : 266 ] MLME_FRMPARSE_WARN_HT_CAP ie->ie_len %d (exp %d) ignore this IE 
757,ii,[ wlan_frameparse.c : 272 ] MLME_FRMPARSE_WARN_HT_CAP remaining_len %d (exp %d) ignore this IE 
756,ii,[ wlan_frameparse.c : 325 ] MLME_FRMPARSE_WARN_HT_OPER ie->ie_len %d (exp %d) ignore this IE 
755,ii,[ wlan_frameparse.c : 331 ] MLME_FRMPARSE_WARN_HT_OPER remaining_len %d (exp %d) ignore this IE 
754,,[ wlan_frameparse.c : 4925 ] FRM_PARSE_IE_ITERATOR ie_buffer_start is NULL 
753,ii,[ wlan_frameparse.c : 4932 ] FRM_PARSE_IE_ITERATOR ERROR remaining_length(%d) < ie_hdr_size(%d) 
752,ii,[ wlan_frameparse.c : 4939 ] FRM_PARSE_IE_ITERATOR ERROR remaining_length(%d) < ie_len(%d) 
751,ii,[ wlan_frameparse.c : 1645 ] FRMPARSE_WARN_MU_EDCA_PARAM ie->ie_len %d (exp %d). ignore this IE 
750,ii,[ wlan_frameparse.c : 1652 ] FRMPARSE_WARN_MU_EDCA_PARAM ie->ie_len %d remaining_len %d. ignore this IE 
749,ii,[ wlan_frameparse.c : 84 ] MLME_FRMPARSE_WARN_QBSS ie->ie_len %d remaining_len %d. ignore this IE 
748,ii,[ wlan_frameparse.c : 89 ] MLME_FRMPARSE_WARN_QBSS ie->ie_len %d (!= %d) 
747,ii,[ wlan_frameparse.c : 1263 ] MLME_FRMPARSE_WARN_SSID ie->ie_len %d (> %d) 
746,ii,[ wlan_frameparse.c : 1270 ] MLME_FRMPARSE_WARN_SSID ie->ie_len %d remaining_len %d. ignore this IE 
745,ii,[ wlan_frameparse.c : 1304 ] MLME_FRMPARSE_WARN_SUPP_RATE ie->len %d (> %d)-> ignore this IE 
744,ii,[ wlan_frameparse.c : 1312 ] MLME_FRMPARSE_WARN_SUPP_RATE ie->ie_len %d remaining_len %d. ignore this IE 
743,I,[ wlan_frameparse.c : 1327 ] MLME_FRMPARSE_WARN_SUPP_RATE skipped unknown rate 0x%x 
742,,[ wlan_frameparse.c : 1336 ] MLME_FRMPARSE_WARN_SUPP_RATE no known rate value 
741,i,[ wlan_frameparse.c : 4634 ] MLME_FRMPARSE_VENDOR_VHT unknown type %d 
740,ii,[ wlan_frameparse.c : 4651 ] MLME_FRMPARSE_WARN_VENDOR_VHT remaining_len %d (exp %d) ignore this IE 
739,I,[ wlan_frameparse.c : 4664 ] MLME_FRMPARSE_WARN_VENDOR_VHT ERROR vht_caps. status %x
 
738,I,[ wlan_frameparse.c : 4678 ] MLME_FRMPARSE_WARN_VENDOR_VHT ERROR vht_oper. status %x
 
737,ii,[ wlan_frameparse.c : 423 ] MLME_FRMPARSE_WARN_VHT_CAP ie->ie_len %d (exp %d) ignore this IE 
736,ii,[ wlan_frameparse.c : 430 ] MLME_FRMPARSE_WARN_VHT_CAP remaining_len %d (exp %d) ignore this IE 
735,ii,[ wlan_frameparse.c : 370 ] MLME_FRMPARSE_WARN_VHT_OPER ie->ie_len %d (exp %d) ignore this IE 
734,ii,[ wlan_frameparse.c : 377 ] MLME_FRMPARSE_WARN_VHT_OPER remaining_len %d (exp %d) ignore this IE 
733,i,[ wlan_frameparse.c : 2074 ] MLME_FRMPARSE_WPA_IE skip parsing as rsn_ie_len (%d) is present 
732,iIII,[ wlan_frameparse.c : 1791 ] MLME_FRMPARSE_WPA_RSN_CIPHER index %d unknown vendor oui 0x%08x 0x%08x 0x%08x 
731,I,[ wlan_frameparse.c : 1818 ] MLME_FRMPARSE_WPA_RSN_CIPHER_ERR can't use_group for suite type 0x%x 
730,iIi,[ wlan_frameparse.c : 1834 ] MLME_FRMPARSE_WPA_RSN_CIPHER index %d unknown suite type 0x%08x cipher_suite_type = %d 
729,iiiII,[ wlan_frameparse.c : 1847 ] MLME_FRMPARSE_WPA_RSN_CIPHER cipher_suite_count %d is_rsn %d suite_type %d (0=group,1=pair,2=group_mgmt) cipher_type 0x%08x ie_status 0x%x 
728,i,[ wlan_frameparse.c : 1885 ] MLME_FRMPARSE_ERROR_WPA_RSN missing version field. remaining_len %d 
727,ii,[ wlan_frameparse.c : 1892 ] MLME_FRMPARSE_ERROR_WPA_RSN version (%d) is not 1. remaining ie_len %d 
726,i,[ wlan_frameparse.c : 1902 ] MLME_FRMPARSE_WARN_WPA_RSN incomplete group cipher suite. remaining_len = %d (< 4) 
725,i,[ wlan_frameparse.c : 1916 ] MLME_FRMPARSE_WARN_WPA_RSN pairwise suite count remaining_len %d (< 2) 
724,ii,[ wlan_frameparse.c : 1924 ] MLME_FRMPARSE_WARN_WPA_RSN incomplete pairwise cipher suite. remaining_len = %d (< %d) 
723,i,[ wlan_frameparse.c : 1938 ] MLME_FRMPARSE_WARN_WPA_RSN incomplete akm suite count remaining_len %d (< 2) 
722,ii,[ wlan_frameparse.c : 1948 ] MLME_FRMPARSE_WARN_WPA_RSN incomplete akm suite. remaining_len = %d (< %d) 
721,i,[ wlan_frameparse.c : 1959 ] MLME_FRMPARSE_WARN_WPA_RSN incomplete rsn caps. remaining_len = %d (< 2) 
720,,[ wlan_frameparse.c : 1970 ] MLME_FRMPARSE_WARN_WPA_RSN rsn_caps.pre_auth set in WPA. 
719,i,[ wlan_frameparse.c : 1987 ] MLME_FRMPARSE_WARN_WPA_RSN pmkid. remaining_len = %d (< 2) 
718,ii,[ wlan_frameparse.c : 1997 ] MLME_FRMPARSE_WARN_WPA_RSN pmkid. remaining_len = %d (< %d) 
717,i,[ wlan_frameparse.c : 2013 ] MLME_FRMPARSE_WARN_WPA_RSN incomplete group mgmt cipher suite. remaining_len = %d (< 4) 
716,iIII,[ wlan_frameparse.c : 1706 ] MLME_FRMPARSE_WPA_RSN_AKM index %d unknown vendor oui 0x%08x 0x%08x 0x%08x 
715,iI,[ wlan_frameparse.c : 1752 ] MLME_FRMPARSE_WPA_RSN_AKM index %d unknown suite type 0x%08x
 
714,iiIII,[ wlan_frameparse.c : 1758 ] MLME_FRMPARSE_WPA_RSN_AKM akm_suite_count %d is_rsn %d proto 0x%08x key_mgmt 0x%08x ie_status 0x%x 
713,i,[ wlan_frameparse.c : 1079 ] MLME_PHYMODE invaild center freq0 phymode=%d 
712,i,[ wlan_frameparse.c : 1180 ] MLME_PHYMODE invaild center freq0 phymode=%d 
711,iiii,[ wlan_frameparse.c : 860 ] wlan_get_rx_nss nss=%d,%d,%d,%d 
710,iiii,[ wlan_frameparse.c : 906 ] wlan_get_tx_nss nss=%d,%d,%d,%d 
794,iii,[ wlan_key_mgmt.c : 40 ] KEYMGMT_ADD_PEER_ENTRY  key_ciper:%d key_len:%d is_mcast:%d 
793,iIi,[ wlan_key_mgmt.c : 77 ] KEYMGMT_ADD_KEY_ENTRY_REINSTALLATION ERROR id=%d flags=0x%x len=%d 
792,i,[ wlan_key_mgmt.c : 104 ] KEYMGMT_ADD_PEER_ENTRY WEP ERROR key_len:%d 
791,i,[ wlan_key_mgmt.c : 120 ] KEYMGMT_ADD_PEER_ENTRY AES CCM ERROR key_len:%d  
790,i,[ wlan_key_mgmt.c : 137 ] KEYMGMT_ADD_PEER_ENTRY AES GCM ERROR key_len:%d  
789,i,[ wlan_key_mgmt.c : 172 ] KEYMGMT_ADD_PEER_ENTRY ERROR key_ciper:%d 
788,iii,[ wlan_key_mgmt.c : 195 ] wal_peer_set_key type=%d, keyid=%d,pairwise=%d failed 
 
787,i,[ wlan_key_mgmt.c : 43 ] KEYMGMT_ADD_PEER_ENTRY open key_ciper:%d 
786,,[ wlan_key_mgmt.c : 57 ] KEYMGMT_ADD_PEER_ENTRY ERROR! wal_peer is NULL 
785,i,[ wlan_key_mgmt.c : 416 ] KEYMGMT_CLR_KEY_ENTRY id=%d 
784,i,[ wlan_key_mgmt.c : 433 ] KEYMGMT_CLR_KEY_ENTRY id=%d 
783,,[ wlan_key_mgmt.c : 244 ] KEYMGMT_ADD_GROUP_KEY ERROR! wal_peer is NULL 
782,i,[ wlan_key_mgmt.c : 270 ] KEYMGMT_ADD_GROUP_KEY WEP ERROR key_len:%d 
781,i,[ wlan_key_mgmt.c : 327 ] KEYMGMT_ADD_GROUP_KEY ERROR key_ciper:%d 
780,iII,[ wlan_key_mgmt.c : 527 ] KEYMGMT_RESET_KEY id=%d peer_addr=%08x%04x 
779,iiIi,[ wlan_key_mgmt.c : 367 ] KEYMGMT_ADD_KEY_ENTRY id=%d key_idx=%d flags=0x%x len=%d 
778,iIi,[ wlan_key_mgmt.c : 382 ] KEYMGMT_ADD_KEY_ENTRY_EXISTING key_idx=%d flags=0x%x len=%d 
777,ii,[ wlan_key_mgmt.c : 394 ] KEYMGMT_ADD_KEY_ENTRY_NO_MEM id=%d key_idx=%d 
776,iiIiII,[ wlan_key_mgmt.c : 479 ] KEYMGMT_INSTALL_KEY_ENTRY id=%d idx=%d key_flags_bitmap=0x%x len=%d peer_addr=0x04%x08%x 
817,ii,[ wlan_beacon.c : 1152 ] WLAN_BEACON_CANCEL_RESYNC: vdev_id=%d, resyncBeacon=%d 
816,II,[ wlan_beacon.c : 1855 ] nextdtim: 0x%08x%08x 
815,II,[ wlan_beacon.c : 651 ] tsf_beacon: 0x%08x%08x 
814,ii,[ wlan_beacon.c : 1124 ] WLAN_BEACON_RESYNC: vdev_id=%d, resyncBeacon=%d 
813,ii,[ wlan_beacon.c : 2331 ] BEACON_RESYNC_ARBITER_ADD_CLIENT: vdev_id=%d, client_id=%d 
812,i,[ wlan_beacon.c : 2314 ] BEACON_RESYNC_ARBITER_CANCEL_ALL_REQUESTS: vdev_id=%d 
811,ii,[ wlan_beacon.c : 2289 ] BEACON_RESYNC_ARBITER_CANCEL_REQUEST: vdev_id=%d, client_id=%d 
810,ii,[ wlan_beacon.c : 2345 ] BEACON_RESYNC_ARBITER_REMOVE_CLIENT: vdev_id=%d, client_id=%d 
809,ii,[ wlan_beacon.c : 2258 ] BEACON_RESYNC_ARBITER_REQUEST: vdev_id=%d, client_id=%d 
808,iii,[ wlan_beacon.c : 2361 ] BEACON_RESYNC_ARBITER_RESOLVE: vdev_id=%d, is_vdev_holding=%d, SLIST_EMPTY(hold_list)=%d 
807,i,[ wlan_beacon.c : 2387 ] BEACON_RESYNC_ARBITER_VDEV_INIT: vdev_id=%d 
806,,[ wlan_beacon.c : 2405 ] arbiter_clinet POOL ALLOC FAILURE 
805,,[ wlan_beacon.c : 2392 ] arbiter_clinet POOL ALLOC FAILURE 
804,i,[ wlan_beacon.c : 2427 ] BEACON_RESYNC_ARBITER_VDEV_DEINIT: vdev_id=%d 
803,,[ wlan_beacon.c : 1049 ] WLAN_BEACON_TBTTOFFSET_UPDATE_HANDLER ERROR! pmac is NULL 
802,iIII,[ wlan_beacon.c : 1086 ] WLAN_BEACON_TBTTOFFSET_UPDATE_HANDLER vdev_map mismatch i:%d vdev_map:0x%x vdev_id_map:0x%x max_diff:0x%x 
801,,[ wlan_beacon.c : 204 ] beacon_init POOL ALLOC FAILURE 
800,iI,[ wlan_beacon.c : 1459 ] _wlan_tsfoor_handler: vdev_id = %d, tesf = 0x%x 
799,iiii,[ wlan_beacon.c : 753 ] QUIET IE STA: period=%d dur=%d, offset=%d, tbtt cnt=%d 
798,ii,[ wlan_beacon.c : 163 ] wlan_beacon_unit_test_module %d %d 
797,,[ wlan_beacon.c : 969 ] WLAN_BEACON_WAL_TBTTOFFSET_UPDATE_HANDLER ERROR! pmac is NULL 
796,ii,[ wlan_beacon.c : 128 ] wlan_beacon_unit_test_beacon_start_stop %d %d 
795,i,[ wlan_beacon.c : 154 ] wlan_beacon_unit_test_slot_time %d 
831,iI,[ wlan_mbssid.c : 686 ] MBSS: NONTRAN_BSSID_CAP IE length: %d, NontxBssidCap: 0x%x 
830,iI,[ wlan_mbssid.c : 691 ] MBSS: SSID IE length:%d ssid:%s 
829,iIIIIIIii,[ wlan_mbssid.c : 707 ] MBSS: Couldn't find (mbssid_ind %d) %x:%x:%x:%x:%x:%x, DP: %d, DC:%d 
828,iiii,[ wlan_mbssid.c : 716 ] MBSS: UPDATE: mbssid_idx:%d, period:%d, *dtim_cnt:%d, vdev_dtim_intval:%d 
827,iiiiii,[ wlan_mbssid.c : 725 ] MBSS: SET: mbssid_idx: %d, dtimperiod:%d, frm_dtimcnt:%d, vdev_dtim_cnt %d, recvd_dtim:%d, settingdtm:%d 
826,i,[ wlan_mbssid.c : 743 ] MBSS: Unhandled wlan_mbss_index_update_type: %d 
825,ii,[ wlan_mbssid.c : 750 ] MBSS: ELEMENT ID: %d, IE length: %d 
824,i,[ wlan_mbssid.c : 461 ] WLAN_MBSSID_GET_NONTRANS_BSSID Big max_bssid_ind:%d 
823,iiIIIIII,[ wlan_mbssid.c : 478 ] MBSSID_GET_NONTRANS_BSSID profile_id = %d bssid_index = %d mac addr = %02x:%02x:%02x:%02x:%02x:%02x 
822,ii,[ wlan_mbssid.c : 445 ] MBSSID_GET_NONTRANS_BSSID_PROF_NUM profile_num = %d max_mbssid_indicator = %d 
821,ii,[ wlan_mbssid.c : 317 ] MBSSID_IS_BSSID_MATCHED fail, len:%d err_code:%d(4:invalid_idx,5:invalid_profile_id) 
820,,[ wlan_mbssid.c : 342 ] MBSSID_IS_SSID_MATCHED legacy case 
819,ii,[ wlan_mbssid.c : 376 ] MBSSID_IS_SSID_MATCHED profile_id = %d ssid_len = %d 
818,i,[ wlan_mbssid.c : 807 ] MBSS: MBSSID_GET_NONTRANS_BSSID_PROF_NUM profile_num = %d 
834,ii,[ wlan_phyerr_internal.c : 121 ] phyerr event err: buf_len:%d>%d 
833,,[ wlan_phyerr_internal.c : 209 ] phyerr event: alloc event failure 
832,iiiii,[ wlan_phyerr_internal.c : 224 ] phyerr event, lo:%d, now_mac:%d, now_os:%d, phy0:%d, phy1:%d 
848,i,[ wlan_dfs_phyerr_offload.c : 384 ] PHYERR offload enable pdev_id=%d 
847,,[ wlan_dfs_phyerr_offload.c : 420 ] PHYERR unexpected offload disable command for HKv2! 
846,iiiiiii,[ wlan_dfs_phyerr_offload.c : 472 ] ADFS_DUMPS WMI_VDEV_ADFS_CH_CFG_CMD center_freq1=%d, center_freq2=%d, chan_width=%d, cac_duration_ms=%d, ocac_mode=%d, flags=%d, vdev_id=%d 
845,ii,[ wlan_dfs_phyerr_offload.c : 510 ] ADFS_DUMPS PROTOCOL-Starting timer for cac_duration_ms:%d, current_time:%d
 
844,i,[ wlan_dfs_phyerr_offload.c : 73 ] ADFS_DUMPS PROTOCOL-Inside wlan_adfs_cac_timer_handler, current_time = %d 
843,iiiii,[ wlan_dfs_phyerr_offload.c : 56 ] ADFS_DUMPS PROTOCOL-Sending WMI_VDEV_ADFS_OCAC_COMPLETE_EVENTID center_freq1=%d, center_freq2=%d, bandwidth=%d, status=%d, vdev_id=%d 
842,,[ wlan_dfs_phyerr_offload.c : 258 ] PHYERR offload cac check not DFS chan 
841,ii,[ wlan_dfs_phyerr_offload.c : 263 ] PHYERR offload not enabled, mac_id=%d vdev_id=%d 
840,i,[ wlan_dfs_phyerr_offload.c : 95 ] PHYERR offload cac timeout vdevId=%d 
839,ii,[ wlan_dfs_phyerr_offload.c : 238 ] PHYERR offload mac_id=%d enabled=%d 
838,,[ wlan_dfs_phyerr_offload.c : 579 ]  register - WMI_SERVICE_DFS_PHYERR_OFFLOAD  
837,i,[ wlan_dfs_phyerr_offload.c : 314 ] PHYERR offload radar det evt disable cac timer vdevId=%d 
836,iiii,[ wlan_dfs_phyerr_offload.c : 348 ] PHYERR offload det mode=%d, chan_freq=%d det_id=%d seg_id=%d 
835,i,[ wlan_dfs_phyerr_offload.c : 346 ] PHYERR offload send radar detection evt WMI pdevId=%d 
851,iii,[ wlan_dfs_phyerr_unit_test.c : 44 ] wlan_dfs_phyerr_offload_unit_test input: vdevId=%d testId=%d num_args=%d 
850,ii,[ wlan_dfs_phyerr_unit_test.c : 60 ] wlan_dfs_phyerr_offload_unit_test input: set radar mac_id=%d cmd=%d 
849,ii,[ wlan_dfs_phyerr_unit_test.c : 107 ] wlan_dfs_phyerr_offload_unit_test input: mac_id=%d enable radar det offload=%d 
860,II,[ wlan_txbf.c : 1436 ] TXBFEE_DBGID_HOST_CONFIG_CMDID  ID=0x%x Value=0x%x 
859,IIIIi,[ wlan_txbf.c : 1175 ] TXBF: SUBFee=0x%x MUBFee=0x%x SUBFer=0x%x MUBFer=0x%x chan->phy_mode=%d 
858,,[ wlan_txbf.c : 1191 ]  VDEV Registration Failed 
857,iI,[ wlan_txbf.c : 1330 ] TXBFEE_DBGID_BRPOLL_RECEIVED vdev_id = %d fbSegBmap=0x%x 
856,,[ wlan_txbf.c : 1352 ] Non-directed GID frame
 
855,i,[ wlan_txbf.c : 1395 ] Gid=%d
 
854,iII,[ wlan_txbf.c : 1404 ] TXBFEE_DBGID_GID_RECEIVED vdev_id = %d gid=0x%x userpos=0x%x 
853,iI,[ wlan_txbf.c : 1378 ] i=%d, membership=0x%x
 
852,iiIi,[ wlan_txbf.c : 1309 ]  TXBFEE_DBGID_NDPA_RECEIVED vdev_id=%d vht_he=%d staInfo=0x%x token_num=%d 
861,I,[ wlan_txbf_unit_test.c : 78 ] WLAN_TXBF_CONFIG param = 0x%x 
864,II,[ unit_test.c : 419 ] UNIT_TEST_GEN  0x%x 0x%x 
863,IIIII,[ unit_test.c : 427 ] UNIT_TEST_GEN  0x%x 0x%x 0x%x 0x%x, 0x%x 
862,,[ unit_test.c : 180 ] DTF Disabled 
890,iiI,[ wlan_regdb_offload.c : 192 ] REGDB set init country command pdev_id=%d, cc_type=%d, cc_value=%x 
889,,[ wlan_regdb_offload.c : 276 ]  register - WMI_SERVICE_REGULATORY_DB  
888,i,[ wlan_regdb_offload.c : 588 ] REGDB EXT send reg rules failed - status=%d 
887,i,[ wlan_regdb_offload.c : 524 ] REGDB send reg rules failed - status=%d 
886,ii,[ wlan_regdb_offload.c : 530 ] REGDB rdCtl: %d %d 
885,II,[ wlan_regdb_offload.c : 537 ] REGDB send default reg rules for alpha2: %c %c 
884,iiiiii,[ wlan_regdb_offload.c : 539 ] REGDB send def reg rules phy_id=%d status_code=%d, ctry_id=%d dom_code=%d, num_2g_rules=%d, num_5g_rules=%d 
883,IIiiii,[ wlan_regdb_offload.c : 542 ] REGDB dfs_reg=%x, phybitmap=%x minbw2g=%d maxbw2g=%d minbw5g=%d maxbw5g=%d 
882,,[ wlan_regdb_offload.c : 430 ] REGDB EXT fail - invalid country code input 
881,,[ wlan_regdb_offload.c : 434 ] REGDB EXT fail - invalid get type 
880,iiiI,[ wlan_regdb_offload.c : 315 ] REGDB send reg rules for mac_id=%d get_type=%d cc_type=%d cc_value=%x 
879,i,[ wlan_regdb_offload.c : 384 ] REGDB send reg rules failed - status=%d 
878,II,[ wlan_regdb_offload.c : 388 ] REGDB send reg rules for alpha2: %c %c 
877,iiiiii,[ wlan_regdb_offload.c : 390 ] REGDB phy_id=%d status_code=%d, ctry_id=%d dom_code=%d, num_2g_rules=%d, num_5g_rules=%d 
876,IIiiii,[ wlan_regdb_offload.c : 393 ] REGDB dfs_reg=%x, phybitmap=%x minbw2g=%d maxbw2g=%d minbw5g=%d maxbw5g=%d 
875,,[ wlan_regdb_offload.c : 330 ] REGDB fail - invalid country code input 
874,,[ wlan_regdb_offload.c : 334 ] REGDB fail - invalid get type 
873,i,[ wlan_regdb_offload.c : 765 ] RegDB EXT Rules Assert - %d
 
872,,[ wlan_regdb_offload.c : 776 ] RegDB EXT wmi buf alloc fail 
871,,[ wlan_regdb_offload.c : 868 ] RegDB - Sent WMI_REG_CHAN_LIST_CC_EXT_EVENT
 
870,II,[ wlan_regdb_offload.c : 636 ] REGDB read reg rules alpha2 %c %c 
869,iiii,[ wlan_regdb_offload.c : 648 ] REGDB max_rules=%d 2g_rules=%d 5g_rules=%d, evt_len=%d 
868,,[ wlan_regdb_offload.c : 652 ] REGDB wmi buf alloc fail 
867,iIII,[ wlan_regdb_offload.c : 715 ] REGDB ruleIdx=%d freq info=%x bw_pwr=%x flag=%x 
866,,[ wlan_regdb_offload.c : 723 ] REGDB send WMI_REG_CHAN_LIST_CC_EVENTID 
865,iiI,[ wlan_regdb_offload.c : 66 ] REGDB test command num_args=%d testId=%d value1=%x 
924,iiIII,[ wlan_beacon_tx_offload.c : 1368 ] WOW_BEACON_OFFLOAD_TX  pdev_id = %d vdev_id = %d completion_status = 0x%x bcn_pending_count = 0x%x bcn_buf_initialized = 0x%x 
923,i,[ wlan_beacon_tx_offload.c : 2577 ] WOW_PROBE_RESP_TX: tx done cb, compl status=%d 
922,iiiiiiI,[ wlan_beacon_tx_offload.c : 955 ] BCN_TMPL_CMDID: vdevid:%d, tmplt_idx:%d, first:%d, last:%d, pp:%d, maxpp:%d, vdev_flags:0x%x 
921,ii,[ wlan_beacon_tx_offload.c : 988 ] tmplt_idx %d >= profile_period %d 
920,IIIII,[ wlan_beacon_tx_offload.c : 1109 ] QUIET IE AP: vdev_id= %x period = %x duration = %x off = %x flag = %x 
919,iI,[ wlan_beacon_tx_offload.c : 1163 ] WOW_PROBE_RESP_TX: PRB TMPL CMDID, probe_resp_len=%d flags=%x 
918,,[ wlan_beacon_tx_offload.c : 1193 ] offload_ctxt POOL ALLOC FAILURE 
917,,[ wlan_beacon_tx_offload.c : 1200 ] buf POOL ALLOC FAILURE 
916,I,[ wlan_beacon_tx_offload.c : 1238 ] QUIET IE AP_swba: TIM  Disable value = %x 
915,I,[ wlan_beacon_tx_offload.c : 1248 ] QUIET IE AP_swba: TIM  Enable value = %x 
914,,[ wlan_beacon_tx_offload.c : 115 ] bcn_ctxt POOL ALLOC FAILURE 
913,I,[ wlan_beacon_tx_offload.c : 2164 ] HE_RTS_THRESHOLD_DBG: enter: he_op_ie rts_thresh: %lu 
912,iiii,[ wlan_beacon_tx_offload.c : 2188 ] HE_RTS_THRESHOLD_DBG: middle: he_rts_load_enable_threshold: %d, load_metric: %d, active_user_count: %d, rx_load_pct: %d 
911,I,[ wlan_beacon_tx_offload.c : 2202 ] HE_RTS_THRESHOLD_DBG: exit: he_op_ie rts_thresh: %lu 
910,IIIIiiI,[ wlan_beacon_tx_offload.c : 1585 ] BEACON TX ignored, vdev id:%x, mac_id:%x, bcn_tx_paused:%x, pdev_id:%x, swba_delay:%d consec_beacon_skip:%d, on_chan = %x 
909,I,[ wlan_beacon_tx_offload.c : 1708 ] WOW_RECV_MGMT frame_type = 0x%x 
908,ii,[ wlan_beacon_tx_offload.c : 2219 ] MU_EDCA_DEBUG: id: %d, update_cnt: %d 
907,iiiii,[ wlan_beacon_tx_offload.c : 2224 ] MU_EDCA_DEBUG: id: %d, BK: cwmin: %d, cwmax: %d, aifsn: %d, edca_timer: %d 
906,iiiii,[ wlan_beacon_tx_offload.c : 2229 ] MU_EDCA_DEBUG: id: %d, BE: cwmin: %d, cwmax: %d, aifsn: %d, edca_timer: %d 
905,iiiii,[ wlan_beacon_tx_offload.c : 2234 ] MU_EDCA_DEBUG: id: %d, VI: cwmin: %d, cwmax: %d, aifsn: %d, edca_timer: %d 
904,iiiii,[ wlan_beacon_tx_offload.c : 2239 ] MU_EDCA_DEBUG: id: %d, VO: cwmin: %d, cwmax: %d, aifsn: %d, edca_timer: %d 
903,I,[ wlan_beacon_tx_offload.c : 3156 ] QUIET IE AP: num_args= %x failed 
902,IIIII,[ wlan_beacon_tx_offload.c : 3168 ] QUIET IE AP: vdev_id= %x period = %x duration = %x off = %x flag = %x 
901,iiiiii,[ wlan_beacon_tx_offload.c : 375 ] OPTDBG: vdevid:%d,  vdev chan_idx:%d, vdev opclass:%d, regdomain:%d, rnr opclass: %d, rnr_chidx:%d 
900,iIIi,[ wlan_beacon_tx_offload.c : 699 ] BCN_TMPL_CMDID: dtim_count_tmpl0:%d, nonTxVdevMap: 0x%x 0x%x Cur_idx:%d 
899,iiii,[ wlan_beacon_tx_offload.c : 732 ] MBSS : BCN_TMPL_CMDID: TMPL0: %d DTIM: %d Cur_pp_index: %d PP:%d
 
898,iii,[ wlan_beacon_tx_offload.c : 758 ] BCN_TMPL_CMDID: dtim_count:%d, pp:%d new_pp_eff_in_bcn:%d 
897,,[ wlan_beacon_tx_offload.c : 3020 ] WOW_PROBE_RESP_TX: wps ie recv, wakeup host 
896,Ii,[ wlan_beacon_tx_offload.c : 3040 ] WOW_PROBE_RESP_TX offload flags = 0x%x enabled = %d 
895,,[ wlan_beacon_tx_offload.c : 299 ] QUIET IE AP_swba: BCN_CTXT Null 
894,I,[ wlan_beacon_tx_offload.c : 304 ] QUIET IE AP_swba: SWBA  Enable value = %x 
893,I,[ wlan_beacon_tx_offload.c : 309 ] QUIET IE AP_swba: SWBA  disable value = %x 
892,ii,[ wlan_beacon_tx_offload.c : 2647 ] WOW_PROBE_RESP_TX: Err sending probe response not on home channel vdev home channel = %d, mac cahnnel = %d 
891,,[ wlan_beacon_tx_offload.c : 2787 ] WOW_PROBE_RESP_TX: send probe resp 
931,iii,[ wlan_nth_beacon_offload.c : 59 ] wlan_nth_bcn_ctx_deint nth_value = %d, timer_status = %d, is_nth_beacon_enable = %d 
930,iii,[ wlan_nth_beacon_offload.c : 120 ] wlan_nth_bcn_ofld_run_timer error can't start timer nvalue = %d, ifup = %d, active = %d 
929,iiiiiIII,[ wlan_nth_beacon_offload.c : 173 ] wlan_nth_bcn_ofld_run_timer timeout_val_ms = %d, nvalue = %d, status = %d, is_nth_beacon_enable = %d, drift_ms = %d, next_tbtt = 0x%x, cur_tsf =0x%x bi_us = 0x%x  
928,iiiii,[ wlan_nth_beacon_offload.c : 339 ] wlan_nth_beacon_ofld_handler bcn received n_value = %d, nth_ctx->tmr_status = %d, is_nth_beacon_enable = %d, WOW_STATE = %d , host_wake_alwd = %d  
927,,[ wlan_nth_beacon_offload.c : 211 ] nth beacon vdev notification registration failed 
926,iii,[ wlan_nth_beacon_offload.c : 222 ] wlan_nth_beacon_to_host_ofld_init nth_value = %d, timer_status = %d, is_ofld_active = %d 
925,iii,[ wlan_nth_beacon_offload.c : 260 ] wlan_update_value_nth_bcn_ofld nth_value = %d, timer_ststus = %d, is_ofld_active = %d  
932,iiiii,[ wlan_nth_beacon_offload_unit_test.c : 26 ] wlan_nth_bcn_offload_unit_test num_args = %d, args[0] = %d, args[1] = %d, vdev_id = %d, ifUp = %d 
949,Ii,[ csa_offload_main.c : 531 ] _csa_action_frame_handler: wbw_ie 0x%x len: %d 
948,II,[ csa_offload_main.c : 56 ] CSA_OFFLOAD_WMI_CHANSWITCH_RECV  cur_ch_freq=0x%x new_ch_freq=0x%x 
947,,[ csa_offload_main.c : 674 ] pause disable 
946,II,[ csa_offload_main.c : 136 ] CSA_OFFLOAD_CSA_TIMER_ERROR  vdev_id=0x%x state=0x%x 
945,iII,[ csa_offload_main.c : 148 ] CSA_OFFLOAD_CSA_TIMER_ERROR vdev_id = %d csa_proc/bcn_tsf=0x%x curr_tsf=0x%x 
944,iII,[ csa_offload_main.c : 158 ] CSA_OFFLOAD_CSA_TIMER_EXP  vdev_id = %d csa_proc=0x%x curr_tsf=0x%x 
943,IIII,[ csa_offload_main.c : 709 ] _csa_vdev_notif_handler: enable:%x pause_until_beacon:%x, csa state:%x, notify:%x
 
942,II,[ csa_offload_main.c : 722 ] csa vdev_start notif,csa ch freq:0x%x, prev csa ch freq:0x%x 
941,III,[ csa_offload_main.c : 289 ] csa handle ie: enable:%x pause_until_beacon:%x, csa state:%x
 
940,iIIiII,[ csa_offload_main.c : 322 ] CSA_OFFLOAD_BEACON_CSA_RECV, XCSA_IE  vdev_id = %d tbtt_cnt=0x%x, curr_chan_freq :0x%x, csa_chan %d csa_freq:0x%x, prev csa ch freq:0x%x 
939,iIIiII,[ csa_offload_main.c : 338 ] CSA_OFFLOAD_BEACON_CSA_RECV, CSA_IE  vdev_id = %d tbtt_cnt=0x%x, curr_chan_freq :0x%x, csa_chan %d csa_freq:0x%x, prev csa ch freq:0x%x 
938,iI,[ csa_offload_main.c : 347 ] CSA_OFFLOAD_CSA_RECV_ERROR_IE vdev_id = %d tbtt_cnt=0x%x 
937,iIi,[ csa_offload_main.c : 400 ] CSA_OFFLOAD_CSA_RECV_ERROR_IE  vdev_id = %d tbtt_cnt=0x%x csa_ies_valid = %d 
936,i,[ csa_offload_main.c : 431 ] CSA_OFFLOAD_CSA_RECV_ERROR_IE: CSWRAP IE len: %d 
935,I,[ csa_offload_main.c : 453 ] pause vdev, csa:%x 
934,iii,[ csa_offload_main.c : 267 ] csa_check_ies_valid chan_valid = %d, tbtt_valid = %d pcl = %d 
933,iI,[ csa_offload_main.c : 118 ] CSA_OFFLOAD_WMI_EVENT_ERROR  vdev_id = %d csa_proc=0x%x 
950,i,[ obss_offload_api.c : 104 ] bss color: SCAN_SCH_START_ALLOC_FAIL, %d 
972,i,[ bss_color_offload_int.c : 697 ] bss color offload: not support: vdev id:%d 
971,ii,[ bss_color_offload_int.c : 705 ] bss color offload: vdev id:%d, enable=%d 
970,iii,[ bss_color_offload_int.c : 86 ] bss color chg ie: new_bss_color=%d countdown=%d remain_time_us=%d 
969,ii,[ bss_color_offload_int.c : 119 ] bss color he op ie: new_rts_thres=%d curr_rts_thres=%d 
968,i,[ bss_color_offload_int.c : 651 ] bss color: bss clr chg timeout hdlr vdev_id=%d 
967,iii,[ bss_color_offload_int.c : 265 ] bss color he op ie: bcn_bss_color=%d bss_color_disabled=%d curr_bss_color=%d 
966,i,[ bss_color_offload_int.c : 504 ] bss color: scan_evt_handler evt->type = %d 
965,,[ bss_color_offload_int.c : 558 ] BSS COLOR: SCAN_START_COMMAND_FAILED, vdev bss NULL 
964,i,[ bss_color_offload_int.c : 605 ] BSS COLOR: SCAN_START_COMMAND_FAILED, %d 
963,i,[ bss_color_offload_int.c : 626 ] 11d: STOP_COMMAND_FAILED, %d 
962,iii,[ bss_color_offload_int.c : 455 ] bss color: check color collision detection vdev_id=%d vdev_mode=%d col_detect=%d 
961,iii,[ bss_color_offload_int.c : 484 ] bss color: check color collision detection evt_type=%d free_slot_timer=%d det_period=%d 
960,iii,[ bss_color_offload_int.c : 159 ] bss color action: iv_len=%d, category=%d, code=%d 
959,i,[ bss_color_offload_int.c : 723 ] bss color offload: not support: vdev id:%d 
958,ii,[ bss_color_offload_int.c : 743 ] bss color offload: collision det cmd: vdev id:%d, evt_type=%d 
957,iii,[ bss_color_offload_int.c : 749 ] bss color vdev cfg: det_per=%d scan_per=%d expiry_per=%d 
956,i,[ bss_color_offload_int.c : 670 ] bss color: obss clr colli det timeout hdlr vdev_id=%d 
955,ii,[ bss_color_offload_int.c : 357 ] bss color: Send evt report vdevId=%d, tx_status=%d 
954,ii,[ bss_color_offload_int.c : 378 ] bss color: event report fails in wow, vdev id:%d, evt_type:%d  
953,iiII,[ bss_color_offload_int.c : 403 ] bss color: event report,vdev id:%d, evt_type:%d, color bitmap:32to63 0x%x 0to31 0x%x 
952,i,[ bss_color_offload_int.c : 436 ] bss color: restart color collision detection vdev_id=%d 
951,i,[ bss_color_offload_int.c : 414 ] bss color: stop color collision detection vdev_id=%d 
974,i,[ bss_color_offload_unit_test.c : 94 ] bss_color ofld unit test fails: bss_color vdev not exist id:%d 
973,iiii,[ bss_color_offload_unit_test.c : 105 ] bss color ofld unit test: args %d %d %d %d 
976,i,[ obss_offload_priv.c : 64 ] bss color: len wrong:%d 
975,ii,[ obss_offload_priv.c : 73 ] bss color: wrong type:%d, sub:%d 
991,iii,[ wlan_quiet_ie_ap.c : 107 ] QUIET IE AP: timer cb-next evt:%d, cac:%d, paused:%d 
990,I,[ wlan_quiet_ie_ap.c : 131 ] QUIET IE AP: quiet duration time-usec:0x%x 
989,i,[ wlan_quiet_ie_ap.c : 59 ] QUIET IE AP: vdev init vdevId=%d 
988,II,[ wlan_quiet_ie_ap.c : 232 ] QUIET IE AP: not appending quiet IE. time_to_quite_period_start = 0x%x, time_to_bcn_tx = 0x%x 
987,iIIi,[ wlan_quiet_ie_ap.c : 276 ] QUIET IE AP: append quiet IE, tbtt cnt=%d dur=0x%x offset=0x%x len=%d 
986,iiI,[ wlan_quiet_ie_ap.c : 188 ] QUIET IE AP: bi_us=%d diff=%d curr_wal_time=0x%x 
985,iiii,[ wlan_quiet_ie_ap.c : 313 ] QUIET IE AP: start quiet IE: module id=%d, vdev id=%d, dur=%d, beaconing_cnt=%d 
984,i,[ wlan_quiet_ie_ap.c : 324 ] QUIET IE AP: start quiet IE: input duration out of range, duration_us = %d 
983,,[ wlan_quiet_ie_ap.c : 335 ] QUIET IE AP: cancel current quiet IE config 
982,III,[ wlan_quiet_ie_ap.c : 380 ] QUIET IE AP: quiet IE Start time=0x%x Curr_time=0x%x timeout=0x%x 
981,iiii,[ wlan_quiet_ie_ap.c : 454 ] QUIET IE AP: test input num_args=%d vdevId=%d dur=%d cnt=%d 
980,,[ wlan_quiet_ie_ap.c : 463 ] QUIET IE AP: test cfg fail 
979,I,[ wlan_quiet_ie_ap.c : 466 ] QUIET IE AP: test cfg success start_time=0x%x 
978,i,[ wlan_quiet_ie_ap.c : 444 ] QUIET IE AP: test cb status=%d 
977,iii,[ wlan_quiet_ie_ap.c : 423 ] QUIET IE AP: post migration,vdevId:%d, cac:%d, vdevPaused:%d 
1004,IiiiiI,[ wlan_quiet_ie_sta.c : 141 ] QUIET IE STA, time-usec:0x%x, vdevId=%d, evt:%d, all_tids_tx_blocked:%d, supend_alwd:%d, period:0x%x 
1003,iiiii,[ wlan_quiet_ie_sta.c : 232 ] QUIET IE STA: vdevId=%d, next_start=%d, period=%d, duration=%d, quiet_enabled=%d 
1002,,[ wlan_quiet_ie_sta.c : 237 ] QUIET IE STA: cancel current quiet IE config 
1001,Ii,[ wlan_quiet_ie_sta.c : 273 ] QUIET IE STA: Quiet period starts in=0x%x, vdevId=%d 
1000,iiii,[ wlan_quiet_ie_sta.c : 327 ] QUIET IE STA: test input num_args=%d vdevId=%d dur=%d per=%d 
999,,[ wlan_quiet_ie_sta.c : 332 ] QUIET IE STA: test cfg, vdev is NULL 
998,,[ wlan_quiet_ie_sta.c : 337 ] QUIET IE STA: test cfg, vdev not up or incorrect mode 
997,,[ wlan_quiet_ie_sta.c : 354 ] QUIET IE STA: test cfg fail 
996,,[ wlan_quiet_ie_sta.c : 357 ] QUIET IE STA: test cfg success 
995,IiiiiIi,[ wlan_quiet_ie_sta.c : 396 ] QUIET IE STA: PS SM callback , time-usec:0x%x, vdevId=%d, next_evt:%d, all_tids_tx_blocked:%d, supend_alwd:%d, period:0x%x, sleep = %d 
994,IIIII,[ wlan_quiet_ie_sta.c : 437 ] QUIET IE STA: time_diff_us = 0x%x , current_quite_ie = 0x%x, sum =0x%x, ref_time = 0x%x, curr_ts=0x%x 
993,Ii,[ wlan_quiet_ie_sta.c : 460 ] QUIET IE STA: wake recved in ON period timer:0x%x, nxt_evnt:%d 
992,Ii,[ wlan_quiet_ie_sta.c : 474 ] QUIET IE STA: wake recved in OFF period timer:0x%x, nxt_evnt:%d 
1009,,[ wlan_hw_data_filtering.c : 264 ] Add NON ARP BC CCE filter 
1008,,[ wlan_hw_data_filtering.c : 268 ] Delete NON ARP BC CCE filter 
1007,,[ wlan_hw_data_filtering.c : 320 ] Add NON ICMPv6 MC CCE filter 
1006,,[ wlan_hw_data_filtering.c : 324 ] Delete NON ICMPv6 MC CCE filter 
1005,iiiiii,[ wlan_hw_data_filtering.c : 65 ] OFFLOAD HDLR CCE UNIT TEST CMD: num_args=%d vdevId=%d args =%d %d %d %d  
1011,i,[ offload_unit_test.c : 128 ] OFFLOAD HDLR UNIT TEST: status = %d 
1010,iii,[ offload_unit_test.c : 173 ] Offload unit test input: vdevid:%d, group=%d, type=%d 
1012,II,[ wlan_pps.c : 124 ] PPS wmi_set_vdev_pkt_pwr_save: old:0x%x, new:0x%x 
1152,,[ wlan_rtt.c : 11076 ] wlan_internal_disable_responder 
1151,,[ wlan_rtt.c : 665 ] Event buffer allocation for cancel measurement response failed 
1150,iii,[ wlan_rtt.c : 4585 ] wlan_oem_rtt_measreq_hdl: client %d running. cannot new req from client: %d. So Dropping req_id: %d 
1149,i,[ wlan_rtt.c : 4608 ] wlan_oem_rtt_measreq_hdl: Request with id %d won't be served because of an error 
1148,i,[ wlan_rtt.c : 4640 ] wlan_oem_rtt_measreq_hdl: asm_req  status %d would be served from call back due to NACK 
1147,IIII,[ wlan_rtt.c : 10853 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1146,IIII,[ wlan_rtt.c : 10913 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1145,IIII,[ wlan_rtt.c : 10924 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1144,iIi,[ wlan_rtt.c : 1020 ] wlan_rtt_band_change_req_init_cb: event: %d init_ctxt: %p rtt_2g: %d 
1143,IIII,[ wlan_rtt.c : 1056 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1142,,[ wlan_rtt.c : 3192 ] RTT_CALL_FLOW: WLAN_RTT_BEACON_RX 
1141,iiiiiiii,[ wlan_rtt.c : 4854 ] wlan_rtt_burst_instance_done: num_burst_done:%d total_bursts:%d curr_state:%d burst_duration:%d, index:%d ftm1_done:%d num_meas:%d ftm_per_burst:%d 
1140,,[ wlan_rtt.c : 4961 ] Wait for NAN module to finish sending NAN ranging termination frame 
1139,iI,[ wlan_rtt.c : 11195 ] wlan_rtt_cancel_all_rtt_operation attached to vdev_id: %d p_pdev_rtt_ctxt: %p 
1138,iiiiii,[ wlan_rtt.c : 3782 ] wlan_rtt_cap_msg_req_hdl: client_id: %d Req:%d Reqid:%d Major:%d Minor:%d Revision:%d 
1137,,[ wlan_rtt.c : 3797 ] Event buffer allocation for wlan_rtt_cap_msg_req response failed 
1136,iIII,[ wlan_rtt.c : 7412 ] RTT_CHANNEL_SWITCH_GRANT  ev_id = %d p_chnl_switch_ctxt = 0x%x p_owner = 0x%x p_rtt_ctxt = 0x%x 
1135,,[ wlan_rtt.c : 3149 ] RTT_CALL_FLOW: WLAN_RTT_DFS_EXIT 
1134,IIII,[ wlan_rtt.c : 10545 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1133,ii,[ wlan_rtt.c : 3310 ] wlan_rtt_dfs_chan_init_handler rtt_ctxt->chnl_switch_ctxt.cb_fn %d rtt_ctxt->chnl_switch_ctxt.owner%d  
1132,iII,[ wlan_rtt.c : 3337 ] RTT_CHANNEL_DFS_SWITCH_HDL  ev = %d sw_ctxt->arg = %p sw_ctxt->cb_fn %p 
1131,,[ wlan_rtt.c : 3132 ] RTT_CALL_FLOW: WLAN_RTT_DFS_TIMEOUT_HANDLER 
1130,iiii,[ wlan_rtt.c : 7636 ] RTT_CHANNEL_SWITCH_REQ  module_id %d duration = %d channel = %d priority = %d 
1129,I,[ wlan_rtt.c : 1921 ] wlan_rtt_free_init_ctxt() usage flags = 0x%x 
1128,II,[ wlan_rtt.c : 1958 ] Unregistered wlan_rtt_vdev_notify_handler() for init context vdev = %p status = 0x%x 
1127,IIiiiii,[ wlan_rtt.c : 6411 ] wlan_rtt_ftm_init_burst_periodic_timeout: dest_mac:%x%x is_multiburst(%d) is_repetitive_ss(%d) current_burst:%d total_bursts:%d curr_state: %d 
1126,iII,[ wlan_rtt.c : 6467 ] wlan_rtt_ftm_init_burst_periodic_timeout: ERR: Some other request is in progress; skip current burst %d for dest_mac:%x%x 
1125,II,[ wlan_rtt.c : 6499 ] Init PTSF fired resp_tsf_h = 0x%x resp_tsf_l = 0x%x 
1124,iii,[ wlan_rtt.c : 6383 ] wlan_rtt_ftm_resp_burst_timeout: ftm_state: %d num_burst_exp: %d no_burst_count: %d 
1123,II,[ wlan_rtt.c : 11158 ] wlan_rtt_get_clear_stats ranging_dur: %x resp_dur: %x  
1122,iii,[ wlan_rtt.c : 5206 ]  wlan_rtt_get_ftm_chnl_code bw:%d preamble:%d phy_mode:%d 
1121,,[ wlan_rtt.c : 5659 ] RTT_ERROR_REPORT :RTT_RESP_CTXT_EXIST 
1120,,[ wlan_rtt.c : 5690 ] RTT_ERROR_REPORT :RTT_RESP_REQ_ACCEPT 
1119,,[ wlan_rtt.c : 5700 ] RTT_ERROR_REPORT :RTT_RESP_BUSY 
1118,IIiIIiII,[ wlan_rtt.c : 3595 ] wlan_rtt_init_handler: Starting initiator with mac_addr = %08x%02x  init_idx = %d init_ctxt_usage_flags = 0x%x pmac: %p mac_id: %d vdev: %p rate_info: 0x%x 
1117,,[ wlan_rtt.c : 3600 ] RTT request on a different vdev than the one set during channel change 
1116,IiI,[ wlan_rtt.c : 3622 ] Registered wlan_rtt_vdev_notify_handler() for init context : vdev = %p vdevid = %d status = 0x%x 
1115,iii,[ wlan_rtt.c : 7317 ] vdev mac id(%d) not same as pmac mac id(%d): change PM lock & set mac address: %d 
1114,iiiiI,[ wlan_rtt.c : 7336 ] Channel Granted(Initiator): RTT requested freq: %d phymode: %d Grant came on freq: %d phymode: %d chan_flags: 0x%04x 
1113,iII,[ wlan_rtt.c : 7369 ] Downgraded the BW: New bw: %d chnl_format: %u rate_info: %u 
1112,II,[ wlan_rtt.c : 2059 ] wlan_rtt_init_scheduler => curr_init:0x%x init_ctxt_usage_flags:0x%x 
1111,ii,[ wlan_rtt.c : 2094 ] wlan_rtt_init_scheduler => diff1:%d diff2:%d 
1110,i,[ wlan_rtt.c : 2124 ] wlan_rtt_init_scheduler => next_mb_slot_index:%d  
1109,i,[ wlan_rtt.c : 2169 ] wlan_rtt_init_scheduler: Skipping initiator with index %d as it may creep into next multiburst start time 
1108,iiii,[ wlan_rtt.c : 2186 ] wlan_rtt_init_scheduler => index:%d curr_index:%d schedule_timeout:%d next_mb_slot_index: %d 
1107,iiiiiiiI,[ wlan_rtt.c : 2747 ] RTT_MEAS_REQ_HEAD ch_mhz = %d, center_freq1 = %d ch_mode = %d sta_num:%d, max_reg_power: %d antenna_max: %d, max_tx_power: %d, ch_flags: 0x%04x 
1106,IIIII,[ wlan_rtt.c : 10231 ] Received FTMR resp_tsf_h = 0x%x resp_tsf_l = 0x%x curslot_slot_idx: 0x%x cur_diff: 0x%x resp_ref_tsf: 0x%x 
1105,III,[ wlan_rtt.c : 10248 ] wlan_rtt_is_burst_in_slot: diff_tesf: %u next_burst_tsf: %u cur_tsf: %u 
1104,IIII,[ wlan_rtt.c : 7696 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1103,iiiIIii,[ wlan_rtt.c : 7751 ] wlan_rtt_local_send()status: %d pmac_mac_id: %d vdev_mac_id: %d selfgen_chm: 0x%x abf: %p peer_type: %d vdev_id: %d 
1102,IIIII,[ wlan_rtt.c : 5182 ] RTT_FTM_PARAM_INFO  arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x arg5 = 0x%x 
1101,iiii,[ wlan_rtt.c : 2892 ] RTT_MEAS_REQ_HEAD  req_id = %d num_chan = %d sps = %d client: %d 
1100,iIii,[ wlan_rtt.c : 7061 ] wlan_rtt_measurement_report: client_id: %d curr_init_ctxt:%p size: %d freq: %d 
1099,iII,[ wlan_rtt.c : 10395 ] nan_ranging_terminate_completion_handler: req_id: %d init_ctxt: %p wait_status: %x 
1098,i,[ wlan_rtt.c : 10418 ] nan_ranging_terminate_completion_handler for req_id: %d is not processed !!! 
1097,iiii,[ wlan_rtt.c : 8811 ] RTT Null frame Tx status: %d tx_fail_count: %d num_meas: %d terminate: %d 
1096,I,[ wlan_rtt.c : 8556 ] RTT add_random_mac_addr failed. status: 0x%x 
1095,i,[ wlan_rtt.c : 4072 ] _wlan_wmi_oem_req: Non TLV format msg received; tlv_head: %d 
1094,iii,[ wlan_rtt.c : 4089 ] wlan_wmi_oem_req: INFO: OEM Req received with sub_type:%d, req_id:%d client: %d 
1093,ii,[ wlan_rtt.c : 3091 ] wlan_rtt_pm_arb_req(): mac_id: %d state: %d  
1092,IIIIII,[ wlan_rtt.c : 5553 ] wlan_rtt_populate_resp_ftm_param: next_sched_tsf: %u resp_ref_tsf: %u partial_tsf: %u diff_tsf: %u current_resp_tsf64: 0x%08x%08x 
1091,IIIIII,[ wlan_rtt.c : 5582 ] wlan_rtt_populate_resp_ftm_param: next_sched_tsf: %u diff_tsf: %u nearest_tsf: %u resp_partial_tsf: %u next_burst_tsf: 0x%08x%08x 
1090,II,[ wlan_rtt.c : 5637 ] wlan_rtt_populate_resp_ftm_param: ftm_param.burst_period: %u resp_param_info.burst_period: %u 
1089,Ii,[ wlan_rtt.c : 498 ] wlan_rtt_proceed: init_ctxt: %p wait_status: %d 
1088,iIIIIIIII,[ wlan_rtt.c : 2693 ] RTT_MEAS_REQ_BODY idx = %d dest_mac_0to31 = 0x%x dest_mac_32to47 = 0x%x sppof_bssid_0to31 = 0x%x spoof_bssid_32to47 = 0x%x control_inf = 0x%x meas_inf = 0x%x meas_params1 = 0x%x meas_params2 = 0x%x 
1087,IIIII,[ wlan_rtt.c : 10493 ] wlan_rtt_ranging_negotiation_status_notif_handler: timeout_us:%u burst_start_time_h:%u burst_start_time_l:%u StartTsf:%u curr_time%u 
1086,iIi,[ wlan_rtt.c : 10519 ] wlan_rtt_ranging_negotiation_status_notif_handler: ranging_ind_data->RangingParams.ReqId %d init_ctxt %p event_handled %d 
1085,IIII,[ wlan_rtt.c : 10669 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1084,iii,[ wlan_rtt.c : 7238 ] wlan_rtt_resp_chan_switch_hdl()  ev_id = %d ftm_state:%d is_ftmr_pending:%d 
1083,II,[ wlan_rtt.c : 3058 ] Unregistered wlan_rtt_vdev_notify_handler() for resp context vdev = %p status = 0x%x 
1082,IIIII,[ wlan_rtt.c : 10188 ] wlan_rtt_resp_free_existing_slot 0x%x 0x%x 0x%x dest_mac:%08x%02x 
1081,iiI,[ wlan_rtt.c : 6310 ] wlan_rtt_resp_ftm1_timeout: ftm_state: %d asap: %d resp_ctxt: %p 
1080,IIIIIIII,[ wlan_rtt.c : 10174 ] wlan_rtt_resp_get_free_slot 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x dest_mac:%08x%02x 
1079,ii,[ wlan_rtt.c : 6144 ] wlan_rtt_resp_init:current session is active: session_index: %d slot: %d 
1078,ii,[ wlan_rtt.c : 6155 ] wlan_rtt_resp_init: Received a frame which we are not in slot send FTM stop frame. session_index: %d slot: %d 
1077,iii,[ wlan_rtt.c : 6020 ] wlan_rtt_resp_init_body: session_active: %d init_new_session: %d ftm_state: %d 
1076,iii,[ wlan_rtt.c : 6024 ] wlan_rtt_resp_init_body: asap: %d ftm_state: %d session_active: %d 
1075,iiI,[ wlan_rtt.c : 6058 ] wlan_rtt_resp_init_body:ftm_state: %d asap: %d resp_ctxt: %p 
1074,III,[ wlan_rtt.c : 6083 ] wlan_rtt_resp_init_body: ftm_state: %u asap: %u resp_ctxt: %p 
1073,IiII,[ wlan_rtt.c : 5830 ] Registered wlan_rtt_vdev_notify_handler() for resp context vdev: %p vdev_type: %d pmac: %p status: 0x%x 
1072,IIII,[ wlan_rtt.c : 5954 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1071,ii,[ wlan_rtt.c : 5969 ] wlan_rtt_resp_init_new_session: slot: %d param_info.status: %d 
1070,iiI,[ wlan_rtt.c : 5978 ] END_FTM_INVALID_REQUEST: ftm_state: %d asap: %d resp_ctxt: %p 
1069,iiiiiiii,[ wlan_rtt.c : 5441 ] wlan_rtt_resp_init_rate: vdev_id: %d phy_mode: %d mhz: %d ftm_chnl_format: %d param_ie_valid: %d tx_bw: %d tx_preamble: %d mcs: %d 
1068,IIIi,[ wlan_rtt.c : 7221 ] Channel Granted(Responder): Responder operating freq = 0x%x pmac = %p Granted on freq: 0x%x phymode: %d 
1067,ii,[ wlan_rtt.c : 10334 ] wlan_rtt_resp_house_keeping: channel_mhz: %d nearest_sched_resp_tsf_ctxt_index: %d 
1066,,[ wlan_rtt.c : 2269 ] All requests done nothing to schedule 
1065,IIII,[ wlan_rtt.c : 1691 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1064,iiiI,[ wlan_rtt.c : 6910 ] RTT_ERROR_WMI_EVENT: ERROR: client_id: %d req_id:%d reason:%d init_ctxt: %p 
1063,,[ wlan_rtt.c : 6954 ] Event buffer allocation for send_rtt_error_report failed 
1062,iIiiiIi,[ wlan_rtt.c : 7111 ] wlan_rtt_send_measurement_report_hdl: client_id: %d curr_init_ctxt: %p token_id:%d frag_idx:%d more_frag: %d buf:%p buf_len:%d 
1061,IIIi,[ wlan_rtt.c : 7816 ] wlan_rtt_send_null_frame: abf: %p channel: %x pmac = %p spoofed_seqno = %d 
1060,Ii,[ wlan_rtt.c : 7834 ] RTT NULL frame Tx failed: abf: %p ret: %d 
1059,,[ wlan_rtt.c : 8339 ] wlan_rtt_send_tm_frame: vdev is seen as NULL in resp_ctxt 
1058,,[ wlan_rtt.c : 8493 ] RTT_ERROR_REPORT :ALLOCATE_FRAME_BUFFER_ERROR 
1057,IiIIiiiiI,[ wlan_rtt.c : 8502 ] wlan_rtt_send_tm_frame: abf: %p freq: %d pmac = %p resp_ctxt: %p tkn = %d follow_tkn = %d tx_bw = %d resp_ctxt ftm state = %d chan_flags = 0x%04x 
1056,II,[ wlan_rtt.c : 8177 ] Sending RTT Trigger frame resp_tsf_h = 0x%x resp_tsf_l = 0x%x 
1055,,[ wlan_rtt.c : 8208 ] RTT_ERROR_REPORT :ALLOCATE_FRAME_BUFFER_ERROR 
1054,IIi,[ wlan_rtt.c : 8232 ] wlan_rtt_send_tmr_frame: channel: %x pmac = %p spoofed_seqno = %d 
1053,,[ wlan_rtt.c : 8273 ] RTT_TIMER_STOP 
1052,I,[ wlan_rtt.c : 8022 ] RTT_CALL_FLOW: WLAN_RTT_SET_VENDOR_IE_HT_VHT_ACK ts = %u 
1051,iii,[ wlan_rtt.c : 11038 ] wlan_rtt_sta_resp_chan_switch: channel.mhz: %d band_center_freq1: %d phy_mode: %d 
1050,IIII,[ wlan_rtt.c : 10965 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1049,i,[ wlan_rtt.c : 1507 ] wlan_rtt_start_burst_periodic_timer: timeout_ms:%dms 
1048,iIIi,[ wlan_rtt.c : 1261 ] wlan_rtt_terminate_all_ftm_resp_context() idx: %d resp_ctxt = %p vdev = %p ftm_state = %d 
1047,iiii,[ wlan_rtt.c : 1339 ] cancel_measurement_req: vdev_type: %d, req_id: %d, free_curr_init: %d, is_cancelled: %d 
1046,iIII,[ wlan_rtt.c : 2027 ] wlan_rtt_terminate_repetitive_ss_request: red_id:%d init_ctxt_usage_flags:0x%x dest_mac :%x %x 
1045,iii,[ wlan_rtt.c : 1210 ] wlan_rtt_terminate_resp_context() state: %d busrt_exp: %d burst_count: %d 
1044,iii,[ wlan_rtt.c : 9125 ] wlan_rtt_tm_ack_handle_completion: ftm_state: %d num_burst_exp: %d no_burst_count: %d 
1043,IiIII,[ wlan_rtt.c : 9157 ] wlan_rtt_tm_ack_handle_completion: init_ftmr_rx_ts: %10u completion_status: %d ftm_tx_ts: %10u init_ftmr_offset: %6u delta_ftm_act: %6u 
1042,i,[ wlan_rtt.c : 9239 ] RTT TM frame Tx status: %d 
1041,i,[ wlan_rtt.c : 9186 ] RTT_TWOSIDED_RESP_CNT  number = %d 
1040,iii,[ wlan_rtt.c : 9206 ] wlan_rtt_tm_ack_success: ftm_state: %d num_burst_exp: %d no_burst_count: %d 
1039,iii,[ wlan_rtt.c : 9211 ] wlan_rtt_tm_ack_success:Don't continue burst: ftm_state: %d num_burst_exp: %d no_burst_count: %d  
1038,iIIiIII,[ wlan_rtt.c : 9590 ] state = %d tsf_sync_info = 0x%x resp_tsf = 0x%x Diff: %d ftm_req_start_time = 0x%x ftm_req_complete_time = 0x%x current_tsf = 0x%x 
1037,II,[ wlan_rtt.c : 9601 ] RTT TM FTM curr_tsf_delta = 0x%x new_tsf_delta = 0x%x 
1036,IIII,[ wlan_rtt.c : 9680 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1035,,[ wlan_rtt.c : 9777 ] RTT_ERROR_REPORT :TM_TOKEN_MISMATCH 
1034,,[ wlan_rtt.c : 9780 ] RTT_ERROR_REPORT :TM_CFR_CAPTURE_ERROR 
1033,,[ wlan_rtt.c : 9782 ] RTT_ERROR_REPORT :TM_SEQUENCE_RESTART 
1032,,[ wlan_rtt.c : 9836 ] RTT_ERROR_REPORT :RTT_GET_TM_NOTWAIT_TM 
1031,,[ wlan_rtt.c : 9854 ] RTT_ERROR_REPORT :RTT_GET_TM_NOTWAIT_TM 
1030,IIiIIII,[ wlan_rtt.c : 9937 ] wlan_rtt_tm_rx_hdl: status: 0x%x RTT_TWOSIDED_RESP_CNT  number = %2d recv_state: %d init_ftmr_tx_ts: %10u ftm_rx_ts: %10u init_ftmr_offset: %6u delta_ftm_act: %6u 
1029,IIII,[ wlan_rtt.c : 7921 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1028,IIII,[ wlan_rtt.c : 7928 ] RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
1027,I,[ wlan_rtt.c : 8654 ] RTT add_random_mac_addr failed. status: 0x%x 
1026,,[ wlan_rtt.c : 9465 ] rtt_tmr_rx_hdl() vdev not found 
1025,,[ wlan_rtt.c : 9471 ] rtt_tmr_rx_hdl() wal_vdev not found 
1024,II,[ wlan_rtt.c : 9507 ] rtt_tmr_rx_hdl() ftmr_rx_ts: %10u begin_tsf_sap_resp: %10u 
1023,,[ wlan_rtt.c : 9526 ] RTT_ERROR_REPORT :RTT_GET_INVALID_TMR_STOP 
1022,,[ wlan_rtt.c : 9546 ] RTT_ERROR_REPORT :RTT_GET_INVALID_TMR_STOP 
1021,iiI,[ wlan_rtt.c : 8872 ] RTT TMR frame Tx status: %d curr_state: %d ftmr_tx_ts: %u 
1020,iiii,[ wlan_rtt.c : 4238 ] RTT_UNIT_TEST_CMD 1  num_args = %d arg0 = %d vdev_id = %d mac_id = %d 
1019,iiiiii,[ wlan_rtt.c : 4301 ] RTT_UNIT_TEST_CMD numFrms= %d ChnlFrmt= %d frmType= %d reportType= %d burstDr= %d asap_mode= %d 
1018,i,[ wlan_rtt.c : 4530 ] RTT_UNIT_TEST_CMD 2  status = %d 
1017,,[ wlan_rtt.c : 4278 ] MAC address not configured 
1016,,[ wlan_rtt.c : 4289 ] Channel not configured 
1015,Iii,[ wlan_rtt.c : 1433 ] wlan_rtt_vdev_notify_handler() vdev = %p vdev_id = %d notification type = %d 
1014,,[ wlan_rtt.c : 10724 ] Event buffer allocation for send_responder_cfg_info response failed 
1013,iiIii,[ wlan_rtt.c : 7015 ] wmi_send_rtt_error_report_event: req_id: %d reason: %d init_ctxt: %p vdev_type: %d nan_req_active: %d 
1178,iIii,[ wlan_rtt_tlv_helper.c : 190 ] RTTTLV_CHECK_AND_PAD_TLVS  is_req = %d buf_ptr = 0x%x buf_len = %d sub_type = %d 
1177,i,[ wlan_rtt_tlv_helper.c : 194 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Couldn't get expected number of TLVs for sub_type=%d
 
1176,iiiiii,[ wlan_rtt_tlv_helper.c : 214 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Invalid TLV length for sub_type=%d Tag_order=%d buf_idx=%d Tag:%d Len:%d TotalLen:%d
 
1175,ii,[ wlan_rtt_tlv_helper.c : 223 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: No TLV attributes found for sub_type=%d Tag_order=%d
 
1174,iii,[ wlan_rtt_tlv_helper.c : 228 ] RTTTLV_CHECK_AND_PAD_TLVS: VERBOSE: [tlv %d]: tag=%d, len=%d
 
1173,iii,[ wlan_rtt_tlv_helper.c : 241 ] RTTTLV_CHECK_AND_PAD_TLVS: VERBOSE: Tag ID expecting is Loop end for loop started at index %d but received tag %d.num_active_loops: %d 
1172,iii,[ wlan_rtt_tlv_helper.c : 247 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Can't get  the first TLV Tag ID (tlv_index:%d) for last entered loop start (cnt=%d) for sub_type=%d
 
1171,iiii,[ wlan_rtt_tlv_helper.c : 255 ] RTTTLV_CHECK_AND_PAD_TLVS: WARN: First TLV Tag ID (%d) for last entered loop start (index=%d) doesn't match; skipping this tlv with tag:%d for sub_type=%d 
1170,iiiii,[ wlan_rtt_tlv_helper.c : 262 ] RTTTLV_CHECK_AND_PAD_TLVS: VERBOSE: First TLV Tag ID (tlv_index:%d) for last entered loop start (total_active_loops=%d) matched (looping loop_cnt:%d) with tag:%d for sub_type=%d 
1169,iii,[ wlan_rtt_tlv_helper.c : 278 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: TLV has wrong tag in order for sub_type=%d. Given=%d, Expected=%d.
 
1168,iii,[ wlan_rtt_tlv_helper.c : 284 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: TLV has wrong tag in order for sub_type=%d. Given=%d, Expected=%d.
 
1167,ii,[ wlan_rtt_tlv_helper.c : 292 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Wrong TLV length %d for loop end for sub_type:%d 
1166,i,[ wlan_rtt_tlv_helper.c : 297 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Loop start and End mismatch for sub_type:%d 
1165,iiii,[ wlan_rtt_tlv_helper.c : 305 ] RTTTLV_CHECK_AND_PAD_TLVS: VERBOSE: Processing of loop %d done for sub_type:%d; left out loop instances:%d TLVs per loop:%d 
1164,iii,[ wlan_rtt_tlv_helper.c : 320 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Exceeded given max loop count %d, for sub_type:%d tlv_index:%d 
1163,ii,[ wlan_rtt_tlv_helper.c : 329 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Wrong TLV length %d for loop start for sub_type:%d 
1162,i,[ wlan_rtt_tlv_helper.c : 334 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Maximum inner loops reached for sub_type:%d 
1161,i,[ wlan_rtt_tlv_helper.c : 367 ] RTTTLV_CHECK_AND_PAD_TLVS: WARN: ERROR Need to handle this tag ID %d for variable length
 
1160,ii,[ wlan_rtt_tlv_helper.c : 378 ] RTTTLV_CHECK_AND_PAD_TLVS: WARN: TLV truncated. tlv_size_diff=%d, curr_tlv_len=%d
 
1159,i,[ wlan_rtt_tlv_helper.c : 393 ] RTTTLV_CHECK_AND_PAD_TLVS: WARN: TLV needs padding. tlv_size_diff=-%d
 
1158,ii,[ wlan_rtt_tlv_helper.c : 458 ] RTTTLV_CHECK_AND_PAD_TLVS: Some loop(cnt = %d) didn't ended properly for sub_type:%d 
1157,i,[ wlan_rtt_tlv_helper.c : 464 ] RTTTLV_CHECK_AND_PAD_TLVS: Successfully processed TLVs for sub_type:%d
 
1156,iii,[ wlan_rtt_tlv_helper.c : 90 ] WMI TLV attribute definitions for is_req:%d found; rtt_cmd_event_id: %d num_of_tlvs:%d 
1155,ii,[ wlan_rtt_tlv_helper.c : 119 ] ERROR: Didn't found WMI TLV attribute definitions for is_req:%d rtt_cmd_event_id: %d 
1154,iiii,[ wlan_rtt_tlv_helper.c : 99 ] ERROR: TLV order %d greater than num_of_tlvs:%d for is_req:%d rtt_cmd_event_id: %d 
1153,iiii,[ wlan_rtt_tlv_helper.c : 106 ] WMI TLV attributes for is_req:%d rtt_cmd_event_id: %d TLV order %d [tlv %d] 
1204,,[ wlan_cfr.c : 1455 ] No free unassociated CFR pool 
1203,ii,[ wlan_cfr.c : 1804 ] wlan_cfr_pm_arb_req(): mac_id: %d state: %d  
1202,iiii,[ wlan_cfr.c : 1606 ] <<< CFR_UNIT_TEST_CMD, num_args = %d arg0 = %d vdev_id = %d mac_id = %d 
1201,,[ wlan_cfr.c : 1639 ] CFR_UNIT_TEST_CMD_SET_TA_AND_MASK, there's some missing argument, cannot set here 
1200,,[ wlan_cfr.c : 1659 ] CFR_UNIT_TEST_CMD_SET_RA_AND_MASK, there's some missing argument, cannot set here 
1199,,[ wlan_cfr.c : 1681 ] CFR_UNIT_TEST_CMD_SET_EXTRA_PARAMS_CAPTURE_GROUP, there's some missing argument, cannot set here 
1198,,[ wlan_cfr.c : 1704 ] CFR_UNIT_TEST_CMD_SET_EXTRA_FIXED_PARAM, there's some missing argument, cannot set here 
1197,,[ wlan_cfr.c : 1724 ] CFR_UNIT_TEST_CMD_WMI_CFR_CAPTURE_FILTER_CMDID, there's some missing argument, cannot set here 
1196,IIIII,[ wlan_cfr.c : 1749 ] wmi_pdev_id = 0x%x filter_type = 0x%x capture_interval = 0x%x capture_duration = 0x%x filter_group_bitmap = 0x%x 
1195,IIIIII,[ wlan_cfr.c : 1758 ] filter_group_id = 0x%x filter_set_valid_mask = 0x%x bw_nss_filter = 0x%x mgmt_subtype_filter = 0x%x ctrl_subtype_filter = 0x%x data_subtype_filter = 0x%x  
1194,IIII,[ wlan_cfr.c : 1765 ] ta_addr.mac_addr31to0 = 0x%x ta_addr.mac_addr47to32 = 0x%x ta_addr_mask.mac_addr31to0 = 0x%x ta_addr_mask.mac_addr47to32 = 0x%x 
1193,IIII,[ wlan_cfr.c : 1772 ] ra_addr.mac_addr31to0 = 0x%x ra_addr.mac_addr47to32 = 0x%x ra_addr_mask.mac_addr31to0 = 0x%x ra_addr_mask.mac_addr47to32 = 0x%x 
1192,i,[ wlan_cfr.c : 1792 ] >>> CFR_UNIT_TEST_CMD, status = %d 
1191,I,[ wlan_cfr.c : 1531 ] wlan_next_cfr_capture_handler: no capture requests in %p 
1190,III,[ wlan_cfr.c : 921 ] Space not available read_index = %x,write_index = %x, max_write_index = %x 
1189,i,[ wlan_cfr.c : 1137 ] gain table index is non zero for chain: %d 
1188,,[ wlan_cfr.c : 1158 ] Invalid gain info. No AoA phase data got captured. 
1187,IIIii,[ wlan_cfr.c : 1184 ] wlan_null_frame_cfr_wmi_ack_hdl: status 0x%08x correlation_info 0x%08x%08x cap_bw %d tx_bw %d 
1186,i,[ wlan_cfr.c : 1144 ] Capping gain to 62, Current gain = %d 
1185,IIIIIIII,[ wlan_cfr.c : 1153 ] gainDB values: %u %u %u %u %u %u %u %u 
1184,I,[ wlan_cfr.c : 1322 ] Invalid operating BW for CFR %x 
1183,I,[ wlan_cfr.c : 1371 ] Invalid CFR capture method %x 
1182,iiIIIi,[ wlan_cfr.c : 743 ] wlan_peer_cfr_capture_cmd_handler: request %d periodicity %d peer MAC 0x%08x%02x context %p status %d 
1181,iIIiI,[ wlan_cfr.c : 43 ] wlan_peer_cfr_capture: vdev %d peer MAC 0x%08x%02x status %d at %p 
1180,,[ wlan_cfr.c : 88 ] WMI_PEER_CFR_CAPTURE_EVENTID evt alloc failed 
1179,I,[ wlan_cfr.c : 1569 ] wlan_periodic_cfr_capture_handler: no capture requests in %p 
1219,II,[ wlan_obss_scan_offload.c : 221 ] obss send: num_of_scans:%x,send cnt:%x 
1218,II,[ wlan_obss_scan_offload.c : 246 ] obss merge: num_of_scans:%x, idx:%x 
1217,ii,[ wlan_obss_scan_offload.c : 392 ] Beacon parser invoked, mac_id:%d, ch:%d 
1216,ii,[ wlan_obss_scan_offload.c : 423 ] obss scan TE-A type=%d, index:%d 
1215,,[ wlan_obss_scan_offload.c : 428 ] obss scan TE-A rec null 
1214,Iiii,[ wlan_obss_scan_offload.c : 464 ] obss scan TE-A found_dup=%x, index:%d, op:%d,ch_id:%d 
1213,iI,[ wlan_obss_scan_offload.c : 420 ] obss scan HT cap present=%d, teb:0x%x 
1212,Ii,[ wlan_obss_scan_offload.c : 148 ] obss scan send action, add ch id:%x, op class:%d 
1211,IiIi,[ wlan_obss_scan_offload.c : 154 ] OBSS_SCAN_SEND_ACTION idx:%x, op class:%d, intolerent len:%x, frame len:%d 
1210,i,[ wlan_obss_scan_offload.c : 700 ] obss scan stop, refer cnt:%d, status 
1209,I,[ wlan_obss_scan_offload.c : 184 ] obss coex action frame buf null, vdev id:%x 
1208,i,[ wlan_obss_scan_offload.c : 571 ] obss scan start vdev id =%d 
1207,i,[ wlan_obss_scan_offload.c : 576 ] obss scan vdev pool alloc failed=%d 
1206,,[ wlan_obss_scan_offload.c : 623 ] Channel not in 2.4 GHz sent 
1205,,[ wlan_obss_scan_offload.c : 635 ] Channel not in 2.4 GHz sent 
1227,II,[ umac_wmi_events.c : 577 ] WMI_CHAN_INFO_EVENT_ALLOC_FAILURE  EventId = 0x%x chan_freq = 0x%x 
1226,iiiiiii,[ umac_wmi_events.c : 585 ] WMI_CHAN_INFO_EVT err_code = %d, freq = %d, cmd_flags = %d, nf = %d, rx_clr_cnt = %d, cycle_cnt = %d, chan_tx_pwr_range = %d 
1225,iiiiii,[ umac_wmi_events.c : 587 ] WMI_CHAN_INFO_EVT chan_tx_pwr_tp = %d, rx_frm_cnt = %d, my_bss_rx_cycle_cnt = %d, rx_11b_mode_data_dur = %d, tx_frm_cnt = %d, mac_clk_mhz = %d 
1224,iII,[ umac_wmi_events.c : 626 ] WMI_EVENT_ALLOC_FAILURE vdev_id = %d EventId = 0x%x AssocId/VdevMap = 0x%x 
1223,iII,[ umac_wmi_events.c : 721 ] WMI_EVENT_ALLOC_FAILURE vdev_id = %d EventId = 0x%x AssocId/VdevMap = 0x%x 
1222,ii,[ umac_wmi_events.c : 99 ] drop mgmt as size:%d,limit:%d 
1221,,[ umac_wmi_events.c : 256 ] BEACON_EVENT_SWBA_SEND_FAILED 
1220,II,[ umac_wmi_events.c : 684 ]  WMI_EVENT_ALLOC_FAILURE EventId = 0x%x AssocId/VdevMap = 0x%x 
1233,,[ wlan_wmi.c : 285 ] wlan_wmi_read_tlv: p_in_tlv is NULL 
1232,,[ wlan_wmi.c : 291 ] wlan_wmi_read_tlv: p_out_tlv is NULL 
1231,III,[ wlan_wmi.c : 314 ] wlan_wmi_read_tlv: type=%u, length=%u, read_len=%u 
1230,,[ wlan_wmi.c : 245 ] wlan_wmi_write_tlv: p_in_tlv is NULL 
1229,,[ wlan_wmi.c : 251 ] wlan_wmi_write_tlv: p_out_tlv is NULL 
1228,III,[ wlan_wmi.c : 271 ] wlan_wmi_write_tlv: type=%u, length=%u, write_len=%u 
1258,iiii,[ wlan_wmi_events.c : 576 ] wlan_debug_mesg_flush_compete stall_type:%d vdev_bmap:%d reason_code1:%d reason_code2:%d 
1257,II,[ wlan_wmi_events.c : 626 ] WMI handle send WMI evt msg fail, evt_id:0x%x, evt_len:0x%x
 
1256,II,[ wlan_wmi_events.c : 630 ] WMI handle send WMI evt msg, evt_id:0x%x, evt_len:0x%x
 
1255,IIIII,[ wlan_wmi_events.c : 262 ] bdf_version = %x ref_design_id=%x, customer_id=%x, project_id=%x, board_data_rev=%x 
1254,iiiii,[ wlan_wmi_events.c : 1700 ] wmi_service_ready_ext_event: pdev_id %d mod_id %d ring_elems_min %d min_buf_align %d min_buf_size %d 
1253,ii,[ wlan_wmi_events.c : 1769 ] SCAN_RADIO_SUPPORT_DBUG WMI_SERVICE_READY_EXT2 san_radio_flag = %d phy_id = %d
 
1252,iiiii,[ wlan_wmi_events.c : 1524 ] wmi_service_ready_ext_event: pdev_id %d mod_id %d ring_elems_min %d min_buf_align %d min_buf_size %d 
1251,IIIIIIII,[ wlan_wmi_events.c : 1547 ] WMI Service Ready Ext: wmi_svc_bitmap(ext) = 0x%08x %08x %08x %08x (%08x %08x %08x %08x) 
1250,III,[ wlan_wmi_events.c : 675 ] DISPLAY_TPC_STATS: 1st event tpcEvSize is %lu wal_pdev_get_reg_array_len is %lu reg_mask is %u 
1249,,[ wlan_wmi_events.c : 679 ] DISPLAY_TPC_STATS: Event size exceeds WMI_SVC_MSG_SIZE!! 
1248,,[ wlan_wmi_events.c : 687 ] DISPLAY_TPC_STATS: WMI tpc stats evt, allocation failed! 
1247,I,[ wlan_wmi_events.c : 914 ] DISPLAY_TPC_STATS: 4th event tpcEvSize is %lu 
1246,I,[ wlan_wmi_events.c : 916 ] DISPLAY_TPC_STATS: wal_pdev_get_ctl_array_len is %lu 
1245,,[ wlan_wmi_events.c : 923 ] DISPLAY_TPC_STATS: Event size exceeds WMI_SVC_MSG_SIZE!! 
1244,,[ wlan_wmi_events.c : 930 ] DISPLAY_TPC_STATS: WMI tpc stats evt, allocation failed! 
1243,I,[ wlan_wmi_events.c : 936 ] DISPLAY_TPC_STATS: event starting ptr is %lu 
1242,,[ wlan_wmi_events.c : 651 ] DISPLAY_TPC_STATS: wmi_tpc_stats_event_complete 
1241,II,[ wlan_wmi_events.c : 750 ] DISPLAY_TPC_STATS: 2nd event tpcEvSize is %lu wal_pdev_get_rates_array_len is %lu 
1240,,[ wlan_wmi_events.c : 754 ] DISPLAY_TPC_STATS: Event size exceeds WMI_SVC_MSG_SIZE!! 
1239,,[ wlan_wmi_events.c : 761 ] DISPLAY_TPC_STATS: WMI tpc stats evt, allocation failed! 
1238,I,[ wlan_wmi_events.c : 767 ] DISPLAY_TPC_STATS: event starting ptr is %lu 
1237,I,[ wlan_wmi_events.c : 826 ] DISPLAY_TPC_STATS: 3rd event tpcEvSize is %lu 
1236,,[ wlan_wmi_events.c : 833 ] DISPLAY_TPC_STATS: Event size exceeds WMI_SVC_MSG_SIZE!! 
1235,,[ wlan_wmi_events.c : 840 ] DISPLAY_TPC_STATS: WMI tpc stats evt, allocation failed! 
1234,,[ wlan_wmi_events.c : 595 ] WOW send initial wakeup wmi cmd 
1312,Ii,[ cmdProcessTlv2.c : 4855 ] %s: #### Getting cal version:bdfvertype: %d  !
 
1311,ii,[ cmdProcessTlv2.c : 2005 ] PHYDBGdump2Handler(Phy:%d, Option:%d)
 
1310,IiI,[ cmdProcessTlv2.c : 2013 ] ### data_ptr %p size %d status 0x%x
 
1309,Ii,[ cmdProcessTlv2.c : 2022 ] ### data_ptr %p stream_cnt %d
 
1308,,[ cmdProcessTlv2.c : 2025 ] ### Data buffer stream ended
 
1307,ii,[ cmdProcessTlv2.c : 2417 ] PHYDBGdumpHandler(Phy:%d, Option:%d)
 
1306,IiI,[ cmdProcessTlv2.c : 2425 ] ### data_ptr %p size %d status 0x%x
 
1305,Ii,[ cmdProcessTlv2.c : 2434 ] ### data_ptr %p stream_cnt %d
 
1304,,[ cmdProcessTlv2.c : 2437 ] ### Data buffer stream ended
 
1303,Ii,[ cmdProcessTlv2.c : 4832 ] %s :set cal version , bdfvertype: %d !
 
1302,i,[ cmdProcessTlv2.c : 4092 ] Channel index out of bounds %d 
1301,i,[ cmdProcessTlv2.c : 4100 ] Power offset Index out of bounds %d 
1300,ii,[ cmdProcessTlv2.c : 4108 ] 2G index %d flag %d 
1299,ii,[ cmdProcessTlv2.c : 4121 ] values written 2G %d 5G %d 
1298,i,[ cmdProcessTlv2.c : 4182 ] Channel index out of bounds %d 
1297,i,[ cmdProcessTlv2.c : 4263 ] Channel index out of bounds %d 
1296,i,[ cmdProcessTlv2.c : 4278 ] Target Power index out of bounds %d 
1295,i,[ cmdProcessTlv2.c : 4293 ] Gain index out of bounds %d 
1294,,[ cmdProcessTlv2.c : 4609 ] OPC_OTP_WRITE:Ready to send response!
 
1293,I,[ cmdProcessTlv2.c : 4610 ] OTP Write status, 0x%x 
1292,,[ cmdProcessTlv2.c : 4622 ] OPC_OTP_WRITE:send response done!
 
1291,,[ cmdProcessTlv2.c : 3041 ] bdGetSizeHandler
 
1290,iIii,[ cmdProcessTlv2.c : 3068 ] bdReadHandler: bdSize %d, offset 0x%x, size %d, source %d
 
1289,i,[ cmdProcessTlv2.c : 3109 ] error in bdReadHandler: status %d
 
1288,Ii,[ cmdProcessTlv2.c : 4509 ] bdWriteHandler: offset 0x%x, size %d
 
1287,ii,[ cmdProcessTlv2.c : 2309 ] combCalGroupHandler(): phyId = %d; cmdid = %d 
1286,IIII,[ cmdProcessTlv2.c : 4734 ] %s: offset %ld, size %ld, totalsize %ld 
1285,III,[ cmdProcessTlv2.c : 4803 ] %s: offset %ld, size %ld 
1284,,[ cmdProcessTlv2.c : 198 ] ftm_termperature_timer_handler::MAC sleeping 
1283,,[ cmdProcessTlv2.c : 1745 ] Failed Rx Stop 
1282,,[ cmdProcessTlv2.c : 1756 ] ### genericUtfCmdHandler: InValid CmdID#### 
1281,i,[ cmdProcessTlv2.c : 493 ]  FATAL ERROR!! Trying to access phy %d which is not present 
1280,i,[ cmdProcessTlv2.c : 504 ]  FATAL ERROR!! Trying to access phy %d which is inactive 
1279,I,[ cmdProcessTlv2.c : 4363 ] modifyBDFOTPFlagsHandler: modifyBdfOtpFlags 0x%x 
1278,,[ cmdProcessTlv2.c : 4381 ] modifyBDFOTPFlagsHandler: pCmdStream is NULL 
1277,,[ cmdProcessTlv2.c : 3741 ] OFDMA TonePlan
 
1276,ii,[ cmdProcessTlv2.c : 626 ] FTM :: pktgen_complete_timer_handler:  pktgen_complete_timer_handler: Pktgen Tx STOP completion callback failure for phyId %d g_pktgen_done_assert_count %d 
1275,iiiiiii,[ cmdProcessTlv2.c : 1122 ] rxHandler: phyId %d rxMode %d wlanMode %d freq %d freq2 %d chainMask %d wifiStandard %d 
1274,i,[ cmdProcessTlv2.c : 1136 ] RX operation not allowed on phyID %d one operation ongoing 
1273,,[ cmdProcessTlv2.c : 4400 ] #### per chain forced pwr TLV called!
 
1272,iI,[ cmdProcessTlv2.c : 2732 ] setPhyRfModeHandler: DBS/SBS is not supported, phyRfMode %d status 0x%x  
1271,I,[ cmdProcessTlv2.c : 1259 ] pdev %u 
1270,iiiiiII,[ cmdProcessTlv2.c : 1295 ] curChan->band_center_freq1 %d, curChan->band_center_freq2 %d, PHYRF_BW_IDX(curChan) %d curChan->phy_mode %d num_20_bw %d rx_CM %x, tx_CM %x 
1269,ii,[ cmdProcessTlv2.c : 1363 ] pilot_evm pilot_evm_dB_mean[%d] = %d 
1268,I,[ cmdProcessTlv2.c : 588 ] FTM :: tlv2SendTxStatus:  timestamp = %ld 
1267,iiii,[ cmdProcessTlv2.c : 3516 ] Tx Gain Control:Chain %d, Gain %d, dacGain %d, forceCal %d 
 
1266,iiiiiiiI,[ cmdProcessTlv2.c : 675 ] FTM :: txHandler: phyId %d txMode %d freq %d freq2 %d wlanMode %d chainMask %d wifiStandard %d timestamp =%ld 
1265,IIII,[ cmdProcessTlv2.c : 850 ] FTM :: txHandler: ret:0x%x, ret1:0x%x, ret2:0x%x, ret3:0x%x 
1264,ii,[ cmdProcessTlv2.c : 868 ] FTM :: txHandler dev running state=%d iterations_taken_to_flush=%d 
1263,iI,[ cmdProcessTlv2.c : 879 ] FTM :: txHandler: Sent response to host with status =%d, timestamp =%ld 
1262,i,[ cmdProcessTlv2.c : 709 ] FTM :: txHandler: TX operation not allowed on phyID %d one operation ongoing 
1261,iiI,[ cmdProcessTlv2.c : 919 ] FTM :: txStatusHandler: INSIDE txStatusHandler phyId =%d pParms->needReport=%d timestamp : %u 
1260,ii,[ cmdProcessTlv2.c : 933 ] FTM :: txStatusHandler: pParms->needReport=%d pParms->stopTx=%d 
1259,IIII,[ cmdProcessTlv2.c : 964 ] FTM :: txStatusHandler: ret:0x%x, ret1:0x%x, ret2:0x%x, ret3:0x%x 
1315,,[ LMGoProcessing.c : 61 ] LM_DBG: NULL pdev return 
1314,Ii,[ LMGoProcessing.c : 78 ] LM_DBG: ABI on-period tx_duration_data %ld(US) current_time(MS) %d 
1313,Ii,[ LMGoProcessing.c : 295 ] LM_DBG: ABI off-period tx_duration_data(US) %ld curTime(MS) %d 
1317,II,[ cmdProcessing.c : 279 ] FTM_DEBUG :: txCmdProcessor, TxMiscFlags : 0x%x txParms->aifsn=0x%x 
1316,iiiii,[ cmdProcessing.c : 391 ] FTM :: txCmdProcessor channel=%d txPwr=%d dataRrate=%d numPkt=%d txChain=%d
 
1344,I,[ tcmd.c : 4941 ] Invalid pdev %lu 
1343,,[ tcmd.c : 1222 ] A: NEW COMMAND ISSUED 
1342,iiiiI,[ tcmd.c : 2388 ] [UL-OFDMA]ruIdx=%d, dataRate=%d, NSS=%d, pktSz=%d, miscFlags=0x%x 
1341,,[ tcmd.c : 4303 ] Could not find valid ruIdx in tone plan 
1340,i,[ tcmd.c : 3607 ] tcmd_cont_rx_begin: phyId=%d, chain mask 0
 
1339,i,[ tcmd.c : 3648 ] tcmd_cont_rx_begin: phyId=%d, tcmd_setup_channel failure
 
1338,Ii,[ tcmd.c : 3203 ] tcmd_cont_rx_cmd - flags 0x%x; act %d 
1337,ii,[ tcmd.c : 3211 ] aId[%d] = %d 
1336,,[ tcmd.c : 3217 ] Could not find valid aID in tone plan 
1335,ii,[ tcmd.c : 3473 ] pilot_evm g_ftmrxstats[phyId].pilotEvmDbMean[%d] = %d 
1334,iii,[ tcmd.c : 2696 ] TPC force glutindex: chain%d: gainindex%d: dacgain=%d
 
1333,iii,[ tcmd.c : 2718 ] PAPRD TCMD: Chain %d Glut Idx %d Gain Idx %d
 
1332,iiii,[ tcmd.c : 2833 ] Setup chan failed: freq %d, freq2 %d, wlanMd %d, bw %d
 
1331,,[ tcmd.c : 4172 ] Enabled SIFS bursting for Tx99 
1330,i,[ tcmd.c : 1808 ] Invalid frequency %d.
 
1329,,[ tcmd.c : 1946 ] 11AC VHT20 
 
1328,i,[ tcmd.c : 2188 ] 165 MHz frequency %d 
1327,i,[ tcmd.c : 2192 ] Invalid frequency %d 
1326,i,[ tcmd.c : 2028 ] pktType Invalid %d
 
1325,Iiiii,[ tcmd.c : 2141 ] get_ch wlanMode: %lu ch: %d freq1 %d freq2 %d, fcMode %d
 
1324,iiII,[ tcmd.c : 3883 ] tcmd_setup_channel_real: phyId=%d,Failure: chan.phy_mode=%d, rx_tcmdParms.u.para.pktType=0x%x, rx_tcmdParms.miscFlags=0x%x
 
1323,II,[ tcmd.c : 3993 ] tcmd() Before GI 0x%x LTF 0x%x 
1322,II,[ tcmd.c : 4028 ] tcmd() After GI 0x%x LTF 0x%x 
1321,iI,[ tcmd.c : 1496 ] A: TCMD TX COMP CB - MADE STOP TX = 2 phyId [%d] | Time : %u 
1320,I,[ tcmd.c : 4453 ] tcmd() Before RC flag 0x%x 
1319,Iii,[ tcmd.c : 4478 ] tcmd() After RC flag 0x%x GI %d LTF %d 
1318,ii,[ tcmd.c : 4630 ] [UL-OFDMA]gi=%d, ltf=%d 
1351,,[ tcmd_rx.c : 335 ] A: RETURN if((g_ftm_frame_enacap_config[phyId].da_addr == NULL) || (g_ftm_frame_enacap_config[phyId].bss_addr == NULL)) 
1350,,[ tcmd_rx.c : 364 ] RX WAL PEER A_PANIC 
1349,ii,[ tcmd_rx.c : 383 ] A: wal_vdev_attach vdevId[%d]=%d 
1348,,[ tcmd_rx.c : 389 ] A: wal_peer_alloc rx peer 1 
1347,,[ tcmd_rx.c : 399 ] A: wal_peer_alloc rx peer 2 
1346,,[ tcmd_rx.c : 352 ] A: page fault condition, all vdev is null 
1345,,[ tcmd_rx.c : 361 ] A: Inside if(g_tcmd_wal_rx_ctxt[phyId].vdev == NULL) 
1369,ii,[ tcmd_tx.c : 1417 ] [MU] sched_algo_mu_tx_peer_assoc() peer[%d] AID %d 
1368,,[ tcmd_tx.c : 1533 ] A: INSIDE tcmd_wal_peer_free 
1367,ii,[ tcmd_tx.c : 1023 ] tcmd_wal_setup_data_rate: rc %d invalid for freq %d 
1366,ii,[ tcmd_tx.c : 418 ] ftm_tid_create_handler: phyId %d, tid %d 
1365,,[ tcmd_tx.c : 1558 ] A: RETURN if((g_ftm_frame_enacap_config[phyId].bss_addr == NULL) || (g_ftm_frame_enacap_config[phyId].da_addr == NULL))  
1364,,[ tcmd_tx.c : 1564 ] A: if((g_tcmd_wal_config[phyId].vdev) == NULL)  
1363,,[ tcmd_tx.c : 1567 ] A: if(((g_bss_peer[phyId]) == NULL) || (g_ftm_ctxt[phyId].peer == NULL))  
1362,,[ tcmd_tx.c : 1572 ] A: RETURN if((g_bss_track_peer != NULL) || (g_ctxt_track_peer != NULL)) 
1361,,[ tcmd_tx.c : 1176 ] A: peer_use_4cal 
1360,iiI,[ tcmd_tx.c : 1196 ] A: g_bss_peer[%d]=%d g_ftm_bss_peer[phyId]= %08x 
1359,I,[ tcmd_tx.c : 1197 ] cwc wal_peer_alloc for bss_peer %08x <= 
1358,I,[ tcmd_tx.c : 1200 ] A: ctxt->peer=0x%x 
1357,iI,[ tcmd_tx.c : 1201 ] A: g_ftm_frame_enacap_config[%d].da_addr=0x%x 
1356,iI,[ tcmd_tx.c : 1202 ] A: g_ftm_frame_enacap_config[%d].bss_addr=0x%x 
1355,Ii,[ tcmd_tx.c : 1212 ] A: wal_peer_alloc ctxt->peer[%08x] %d times  
1354,,[ tcmd_tx.c : 1215 ] A: wal_peer_alloc peer_use_4cal ctxt->peer  
1353,iiI,[ tcmd_tx.c : 1179 ] A: g_bss_peer[%d]=%d g_ftm_bss_peer[phyId]= %08x 
1352,,[ tcmd_tx.c : 1186 ] A: peer_use_4cal wal_peer_alloc bss_peer 
1457,iii,[ tpcCal.c : 586 ] chk1 Max_TX_CAL_Gain_ID_5G:%d Max_TX_CAL_Gain_ID_2G %d Max_TX_CAL_Gain_ID_6G %d 
1456,IIII,[ tpcCal.c : 680 ] tpccal::5G opcChan[%u] %u, tpcChan[%u] %u 
1455,IIII,[ tpcCal.c : 700 ] tpccal::6G opcChan[%u] %u, tpcChan[%u] %u 
1454,Ii,[ tpcCal.c : 760 ] greenTxGainIndGrpFlag2G:%x, greenTxGainIndGrpFlag5G:%d 
 
1453,iiii,[ tpcCal.c : 845 ]  5G IdxGainEndGrp1:%d IdxGainEndGrp2:%d IdxGainEndGrp3:%d IdxGainEndGrp4:%d
 
1452,i,[ tpcCal.c : 633 ] tpccal chan::6g %d 
1451,IIII,[ tpcCal.c : 660 ] tpccal::2G opcChan[%u] %u, tpcChan[%u] %u 
1450,iiiii,[ tpcCal.c : 1210 ] freq %d gIdx %d dacGain %d paCfg %d chMask %d
 
1449,III,[ tpcCal.c : 1248 ] tpccal::Stopping tx before starting for Chan %u, Chain %u, Gain %u 
1448,,[ tpcCal.c : 2338 ] tpccal::Generating Caldata 
1447,ii,[ tpcCal.c : 2382 ] tpcCal::Generating Caldata for Channel %d dacGainforCal %d 
1446,i,[ tpcCal.c : 2386 ] tpcCal::Generating Caldata for Chain %d 
1445,iii,[ tpcCal.c : 2392 ] tpcCal::Generating Caldata for GLUT Gain Idx %d txgainIdx %d meas_pwr %d 
1444,iii,[ tpcCal.c : 2402 ] tpcCal::Generating Caldata for GLUT EXT Gain Idx %d txgainIdx %d meas_pwr %d 
1443,iii,[ tpcCal.c : 2412 ] tpcCal::Generating Caldata for PLUT Gain Idx %d pdadc_read %d meas_pwr %d 
1442,iii,[ tpcCal.c : 2454 ] tpcCal::Generating Caldata for Chain %d sbsOffset %d NUM_CAL_GAINS_SELECTED_4_GLUT:%d 
1441,iii,[ tpcCal.c : 2461 ] tpcCal::Generating Caldata for GLUT Gain Idx %d txgainIdx %d meas_pwr %d 
1440,iiii,[ tpcCal.c : 2471 ] tpcCal::Generating Caldata for GLUT EXT Gain Idx %d txgainIdx %d meas_pwr %d numGlutEntries_5G:%d 
1439,iii,[ tpcCal.c : 2481 ] tpcCal::Generating Caldata for PLUT Gain Idx %d pdadc_read %d meas_pwr %d 
1438,iii,[ tpcCal.c : 2499 ] phyId:%d cmask:%d pwrAtPdadc:%d 
1437,III,[ tpcCal.c : 1670 ] getNextLoop fail curLoop->idxCalPt %u, Chain %u, Gain %u 
1436,iiiii,[ tpcCal.c : 1697 ] bef, band %d ch %d numCh %d chain %d gain %d
 
1435,,[ tpcCal.c : 1702 ] end loop0
 
1434,iiii,[ tpcCal.c : 1715 ] inc calPt %d ch %d chn %d, numGain %d
 
1433,ii,[ tpcCal.c : 1723 ] inc chain AI %d %d
 
1432,ii,[ tpcCal.c : 1731 ] inc ch AI %d %d
 
1431,ii,[ tpcCal.c : 1739 ] inc band AI %d %d
 
1430,,[ tpcCal.c : 1743 ] end loop
 
1429,iiii,[ tpcCal.c : 1804 ] pwr est %d band %d numEst %d, idx %d 
1428,iiiii,[ tpcCal.c : 1808 ] sG %d %d %d %d %d  
1427,i,[ tpcCal.c : 1809 ] %d
 
1426,i,[ tpcCal.c : 3077 ] available_gainIdxs:%d 
1425,iiii,[ tpcCal.c : 3083 ] Iteration m:%d glutsfilled[%d]:%d Max_Glut_Map[band][grpId]:%d 
1424,i,[ tpcCal.c : 3084 ] tpcCalResult[band][chan].measPwr[chain][m]:%d 
1423,,[ tpcCal.c : 3087 ] ERR: BAD CAL TARGETs CONFIGURED for:  
1422,i,[ tpcCal.c : 3094 ] Picked limiting gainidx:%d 
1421,i,[ tpcCal.c : 3103 ] Picked gainidx:%d  
1420,,[ tpcCal.c : 3107 ] Moving up gainidxs to guarantee GLUT count! 
1419,ii,[ tpcCal.c : 3110 ] currIndx:%d Updated endPwrIdxGrp:%d 
1418,,[ tpcCal.c : 3115 ] BAD CAL TARGETs CONFIGURED for 
1417,ii,[ tpcCal.c : 3120 ] Picked max gainidx:%d from group :%d  
1416,,[ tpcCal.c : 3123 ] Invalid pick_glut_entry condition! 
1415,,[ tpcCal.c : 1986 ] tpccal::Post processing CLPC Caldata 
1414,,[ tpcCal.c : 2112 ] tpccal::Post processing CLPC Caldata 
1413,,[ tpcCal.c : 1880 ] tpccal::Post processing OLPC Caldata 
1412,,[ tpcCal.c : 1888 ] pp OLPC
 
1411,iiiii,[ tpcCal.c : 1911 ] meaPwr %d tgtPwr %d, bn %d ch %d chn %d, 
 
1410,i,[ tpcCal.c : 1912 ] numValidMeas = %d
 
1409,iiii,[ tpcCal.c : 1919 ] bkof %d bn %d ch %d chn %d
 
1408,iiii,[ tpcCal.c : 1930 ] stPwrIdx %d bn %d ch %d chn %d
 
1407,iiiiiiii,[ tpcCal.c : 1956 ] iMeas %d iGainIdx %d tgt %d ch %d chn %d sel pwr %d gIdx %d dac %d
 
1406,,[ tpcCal.c : 3141 ] postProcessingOLPCCALData_gtx 
1405,iiii,[ tpcCal.c : 3172 ] BegiN: Band:%d chan:%d startPwrIdxGrp:%d  endPwrIdxGrp:%d  
1404,ii,[ tpcCal.c : 3173 ] gtx tgtpwridx:%d , GlutPwrMapGrpNum:%d  
1403,iii,[ tpcCal.c : 3180 ] gtx startPwrIdxGrp:%d , endPwrIdxGrp:%d modifiedTarget:%d 
1402,i,[ tpcCal.c : 3182 ] endPwrIdxGrp:%d 
1401,iii,[ tpcCal.c : 3188 ] gtx startPwrIdxGrp:%d , endPwrIdxGrp:%d modifiedTarget:%d 
1400,i,[ tpcCal.c : 3190 ] endPwrIdxGrp:%d 
1399,iiii,[ tpcCal.c : 3197 ] gtx startPwrIdxGrp:%d , endPwrIdxGrp:%d tpcCfg[band].IdxGainEndGrp3:%d modifiedTarget:%d 
1398,i,[ tpcCal.c : 3199 ] endPwrIdxGrp:%d 
1397,iiii,[ tpcCal.c : 3205 ] gtx startPwrIdxGrp:%d , endPwrIdxGrp:%d tpcCfg[band].IdxGainEndGrp4:%d modifiedTarget:%d 
1396,i,[ tpcCal.c : 3207 ] endPwrIdxGrp:%d 
1395,iii,[ tpcCal.c : 3211 ] gtx Invalid TPC_GLUT_PWR_MAP_GRP Id ! from Band:%d Chain:%d tgtpwridx:%d 
1394,ii,[ tpcCal.c : 1032 ] Sending to host freq2G %d, freq5G %d
 
1393,iii,[ tpcCal.c : 1573 ] Sending to host freq2G %d, freq5G %d, chain %d 
1392,iiii,[ tpcCal.c : 1574 ] gain %d pwr %d numChain %d numCalpt %d
 
1391,IIII,[ tpcCal.c : 1578 ] tpccal::Sending to host to look for measurements inChan2G %u, Chan5G %u, ChainMask(User) %u, Gain %u 
1390,iii,[ tpcCal.c : 1580 ] Sending to host freq2G %d, freq5G %d, chain %d
 
1389,iiii,[ tpcCal.c : 1581 ] gain %d pwr %d numChain %d numCalpt %d
 
1388,,[ tpcCal.c : 2291 ] tpccal::Sending Caldata to host 
1387,,[ tpcCal.c : 1317 ] tpccal::Starting ... 
1386,,[ tpcCal.c : 1414 ] TPC Cal message check 
 
1385,ii,[ tpcCal.c : 1456 ] tpcCALScheme: %d, phyID %d
 
1384,,[ tpcCal.c : 1850 ] tpccal::Completed 
1383,,[ tpcCal.c : 1866 ] FTM_REGEN_CALDB: Initiating cold boot calibration in FTM...
 
1382,,[ tpcCal.c : 2709 ] tpccal::Out of sync power measurement report!
 
1381,iIIII,[ tpcCal.c : 2742 ] tpccal::Got measurement %d from host for Chan %u Chain %u Chain(user) %u Gain %u 
1380,iIIIII,[ tpcCal.c : 2762 ] tpccal::Thermoffset %d for Band %u tpcChan %u opcChan[%u] %u  Chain %u 
1379,iiii,[ tpcCal.c : 2778 ] Got Power from host Chan %d ,  GainIdx %d , MeasPwr  %d , Read pdadc %d  
1378,ii,[ tpcCal.c : 2831 ] Received identical power meas:%d prevMeas:%d .Failing calloop 
1377,iii,[ tpcCal.c : 2860 ] Get 10Log(pdadc) prev:%d curr:%d slope:%d 
1376,ii,[ tpcCal.c : 2863 ] Get Power meas:%d prevMeas:%d 
1375,iiii,[ tpcCal.c : 2864 ]  calFail:%d, gainIdx:%d, idxCalPt:%d skipSlope_gtx_bndry:%d 
1374,i,[ tpcCal.c : 2868 ] skipping slope for gainIdx = %d 
1373,III,[ tpcCal.c : 1835 ] tpccal::Starting tx for Chan %u, Chain %u, Gain %u 
1372,iiiii,[ tpcCal.c : 3046 ] Write to tpcCalPostProcResult[%d][%d].olpc.measPwrExt[%d][%d]:%d 
1371,iiiii,[ tpcCal.c : 3053 ] Write to tpcCalPostProcResult[%d][%d].olpc.measPwr[%d][%d]:%d 
1370,ii,[ tpcCal.c : 3063 ] glutsfilled[%d]:%d 
1459,ii,[ xtalCal.c : 252 ] [TLV2_CTRL_W_OTP]capIn=%d, capOut=%d 
1458,ii,[ xtalCal.c : 256 ] [ERROR][TLV2_CTRL_W_OTP]OTP has data %d, %d 
1478,Iiii,[ tpcOnepointCal.c : 296 ] tpcOnepointCal::Starting Tx for phy %u, freq %d, chainMask %d, txPwr_db2 %d 
1477,Iiii,[ tpcOnepointCal.c : 299 ] tpcOnepointCal::Stopping Tx for phy %u, freq %d, chainMask %d, txPwr_db2 %d 
1476,iii,[ tpcOnepointCal.c : 529 ] tpcOnepointCal::Failure at BandIdx:%d chanIdx:%d chainIdx:%d 
1475,,[ tpcOnepointCal.c : 539 ] tpcOnepointCal:: end loop 1 
1474,,[ tpcOnepointCal.c : 549 ] tpcOnepointCal:: break 
1473,,[ tpcOnepointCal.c : 595 ] tpcOnepointCal:: end loop 
1472,i,[ tpcOnepointCal.c : 136 ] tpccal chan::2g %d 
1471,ii,[ tpcOnepointCal.c : 170 ] tpcOnepointCal::TPC_DBG 5G numChain %d 2G numChain %d 
1470,i,[ tpcOnepointCal.c : 142 ] tpccal chan::5g %d 
1469,i,[ tpcOnepointCal.c : 148 ] tpccal chan::6g %d 
1468,ii,[ tpcOnepointCal.c : 613 ] tpcOnepointCal::TPC_DBG band %d idxChan %d 
1467,IIII,[ tpcOnepointCal.c : 431 ] tpcOnepointCal::Requesting pwr measurement for phy %u, freq %u, chainMask %u,tgtPwr_db8 %u 
1466,IIII,[ tpcOnepointCal.c : 445 ] tpcOnepointCal::Requesting pwr measurement for phy %u, freq %u, chainMask %u,tgtPwr_db8 %u 
1465,IIII,[ tpcOnepointCal.c : 461 ] tpcOnepointCal::Requesting pwr measurement for phy %u, freq %u, chainMask %u,tgtPwr_db8 %u 
1464,,[ tpcOnepointCal.c : 668 ] tpcOnepointcal::Completed 
1463,,[ tpcOnepointCal.c : 322 ] tpcOnepointCAL::Starting... 
1462,,[ tpcOnepointCal.c : 711 ] tpcOnepointcal::Failure, -999 power detected 
1461,IIIiiI,[ tpcOnepointCal.c : 739 ] tpcOnepointCal::Pwr measurement for phy %u, freq %u, chainMask %u, glutOffset %d, thermOffset %d, measPwr_db8 is %u 
1460,,[ tpcOnepointCal.c : 102 ] tpcOnepointCal::tpcPowerMeasurementDelayTimeout 
1487,iiiiii,[ rxGainCal.c : 132 ] rxGainCal:: Starting Rx on phyId %d, is2Ghz %d, Chain %d Chan %d, rxMode %d refISS Level %d 
1486,i,[ rxGainCal.c : 213 ] rxGainCal:: Error on chainIdx %d
 
1485,i,[ rxGainCal.c : 223 ] rxGainCal:: Error on chainIdx %d
 
1484,i,[ rxGainCal.c : 237 ] rxGainCal:: Error on chainIdx status %d
 
1483,ii,[ rxGainCal.c : 281 ] rxGainCal:: Host error: phyId %d,  veryFirstRxGainCal %d 
1482,iiiiii,[ rxGainCal.c : 295 ] rxGainCal:: Host error: phyId %d, chainIdx %d, ChanIdx %d, Expected Pkt Cnt %d, Actual Pkt Cnt %d,  rxGainCalState.status %d 
1481,iiiiiii,[ rxGainCal.c : 337 ] rxGainCal:: Saving Results for phyId %d, chainIdx %d, ChanIdx %d, PNFdBr %d, PNFdBm %d, Expected Pkt Cnt %d, Actual Pkt Cnt %d 
1480,iiiiii,[ rxGainCal.c : 343 ] rxGainCal:: Saving Results for phyId %d, chainIdx %d, ChanIdx %d, Expected Pkt Cnt %d, Actual Pkt Cnt %d totalPkt=%d 
1479,,[ rxGainCal.c : 353 ] nextLoopRxCal is NULL 
1488,ii,[ wmi_ftm_attach.c : 227 ] ERROR: ftm_parse_unifiedcmd: dataLen %d is LESS than sizeof(segHdrInfo) %d 
1501,III,[ whal_debug.c : 5561 ] assert:r0=0x%x, r1=0x%x, line:0x%x
 
1500,ii,[ whal_debug.c : 5724 ] config_reg_dump: Entries exceeded MAX REG DUMP ENTRY :%d! :%d 
 
1499,I,[ whal_debug.c : 5729 ] config_reg_dump: Invalid register physical address! :0x%x 
 
1498,iIIII,[ whal_debug.c : 3583 ] CRYPTO_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
1497,iII,[ whal_debug.c : 3453 ] HWSCH_TRACER_LOG: mac(%d), tbus_index(0x%x), debug_trace(0x%x) 
1496,iIIII,[ whal_debug.c : 3551 ] PDG_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
1495,iIIII,[ whal_debug.c : 4378 ] RXDMA1_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
1494,iIIII,[ whal_debug.c : 4324 ] RXDMA_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
1493,iIIII,[ whal_debug.c : 3647 ] RXOLE_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
1492,iIIII,[ whal_debug.c : 3518 ] RXPCU_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
1491,iIIII,[ whal_debug.c : 4434 ] TXDMA_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
1490,iIIII,[ whal_debug.c : 3615 ] TXOLE_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
1489,iIIII,[ whal_debug.c : 3486 ] TXPCU_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
1508,II,[ whal_hwsch.c : 3661 ] hwsch2_wdog_timeout: reg_wdog=%x, reg_cmd_ring_wdog=%x 
1507,II,[ whal_hwsch.c : 3853 ] cca_watchdog=%x, reg_axi_err=%x 
1506,II,[ whal_hwsch.c : 3898 ] ul-q(%i), reg:%x 
1505,III,[ whal_hwsch.c : 3904 ] val_0=%x, val_1=%x, val_2=%x 
1504,I,[ whal_hwsch.c : 4056 ] WHAL_FATAL_ERR_UNKNOWN:%x 
1503,i,[ whal_hwsch.c : 4070 ] WHAL_FATAL_ERR_UNKNOWN: pdev_id:%d - Ignore, since wdog statuses got cleared 
1502,iiIii,[ whal_hwsch.c : 4665 ] config_txop_sel (pdev=%d,q=%d): reg=0x%x, lifetime_exp=%d, txop_sel=%d 
1510,II,[ whal_interrupt.c : 997 ] Clear false RXPCU WDOG, status %x, limit %x 
1509,I,[ whal_interrupt.c : 1713 ] GetPendingInterrupts-whalPending:0x%x 
1512,ii,[ whal_wmac_recipes.c : 144 ] whal_wmac_clr_rogue_ap_type_by_mask: rogue_ap_bit_mask[%d]: %d 
1511,ii,[ whal_wmac_recipes.c : 164 ] whal_wmac_set_rogue_ap_type: rogue_ap_bit_mask[%d]: %d 
1513,,[ whal_cce.c : 463 ] poll MCMN_R0_MCMN_MAC_IDLE/HWIO_MCMN_R0_MCMN_MAC_IDLE_RXOLE_BMSK timeout
 
1519,III,[ whal_recv.c : 6743 ] fse_watchdog %x, sm_state_reg %x, cache_response %x 
1518,II,[ whal_recv.c : 5652 ] rssi_legacy rssi_comb,rssi_comb_ppdu :0x%x chain0, 1:0x%x 
1517,iii,[ whal_recv.c : 1558 ] startPcuReceive on mac:%d, phy_is_off:%d leave_phy_off:%d 
1516,I,[ whal_recv.c : 9263 ] TxRx overlap TLV_READY reg_val: 0x%x
 
1515,Ii,[ whal_recv.c : 9097 ] %s: invalid lmac id %d
 
1514,,[ whal_recv.c : 9128 ] Link desc leakage due to SFM issue Jira 1206
 
1544,,[ whal_recv_recovery.c : 79 ] SW2RXDMA_BUF ring empty 
1543,,[ whal_recv_recovery.c : 122 ] FW2RXDMA_BUF ring empty 
1542,,[ whal_recv_recovery.c : 143 ] RX_RING_FW_BUF ring empty caused by RX_RING_WMI_EVT 
1541,,[ whal_recv_recovery.c : 167 ] FW2RXDMA_STATBUF ring empty 
1540,,[ whal_recv_recovery.c : 174 ] FW2RXDMA_STATBUF ring empty 
1539,,[ whal_recv_recovery.c : 199 ] WBM2RXDMA_LINK ring empty 
1538,,[ whal_recv_recovery.c : 206 ] WBM2RXDMA_LINK ring empty 
1537,,[ whal_recv_recovery.c : 231 ] FW2RXDMA_LINK ring empty 
1536,,[ whal_recv_recovery.c : 86 ] SW2RXDMA_BUF ring empty 
1535,,[ whal_recv_recovery.c : 238 ] FW2RXDMA_LINK ring empty 
1534,,[ whal_recv_recovery.c : 265 ] MO SW2RXDMA_BUF ring empty 
1533,,[ whal_recv_recovery.c : 272 ] MO SW2RXDMA_BUF ring empty 
1532,,[ whal_recv_recovery.c : 297 ] MO FW2RXDMA_STATBUF ring empty 
1531,,[ whal_recv_recovery.c : 304 ] MO FW2RXDMA_STATBUF ring empty 
1530,,[ whal_recv_recovery.c : 329 ] MO FW2RXDMA_LINK ring empty 
1529,,[ whal_recv_recovery.c : 336 ] MO FW2RXDMA_LINK ring empty 
1528,IIIIII,[ whal_recv_recovery.c : 382 ] ring type [0x%x] empty error ts-0x%x, pre hp:0x%x, ts 0x%x, hp 0x%x, tp 0x%x 
1527,IiI,[ whal_recv_recovery.c : 393 ] ring type [0x%x] wmi pending:%d, empty %x 
1526,,[ whal_recv_recovery.c : 115 ] FW2RXDMA_BUF ring empty 
1525,IIIIIIII,[ whal_recv_recovery.c : 516 ] ring [0x%x] full ts-0x%x, hp 0x%x, tp 0x%x, reo2sw1: 0x%x, reo2sw4:0x%x, reo2tcl:0x%x, rxdma2sw:0x%x 
1524,IiIIII,[ whal_recv_recovery.c : 1738 ] RXDMA hang type [0x%x], cnt %d, error ts-0x%x, rin type: %x, mask 0x%x:0x%x 
1523,IiIII,[ whal_recv_recovery.c : 974 ] RXOLE hang type [0x%x], cnt %d, error ts-0x%x, rin type: %x, mask 0x%x 
1522,IIII,[ whal_recv_recovery.c : 1151 ] RXPCU hang type [0x%x] empty error ts-0x%x, mask 0x%x, 0x%x 
1521,IIII,[ whal_recv_recovery.c : 1871 ] RXCRYPTO hang type [0x%x] empty error ts-0x%x, mask 0x%x, 0x%x 
1520,i,[ whal_recv_recovery.c : 762 ] TXRX OVLAP hit on MAC-%d 
1559,iiiii,[ whal_reset.c : 3644 ] channelSwitch: INI = %d TPC = %d Cal = %d Tot = %d PF = %d 
1558,i,[ whal_reset.c : 2763 ] whalConfigProxyStaParams Unhandled BSS_ID :%d  
1557,,[ whal_reset.c : 1175 ] DEBUG_RESTORE::Invalid access type 
 
1556,II,[ whal_reset.c : 1192 ] DEBUG_RESTORE::Read::addr=0x%x, value=0x%x
 
1555,IiiI,[ whal_reset.c : 1209 ] DEBUG_RESTORE::Bitmask Read::addr=0x%x, bitmask=%d, bitshift=%d, value=0x%x 
 
1554,II,[ whal_reset.c : 1222 ] DEBUG_RESTORE::Write::addr=0x%x, value=0x%x 
 
1553,IiiI,[ whal_reset.c : 1240 ] DEBUG_RESTORE::Bitmask Write::addr=0x%x, bitmask=%d, bitshift=%d, value=0x%x 
 
1552,i,[ whal_reset.c : 1245 ] DEBUG_RESTORE::Invalid num_args_type at idx = %d
 
1551,,[ whal_reset.c : 1137 ] DEBUG_CACHE::Invalid Access type 
 
1550,I,[ whal_reset.c : 1600 ] whalSetMACNAVOverrideCfg: value = 0x%x 
1549,,[ whal_reset.c : 1069 ] DEBUG_CACHE::Clearing the cache 
 
1548,,[ whal_reset.c : 1114 ] DEBUG_CACHE::Invalid num args type 
 
1547,,[ whal_reset.c : 1075 ] DEBUG_CACHE::Invalid address 
 
1546,,[ whal_reset.c : 1081 ] DEBUG_CACHE::Reseting the cache idx 
 
1545,iIiiI,[ whal_reset.c : 1047 ] DEBUG_CACHE::args_type=%d, addr=0x%x, bitmask=%d, bitshift=%d, value=0x%x 
 
1579,iiIIII,[ whal_rtt.c : 1132 ] DEBUG-TKNS: %d,%d,%lu,%lu,%lu,%lu 
1578,IIIIIIIIi,[ whal_rtt.c : 1144 ] DEBUG-PERF: %lu,%lu,%lu,%lu,%lu,%lu,%lu,%lu,%d 
1577,II,[ whal_rtt.c : 1150 ] DEBUG-PERF: %lu,%lu 
1576,iiIIIIII,[ whal_rtt.c : 1101 ] DEBUG-PERF: %d,%d,%lu,%lu,%lu,%lu,%lu,%lu 
1575,II,[ whal_rtt.c : 1107 ] DEBUG-PERF: %lu,%lu 
1574,IIIIIIIII,[ whal_rtt.c : 575 ] RXLocInf1 0x%08x,0x%08x,0x%08x,0x%08x,0x%08x,0x%08x,0x%08x,0x%08x,0x%08x 
1573,I,[ whal_rtt.c : 576 ] RXLocInf2 %u 
1572,,[ whal_rtt.c : 232 ] whal_rtt_frame_prepare() HW is already prepared for RTT return !!! 
1571,,[ whal_rtt.c : 354 ] whal_rtt_frame_recover() HW was not configured for RTT!!! return 
1570,I,[ whal_rtt.c : 700 ] ar_wal_get_rssi_chain: invalid rssi_info for %p 
1569,II,[ whal_rtt.c : 708 ] ar_wal_rtt_get_rssi_chain: rssi_info 0x%08x%08x 
1568,IiIiii,[ whal_rtt.c : 1080 ] rtt_get_toda: txrx_msg_buf=%p toda_type=%d toda_phy_clk=%u ppdu_id=%d txrx_delay=%d status=%d 
1567,ii,[ whal_rtt.c : 556 ] rtt_get_tx_rate: rate: %d bit_rate_kbps: %d 
1566,Ii,[ whal_rtt.c : 939 ] recv sta rssi 0x%08x chain:%d 
1565,ii,[ whal_rtt.c : 1183 ] rtt_recv_sta_get_rxbw: rx_bw=%d rx_preamble=%d 
1564,iiIIiIi,[ whal_rtt.c : 184 ] whal_rtt_recv_sta_txrx_chain_handle_event: mode %d event %d tx_mask 0x%02x rx_mask 0x%02x tx_dirty %d rtt_selfgen_tx_chain_idx %u rtt_rx_chain_idx %d 
1563,Ii,[ whal_rtt.c : 966 ] send sta rssi 0x%08x chain:%d 
1562,I,[ whal_rtt.c : 1225 ] rtt_send_sta_get_rxbw: rtt_pkt_bw=0x%x 
1561,I,[ whal_rtt.c : 1205 ] rtt_send_sta_get_txbw: packet_bw=0x%x 
1560,,[ whal_rtt.c : 1344 ] ar_wal_rtt_tx_ppdu_completion_handler: excess zero values in receive_rssi_info 
1581,iii,[ whal_cfir.c : 253 ] whal_cfir_configure: rtt %d capture_cfr %d capture_cir %d 
1580,iiI,[ whal_cfir.c : 193 ] whal_cfir_enable: enaRttPerBurst %d enaFixedStrChain %d fixedStrChainIdx 0x%02x 
1583,I,[ whal_tqm.c : 402 ] link_Desc_tshd register value:%02x 
1582,I,[ whal_tqm.c : 412 ] link_Desc_tshd register value:%02x 
1603,IIIIII,[ whal_xmit.c : 20680 ] fsm_client0 = %lu, fsm_client1 = %lu, fsm_client2 = %lu,  fsm_client3 = %lu, fsm_client4 = %lu,  fsm_client5 = %lu 
1602,IIIIiII,[ whal_xmit.c : 20682 ] fsm_client6 = %lu, fsm_client7 = %lu,  fsm_client8 = %lu, fsm_client9 = %lu, num of times sfm issue got hit = %d, sfm_status = %u, sfm_limit = %u 
1601,i,[ whal_xmit.c : 20532 ] NAN virtual CCA: war_enable=%d 
1600,iiIII,[ whal_xmit.c : 15190 ] TPCDBG: HWAdjust: tpc=%d,%d cm=%x c=%08x:%08x 
1599,ii,[ whal_xmit.c : 11024 ] InfoTPC: Max TPC = %d Min TPC = %d
 
1598,iiiiii,[ whal_xmit.c : 5468 ] UL_RESP_TPC_DBG : rix %d, rc_flags %d, num_chain %d, tx_mask %d, ctl_pwr %d, chan %d 
1597,II,[ whal_xmit.c : 20284 ] FIPS hp %x tp %x 
1596,I,[ whal_xmit.c : 20302 ] FIPS nxt_p %x 
1595,,[ whal_xmit.c : 20326 ] FIPS hp null 
1594,I,[ whal_xmit.c : 20355 ] FIPS %x 
1593,,[ whal_xmit.c : 20366 ] FIPS nxt_p null 
1592,I,[ whal_xmit.c : 20394 ] FIPS %x 
1591,I,[ whal_xmit.c : 20443 ] FIPS %x 
1590,,[ whal_xmit.c : 20553 ] NAN disable CCA profiling 
1589,iiIII,[ whal_xmit.c : 4833 ] TPCDBG: selfGen: tpc=%d,%d cm=%x c=%08x:%08x 
1588,II,[ whal_xmit.c : 9912 ] whalSetupCbfRateParams: rate code %x, flags %x 
1587,I,[ whal_xmit.c : 20112 ] TXDMA WDG TXDMA_R1_DEBUG_STATES_0 reg_val: 0x%x
 
1586,III,[ whal_xmit.c : 5238 ] Old mcs %x New mcs %x New rate_mask %x 
1585,iIII,[ whal_xmit.c : 15769 ] TPCDBG: override: tpc=%d reason=%x c=%08x:%08x 
1584,II,[ whal_xmit.c : 16430 ] Info: TPC = %u, %u
 
1605,iIIII,[ data_rx.c : 658 ] DATA_TXRX_DBGID_DUP_CHECK vdev_id = %d tcp_info=0x%x SN=0x%x last_pn_valid=0x%x offset_winsize=0x%x 
1604,iIIII,[ data_rx.c : 749 ] DATA_TXRX_DBGID_DUP_CHECK vdev_id = %d SN=0x%x Len=0x%x WalRxCnt=0x%x DataRxCnt=0x%x 
1607,III,[ data_rx_pn.c : 151 ] DATA_TXRX_DBGID_REPLAY_CHECK_WAR KeyId=0x%x oldPN=0x%llx newPN=0x%llx 
1606,IIII,[ data_rx_pn.c : 194 ] DATA_TXRX_DBGID_REPLAY_CHECK 0x%x KeyId=0x%x oldPN=0x%x newPN=0x%x 
1614,ii,[ blockack.c : 413 ] ADDBA Req dropped WEP:%d MFP_SUPPORT:%d 
1613,ii,[ blockack.c : 204 ] wal_ba_event_peer_rx: amsdusupported=%d, buffersize=%d 
1612,ii,[ blockack.c : 1661 ] wal_ba_rx_sm: their_buf_size:%d, our_buf_size:%d 
1611,ii,[ blockack.c : 2046 ] wal_ba_send_addba_rsp: amsdusupported=%d, buffersize=%d 
1610,,[ blockack.c : 2524 ] BA-Link-Monitor implementation Start 
1609,I,[ blockack.c : 505 ] wal_ba_start_tear_down,tid:%x
 
1608,i,[ blockack.c : 1138 ] Error: ba_handle is NULL for wal_peer_id = %d 
1619,iii,[ wal_lp_bar.c : 191 ] LP_BAR_DBG: lp_complete_cnt=%d,tid_num = %d, session_id = %d 
1618,,[ wal_lp_bar.c : 45 ] LP_BAR_DBG: Local frame completion 
1617,,[ wal_lp_bar.c : 78 ] LP_BAR_DBG: Alloc failed 
1616,,[ wal_lp_bar.c : 90 ] LP_BAR_DBG: BA session not established 
1615,Iiiii,[ wal_lp_bar.c : 112 ] LP_BAR_DBG: Resp_ctxt info = %x, peer_id = %d,tid_num = %d, session_id = %d, repeat_cnt = %d 
1626,iiiIIi,[ htt_tgt_rx.c : 333 ] htt_tgt_fse_setup:[%d] [%d] [%d] [0x%lx] [0x%lx] RT: [%d]
 
1625,iiiii,[ htt_tgt_rx.c : 396 ] htt_tgt_fse_operation pdev,ipsec,src/dest ports,proto:[%d][%d] [%d][%d] [%d]
 
1624,IIIIIIII,[ htt_tgt_rx.c : 406 ] IP src [%x][%x][%x][%x] dest [%x][%x][%x][%x]
 
1623,II,[ htt_tgt_rx.c : 483 ] 3-tuple Configuration value rcvd : 
 flow_id_toeplitz_enable : [%x]
 toeplitz_2_or_4_field_enable : [%x]
 
1622,IIIIIII,[ htt_tgt_rx.c : 751 ] ring_selection_cfg [%x] [%x] [%x] [%x] [%x] [%x] [%x]
 
1621,iiiiii,[ htt_tgt_rx.c : 60 ] htt_tgt_sring_setup [%d] [%d] [%d] [%d] [%d] [%d]
 
1620,i,[ htt_tgt_rx.c : 640 ] htt_tgt_sring_setup_done -[%d]
 
1628,III,[ htt_tgt_rx_event.c : 334 ] RX event msg buf_len type[%x] peer_id [%x] vdev_id [%x]
 
1627,IIIIII,[ htt_tgt_rx_event.c : 706 ] htt_tgt_rx_event_backpressure -[%x], [%x], [%x], [%x], [%x], [%x]
 
1630,III,[ mac_core_main.c : 225 ] assert:r0=0x%x, r1=0x%x, line:0x%x
 
1629,I,[ mac_core_main.c : 147 ] mac_core_work_loop_init: invalid wlan_driver_mode 0x%x 
1642,iii,[ pktgen.c : 196 ] pktgen_calc_aggr_size: adjust pkt len: orig=%d adjust=%d mpdu=%d 
1641,iii,[ pktgen.c : 1651 ] pktgen_tx_msg_handler msg hdlr: pkt len = %d pdev_id = %d mode = %d
 
1640,I,[ pktgen.c : 1611 ] pktgen_data_tx_start_msg_send  dev->running=0x%x 
1639,,[ pktgen.c : 1810 ] pktgen_data_tx_stop_msg_send
 
1638,I,[ pktgen.c : 852 ] %s: Unable to get tcl entry 
 
1637,I,[ pktgen.c : 870 ] %s: Unable to get tcl entry 
 
1636,II,[ pktgen.c : 1146 ] %s: we're dead - %u is in use now
Bitmap  
1635,I,[ pktgen.c : 1155 ] 0x%X  
1634,I,[ pktgen.c : 750 ] Tx done MAC id %lu
 
1633,II,[ pktgen.c : 1284 ] %s: we're dead - try to free cookie %lu notused
Bitmap: 
1632,I,[ pktgen.c : 1293 ] 0x%x  
1631,,[ pktgen.c : 1296 ] 
 
1648,IIii,[ pktlog.c : 201 ] _pktlog_getbuf: pool_list_alloc failed with size %u type=%u qheap=%d missed=%d 
1647,i,[ pktlog.c : 357 ] Dropped buffer for pktlog_type:%d 
1646,I,[ pktlog.c : 774 ] FLUSHSTATS INFRA_4 HIF RINGSEND buffer:0x%x  
1645,I,[ pktlog.c : 710 ] _pktlog_disable: already disabled, bmap=0x%x 
1644,I,[ pktlog.c : 584 ] _pktlog_enable: already enabled, bmap=0x%x 
1643,II,[ pktlog.c : 589 ] _pktlog_enable: enable %u evlist %08x 
1654,iii,[ wal_channel_change_hw.c : 653 ] ADFS_DUMPS MAC-Received agile channel command for center_freq1:%d center_freq2:%d flags=%d 
 
1653,i,[ wal_channel_change_hw.c : 659 ] ADFS_DUMPS rc=%d
 
1652,IiIIII,[ wal_channel_change_hw.c : 410 ] WAL_DBGID_CHANNEL_CHANGE_FORCE_RESET: mhz = %04d mac_id = %d phy_mode = %02d flags = 0x%04x rx_stop|tx_stop = 0x%x pf_cnt = %02d 
1651,IiIII,[ wal_channel_change_hw.c : 419 ] WAL_DBGID_CHANNEL_CHANGE: mhz = %04d mac_id = %d phy_mode = %02d flags = 0x%04x pf_cnt = %02d 
1650,ii,[ wal_channel_change_hw.c : 507 ]  phyId %d Caling DPD SM for home channel %d
 
1649,iiii,[ wal_channel_change_hw.c : 573 ] GreenAP wal_set_greenap_channel error tx/rx chainmask: %d/%d, phy_mode: %d, flag: %d 
1677,ii,[ ar_wal_tx_de.c : 2847 ] security: sw_peer_id=%d WAL_DBGID_TX_EAPOL_PKT type=%d 
1676,iiiiI,[ ar_wal_tx_de.c : 2944 ] security: sw_peer_id=%d WAL_DBGID_TX_EAPOL_PKT M%d or G%d key_type:%d key_val:0x%02x 
1675,,[ ar_wal_tx_de.c : 1901 ] DE classify: invalid bcast mcast 
1674,ii,[ ar_wal_tx_de.c : 2032 ] DE enq: ARP req|actual_tid_num = %d %d 
1673,ii,[ ar_wal_tx_de.c : 2068 ] DE enq: DHCP|actual_tid_num = %d %d 
1672,i,[ ar_wal_tx_de.c : 2512 ] Drop frame: qos_to_nonqos_switch in progress, peer_id:%d 
1671,,[ ar_wal_tx_de.c : 2577 ] WAL_DBGID_TX_EAPOL_PKT peer is disassoced 
1670,,[ ar_wal_tx_de.c : 2584 ] WAL_DBGID_TX_EAPOL_PKT qpeer is not valid 
1669,iiIiIiI,[ ar_wal_tx_de.c : 1726 ] DE enq: sw_peer_id=%d tid=%d fc=0x%x type=%d msdu_flags=0x%x len=%d id=0x%x 
1668,ii,[ ar_wal_tx_de.c : 414 ] wal_tx_de_wbm_complete_handler vdev_id = %d, buffer_id = %d 
1667,ii,[ ar_wal_tx_de.c : 420 ] wal_tx_de_wbm_complete_handler WAL_BUFFERID_TX_DELETE_ALL_PEER_TCL_DUMMY_FRAME vdev_id = %d, peer_id = %d 
1666,i,[ ar_wal_tx_de.c : 431 ] wal_tx_de_wbm_complete_handler WAL_VDEV_DEL_ALL_PEER_TCL_DUMMY_FRAME_DONE vdev_id = %d 
1665,ii,[ ar_wal_tx_de.c : 436 ] wal_tx_de_wbm_complete_handler WAL_BUFFERID_TX_DELETE_ALL_PEER_TQM_DUMMY_FRAME vdev_id = %d, peer_id = %d 
1664,i,[ ar_wal_tx_de.c : 447 ] wal_tx_de_wbm_complete_handler WAL_VDEV_DEL_ALL_PEER_TQM_DUMMY_FRAME_DONE vdev_id = %d 
1663,i,[ ar_wal_tx_de.c : 462 ] wal_tx_de_wbm_complete_handler WAL_VDEV_DEL_ALL_PEER_TCL_DUMMY_FRAME_DONE & WAL_VDEV_DEL_ALL_PEER_TQM_DUMMY_FRAME_DONE vdev_id = %d 
1662,iii,[ ar_wal_tx_de.c : 465 ] wal_tx_de_wbm_complete_handler vdev_id = %d, thread_id = %d, msg_id = %d 
1661,iii,[ ar_wal_tx_de.c : 484 ] qos_to_nonqos_switch: Received tcl dummy frame compl peer_id:%d status:%d buffer_id:%d 
1660,,[ ar_wal_tx_de.c : 498 ] qos_to_nonqos_switch: Received tqm dummy frame compl in wbm2fw release ring 
1659,IiIiii,[ ar_wal_tx_de.c : 3116 ] DE wbm2fw: cookie=0x%x sw_peer_id=%d flags=0x%x msdu_len=%d rel_md=%d,rel_reason=%d 
1658,i,[ ar_wal_tx_de.c : 3788 ] wal_tx_de_delete_all_peer_handler vdev_id = %d 
1657,,[ ar_wal_tx_de.c : 3231 ] invalid_msdu - about to free to FW 
1656,,[ ar_wal_tx_de.c : 3236 ] invalid_msdu - about to free to host 
1655,IIII,[ ar_wal_tx_de.c : 3768 ] restore SN: tid=%x, mpdu_last_seq_num=%X, frameq=%p %x 
1752,,[ wal_phy_dev_hw.c : 10564 ] AWGN_INT_DBG : cca_int reduce BW 20Mhz
 
1751,,[ wal_phy_dev_hw.c : 10567 ] AWGN_INT_DBG : cca_int reduce BW 40Mhz
 
1750,,[ wal_phy_dev_hw.c : 10571 ] AWGN_INT_DBG : cca_in Primary
 
1749,,[ wal_phy_dev_hw.c : 10575 ] AWGN_INT_DBG : cca_int reduce BW 80Mhz
 
1748,,[ wal_phy_dev_hw.c : 10585 ] AWGN_INT_DBG : cca_int ack restore 
 
1747,i,[ wal_phy_dev_hw.c : 10591 ] AWGN_INT_DBG : cca_int bw restore cur_bw  = %d
 
1746,I,[ wal_phy_dev_hw.c : 10606 ] AWGN_INT_DBG : bw_drop cca_seg =0x%x
 
1745,i,[ wal_phy_dev_hw.c : 10614 ] AWGN_INT_DBG : bw_drop restore cur_bw  = %d
 
1744,,[ wal_phy_dev_hw.c : 10622 ] AWGN_INT_DBG : pkt_drop ack blk 
 
1743,,[ wal_phy_dev_hw.c : 10629 ] AWGN_INT_DBG : pkt_drop ack restore 
 
1742,Iiii,[ wal_phy_dev_hw.c : 10635 ] AWGN_INT_DBG : Sending WMI Event cca_seg =0x%x cca_int = %d  pkt_drop = %d bw_drop = %d
 
1741,iII,[ wal_phy_dev_hw.c : 6952 ] RXPCU WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1740,iIII,[ wal_phy_dev_hw.c : 6979 ] TXPCU WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x, PhyErr 0x%x 
1739,iII,[ wal_phy_dev_hw.c : 7004 ] TXDMA WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1738,iII,[ wal_phy_dev_hw.c : 7044 ] RXOLE WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1737,iII,[ wal_phy_dev_hw.c : 7061 ] TXOLE WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1736,iII,[ wal_phy_dev_hw.c : 7074 ] CRYPTO WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1735,iII,[ wal_phy_dev_hw.c : 7095 ] RXDMA WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1734,iII,[ wal_phy_dev_hw.c : 7112 ] PDG WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1733,iII,[ wal_phy_dev_hw.c : 7137 ] HWSCH WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1732,iII,[ wal_phy_dev_hw.c : 7217 ] MXI WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1731,iII,[ wal_phy_dev_hw.c : 7227 ] AMPI WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1730,I,[ wal_phy_dev_hw.c : 8938 ] WAL_DBGID_DEV_TX_TIMEOUT  0x%x 
1729,iIIIII,[ wal_phy_dev_hw.c : 8246 ]  %d [CCA:myRxFrame]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1728,iIIIII,[ wal_phy_dev_hw.c : 8251 ] %d [CCA:rxFrame]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1727,iIIIII,[ wal_phy_dev_hw.c : 8256 ] %d [CCA:rx_busy_cnt]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1726,iIIIII,[ wal_phy_dev_hw.c : 8261 ] %d [CCA:tx_frame_cnt]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1725,iII,[ wal_phy_dev_hw.c : 7328 ] CRYPTO panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1724,iII,[ wal_phy_dev_hw.c : 7659 ] PDG panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1723,iII,[ wal_phy_dev_hw.c : 7782 ] HWSCH panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1722,iII,[ wal_phy_dev_hw.c : 7799 ] MXI panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1721,iII,[ wal_phy_dev_hw.c : 7869 ] AMPI panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1720,iII,[ wal_phy_dev_hw.c : 7882 ] TXOLE panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1719,iII,[ wal_phy_dev_hw.c : 7961 ] RXOLE panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1718,iII,[ wal_phy_dev_hw.c : 7974 ] SFM panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1717,iII,[ wal_phy_dev_hw.c : 8007 ] RXDMA1 panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1716,iII,[ wal_phy_dev_hw.c : 8021 ] RXDMA_SRC_RNG panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1715,iII,[ wal_phy_dev_hw.c : 8034 ] RXDMA_DST_RNG panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1714,iII,[ wal_phy_dev_hw.c : 8049 ] RXDMA1_SRC_RNG panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1713,iII,[ wal_phy_dev_hw.c : 8061 ] RXDMA1_DST_RNG panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1712,iII,[ wal_phy_dev_hw.c : 8073 ] MCMN panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1711,iII,[ wal_phy_dev_hw.c : 7381 ] TXPCU0 panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1710,iII,[ wal_phy_dev_hw.c : 7522 ] TXDMA panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1709,iII,[ wal_phy_dev_hw.c : 7623 ] RXDMA panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1708,iII,[ wal_phy_dev_hw.c : 7635 ] RXPCU0 panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1707,iII,[ wal_phy_dev_hw.c : 7647 ] RXPCU1 panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
1706,,[ wal_phy_dev_hw.c : 2053 ] Don't reset as CHIP IS IN POWER DOWN STATE 
1705,II,[ wal_phy_dev_hw.c : 2541 ] ctrl_path_stats_dbg: mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x
 
1704,I,[ wal_phy_dev_hw.c : 6797 ] PHY M3 requested WARM reset for PHY: %x 
 
1703,III,[ wal_phy_dev_hw.c : 6810 ] M3SSR asserted on pdev:%x  MAC_ID:%x  ts:%x  
 
1702,I,[ wal_phy_dev_hw.c : 6817 ] PHY M3 Assert for PHY: %x 
 
1701,Iii,[ wal_phy_dev_hw.c : 10497 ] AWGN_INT_DBG  get = 0x%x period = %d inited = %d  
1700,IIIII,[ wal_phy_dev_hw.c : 10237 ] AWGN_INT_DBG register read ed = 0x%x gi = 0x%x sec_mask = 0x%x seg =0x%x intr = 0x%x
 
1699,IiiiiIii,[ wal_phy_dev_hw.c : 10257 ] AWGN_INT_DBG  compute_cca current_time = %ld cca1 = %d cca2 = %d ed_mu = %d  gi_mu = %d cc_cnt = %ld tx_frm = %d rx_frm = %d
 
1698,iiiiii,[ wal_phy_dev_hw.c : 10269 ] AWGN_INT_DBG tx_frame_1 = %d tx_frame = %d rx_frame_1 = %d rx_frame = %d cc_1 = %d cc = %d
 
1697,iii,[ wal_phy_dev_hw.c : 10274 ] AWGN_INT_DBG tx_prop = %d rx_prop = %d cc_diff = %d
 
1696,iii,[ wal_phy_dev_hw.c : 10308 ] AWGN_INT_DBG p_cca1 = %d p_cca2 = %d time_diff = %d
 
1695,IIiiiiii,[ wal_phy_dev_hw.c : 10331 ] AWGN_INT_DBG cur_time = 0x%x current_time = %ld cca1 = %d cca2 = %d ed_mu = %d gi_mu = %d awgn_cca_edmu_ind = %d interference_count = %d
 
1694,iiiiii,[ wal_phy_dev_hw.c : 10372 ] AWGN_INT_DBG tx_frame_1 = %d tx_frame = %d rx_frame_1 = %d rx_frame = %d cc_1 = %d cc = %d
 
1693,iii,[ wal_phy_dev_hw.c : 10377 ] AWGN_INT_DBG tx_prop = %d fudge_fact = %d cc_diff = %d
 
1692,III,[ wal_phy_dev_hw.c : 10393 ] AWGN_INT_DBG compute_seg ed_mu = 0x%x gi_mu = 0x%x int_detected = 0x%x
 
1691,II,[ wal_phy_dev_hw.c : 10414 ] AWGN_INT_DBG  Interrrupt Not detected gi_mask = 0x%x sec_mask = 0x%x
 
1690,I,[ wal_phy_dev_hw.c : 10432 ] AWGN_INT_DBG  Interrupt  detected at Segment = 0x%x
 
1689,I,[ wal_phy_dev_hw.c : 10446 ] AWGN_INT_DBG  Interrupt  detected at Segment = 0x%x
 
1688,II,[ wal_phy_dev_hw.c : 10470 ] AWGN_INT_DBG  Pri gi_mask = 0x%x mask = 0x%x
 
1687,II,[ wal_phy_dev_hw.c : 10485 ] AWGN_INT_DBG Sec gi_mask = 0x%x mask = 0x%x
 
1686,ii,[ wal_phy_dev_hw.c : 1930 ] WAL_PDEV_RESUME_REQ req = %d, is_pdev_pause = %d 
1685,iiiii,[ wal_phy_dev_hw.c : 1843 ] WAL_PDEV_SUSPEND_REQ req = %d, reason %d, is_pdev_pause = %d, force_sync = %d, resume_inline = %d 
1684,iIIIII,[ wal_phy_dev_hw.c : 8443 ]  %d [TX_RX_STATS:hw_queued]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1683,iIIIII,[ wal_phy_dev_hw.c : 8452 ]  %d [TX_RX_STATS:hw_reaped]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1682,iIIIII,[ wal_phy_dev_hw.c : 8462 ]  %d [TX_RX_STATS:hw_flush]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1681,iIIIII,[ wal_phy_dev_hw.c : 8472 ]  %d [TX_RX_STATS:hw_filt]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1680,iIIIII,[ wal_phy_dev_hw.c : 8482 ]  %d [TX_RX_STATS:ppdu_recvd]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1679,iIIIII,[ wal_phy_dev_hw.c : 8492 ]  %d [TX_RX_STATS:mpdu_cnt_fcs_ok]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1678,iIIIII,[ wal_phy_dev_hw.c : 8502 ]  %d [TX_RX_STATS:ppdu_recvd]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
1773,II,[ wal_soc_dev_hw.c : 525 ] TCL0 panic interrupt mask : 0x%x, total count 0x%x
 
1772,II,[ wal_soc_dev_hw.c : 536 ] TCL1 panic interrupt mask : 0x%x, total count 0x%x
 
1771,II,[ wal_soc_dev_hw.c : 627 ] TQM0 panic interrupt mask : 0x%x, total count 0x%x
 
1770,II,[ wal_soc_dev_hw.c : 660 ] TQM1 panic interrupt mask : 0x%x, total count 0x%x
 
1769,II,[ wal_soc_dev_hw.c : 723 ] TQM2 panic interrupt mask : 0x%x, total count 0x%x
 
1768,II,[ wal_soc_dev_hw.c : 850 ] APB panic interrupt mask : 0x%x, total count 0x%x
 
1767,II,[ wal_soc_dev_hw.c : 1016 ] GXI panic interrupt mask : 0x%x, total count 0x%x
 
1766,II,[ wal_soc_dev_hw.c : 859 ] MEM panic interrupt mask : 0x%x, total count 0x%x
 
1765,II,[ wal_soc_dev_hw.c : 868 ] WBM0 panic interrupt mask : 0x%x, total count 0x%x
 
1764,II,[ wal_soc_dev_hw.c : 928 ] WBM1 panic interrupt mask : 0x%x, total count 0x%x
 
1763,II,[ wal_soc_dev_hw.c : 944 ] WBM2 panic interrupt mask : 0x%x, total count 0x%x
 
1762,II,[ wal_soc_dev_hw.c : 957 ] RE0 panic interrupt mask : 0x%x, total count 0x%x
 
1761,II,[ wal_soc_dev_hw.c : 966 ] REO1 panic interrupt mask : 0x%x, total count 0x%x
 
1760,II,[ wal_soc_dev_hw.c : 975 ] REO2 panic interrupt mask : 0x%x, total count 0x%x
 
1759,II,[ wal_soc_dev_hw.c : 984 ] REO3 panic interrupt mask : 0x%x, total count 0x%x
 
1758,I,[ wal_soc_dev_hw.c : 991 ] SM_IX_2 value:%x 
1757,II,[ wal_soc_dev_hw.c : 1007 ] REO4 panic interrupt mask : 0x%x, total count 0x%x
 
1756,I,[ wal_soc_dev_hw.c : 1748 ] PN dummy MSDU(%x) returned 
1755,i,[ wal_soc_dev_hw.c : 1305 ] Enter/Exit  WoW mode :%d 
1754,,[ wal_soc_dev_hw.c : 1348 ] Entering into WoW mode is done 
1753,,[ wal_soc_dev_hw.c : 1367 ] Exiting from WoW mode is done 
1774,iIiiii,[ ar_wal_vdev_hw.c : 404 ] VDEV migration sync: ba_migrate, thread_id=%d, peer=%p, vdev_id=%d, vdev_type=%d, pdev_id=%d:%d 
1783,iiii,[ wal_soc_debug.c : 233 ] wal_unit_test: num_args = %d test_cmd = %d arg[1] = %d arg[2] = %d  
1782,,[ wal_soc_debug.c : 713 ] Recorded page fault count reset to 0 
1781,i,[ wal_soc_debug.c : 715 ] Total page fault count: %d 
1780,i,[ wal_soc_debug.c : 719 ] Recorded page fault count: %d 
1779,i,[ wal_soc_debug.c : 721 ] Total page fault count: %d 
1778,IIIII,[ wal_soc_debug.c : 859 ] pcss_ring_feeder num_interrupts:%u, num_pcss_elem_zero:%u, num_in_elem_zero:%u, num_out_elem_zero:%u, num_elem_moved:%u
 
1777,iiii,[ wal_soc_debug.c : 991 ] wal_unit_test: num_args = %d test_cmd = %d arg[1] = %d arg[2] = %d  
1776,I,[ wal_soc_debug.c : 582 ] page fault in wow: 0x%x 
1775,i,[ wal_soc_debug.c : 712 ] Recorded page fault count: %d 
1784,Ii,[ direct_dma_config.c : 212 ] dma_prepare %p status %d 
1790,IIIIIIII,[ host_ring_reader.c : 348 ] host ring reader %p has base address 0x%08x%08x, %u elements, tail address 0x%08x%08x, head address 0x%08x%08x 
1789,IIIIII,[ host_ring_reader.c : 162 ] host_ring_reader_read_elems: reader %p head_idx %u tail_idx %u shadow_tail_idx %u num_avail %u num_free %u 
1788,III,[ host_ring_reader.c : 183 ] tail dirty host ring reader %p head index is %u, shadow tail index is %u 
1787,II,[ host_ring_reader.c : 81 ] host_ring_reader_read_elems_compl: host ring reader %p read %u elements 
1786,I,[ host_ring_reader.c : 298 ] host ring reader %p stop request 
1785,IIIi,[ host_ring_reader.c : 39 ] host ring reader %p failed to copy from address 0x%08x%08x with status %d 
1795,iiI,[ pcss_ring_feeder.c : 241 ] PHY %d ring %d has %u elements remaining 
1794,III,[ pcss_ring_feeder.c : 267 ] pcss_ring_feeder_handle_ipc : head = %u shadow_head = %u and num_elems = %u for out_ring 
1793,I,[ pcss_ring_feeder.c : 278 ] pcss_ring_feeder_handle_ipc : num elems_dmaed = %u for out_ring 
1792,iiII,[ pcss_ring_feeder.c : 382 ] PHY %d ring %d needs %u elements; have %u 
1791,iiIIIIII,[ pcss_ring_feeder.c : 499 ] pcss_ring_status_print: PHY %d ring %d event %c%u head_idx %u tail_idx %u num_avail %u num_free %u 
1824,IIiIi,[ ar_wal_local_frames.c : 2389 ] LOCAL abf completion internal,peer=%x,abf=%x,flags=%d,abf_thread=%x,cur_thread=%d 
1823,IIiIi,[ ar_wal_local_frames.c : 2396 ] LOCAL abf completion internal,peer=%x,abf=%x,flags=%d,abf_thread=%x,cur_thread=%d 
1822,IIiIiI,[ ar_wal_local_frames.c : 2301 ] LOCAL abf completion msg:peer_id=%x,abf=%x,flag=%d,abf_thread=%x,cur_thread=%d,target_thread=%x 
1821,IIIiII,[ ar_wal_local_frames.c : 2258 ] Deliver LOCAL buffer sending msg failure: tid=%x,peer=%x,abf=%x,flag=%d,target_thread=%x, is_data:%x 
1820,ii,[ ar_wal_local_frames.c : 1237 ] Local data send: use default tid, requested TID:%d, tid_alloc_status=%d 
1819,II,[ ar_wal_local_frames.c : 1439 ] Local EAPOL M4 duplicated, peer:%x, qpeer-flag=%x 
1818,iiI,[ ar_wal_local_frames.c : 1494 ] Local data send: use tqm-tid %d, num:%d, flags:0x%x 
1817,iiIII,[ ar_wal_local_frames.c : 1558 ] local_data_frame_send  vdev_id=%d mac_id=%d seq_num=0x%x type=0x%x status =0x%x 
1816,I,[ ar_wal_local_frames.c : 188 ] MGMT_TX_WMI_FROM_HOST TX COMP: flags = 0x%x 
1815,IIIiii,[ ar_wal_local_frames.c : 384 ] local_frame_handle_completion: SN=0x%x/0x%x, type=0x%x, thread=%d/%d, status=%d 
1814,iii,[ ar_wal_local_frames.c : 388 ] local_frame_handle_completion: thread=%d/%d, status=%d 
1813,iiIIIIi,[ ar_wal_local_frames.c : 328 ] WAL_DBGID_TX_MGMT_COMP_DESCID_STATUS vdev_id=%d mac_id=%d dec_id=0x%x tx_status=0x%x tid=0x%x buffer_id=0x%x reset_cnt=%d 
1812,iI,[ ar_wal_local_frames.c : 332 ] WAL_DBGID_TX_MGMT_COMP_DESCID_STATUS vdev_id=%d  tx_status=0x%x 
1811,IIIIiiIiI,[ ar_wal_local_frames.c : 477 ] local_frame_handle_completion_tqm, DA:%X-%X,type=0x%X,DATA:0x%X,thread=%d/%d,cookie=%X,status=%d,flags=0x%x 
1810,ii,[ ar_wal_local_frames.c : 925 ] WAL_DBGID_TX_MGMT_ENQUEUE_FAILED vdev_id = %d tid:%d 
1809,iiIIIII,[ ar_wal_local_frames.c : 1100 ] WAL_DBGID_TX_MGMT_DESCID_SEQ_TYPE_LEN vdev_id=%d mac_id=%d cookie=0x%x seq_num=0x%x type=0x%x len=0x%x tid_flg=0x%x 
1808,iiIIIII,[ ar_wal_local_frames.c : 1111 ] DBG WAL_DBGID_TX_MGMT_DESCID_SEQ_TYPE_LEN vdev_id=%d mac_id=%d cookie=0x%x seq_num=0x%x type=0x%x len=0x%x tid_flg=0x%x 
1807,IIi,[ ar_wal_local_frames.c : 1128 ] ctrl_path_stats_dbg: mac_address equal mac_0 = 0x%x mac_2 =0x%x subtype = %d
 
1806,i,[ ar_wal_local_frames.c : 2186 ] send local buffer fail: sw_peer_id=%d migration in progress  
1805,II,[ ar_wal_local_frames.c : 2216 ] send local buffer fail: status=%x, flags=%x 
1804,IIII,[ ar_wal_local_frames.c : 2150 ] local_data, peer(%p, sw_peer_id:%x) pdev mismatch(%p:%p) 
1803,IIII,[ ar_wal_local_frames.c : 2095 ] local_mgmt, peer(%p, sw_peer_id:%x) pdev mismatch(%p:%p) 
1802,ii,[ ar_wal_local_frames.c : 1726 ] WAL_DBGID_TX_MGMT_ENQUEUE_FAILED vdev_id = %d tid:%d 
1801,IIII,[ ar_wal_local_frames.c : 1763 ] host_mgmt, peer(%p, sw_peer_id:%x) pdev mismatch(%p:%p) 
1800,Ii,[ ar_wal_local_frames.c : 1780 ] MGMT_TX_WMI_FROM_HOST flags = %x, is_wmi = %d 
1799,iiIIII,[ ar_wal_local_frames.c : 1894 ] WAL_DBGID_TX_MGMT_DESCID_SEQ_TYPE_LEN vdev_id=%d mac_id=%d cookie=0x%x seq_num=0x%x type=0x%x len=0x%x 
1798,iiIIII,[ ar_wal_local_frames.c : 1903 ] DBG WAL_DBGID_TX_MGMT_DESCID_SEQ_TYPE_LEN vdev_id=%d mac_id=%d cookie=0x%x seq_num=0x%x type=0x%x len=0x%x 
1797,IIi,[ ar_wal_local_frames.c : 1919 ] ctrl_path_stats_dbg: mac_address equal mac_0 = 0x%x mac_2 =0x%x subtype = %d
 
1796,iIiiI,[ ar_wal_local_frames.c : 1954 ] WAL_DBGID_MGMT_TX_FAIL vdev_id=%d, err_code=%x, cookie=%d, status=%d, fc[0]=%x 
1839,i,[ ar_wal_monitor.c : 1320 ] dev-%d:POLICY_ENFORCE_STATE --> MONITOR_TIMER_RUNNING_STATE 
1838,i,[ ar_wal_monitor.c : 381 ] dev-%d:TIMER_RUNNING_STATE  --> MONITOR_STATS_COLLECTION_STATE 
1837,i,[ ar_wal_monitor.c : 408 ] dev-%d:WAIT_POLICY_ENFORCE_STATE -->                 MONITOR_POLICY_ENFORCE_STATE 
1836,i,[ ar_wal_monitor.c : 840 ] dev-%d:STATS_COLLECTION_STATE -->                 MONITOR_WAIT_POLICY_ENFORCE_STATE 
1835,ii,[ ar_wal_monitor.c : 852 ] dev-%d:STATS_COLLECTION_STATE -->                 MONITOR_STATS_COLLECTION_STATE last_peer_idx:%d 
1834,i,[ ar_wal_monitor.c : 356 ] dev-%d:INIT_STATE  --> MONITOR_TIMER_RUNNING_STATE 
1833,IIiI,[ ar_wal_monitor.c : 360 ] %s %s send signal=%d to thread=%s to start timer 
 
1832,IIiI,[ ar_wal_monitor.c : 94 ] %s %s send signal=%d to thread=%s to yield 
 
1831,iiii,[ ar_wal_monitor.c : 1047 ] CONGCTRL HOST_CONTROL UPDATE aid:%d tid_num:%d threshold_1:%d threshold_2:%d
 
1830,iii,[ ar_wal_monitor.c : 1073 ] CONGCTRL HOST_CONTROL UPDATE aid:%d tid_num:%d new drop_threshold:%d  
1829,iii,[ ar_wal_monitor.c : 1114 ] CONGCTRL FW_CONTROL UPDATE aid:%d tid_num:%d new drop_threshold:%d  
1828,iiI,[ ar_wal_monitor.c : 1175 ] CONGCTRL peer_id:%d tid_num:%d msduq_mask:0x%08x 
1827,iiiiiii,[ ar_wal_monitor.c : 967 ] CONGCTRL HOST_CONTROL peer_id:%d tid_num:%d traffic_enq:%d drop:%d deq:%d old_threshold:%d new_threshold:%d 
1826,iii,[ ar_wal_monitor.c : 714 ] qstats_update peer_id:%d tid_num:%d qtype:%d 
1825,IIIIIi,[ ar_wal_monitor.c : 275 ] _wal_txrx_monitor_pdev_record: type %x rx msdu %x ppdu %x, tx msdu %x ppdu %x phy_mode %d
 
1860,,[ ar_wal_ast.c : 419 ] WAL_DBGID_AST_ENTRY_FULL WAL_ENOSPC 
1859,,[ ar_wal_ast.c : 1517 ] WAL_DBGID_AST_ENTRY_EXIST WAL_EEXIST 
1858,IIII,[ ar_wal_ast.c : 1526 ] WAL_AST_ALLOC_PEER peer_mac:0x%x ast_index:0x%x sw_peer_id:0x%x ast_flags:0x%x 
1857,i,[ ar_wal_ast.c : 1476 ] ar_wal_ast_dummy_alloc_peer ast_index = %d 
1856,III,[ ar_wal_ast.c : 491 ] WAL_DBGID_AST_DEL_WDS_ENTRY  0x%x 0x%x 0x%x 
1855,IIII,[ ar_wal_ast.c : 1659 ] WAL_DBGID_AST_ADD_MONITOR_DIRECT_ENTRY  0x%x 0x%x 0x%x 0x%x 
1854,IIII,[ ar_wal_ast.c : 1678 ] WAL_DBGID_AST_ADD_MONITOR_DIRECT_ENTRY  0x%x 0x%x 0x%x 0x%x 
1853,IIIIi,[ ar_wal_ast.c : 1683 ] WAL_DBGID_AST_ADD_MONITOR_DIRECT_ENTRY  0x%x 0x%x 0x%x 0x%x pdev_id:%d 
1852,IIIII,[ ar_wal_ast.c : 1118 ] WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x 
1851,IIIII,[ ar_wal_ast.c : 1152 ] WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x 
1850,IIIIIi,[ ar_wal_ast.c : 1161 ] WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x pdev_id:%d 
1849,II,[ ar_wal_ast.c : 1827 ] WAL_DBGID_AST_DEL_ALL_MONITOR_DIRECT_ENTRY  0x%x 0x%x 
1848,II,[ ar_wal_ast.c : 1295 ] WAL_DBGID_AST_FREE_WDS_ENTRY des_mac is not next_hop or monitor direct 0x%x 0x%x 
1847,IIII,[ ar_wal_ast.c : 1730 ] WAL_DBGID_AST_DEL_MONITOR_DIRECT_ENTRY  0x%x 0x%x 0x%x 0x%x 
1846,IIII,[ ar_wal_ast.c : 1771 ] WAL_DBGID_AST_DEL_MONITOR_DIRECT_ENTRY  0x%x 0x%x 0x%x 0x%x 
1845,I,[ ar_wal_ast.c : 2196 ] SW peer key not found, peer_mac-0x%x 
1844,IiIIIII,[ ar_wal_ast.c : 2209 ] Update reorder queue peer_mac-0x%x, sw_peer_id-%d, queue_addr-0x%x:0x%x, queue-%x, ba_win-0x%x:0x%x 
1843,IIi,[ ar_wal_ast.c : 1210 ] WAL_DBGID_AST_UPDATE_WDS_ENTRY FAILED due to peer mac search failed 0x%x 0x%x pdev_id:%d 
1842,IIi,[ ar_wal_ast.c : 1218 ] WAL_DBGID_AST_UPDATE_WDS_ENTRY FAILED due to dest mac search failed 0x%x 0x%x pdev_id:%d 
1841,IIII,[ ar_wal_ast.c : 1239 ] WAL_DBGID_AST_UPDATE_WDS_ENTRY 0x%x 0x%x 0x%x 0x%x 
1840,IIII,[ ar_wal_ast.c : 1246 ] WAL_DBGID_AST_UPDATE_WDS_ENTRY des_mac is not next_hop 0x%x 0x%x 0x%x 0x%x 
1947,ii,[ ar_wal_peer.c : 9666 ] _wal_peer_alloc_tid: got tid flush handle for tidno %d sw_peer_id:%d
 
1946,IiiiI,[ ar_wal_peer.c : 9748 ] ul_dbg_tid_alloc: peer=0x%x, tidno=%d, ac=%d, timeout_ms=%d, tid_ptr=0x%x 
1945,i,[ ar_wal_peer.c : 9798 ] _wal_peer_alloc_tid: adding tid %d to temp tid list
 
1944,iIIIIII,[ ar_wal_peer.c : 1001 ] PEER_DELETE_DBG: pdev_id: %d ar_wal_peer_clean_up_flow:%x,%x,%x,%x,%x, invalidate:%x 
 
1943,iIIIII,[ ar_wal_peer.c : 1022 ] pdev_id: %d ar_wal_peer_clean_up_flow:%x,%x,%x,%x,%x, 
1942,III,[ ar_wal_peer.c : 1035 ] ar_wal_peer_clean_up_flow:%x,%x,%x 
1941,IIIiII,[ ar_wal_peer.c : 3166 ] FREE_AST_ENTRY: peer=%p mac_addr=0x%x %x invalidate=%d ast_index=0x%x valid_bmap[ast_index]=0x%x 
1940,ii,[ ar_wal_peer.c : 9907 ] _ar_wal_peer_free_tid:                sw_peer_id=%d, tidno=%d 
1939,ii,[ ar_wal_peer.c : 9921 ] _ar_wal_peer_free_tid: sending tid flush cmd to tac thread_id=%d, tidno=%d
 
1938,iiIiII,[ ar_wal_peer.c : 13213 ] mpdu_reconstruct_block_cb:pdev(%d)peer %d,flags=0x%x,del=%d,block=0x%x,recon=0x%x 
1937,IIIIII,[ ar_wal_peer.c : 4839 ] pdev(%x)peer %x blocked for tidLen update,refcnt=%x,htc=%x,remap=%x,security=%x 
1936,iIiI,[ ar_wal_peer.c : 5010 ] security: ar_wal_peer_set_key_block_cb: peer_id:%d  peer_flags:%02x authrized:%d qpeer_flags:%x 
1935,iIi,[ ar_wal_peer.c : 5053 ] security: ar_wal_peer_set_mcast_key_block_cb: peer_id:%d  peer_flags:%02x authrized:%d 
1934,,[ ar_wal_peer.c : 8913 ] qdepth_thresh_update_cmd_handler:                     Invalid sw_peer_key 
1933,,[ ar_wal_peer.c : 8920 ] qdepth_thresh_update_cmd_handler:                     Invalid peer 
1932,,[ ar_wal_peer.c : 8930 ] qdepth_thresh_update_cmd_handler:                    is_self_peer or bss_peer 
1931,,[ ar_wal_peer.c : 8941 ] qdepth_thresh_update_cmd_handler:                    peer delete in progress 
1930,i,[ ar_wal_peer.c : 8962 ] qdepth_thresh_update_cmd_handler:                    not valid TID give tidno:%d 
1929,i,[ ar_wal_peer.c : 8974 ] qdepth_thresh_update_cmd_handler:                   not valid tqm tid tidno:%d 
1928,ii,[ ar_wal_peer.c : 8991 ] qdepth_thresh_update_cmd_handler:                        qtype:%d host_drop_th:%d  
1927,ii,[ ar_wal_peer.c : 9950 ] _ar_wal_peer_tidq_empty: thread_id =%d,tidq->tid_num=%d
 
1926,IIIIIII,[ ar_wal_peer.c : 4749 ] update MPDUq hdrlen, peer=%x,tid_num=%x,tid_flg=%x %x,orig=%x,new=%x,wow=%x 
1925,,[ ar_wal_peer.c : 11775 ] wal_htt_peer_stats_reset: Peer pointer is NULL  
1924,IIi,[ ar_wal_peer.c : 2364 ] WAL_ALLOC_PEER_AST_FAIL peer_addr 0x04%x08%x type %d  
1923,i,[ ar_wal_peer.c : 2659 ] PEER_ALLOC: peer_id=%d: Fail to allocate wmm_param 
1922,II,[ ar_wal_peer.c : 2867 ] ADDR_TYPE_A: mac_adr_31_0=0x%x, mac_addr_32_47=0x%x 
1921,II,[ ar_wal_peer.c : 2870 ] ADDR_TYPE_B peer: mac_adr_31_0=0x%x, mac_addr_32_47=0x%x 
1920,II,[ ar_wal_peer.c : 2873 ] ADDR_TYPE_C self: mac_adr_31_0=0x%x, mac_addr_32_47=0x%x 
1919,III,[ ar_wal_peer.c : 12201 ] OMI: Change a_ctrl from 0x%lx to 0x%lx, ULMU Disable is 0x%lx
 
1918,ii,[ ar_wal_peer.c : 3709 ] wal_peer_delete_conf_msg_hdlr: peer=%d,num_del_in_pro=%d 
1917,ii,[ ar_wal_peer.c : 3732 ] wal_peer_delete_conf_msg_hdlr: peer = %d, pdev_peer_deletes_in_progress = %d
 
1916,iiI,[ ar_wal_peer.c : 3632 ] _wal_peer_del_msg_hdlr:  thread_id =%d, sw_peer_id=%d, peer->peer_flgs=0x%x
 
1915,iii,[ ar_wal_peer.c : 3919 ] wal_peer_delete_resume: peer = %d, delete_in_progress %d pdev_peer_deletes_in_progress = %d
 
1914,iII,[ ar_wal_peer.c : 13060 ] security: WAL_DBGID_SECURITY_PM4_SENT peer_id:%d, peer_flag:0x%x, qpeer_flag:0x%x 
1913,i,[ ar_wal_peer.c : 10643 ] wal_peer_mcast_cfg AST entry not found for key_id:%d 
1912,Iii,[ ar_wal_peer.c : 10647 ] wal_peer_fill_mcast_key_info: peer :%0x key_id:%d key_id_type:%d 
1911,ii,[ ar_wal_peer.c : 3841 ] _wal_peer_free: peer = %d delete_in_progress %d 
1910,iii,[ ar_wal_peer.c : 10722 ] wal_pm_mcast_cfg: enable :%d encr_en:%d decap_type:%d 
1909,Ii,[ ar_wal_peer.c : 10608 ] _wal_peer_mcast_key_id_update: peer :%0x key_id:%d 
1908,IIII,[ ar_wal_peer.c : 12807 ] peer_migrate failed: rx:%x, tx:%x MAC:%x, reset_cause %x 
1907,iiIiI,[ ar_wal_peer.c : 13256 ] mpdu_reconstruct:pdev(%d)peer %d,flags=0x%x,del=%d,recon=0x%x 
1906,,[ ar_wal_peer.c : 13300 ] reconstruct_tqm_mpdus: no TIDs to block 
1905,iIII,[ ar_wal_peer.c : 13139 ] Index= %d,  time_stamp_32_61 = 0x%x, time_stamp_0_31= 0x%x, flags = 0x%x  
1904,II,[ ar_wal_peer.c : 13144 ] A_TIMER_CURRENT_TIME_IN_TICKS time_stamp_32_61 = 0x%x time_stamp_0_31 = 0x%x  
1903,iIiiiI,[ ar_wal_peer.c : 4083 ] security: wal_peer_set_key: peer:%d, key_info:%p, key_id:%d is_mcast:%d key_type:%d key_flags:%02x  
1902,i,[ ar_wal_peer.c : 4106 ] _wal_peer_set_key: key_id:%d ignored, PMF 
1901,i,[ ar_wal_peer.c : 4306 ] _wal_peer_set_key: is_already_set_key_pending:%d 
1900,II,[ ar_wal_peer.c : 4421 ] WAL_DBGID_SECURITY_UCAST_KEY_SET  0x%x MAC:%x 
1899,I,[ ar_wal_peer.c : 4430 ] WAL_DBGID_SECURITY_MCAST_KEY_SET  0x%x 
1898,iI,[ ar_wal_peer.c : 4597 ] security: postponing set key for peer_id:%d peer_flags:%02x 
1897,iI,[ ar_wal_peer.c : 4627 ] security: wal_peer_set_key: peer:%d  peer_flags:%02x 
1896,i,[ ar_wal_peer.c : 5516 ] WAL_DBGID_SECURITY_SAFE_MODE on: %d  
1895,iIIII,[ ar_wal_peer.c : 5947 ] security: WAL_DBGID_SECURITY_ENCR_EN, peer %d, refcnt=%x,htc=%x,remap=%x,security=%x 
1894,I,[ ar_wal_peer.c : 6331 ] OMI: Set new nss = 0x%lx
 
1893,I,[ ar_wal_peer.c : 6338 ] OMI: Set new bw = 0x%lx
 
1892,I,[ ar_wal_peer.c : 6344 ] OMI: Set new a_ctrl = 0x%lx
 
1891,I,[ ar_wal_peer.c : 6356 ] HTC-block tids, peer:%x 
1890,I,[ ar_wal_peer.c : 6438 ] WAL_DBGID_SET_M4_SENT_MANUALLY PEER = 0X%X 
1889,I,[ ar_wal_peer.c : 6443 ] WAL_DBGID_UNSET_M4_SENT_MANUALLY  peer = 0x%x 
1888,I,[ ar_wal_peer.c : 6522 ] WAL_PEER_PARAM_FW_CONGESTION_DISABLE:%x 
1887,iii,[ ar_wal_peer.c : 5572 ] qos: flag: %d and peer_id is %d and qos_flag_rcvd:%d 
1886,,[ ar_wal_peer.c : 5596 ] qos_to_nonqos_switch: Sent dummy frame request to TX_DE 
1885,Ii,[ ar_wal_peer.c : 5603 ] nonqos to qos switch received during peer assoc for peer = %p, peer->qos_enabled = %d 
1884,iI,[ ar_wal_peer.c : 5668 ] security: set_param_authorized: peer:%d  peer_flags:%02x 
1883,iii,[ ar_wal_peer.c : 5720 ] DYN_MIMO_PS : sw_peer_id %d, dyn_mimo_ps %d, force_dyn_mimo_ps %d 
 
1882,Iii,[ ar_wal_peer.c : 5801 ] security: WAL_PEER_PARAM_TX_KEYID peer_key:%p and peer:%d val:%d 
 
1881,iiIii,[ ar_wal_peer.c : 12926 ] PDEV:%d, peer id=%d, QCU:%x/%d, ena=%d 
1880,,[ ar_wal_peer.c : 11213 ] _wal_peer_state_publish: Entry  
1879,ii,[ ar_wal_peer.c : 11218 ] _wal_peer_state_publish: bytes is %d, less than output size = %d  
1878,iiii,[ ar_wal_peer.c : 11247 ] _wal_peer_state_publish: peer_keyid0_ast_index is %d, vdev_id = %d, qos_enabled = %d, ba_tx_state_bmap = %d 
1877,iiiiii,[ ar_wal_peer.c : 11256 ] _wal_peer_state_publish: mac_address is %d:%d:%d:%d:%d:%d  
1876,,[ ar_wal_peer.c : 11262 ] _wal_peer_state_publish: Exit  
1875,,[ ar_wal_peer.c : 11992 ] Memory ERROR: Cannot retrieve peer stats
 
1874,,[ ar_wal_peer.c : 11996 ] Invalid stats. Please try again
 
1873,iIi,[ ar_wal_peer.c : 5072 ] security: wal_peer_tid_flush_handler: peer_id:%d  peer_flags:%02x authrized:%d 
1872,ii,[ ar_wal_peer.c : 9392 ] wal_peer_tid_free_mem: sw_peer_id=%d, tidno = %d 
1871,i,[ ar_wal_peer.c : 9423 ] qos_to_nonqos_switch: it is last data TID got deleted peer_id:%d 
1870,i,[ ar_wal_peer.c : 9451 ] delete_all_peer wal_peer_tid_free_mem: WLAN_THREAD_COMM_FUNC_VDEV_DEL_ALL_PEER peer_id:%d 
1869,II,[ ar_wal_peer.c : 12688 ] TRIGGER PDEV MISMATCH, thread:%x, tid:%x 
1868,i,[ ar_wal_peer.c : 3536 ] qos_to_nonqos_switch: wal_qos_to_nonqos_conf_msg_hdlr switching is done peer_id:%d 
1867,ii,[ ar_wal_peer.c : 3494 ] qos_to_nonqos_switch: wal_qos_to_nonqos_switch_msg_hdlr peer_id:%d thread_id:%d 
1866,IIIIIII,[ ar_wal_peer.c : 4693 ] security:pdev(%x)peer %x,flag %x, unblocked for tidLen update,refcnt=%x,htc=%x,remap=%x,security=%x 
1865,iII,[ ar_wal_peer.c : 5175 ] security: wal_tqm_setkey_update_sync_cb_func: sw_peer_id:%d peer_flags:0x%x, qpeer_flags=0x%x 
1864,II,[ ar_wal_peer.c : 5201 ] security: wal_tqm_setkey_update_unblock_cb_func: peer:%p  peer_flags:%02x 
1863,ii,[ ar_wal_peer.c : 546 ] HW overwritten tx_flow_number:%d and corressponding sw_peer_id:%d 
1862,iii,[ ar_wal_peer.c : 11083 ] wal_vdev_delete_all_peer_queue_dummy_frame_into_tcl: vdev = %d, sw_cookie = %d, buffer_id = %d 
 
1861,iii,[ ar_wal_peer.c : 10970 ] wal_vdev_delete_all_peer_queue_dummy_frame_into_tqm: vdev = %d, sw_cookie = %d, buffer_id = %d 
 
1954,I,[ wal_rc.c : 212 ] Phy rate=0, rix=%x 
1953,Iiii,[ wal_rc.c : 372 ] CHAINMASk_DBG overwrite tx chainmask, peer%p, sw_peer_id:%d  rate_Sched_chainmask %d tx_mask %d 
1952,i,[ wal_rc.c : 1444 ] [HT Sig]MCS value is not correct (%d) 
1951,i,[ wal_rc.c : 1655 ] [he_sig_b2_ofdma]MCS value is not correct (%d) 
1950,i,[ wal_rc.c : 1780 ] [he_sig_a]MCS value is not correct (%d) 
1949,i,[ wal_rc.c : 1525 ] MCS value is not correct (%d) 
1948,IIII,[ wal_rc.c : 2685 ] MU_EDCA_DEBUG: total_msdu: %lu, tcp_msdu: %lu, udp_msdu: %lu, other_msdu: %lu 
1958,iiiiiii,[ wal_rc_ul.c : 344 ] UL_PSD_BOOST_DBG: AID: %d, bw: %d, ref_mcs: %d, ref_nss: %d, ru_try: %d, boosted mcs: %d, boosted nss: %d 
1957,iiiIIi,[ wal_rc_ul.c : 546 ] UL_PSD_BOOST_DBG: idx: %d, AID: %d, MRU RU Size: %d, Out of Date Bmap: 0x%08x, Invalid RU Size Bmap: 0x%08x, Lgest uptodate ru: %d 
1956,iiIiiiiiI,[ wal_rc_ul.c : 569 ] UL_PSD_BOOST_DBG: idx: %d, AID: %d, cur_time: %u, ru_size: %d, dst_mcs: %d, dst_nss: %d, src_mcs: %d, src_nss: %d, src_tstamp: %u 
1955,iiiiiiiii,[ wal_rc_ul.c : 700 ] UL_TPC_DBG: AID: %d, bw: %d, ru_size: %d, mcs: %d, delta_p_mcs_100x: %d, delta_p_ru_100x: %d, rssi_ref_100x: %d, target_rssi_error_100x: %d => target_rssi_100x: %d 
1960,IiI,[ ar_wal_rtt.c : 93 ] Deliver RX Ind msg:%p s_thr:%d to RT at ticks:0x%x 
1959,i,[ ar_wal_rtt.c : 34 ] _wal_fac_handler: report type %d  
1981,IIIIII,[ ar_wal_rx.c : 2386 ] rxdma_error_code: %x, sw_peer_id =%x ,sw group_id %x, %x,%x, ts= %u 
1980,IIIII,[ ar_wal_rx.c : 2556 ] rx msg 0x%p, head:0x%p, 0x%p, %x buffers, ts: %u 
1979,IIi,[ ar_wal_rx.c : 2642 ] ctrl_path_stats_dbg rx: mac_address equal mac_0 = 0x%x mac_2 =0x%x subtype = %d
 
1978,IIII,[ ar_wal_rx.c : 2016 ] rx pop ppdu %x, sw_frame_group_id %x, err code %x, peer %p 
1977,iII,[ ar_wal_rx.c : 4494 ] RX PhyErr:dev=%d,err=%x,rx_err_cnt=%x 
1976,iiiiii,[ ar_wal_rx.c : 4585 ] RX PPDU dev: %d peer_id: %d ts: %d mcs: %d nss: %d,dur: %d 
 
1975,iiiiiII,[ ar_wal_rx.c : 4595 ] RX PPDU dev: %d peer_id: %d seq_no: %d mpdu_ok: %d mpdu_fail: %d fcs_err_bmap_L32 0x: %x fcs_err_bmap_U32 0x: %x 
 
1974,iiII,[ ar_wal_rx.c : 6951 ] rx resume on pdev :%d, module:%d, flag:%x, caller:0x%x 
1973,IiI,[ ar_wal_rx.c : 632 ] pdev %x, rx reap error sq %d, buffer 0x%x 
1972,I,[ ar_wal_rx.c : 680 ] drop encrypted frame without key %x 
1971,IiI,[ ar_wal_rx.c : 791 ] pdev %x, rx reap normal sq %d, buffer[%x] 
1970,iiiII,[ ar_wal_rx.c : 6864 ] rx_suspend on pdev:%d, module:%d, status:%d, flags %x, caller: %x 
1969,i,[ ar_wal_rx.c : 1657 ] wal_rx_delete_all_peer_hdlr vdev_id = %d 
1968,IIIIIII,[ ar_wal_rx.c : 7205 ] wal_rx_restore_ring_from_offload: [%x] [%x] [%x] [%x] [%x] [%x] [%x]
 
1967,II,[ ar_wal_rx.c : 7224 ] wal_rx_setup_ring_for_offload: [%x] [%x]
 
1966,III,[ ar_wal_rx.c : 1493 ] rx local notify: 0x%p, flags: 0x%x, ts: %u 
1965,IIII,[ ar_wal_rx.c : 1567 ] %s: empty len: 0x%x, addr:0x%x:0x%x 
1964,IIII,[ ar_wal_rx.c : 1606 ] %s: offload len: 0x%x, addr:0x%x:0x%x 
1963,III,[ ar_wal_rx.c : 7810 ] %s: filter0 (0x%x) filter1 (0x%x)
 
1962,IIIIII,[ ar_wal_rx.c : 7076 ] WAL_DBGID_RX_BA_SETUP  0x%x 0x%x 0x%x 0x%x 0x%x MAC:%x 
1961,iiIIII,[ ar_wal_rx.c : 6295 ] rx_suspend_resume_msg on pdev:%d, data_value:%d, status ring flag %x, head %x, tail %x, ms:%x 
1997,IiI,[ ar_wal_rx_recovery.c : 291 ] pdev %x, rx empty recovery sq %d, buffer[%x] 
1996,IiI,[ ar_wal_rx_recovery.c : 321 ] pdev %x, rx reap recovery sq %d, buffer[%x] 
1995,iii,[ ar_wal_rx_recovery.c : 814 ] RX phy error count: CNT_1:%d CNT_2:%d CNT_3:%d 
1994,iII,[ ar_wal_rx_recovery.c : 1014 ] UL OFDMA usr index: %d, Qos Control value: 0x%x, Qos Control count: 0x%x
 
1993,ii,[ ar_wal_rx_recovery.c : 1219 ] pkt_route: %d type_bmap: %d 
1992,iIIII,[ ar_wal_rx_recovery.c : 1261 ] RX ppdu sfm no resource drop count is valid? %d :%x,%x mpdu drop count:%x,%x 
1991,IIi,[ ar_wal_rx_recovery.c : 1360 ] SFM_PENDING_RXPCU DETECTION_TYPE: 0x%x RECOVERY_TYPE = 0x%x NUM_RESETS : %d 
1990,I,[ ar_wal_rx_recovery.c : 1428 ] RX set crash mask 0x%x 
1989,,[ ar_wal_rx_recovery.c : 1432 ] clear crash mask 
1988,I,[ ar_wal_rx_recovery.c : 1444 ] g_dbg_local_buf_debug_enable %x 
1987,iiI,[ ar_wal_rx_recovery.c : 1507 ] mu edca timer stop thru frame handler: pdev_id=%d, peer_id=%d, ac_bitmap = %08x 
1986,iII,[ ar_wal_rx_recovery.c : 987 ] UL OFDMA usr index: %d, HE Control value: 0x%x, HE Control count: 0x%x
 
1985,IIII,[ ar_wal_rx_recovery.c : 541 ] SFM_PENDING_RXPCU (SFM_REG) detected dev_id:0x%x,rxpcu_sfm_num_dwords=0x%x,MCMN_R0_MCMN_MAC_IDLE=0x%x,detection_type= 0x%x 
1984,i,[ ar_wal_rx_recovery.c : 486 ] restart remote timers for pdev:%d 
1983,ii,[ ar_wal_rx_recovery.c : 456 ] wal_rx_rings_reset pdev:%d, cnt:%d 
1982,,[ ar_wal_rx_recovery.c : 515 ] SFM_PENDING_RXPCU ignored.. 
2005,i,[ ar_wal_rx_refill.c : 77 ] Skip host ring TP updating for inactive pdev %d 
2004,i,[ ar_wal_rx_refill.c : 164 ] Skip monitor ring HP updating for inactive pdev %d 
2003,i,[ ar_wal_rx_refill.c : 266 ] Skip refill ring HP updating on pdev %d 
2002,ii,[ ar_wal_rx_refill.c : 1958 ] pdev %d CE pending in refill ring %d  
2001,ii,[ ar_wal_rx_refill.c : 1967 ] pdev %d CE pending in dest ring %d  
2000,ii,[ ar_wal_rx_refill.c : 1975 ] pdev %d CE pending in dest ring %d  
1999,ii,[ ar_wal_rx_refill.c : 1984 ] pdev %d CE pending in src ring %d  
1998,,[ ar_wal_rx_refill.c : 1441 ] Buffer leaked! 
2026,I,[ ar_wal_rx_uplink.c : 1436 ] ul_dbg_fake_qdepth_timer_handler:  pdev=0x%x 
2025,Ii,[ ar_wal_rx_uplink.c : 1474 ] ul_dbg_fake_qdepth_updated:  peer=0x%x, ac=%d 
2024,iii,[ ar_wal_rx_uplink.c : 1793 ] FDRSSI: rx done %d, ipc done %d, flush out %d.
 
2023,iiiiiiii,[ ar_wal_rx_uplink.c : 1632 ] UL_ACTIVITY_DBG: TRIG_TYPE=%d, NUM_USER=%d, RX_DONE=%d, TX_DONE=%d, RX_FLUSH_TIMEOUT=%d CMD_RESULT=%d TSF=%d TSTAMP_MS=%d 
2022,iiiiiiiii,[ ar_wal_rx_uplink.c : 1692 ] UL_ACTIVITY_DBG_USR: PEER_ID=%d, USER_INDEX=%d, BASIC_FAIL=%d, BASIC_SUCCESS=%d, QDEPTH_RESET=%d, BASIC_TRIG=%d, BSR_TRIG=%d, RX_DONE=%d, UL_MPDU_OK=%d 
2021,iIii,[ ar_wal_rx_uplink.c : 885 ] smart_basic_trig : qos_ctrl_info sample_count=%d, average_ul_qdepth_bytes=%u, qdepth_curr=%d, is_11ax_pkt=%d 
2020,Iiiiiiii,[ ar_wal_rx_uplink.c : 893 ] smart_basic_trig : qos_ctrl_info buffer_depletion_time=%lu, buffer_filling_interval=%d, buffer_filling_interval_bytes=%d, received_bytes=%d, bsr_trig=%d, ignore_received_bytes=%d, ac=%d, aid=%d 
 
2019,iiIIIIII,[ ar_wal_rx_uplink.c : 918 ] ul_dbg_update_peer_ul_data QOS_BITMAP: peer_aid=%d, tid_num=%d, ul_tid_state=0x%x, tid_bitmap=0x%x, eosp_bitmap=0x%x, qsize=%u, qos_ctrl_15_8=%u, ul_trig_info=0x%x 
2018,IIIIII,[ ar_wal_rx_uplink.c : 930 ] ul_dbg_update_peer_ul_data_for_bsr: time_delta=%u,qdepth_prev=%u, qdepth_curr=%u, time_now_ms=%u, bsr_timeout_ms=%u, last_non_zero_update_ts=%u 
2017,iiIIIII,[ ar_wal_rx_uplink.c : 942 ] ULMU_QUEUE_TRACK: peer_aid=%d ,peer_aid=%d, rx_mpdu_ok: %lu, rx_mpdu_fail: %lu, rx_mpdu_bytes_count: %lu, tcp_ack_msdu_cnt=%lu, ppdu_dur_us=%u 
2016,iIIIIII,[ ar_wal_rx_uplink.c : 951 ] ul_dbg_efficiency: peer_aid=%d,rx_mpdu_ok: %lu, rx_mpdu_fail: %lu, rx_mpdu_bytes_count: %lu, extra_delim_bytes: %lu, tcp_ack_msdu_cnt=%lu, ppdu_dur_us=%u 
2015,iIIIII,[ ar_wal_rx_uplink.c : 979 ] UL_MAX_PPDU_SIZE_DBG_1: aid: %d,average_mpdu_len: %lu, rx_mpdu_count: %lu, rx_mpdu_bytes_count: %lu, rx_null_delim_bytes: %lu, sum_qdepth_bytes: %lu 
2014,iII,[ ar_wal_rx_uplink.c : 1018 ] UL_MAX_PPDU_SIZE_DBG_2: aid: %d, rx_mpdu_bytes_count: %lu, ul_ofdma_estimated_max_ppdu_bytes: %lu 
2013,iiiiiiiii,[ ar_wal_rx_uplink.c : 2185 ] FDRSSI:  AID: %d, ul_mu_type %d, trigger_type %d, user %d, nss %d, ru_start %d,  min_total_gain %d, Raw %d, Final %d.
 
2012,iiiiiiiii,[ ar_wal_rx_uplink.c : 2058 ] UL_MUMIMO_DBG, EVM, mu_type %d, user %d, stream %d, pilot %d, raw_evm %d, sig_pwr_db4 %d, evm_pwr_db4 %d, pilot_evm_dB %d, mean_pilot_evm %d 
2011,IIII,[ ar_wal_rx_uplink.c : 366 ] ul_dbg_update_peer_queue_stats_from_HT_CTRL: aci_bitmap=0x%x, aci_high=0x%x, qsize_all=%u, qsize_high=%u 
2010,iIIIIII,[ ar_wal_rx_uplink.c : 518 ] ul_dbg_update_peer_queue_stats_from_HT_CTRL ac=%d, time_delta=%u, qdepth_prev=%u, qdepth_curr=%u, time_now_ms=%u, bsr timeout=%u, last_non_zero_qdepth_ts=%u 
2009,iIi,[ ar_wal_rx_uplink.c : 438 ] UL_MUMIMO_DBG: update from_htctrl. aid %d,  queue size %u, ptid_tidno=%d reset UL implicit 
2008,Iiiiiiii,[ ar_wal_rx_uplink.c : 478 ] smart_basic_trig : stats_from_htctrl_field buffer_depletion_time=%lu, buffer_filling_interval=%d, buffer_filling_interval_bytes=%d, sample_count=%d, smart_basic_trigger=%d, qdepth_curr=%d, ac=%d, aid=%d 
 
2007,IIiI,[ ar_wal_rx_uplink.c : 1185 ] ul_dbg_update_peer_ul_data: peer=0x%x, ul_rate_info=0x%x, bsr_recvd=%d, bsr_trig=%u 
2006,IIIIIIII,[ ar_wal_rx_uplink.c : 1194 ] ul_dbg_update_peer_ul_data: fc_valid:%x, fc_field:0x%x, ht_ctrl_valid=%x, ht_control_field=0x%x,ht_ctrl_null_valid=%x, ht_control_null_field=0x%x,qos_data_tid_bitmap=0x%x, qos_data_tid_eosp_bitmap=0x%x 
2045,,[ wal_htt_ppdu_stats.c : 519 ] Dropped ppdu stats due to ring full 
2044,,[ wal_htt_ppdu_stats.c : 1054 ] Dropped ppdu stats due to full QHEAP 
2043,,[ wal_htt_ppdu_stats.c : 1681 ] Dropped ppdu stats due to full QHEAP 
2042,,[ wal_htt_ppdu_stats.c : 1735 ] Dropped ppdu stats due to full QHEAP 
2041,,[ wal_htt_ppdu_stats.c : 1796 ] Dropped mgmt ppdu tlv due to ring full 
2040,,[ wal_htt_ppdu_stats.c : 1853 ] Dropped ppdu stats due to full QHEAP 
2039,,[ wal_htt_ppdu_stats.c : 627 ] Dropped ppdu stats due to full QHEAP 
2038,,[ wal_htt_ppdu_stats.c : 1209 ] Dropped ppdu stats due to full QHEAP 
2037,,[ wal_htt_ppdu_stats.c : 773 ] Dropped ppdu stats due to full QHEAP 
2036,,[ wal_htt_ppdu_stats.c : 992 ] Dropped ppdu stats due to full QHEAP 
2035,,[ wal_htt_ppdu_stats.c : 934 ] Dropped ppdu stats due to full QHEAP 
2034,,[ wal_htt_ppdu_stats.c : 1418 ] Dropped ppdu stats due to full QHEAP 
2033,,[ wal_htt_ppdu_stats.c : 1317 ] Dropped tqm ppdu stats due to ring full 
2032,,[ wal_htt_ppdu_stats.c : 1331 ] Dropped tqm ppdu stats due to full QHEAP 
2031,,[ wal_htt_ppdu_stats.c : 1517 ] Dropped tac ppdu stats due to full QHEAP 
2030,,[ wal_htt_ppdu_stats.c : 1996 ] Dropped ppdu stats due to full QHEAP 
2029,I,[ wal_htt_ppdu_stats.c : 1943 ] Dropped FLUSHSTATS INFRA_3_X HTT RINGFULL!!! CANCEL buffer:0x%x  
2028,I,[ wal_htt_ppdu_stats.c : 1962 ] FLUSHSTATS INFRA_3_0 HTT RINGSEND buffer:0x%x  
2027,i,[ wal_htt_ppdu_stats.c : 1898 ] Dropped self gen ppdu tlv due to ring full ring_id:%d 
2046,iiii,[ ar_wal_thermal.c : 433 ] pdev_id(%d),tx_chainmask(%d), rx_chainmask(%d), num_chains(%d) 
2071,IIII,[ ar_wal_tqm.c : 608 ] peer_id=0x%x, _set_flow_to_be_cleanup:%x, tx_flow_number:%x,caller:%x 
2070,ii,[ ar_wal_tqm.c : 733 ] qos:  %d and peer_id is %d tickle tid 
2069,I,[ ar_wal_tqm.c : 771 ] wal_tqm_process_flow_not_empty_status new flow:%x  
2068,ii,[ ar_wal_tqm.c : 7312 ] soft_msduq_delete: Requesting soft msduq delete :%d qtype:%d 
2067,IIIIII,[ ar_wal_tqm.c : 6345 ] PEER_DELETE_DBG: wal_tqm_delete_tid:%x,%x,%x,%x,%x, invalidate:%x 
 
2066,i,[ ar_wal_tqm.c : 405 ] wal_tqm_flow_empty_helper not_init, counter:%d 
2065,II,[ ar_wal_tqm.c : 353 ] wal_tqm_flow_update_helper not_init, fw_initialized:%x, counter:%x 
2064,I,[ ar_wal_tqm.c : 1225 ] FLUSHSTATS INFRA_5 TQM FREE buffer:0x%x  
2063,,[ ar_wal_tqm.c : 4250 ] TCL rings unpaused 
2062,i,[ ar_wal_tqm.c : 4256 ] Fired timer again             TQM link descriptor counter:%d 
2061,iii,[ ar_wal_tqm.c : 2369 ] qos_to_nonqos_switch: Received tqm add_msdu status peer_id:%d status:%d buffer_id:%d 
2060,iiii,[ ar_wal_tqm.c : 2666 ] Fired timer and paused TCL rings             ring link descriptor counters mac0:%d mac1:%d mac2:%d sum:%d 
2059,IIII,[ ar_wal_tqm.c : 2426 ] peer_id= 0x%x, wal_tqm_process_flush_cache_status:%x,%x,%x 
2058,,[ ar_wal_tqm.c : 1070 ] wal_tqm_process_gen_mpdus_status: Null ptid 
2057,III,[ ar_wal_tqm.c : 1939 ] qstats_status peer_id:%u tid_num:%u qtype:%u 
2056,IIIII,[ ar_wal_tqm.c : 1568 ] FLUSHSTATS TQM remove_mpdu_status TLV:0x%x peerid:%u cmd_reason:%u mpdu:%u msdu:%u flushed 
2055,IIII,[ ar_wal_tqm.c : 1618 ] peer_id= 0x%x, wal_tqm_process_remove_msdu_status:%x,%x,%x 
2054,IIiII,[ ar_wal_tqm.c : 1738 ] FLUSHSTATS TQM remove_msdu_status TLV:0x%x peerid:%u cmd_reason:%d mpdu:%u msdu:%u flushed 
2053,ii,[ ar_wal_tqm.c : 436 ] _wal_tqm_process_update_tx_msdu_flow_status tx_flow_number:%d update_requirements_not_met:%d  
2052,Ii,[ ar_wal_tqm.c : 1282 ] FLUSHSTATS INFRA_0_X TQM copy flush_tlv:0x%x discarded, FAILED due to pool_alloc fail_count:%d 
2051,I,[ ar_wal_tqm.c : 1288 ] FLUSHSTATS INFRA_0 TQM ALLOC buffer:0x%x  
2050,III,[ ar_wal_tqm.c : 1298 ] FLUSHSTATS INFRA_1 TQM copied flush_tlv:0x%x to buffer:0x%x now rem_sz:%u bytes 
2049,II,[ ar_wal_tqm.c : 1246 ] FLUSHSTATS INFRA_2 TQM SEND buffer:0x%x of size:%u 
2048,ii,[ ar_wal_tqm.c : 2057 ] soft_msduq_delete: msduq got deleted :%d qtype:%d 
2047,ii,[ ar_wal_tqm.c : 2061 ] soft_msduq_delete: delete req dropped :%d qtype:%d 
2076,IIIIII,[ ar_tx_q_enque.c : 430 ] tx_q_enque_tqm_bypass: tid_num=0x%x, pdev_id=0x%0x, tid_paused=0x%x, type=0x%0x, len=0x%0x, num_mpdus_in_fq=0x%0x 
2075,IIIIIIII,[ ar_tx_q_enque.c : 685 ] pn_alloc:fc=%x,comp_type=%x,flen=%lx,msdu_flags=%lx,id=%x,buffer_id=%x,enque_id=%x,pending_local=%x 
2074,II,[ ar_tx_q_enque.c : 963 ] WAL_DBGID_TX_DISCARD id: %x, flag:%lx
 
2073,IIIIIII,[ ar_tx_q_enque.c : 773 ] pn_alloc_complete:fc=%x,flen=%lx,msdu_flags=%lx,tid_num=%x,enque_id=%x,pn_idx=%x,pn=%llx 
2072,IIIIII,[ ar_tx_q_enque.c : 816 ] pn_alloc failed: id:%x,flags:%x,tid_no:%x,fc:%x,enqeu_id=%x,pending_local=%x 
2216,IIIIIIIIIII,[ ar_wal_tx_dbg.c : 850 ] txbf_su_ppdu_stats (legacy su = %lu)(ol ac su = %lu)(txbf ac su =  %lu)(txbf ac %% = %lu)(ol ax su = %lu)(txbf ax su =  %lu)(txbf ax %% = %lu) 
2215,III,[ ar_wal_tx_dbg.c : 1800 ] TXDEWDOG TQM1:%u dummy_queued:%u last_time:%u 
2214,,[ ar_wal_tx_dbg.c : 2097 ] No ul_resp_vdev or BSS-peer assigned !! 
2213,I,[ ar_wal_tx_dbg.c : 2102 ] invalid ACTRL:%x 
2212,iii,[ ar_wal_tx_dbg.c : 2166 ] fudge_txtime=%d, legacy_burst_per=%d, vht_burst_per=%d 
2211,iii,[ ar_wal_tx_dbg.c : 2249 ] mu_mimo_ppdu_dur_hist_200us_bin_%d (Nr_%d) : %d 
2210,III,[ ar_wal_tx_dbg.c : 899 ] txbf_su_mpdu_stats AX OL(ol ax su tried = %lu)(ol ax su failed = %lu)(ol ax su retried = %lu) 
2209,iiiiiiiii,[ ar_wal_tx_dbg.c : 2265 ] mu_mimo_total_txop_ms_hist_MU%d_bin_%d - %d (Nr_%d) : %d, %d, %d, %d, %d 
2208,iiii,[ ar_wal_tx_dbg.c : 2274 ] mu_mimo_mpdus_failed_hist_%d - %d (Nr_%d) : %d 
2207,iiii,[ ar_wal_tx_dbg.c : 2279 ] mu_mimo_mpdus_failed_hist_%d - %d (Nr_%d) : %d 
2206,iii,[ ar_wal_tx_dbg.c : 2288 ] mu_mimo_mpdus_tried_hist_%d (Nr_%d) : %d 
2205,iiii,[ ar_wal_tx_dbg.c : 2293 ] mu_mimo_mpdus_tried_hist_%d - %d (Nr_%d) : %d 
2204,iiii,[ ar_wal_tx_dbg.c : 2298 ] mu_mimo_mpdus_tried_hist_%d - %d (Nr_%d) : %d 
2203,ii,[ ar_wal_tx_dbg.c : 2326 ] mu_mimo : Number of MU Sequences Posted (Nr_%d) : %d 
 
2202,iiiiiiii,[ ar_wal_tx_dbg.c : 2339 ] mu_mimo (Nr_%d) : Num of PPDUs Posted Per Burst [%d-%d] : %d,%d,%d,%d,%d 
 
2201,iiiiiiii,[ ar_wal_tx_dbg.c : 2353 ] mu_mimo (Nr_%d) : Num of MU PPDUs completed per burst  [%d-%d] : %d,%d,%d,%d,%d 
 
2200,ii,[ ar_wal_tx_dbg.c : 2359 ] mu_mimo (Nr_%d) : MU seq. termination status WAL_TX_ISR_SCHED_SUCCESS : %d 
 
2199,IIIIII,[ ar_wal_tx_dbg.c : 916 ] txbf_su_mpdu_stats AX (txbf sifs ax su tried = %lu)(txbf sifs ax su failed = %lu)(txbf sifs ax su retried = %lu)(txbf rbo ax su tried = %lu)(txbf rbo ax su failed = %lu)(txbf rbo ax su retried = %lu) 
2198,ii,[ ar_wal_tx_dbg.c : 2363 ] mu_mimo (Nr_%d) : MU seq. termination status WAL_TX_ISR_SCHED_FILTER: %d 
 
2197,ii,[ ar_wal_tx_dbg.c : 2367 ] mu_mimo (Nr_%d) : MU seq. termination status WAL_TX_ISR_SCHED_RESP_TIMEOUT: %d 
 
2196,ii,[ ar_wal_tx_dbg.c : 2371 ] mu_mimo (Nr_%d) : MU seq. termination status WAL_TX_ISR_SCHED_RATES_EXHAUSTED: %d 
 
2195,ii,[ ar_wal_tx_dbg.c : 2375 ] mu_mimo (Nr_%d) : MU seq. termination status WAL_TX_ISR_SCHED_DATA_EXHAUSTED: %d 
 
2194,ii,[ ar_wal_tx_dbg.c : 2379 ] mu_mimo (Nr_%d) : MU seq. termination status WAL_TX_ISR_SCHED_SEQ_ABORT: %d 
 
2193,ii,[ ar_wal_tx_dbg.c : 2383 ] mu_mimo (Nr_%d) : MU seq. termination status WAL_TX_ISR_SCHED_NOTIFY_FRAME_ENCOUNTERED: %d 
 
2192,ii,[ ar_wal_tx_dbg.c : 2387 ] mu_mimo (Nr_%d) : MU seq. termination status WAL_TX_ISR_SCHED_COMPLETION: %d 
 
2191,ii,[ ar_wal_tx_dbg.c : 2391 ] mu_mimo (Nr_%d) : MU seq. termination status WAL_TX_ISR_SCHED_IN_PROGRESS: %d 
 
2190,II,[ ar_wal_tx_dbg.c : 2408 ] TXDEWDOG prev_timeout:%u current_timeout:%u 
2189,II,[ ar_wal_tx_dbg.c : 2504 ] read addr: 0x%x, value = 0x%x 
2188,II,[ ar_wal_tx_dbg.c : 927 ] txbf_snd_stats(txbf_ac_snd = %lu)(txbf_ax_snd = %lu) 
2187,IIIII,[ ar_wal_tx_dbg.c : 2605 ] ax_mu_mimo_ndpa_sch_status : WHAL_TXERR_NONE = %lu,WHAL_TXERR_RESP = %lu,WHAL_TXERR_FILT = %lu,WHAL_TXERR_FIFO = %lu,WHAL_TXERR_SWABORT = %lu
 
2186,IIIII,[ ar_wal_tx_dbg.c : 2619 ] ax_mu_mimo_ndp_sch_status : WHAL_TXERR_NONE = %lu,WHAL_TXERR_RESP = %lu,WHAL_TXERR_FILT = %lu,WHAL_TXERR_FIFO = %lu,WHAL_TXERR_SWABORT = %lu
 
2185,IIIII,[ ar_wal_tx_dbg.c : 2633 ] ax_mu_brp_sch_status : WHAL_TXERR_NONE = %lu,WHAL_TXERR_RESP = %lu,WHAL_TXERR_FILT = %lu,WHAL_TXERR_FIFO = %lu,WHAL_TXERR_SWABORT = %lu
 
2184,I,[ ar_wal_tx_dbg.c : 2639 ] ax_mu_brp_trigger_hw_paused = %lu
 
2183,IIIIIII,[ ar_wal_tx_dbg.c : 2658 ] ax_mu_mimo_ndp_sch_flag_err : WHAL_SCH_TSFLAG_FLUSH_RCVD_ERR = %lu,WHAL_SCH_TSFLAG_FILT_SCHED_CMD_ERR = %lu,WHAL_SCH_TSFLAG_RESP_MISMATCH_ERR = %lu,WHAL_SCH_TSFLAG_RESP_CBF_MIMO_CTRL_MISMATCH_ERR = %lu,WHAL_SCH_TSFLAG_RESP_CBF_BW_MISMATCH_ERR = %lu,WHAL_SCH_TSFLAG_RETRY_COUNT_FAIL_ERR = %lu,WHAL_SCH_TSFLAG_RESP_TOO_LATE_RECEIVED_ERR = %lu
 
2182,IIIIIII,[ ar_wal_tx_dbg.c : 2676 ] ax_mu_mimo_brp_sch_flag_err : WHAL_SCH_TSFLAG_FLUSH_RCVD_ERR = %lu,WHAL_SCH_TSFLAG_FILT_SCHED_CMD_ERR = %lu,WHAL_SCH_TSFLAG_RESP_MISMATCH_ERR = %lu,WHAL_SCH_TSFLAG_RESP_CBF_MIMO_CTRL_MISMATCH_ERR = %lu,WHAL_SCH_TSFLAG_RESP_CBF_BW_MISMATCH_ERR = %lu,WHAL_SCH_TSFLAG_RETRY_COUNT_FAIL_ERR = %lu,WHAL_SCH_TSFLAG_RESP_TOO_LATE_RECEIVED_ERR = %lu
 
2181,IIIII,[ ar_wal_tx_dbg.c : 2690 ] ax_mu_mimo_ndpa_user_status : WHAL_TXERR_NONE = %lu,WHAL_TXERR_RESP = %lu,WHAL_TXERR_FILT = %lu,WHAL_TXERR_FIFO = %lu,WHAL_TXERR_SWABORT = %lu
 
2180,IIIII,[ ar_wal_tx_dbg.c : 2704 ] ax_mu_mimo_ndp_user_status : WHAL_TXERR_NONE = %lu,WHAL_TXERR_RESP = %lu,WHAL_TXERR_FILT = %lu,WHAL_TXERR_FIFO = %lu,WHAL_TXERR_SWABORT = %lu
 
2179,IIIII,[ ar_wal_tx_dbg.c : 2718 ] ax_mu_mimo_ndp_user_flag_err : WHAL_USER_TSFLAG_RESP_MISMATCH_ERR = %lu,WHAL_USER_TSFLAG_RESP_MIMO_CTRL_MISMATCH_ERR = %lu,WHAL_USER_TSFLAG_RESP_CRC_FAIL_ERR = %lu,WHAL_USER_TSFLAG_RESP_TIMEOUT_ERR = %lu,WHAL_USER_TSFLAG_RESP_PROT_TIMEOUT_ERR = %lu
 
2178,IIIII,[ ar_wal_tx_dbg.c : 2732 ] ax_mu_brp_user_flag_err : WHAL_USER_TSFLAG_RESP_MISMATCH_ERR = %lu,WHAL_USER_TSFLAG_RESP_MIMO_CTRL_MISMATCH_ERR = %lu,WHAL_USER_TSFLAG_RESP_CRC_FAIL_ERR = %lu,WHAL_USER_TSFLAG_RESP_TIMEOUT_ERR = %lu,WHAL_USER_TSFLAG_RESP_PROT_TIMEOUT_ERR = %lu
 
2177,iii,[ ar_wal_tx_dbg.c : 939 ] %dms Burst: avg_txop_burst(ms) = %d,txop_on_burst_complete(ms) = %d 
 
2176,,[ ar_wal_tx_dbg.c : 2879 ] DEBUG_CACHE::Invalid Reg Operation 
 
2175,Ii,[ ar_wal_tx_dbg.c : 3088 ] sifs burst enable: 0x%x, pdev=%d
 
2174,i,[ ar_wal_tx_dbg.c : 3111 ] # of MU-RTS : %d 
 
2173,IIIIII,[ ar_wal_tx_dbg.c : 3210 ] flush_38_hist: %02d %02d %02d %02d %02d %02d 
2172,i,[ ar_wal_tx_dbg.c : 3281 ] WAL_PPDU: MU PPDU VAL:%d 
2171,i,[ ar_wal_tx_dbg.c : 3323 ] g_ack_all_6Mbps : %d 
 
2170,IIIII,[ ar_wal_tx_dbg.c : 3378 ] PHYDBG: g_dbg_phydbg_default_events: 0x%08x, g_dbg_phydbg_pmi_events: 0x%08x, g_dbg_phydbg_mpi_events: 0x%08x, g_dbg_phydbg_rxtd_events: 0x%08x, g_dbg_phydbg_robe_events: 0x%08x 
2169,IIIII,[ ar_wal_tx_dbg.c : 3542 ] twt_dbg_leak_hist_dl: Bins0-4: %u, %u, %u, %u, %u 
2168,IIIII,[ ar_wal_tx_dbg.c : 3547 ] twt_dbg_leak_hist_dl: Bins5-9: %u, %u, %u, %u, %u 
2167,IIIII,[ ar_wal_tx_dbg.c : 3553 ] twt_dbg_leak_hist_ul: Bins0-4: %u, %u, %u, %u, %u 
2166,iiiiiiii,[ ar_wal_tx_dbg.c : 1141 ] sched_cmd_result[0] to sched_cmd_result[6] for HWQ id %d = {%d,%d,%d,%d,%d,%d,%d}
 
2165,IIIII,[ ar_wal_tx_dbg.c : 3559 ] twt_dbg_leak_hist_ul: Bins0-4: %u, %u, %u, %u, %u 
2164,i,[ ar_wal_tx_dbg.c : 3995 ] SelfGenResp: Dev id %d is in power saving state, not able to print. 
2163,ii,[ ar_wal_tx_dbg.c : 4054 ] LOCAL: msduq_pool_ctxt total_alloc_cnt:%d cur_alloc_cnt:%d 
2162,ii,[ ar_wal_tx_dbg.c : 4058 ] REMOTE: msduq_pool_ctxt total_alloc_cnt:%d cur_alloc_cnt:%d 
2161,ii,[ ar_wal_tx_dbg.c : 4063 ] LOCAL:  tid_swap_pool_ctxt total_alloc_cnt:%d cur_alloc_cnt:%d 
2160,ii,[ ar_wal_tx_dbg.c : 4066 ] REMOTE: tid_swap_pool_ctxt total_alloc_cnt:%d cur_alloc_cnt:%d 
2159,ii,[ ar_wal_tx_dbg.c : 4071 ] LOCAL: tid_state_pool total_alloc_cnt:%d cur_alloc_cnt:%d 
2158,ii,[ ar_wal_tx_dbg.c : 4074 ] REMOTE: tid_state_pool total_alloc_cnt:%d cur_alloc_cnt:%d 
2157,ii,[ ar_wal_tx_dbg.c : 4078 ] LOCAL: ul_tid_state_pool total_alloc_cnt:%d cur_alloc_cnt:%d 
2156,ii,[ ar_wal_tx_dbg.c : 4081 ] REMOTE: ul_tid_state_pool total_alloc_cnt:%d cur_alloc_cnt:%d 
2155,iiiiiii,[ ar_wal_tx_dbg.c : 1151 ] sched_cmd_result[7] to sched_cmd_result[12] for HWQ id %d = {%d,%d,%d,%d,%d, %d}
 
2154,ii,[ ar_wal_tx_dbg.c : 4289 ]  Profile Enabled : %d   hist_intvl : %d 
2153,iiii,[ ar_wal_tx_dbg.c : 4317 ]  Profile ID : %d  Count: %d  Min : %d  Max : %d  
2152,iiiii,[ ar_wal_tx_dbg.c : 4329 ]  Profile ID : %d  hist_intvl: %d  hist[0] : %d  hist[1] : %d  hist[2] : %d  
2151,,[ ar_wal_tx_dbg.c : 4469 ] ctrl_path_stats_dbg : Disabling peer_dbg logs
 
2150,,[ ar_wal_tx_dbg.c : 4476 ] ctrl_path_stats_dbg : Error seen 
 Usage 
ctrl_path_stats_dbg: To Enable  Stats: wifitool athX setUnitTestCmd 0x48 8 244 1 <mac_addr_0> <mac_addr_1> <mac_addr_2>  <mac_addr_3> <mac_addr_4> <mac_addr_5>
ctrl_path_stats_dbg: To Disable Stats: wifitool athX setUnitTestCmd 0x48 2 244 0
 
2149,IIIIII,[ ar_wal_tx_dbg.c : 4499 ] ctrl_path_stats_dbg : args[2] = 0x%x args[3] = 0x%x args[4] = 0x%x args[5] = 0x%x args[6] = 0x%x args[7] = 0x%x
 
2148,II,[ ar_wal_tx_dbg.c : 4502 ] ctrl_path_stats_dbg : mac_addr_31_0 = 0x%x mac_addr_47_32 = 0x%x
 
2147,,[ ar_wal_tx_dbg.c : 4504 ] ctrl_path_stats_dbg: SW Peer ID Check
 
2146,i,[ ar_wal_tx_dbg.c : 4507 ] ctrl_path_stats_dbg: vdev %d 
 
2145,,[ ar_wal_tx_dbg.c : 4515 ] ctrl_path_stats_dbg: bss  
2144,i,[ ar_wal_tx_dbg.c : 1199 ] TX_IST_TRIGGER SENT %d
 
2143,,[ ar_wal_tx_dbg.c : 4517 ] ctrl_path_stats_dbg: self  
2142,iII,[ ar_wal_tx_dbg.c : 4520 ] ctrl_path_stats_dbg: peer %d, mac %x %x
 
2141,iII,[ ar_wal_tx_dbg.c : 4522 ] ctrl_path_stats_dbg: sw_peer_id found peer %d, mac %x %x
 
2140,,[ ar_wal_tx_dbg.c : 4557 ] s_stats!ERROR!:use:wifitool athX setUnitTestCmd 0x48 2 260 0/1 
 
2139,II,[ ar_wal_tx_dbg.c : 4615 ] s_stats: dbg_num_bufs: %u, dbg_num_evt: %u 
 
2138,III,[ ar_wal_tx_dbg.c : 4616 ] s_stats: HOST_ring_HI : %u, TI : %u, S_TI : %u  
2137,IIII,[ ar_wal_tx_dbg.c : 4617 ] s_stats: IN/SHADOW_ring_HI : %u, TI : %u, S_TI : %u, S_HI : %u 
2136,IIII,[ ar_wal_tx_dbg.c : 4618 ] s_stats: OUT_ring_HI : %u TI : %u, S_TI : %u, S_HI : %u 
2135,IIIII,[ ar_wal_tx_dbg.c : 4621 ] s_stats: IPC_ring_%u : HI : %u TI : %u, S_TI : %u, S_HI : %u 
2134,,[ ar_wal_tx_dbg.c : 4623 ] s_stats: VREG_DET0 : 
 
2133,IIIIII,[ ar_wal_tx_dbg.c : 871 ] txbf_su_mpdu_stats (legacy su tried = %lu)(legacy su failed = %lu)(legacy su retried = %lu) ------------------------txbf_su_mpdu_stats AC OL(ol ac su tried = %lu)(ol ac su failed = %lu)(ol ac su retried = %lu) 
2132,,[ ar_wal_tx_dbg.c : 1243 ] pdev_id can't be > 2, usage: wifitool ath0 setUnitTestCmd 0x48 2 56 <pdev_id> 
2131,III,[ ar_wal_tx_dbg.c : 4624 ] s_stats: ScanPri : %u, SCount : %u, SPrd : %u 
 
2130,III,[ ar_wal_tx_dbg.c : 4625 ] s_stats: ChnMask : %u, SEna : %u, SUpdtMask : 0x%x 
 
2129,IIII,[ ar_wal_tx_dbg.c : 4626 ] s_stats: SRdyIntrpt : %u, SPfmd : %u, IntrptsSent : %u, Scanpending : %u 

 
2128,,[ ar_wal_tx_dbg.c : 4628 ] s_stats: VREG_DET1: 
 
2127,III,[ ar_wal_tx_dbg.c : 4629 ] s_stats: ScanPri : %u, SCount : %u, SPrd : %u 
 
2126,III,[ ar_wal_tx_dbg.c : 4630 ] s_stats: ChnMask : %u, SEna : %u, SUpdtMask : 0x%x 
 
2125,IIII,[ ar_wal_tx_dbg.c : 4631 ] s_stats: SRdyIntrpt : %u, SPfmd : %u, IntrptsSent : %u , Scanpending : %u 
 
2124,,[ ar_wal_tx_dbg.c : 4634 ] s_stats: VREG_DET_AGILE : 
 
2123,III,[ ar_wal_tx_dbg.c : 4635 ] s_stats: ScanPri : %u, SCount : %u, SPrd : %u 
 
2122,III,[ ar_wal_tx_dbg.c : 4636 ] s_stats: ChnMask : %u, SEna : %u, SUpdtMask : 0x%x 
 
2121,iiiiiiii,[ ar_wal_tx_dbg.c : 1263 ] WHAL_STATS for pdev id =  %d: last_unpause_ppdu_id = %d hwsch_unpause_wait_tqm_write = %d hwsch_dummy_tlv_skipped = %d hwsch_misaligned_offset_received = %d hwsch_reset_count = %d hwsch_dev_reset_war = %d hwsch_delayed_pause = %d 
2120,IIII,[ ar_wal_tx_dbg.c : 4637 ] s_stats: SRdyIntrpt : %u, SPfmd : %u, IntrptsSent : %u, Scanpending : %u 
 
2119,iiii,[ ar_wal_tx_dbg.c : 5020 ] delimiter user track: Number of total MU PPDU %d, MU PPDUs with delimiter users: %d, Percent:%d                    Average MU number of delimiter users %d 
2118,i,[ ar_wal_tx_dbg.c : 5416 ] Num of sched commands dropped due to session ID mismatch - %d 
2117,i,[ ar_wal_tx_dbg.c : 5417 ] Num of sched commands during TX abort - %d 
2116,ii,[ ar_wal_tx_dbg.c : 5419 ] Num of seq start during resume: ISR - %d, DSR - %d 
2115,,[ ar_wal_tx_dbg.c : 5433 ] TX abort/resume in progress. Ignoring request! 
2114,iiii,[ ar_wal_tx_dbg.c : 5453 ] SFM_FLUSH_ISSUE sfm_wdg_with_flush_issue = %d, sfm_wdg_without_flush_issue = %d sfm_fatal_unknown = %d, num of times sfm issue got hit = %d 
2113,i,[ ar_wal_tx_dbg.c : 5480 ] NOC PENDING TRANSACTIONS pending_noc_transactions_during_reset = %d 
2112,iiiii,[ ar_wal_tx_dbg.c : 5572 ] CONG_CTRL Multicast_DBG buf_id:%d hcm_bin_idx:%d cur:%d, min:%d, max:%d 
2111,iI,[ ar_wal_tx_dbg.c : 5638 ] mu edca timer stop: pdev_id = %d, ac_bitmap = %08x 
2110,iiiiiiii,[ ar_wal_tx_dbg.c : 1283 ] hwsch_long_delayed_pause = %d sch_rx_ppdu_no_response = %d sch_selfgen_response = %d sch_rx_sifs_resp_trigger = %d sch_mpdu_info_bitmap_missed = %d hwsch_qcdd03911334 = %d hwsch_qcdd04031456 = %d hwsch_qcdd03955078 = %d 
2109,iiiii,[ ar_wal_tx_dbg.c : 5695 ] tqm_sync_pipeling_stats: tqm_sync_sent = %d, tqm_sync_proc = %d, TAC/IST post = %d, tqm_sync_not_proc = %d, tqm_ist post = %d 
2108,i,[ ar_wal_tx_dbg.c : 5717 ] MAC clock gating: %d 
2107,,[ ar_wal_tx_dbg.c : 5814 ]  HW_ERR_REINJECTION : Invalid no. of arguments during mac flush err injection 
2106,,[ ar_wal_tx_dbg.c : 5832 ]  HW_ERR_REINJECTION : Invalid host ring id during host ring bkpressure err injection 
2105,,[ ar_wal_tx_dbg.c : 5835 ]  HW_ERR_REINJECTION : Invalid no. of arguments during host ring bkpressure err injection 
2104,,[ ar_wal_tx_dbg.c : 5853 ]  HW_ERR_REINJECTION : Invalid fw ring id during fw ring bkpressure err injection 
2103,,[ ar_wal_tx_dbg.c : 5856 ]  HW_ERR_REINJECTION : Invalid no. of arguments during fw ring bkpressure err injection 
2102,,[ ar_wal_tx_dbg.c : 5873 ]  HW_ERR_REINJECTION : Invalid hw ring id during hw ring bkpressure err injection 
2101,,[ ar_wal_tx_dbg.c : 5876 ]  HW_ERR_REINJECTION : Invalid no. of arguments during hw ring bkpressure err injection 
2100,,[ ar_wal_tx_dbg.c : 5891 ]  HW_ERR_REINJECTION : Invalid no. of arguments during rx abort err injection 
2099,iiiiiiii,[ ar_wal_tx_dbg.c : 1303 ] hwsch_backpressure_wdog = %d hwsch_pause_wdog = %d hwsch_fes_start_wdog = %d hwsch_life_time_expiry_valid_fes_offset = %d crypto_wdog_tmout = %d hwsch_fes_end_offset_wraparound = %d pdg_sfm_leak_rst_cnt = %d hwsch_cmd_ring_reset_war_dummy_completions = %d 
2098,i,[ ar_wal_tx_dbg.c : 5917 ] RTT LUT enabled : %d 
2097,,[ ar_wal_tx_dbg.c : 5991 ] AWGN_INT_DBG  Wrong Input: wifitool athX setUnitTestCmd 0x48 4 400  1 <intr enable/disable> <seg_index> 
2096,ii,[ ar_wal_tx_dbg.c : 5996 ] AWGN_INT_DBG : intr = %d seg = %d 
2095,,[ ar_wal_tx_dbg.c : 6004 ] AWGN_INT_DBG Wrong Input: wifitool athX setUnitTestCmd 0x48 3 400  2 <awgn_logs enable/disable> 
2094,ii,[ ar_wal_tx_dbg.c : 6008 ] AWGN_INT_DBG : intr = %d seg = %d 
2093,,[ ar_wal_tx_dbg.c : 6016 ] AWGN_INT_DBG Wrong Input: wifitool athX setUnitTestCmd 0x48 4 400  3 <tx_prop> <rx_prop> 
2092,ii,[ ar_wal_tx_dbg.c : 6021 ] AWGN_INT_DBG : tx_prop = %d rx_prop = %d 
2091,,[ ar_wal_tx_dbg.c : 6025 ] AWGN_INT_DBG : wrong input
 
2090,ii,[ ar_wal_tx_dbg.c : 6125 ] g_dbg_mgmt_drop_alloc_fail_peer_paused =%d, g_dbg_mgmt_drop_alloc_fail_peer_unpaused=%d 
2089,iiiiiiii,[ ar_wal_tx_dbg.c : 1323 ] hwsch_flush_not_done = %d flush_tx_not_idle = %d hwsch_wd_unknown_reset = %d hwsch_mtu_wrap_wdog = %d crypto_fatal_unknown = %d txdma_fatal_unknown = %d sfm_fatal_unknown = %d mcmn_fatal_unknown = %d 
2088,iiiiiiii,[ ar_wal_tx_dbg.c : 1343 ] txpcu_wdog_tout = %d txpcu_recd_lt_mpdu = %d txpcu_recd_gt_mpdu= %d pdg_fatal_unknown = %d hwsch_fatal_unknown = %d hwsch_wdog_unknown = %d mxi_fatal_unknown = %d txole_fatal_unknown = %d 
2087,iiiiiii,[ ar_wal_tx_dbg.c : 1391 ] tx_flush_tlv_tag_oor_err = %d tx_flush_tlv_len_oor_err = %d tx_flush_tlv_taglen_mismatch_err = %d tx_flush_unexpected_tlv_end_err = %d tx_steer_frm_cnt = %d tx_flush_txdma_sfm_busy = %d phy_warm_reset = %d 
2086,,[ ar_wal_tx_dbg.c : 1407 ] pdev_id can't be > 2, usage: wifitool ath0 setUnitTestCmd 0x48 2 57 <pdev_id> 
2085,,[ ar_wal_tx_dbg.c : 1418 ] No ul_resp_vdev assigned !! 
2084,II,[ ar_wal_tx_dbg.c : 1422 ] ac:%x already in MU mode, reset timer to %x 
2083,IIIIII,[ ar_wal_tx_dbg.c : 888 ] txbf_su_mpdu_stats AC (txbf sifs ac su tried = %lu)(txbf sifs ac su failed = %lu)(txbf sifs ac su retried = %lu)(txbf rbo ac su tried = %lu)(txbf rbo ac su failed = %lu)(txbf rbo ac su retried = %lu) 
2082,I,[ ar_wal_tx_dbg.c : 1425 ] ac:%x switch to MU mode 
2081,I,[ ar_wal_tx_dbg.c : 1570 ] flush hwq mask:%x 
2080,I,[ ar_wal_tx_dbg.c : 1575 ] flush hwq mask:%x, ul_resp is not enabled 
2079,iii,[ ar_wal_tx_dbg.c : 1652 ] g_eapol_rekey_min_rate_enable num_args:%d %d, %d  
2078,IIII,[ ar_wal_tx_dbg.c : 1797 ] TXDEWDOG TCL1:%u full_ignore:%u dummy_queued:%u last_time:%u 
2077,III,[ ar_wal_tx_dbg.c : 517 ] data_stall debug support is not allowed as the vdev_type is not            STA pdev_id:8/vdev_id:8 0x%08x vdev:0x%x pdev:0x%x 
2217,ii,[ ar_wal_tx_send_selfgen.c : 3746 ] UL_MUMIMO_DBG, seq_type %d, is_ul_mumimo: %d 
2224,,[ ar_wal_tx_halphy_send.c : 629 ]  HALPHY_TX_TBTT_FLUSH : DPD packet is flushed out  
2223,,[ ar_wal_tx_halphy_send.c : 638 ]  HALPHY_TX_ABORT : DPD packet is  aborted 
2222,,[ ar_wal_tx_halphy_send.c : 737 ]  tx_send_halphy_abort_ppdu : DPD packet is  aborted 
2221,i,[ ar_wal_tx_halphy_send.c : 241 ] PAPRD dpd start tlv event : start evt latency %d 
2220,i,[ ar_wal_tx_halphy_send.c : 1250 ]  wal_check_ppdu_status DPD ppdu is stuck in the hardware queue %d 
2219,i,[ ar_wal_tx_halphy_send.c : 1236 ]  thread id %d 
2218,iiiii,[ ar_wal_tx_halphy_send.c : 908 ] PAPRD Total PHY OFF %d Tx suspend fail %d Rx suspend fail %d Tx suspend %d, Tx suspend %d 
2230,,[ ar_wal_tx_disa_send.c : 253 ] disa  tx_frame   NOT EXPECTED since no status would be recv  
2229,,[ ar_wal_tx_disa_send.c : 116 ] wal_sw_peer_key allocation failed...!!! 
2228,,[ ar_wal_tx_disa_send.c : 119 ] wal_sw_peer_key allocation SUCCESS 
2227,i,[ ar_wal_tx_disa_send.c : 199 ]  DISA tx_frame  tx_buf_count %d   
2226,i,[ ar_wal_tx_disa_send.c : 222 ]  DISA tx_frame  After  Delay tx_buf_count %d   
2225,i,[ ar_wal_tx_disa_send.c : 212 ]  DISA tx_frame  After  Delay tx_buf_count %d   
2231,iI,[ ar_wal_tx_flush.c : 414 ] _wal_peer_flush_tids: send msg to SCHED_ALGO, thread_id =%d tid_bitmap=0x%x
 
2232,i,[ ar_wal_tx_send_isr.c : 495 ] TX_IST_TRIGGER RECEIVED %d
 
2277,I,[ ar_wal_tx_send.c : 11981 ] TX_ABORT FAILED 0x%x 
2276,Ii,[ ar_wal_tx_send.c : 3650 ] tx_send_attach failed 0x%x, line:%d 
2275,iiii,[ ar_wal_tx_send.c : 12335 ] CONSECUTIVE_FLUSH9: pdev id %d,reset_mode %d consecutive flush 9 happen for %d times.Total WAR trigger %d times. 
2274,ii,[ ar_wal_tx_send.c : 16579 ] pdev %d, WIFIMISSING_MPDU_INFO_E cnt: %d
 
2273,i,[ ar_wal_tx_send.c : 16670 ] Retried BAR for %d times, clear BAR flag
 
2272,iI,[ ar_wal_tx_send.c : 16683 ] BAR tx failure tid_num: %d, tid_flags:0x%x
 
2271,II,[ ar_wal_tx_send.c : 16897 ] TX resuming on MAC: %p, %lx
 
2270,III,[ ar_wal_tx_send.c : 16932 ] seq not cleaned ! queue_id:%x, txq:%p, seq_ctrl:%p
 
2269,ii,[ ar_wal_tx_send.c : 10805 ] tx_send_dsr_ppdu_done increment peer->consecutive_eap_cnt : %d, sw_peer_id: %d 
2268,ii,[ ar_wal_tx_send.c : 10812 ] tx_send_dsr_ppdu_done clear peer->consecutive_eap_cnt : %d, sw_peer_id: %d 
2267,Iii,[ ar_wal_tx_send.c : 10826 ] tx_send_dsr_proc_ppdu_done consecutive_pm_filter_cnt %0x %d, %d MAC reset counter
 
2266,iiiIIiii,[ ar_wal_tx_send.c : 10889 ] twt_dbg/ul_tcp: dsr_proc_ppdu_done txqid=%d, sched_id=%d, tx_status=%d, peer=%u, ftype=%u, queued=%d, tried=%d, failed=%d 
 
2265,II,[ ar_wal_tx_send.c : 17586 ] Pause UL ring - wal_txq_id:%x,wal_txq_id_sta_ul:%x 
2264,iiiiiIII,[ ar_wal_tx_send.c : 17602 ] TTL tid:%d ppdu:%d %d,cmd:%d txq_id:%d,flg:%x %x,caller:%x 
2263,iiii,[ ar_wal_tx_send.c : 17458 ] MSDUTTL TQM peer_id:%d deq:%d tid_num:%d qtype:%d 
2262,I,[ ar_wal_tx_send.c : 18440 ] Received GTK frame for Qpeer=%p, but PTK not set 
2261,III,[ ar_wal_tx_send.c : 19379 ] pdev:%u, RING(%x) pause finished(%x) 
2260,III,[ ar_wal_tx_send.c : 19449 ] pdev:%u, pause ring(%x:%x) 
2259,Iiiii,[ ar_wal_tx_send.c : 7997 ] allow_n_flags 0x%x sendn_frms_allowed %d sendn_frms_tried %d subfrms_max %d encap_type %d 
2258,II,[ ar_wal_tx_send.c : 18263 ] peer:%p, tid:16/SSN:16 0x%08x 
2257,II,[ ar_wal_tx_send.c : 18269 ] peer:%p, PN=%X 
2256,I,[ ar_wal_tx_send.c : 6100 ] legacy frame with HT-ctrl, tid=%x 
2255,II,[ ar_wal_tx_send.c : 6400 ] ppdu start time (%u) is in the past of current tsf (%u), deliver 1ms 
2254,iiIiI,[ ar_wal_tx_send.c : 18836 ] tx_send_stop_mu_edca_timer: pdev:%d can't stop muedca timer vdev:%d mu_resp:%08X mu_edca_en:%d ac_bitmap:%08x 
2253,ii,[ ar_wal_tx_send.c : 18864 ] tx_send_stop_mu_edca_timer: pdev:%d ac:%d stop muedca timer and back to legacy edca 
2252,iiIiI,[ ar_wal_tx_send.c : 12931 ] tx_send_stop_muedca_timer: pdev:%d can't stop muedca timer vdev:%d mu_resp:%08X mu_edca_en:%d ac_bitmap:%08x 
2251,,[ ar_wal_tx_send.c : 16306 ] INVALID TPC REGISTER 
 
2250,IIIIIIIII,[ ar_wal_tx_send.c : 14463 ] TXPPDU_0 peerid_tidnum_hwq:0x%08x ppdu_id:0x%08x tstamp:0x%08x%08x dur:%5u sw_sched_id__mpdutried__failed:0x%08x mcs_nss_bw_pream:0x%08x seqnum__sifs__sch:0x%08x tries__fes__flush:0x%08x 
2249,IIIII,[ ar_wal_tx_send.c : 14479 ] TXPPDU_1_064 ssn__basn:0x%08x enq_bitmap:%08x_%08x compl_bitmap:%08x_%08x 
2248,IIIIIIIII,[ ar_wal_tx_send.c : 14493 ] TXPPDU_1_256 ssn__basn:0x%08x compl_bitmap:%08x_%08x_%08x_%08x_%08x_%08x_%08x_%08x 
2247,IIIIII,[ ar_wal_tx_send.c : 14511 ] TXPPDU_2 sched_id:%08x sch_flg:%08x swppdu_flg:%08x msdu_mpdu:%08x tpc:%08x cm:%x 
2246,III,[ ar_wal_tx_send.c : 19311 ] pdev:%u, RING(%x) pause WAR triggered(%x) 
2245,i,[ ar_wal_tx_send.c : 14030 ] delimiter user track: peer:%d runs out of data 
2244,i,[ ar_wal_tx_send.c : 14101 ] delimiter user track: peer:%d runs out of data 
2243,IiiI,[ ar_wal_tx_send.c : 15191 ] TXPPDU_0 ppdu_id:0x%08x sched_result:%d flush_reason:%d uid1__uid2:0x%08x 
2242,IIIiiii,[ ar_wal_tx_send.c : 15298 ] dsr_ppdu_done pdev/FC=%X tid=0x%X cmd_result/flush=0x%X cca=%d tx=%d rx=%d cycle=%d
 
2241,iiIiiiiII,[ ar_wal_tx_send.c : 14703 ] twt_dbg: update_dl_stats txqid=%d, sched_id=%d, ftype=%u, tx_status=%d, queued=%d, tried=%d, failed=%d,sched_ref_time_start=%u, sched_ref_time_end=%u 
 
2240,IIIII,[ ar_wal_tx_send.c : 14739 ] twt_dbg_leak: update_dl_stats: start_tsTstamp=%u, duration_us=%u, sch_eval_end_ts=%u, twt_sp_end=%u, offset_tsf2=%u 
 
2239,I,[ ar_wal_tx_send.c : 14743 ] twt_dbg_leak: update_dl_stats twt_sp leakage detected by %u us 
2238,iiiIIIII,[ ar_wal_tx_send.c : 14775 ] twt_dbg_leak_ul: update_ul_stats: txqid=%d, sched_id=%d, tx_sw_status=%d, fes_start=%u, fes_end=%u, fes_duration=%u, sched_ref_time_start=%u, sched_ref_time_end=%u 
 
2237,IIII,[ ar_wal_tx_send.c : 14810 ] twt_dbg_leak_ul: update_ul_stats: sch_eval_start_ts=%u, sch_eval_end_ts=%u, twt_sp_end=%u, offset_tsf2=%u 
 
2236,I,[ ar_wal_tx_send.c : 14814 ] twt_dbg_leak_ul: update_ul_stats twt_sp leakage detected by %u us 
2235,IIIIIIII,[ ar_wal_tx_send.c : 12777 ] update_hw_wmm_params: ac:%x,ul_resp=%x,txqid=%x,cw_min/cw_max:%x,aifs:%x,type=%x,txop_limit=%x %x 
2234,iIi,[ ar_wal_tx_send.c : 2325 ] update pdev(%d) vdev(%p) wmm params, type=%d 
2233,,[ ar_wal_tx_send.c : 2366 ] MU-EDCA being used while update its WMM parameters. 
2280,,[ ar_wal_tx_seq.c : 4044 ] CW reset 
2279,iiiiiiiI,[ ar_wal_tx_seq.c : 6101 ] 6G FCC: BW recipe state: max_bw_restricted - %d, max_queued_bw - %d, current_transmitted_bw - %d, resp_bw - %d, num_intereference_at_sec[%d/%d/%d], curr_time_us = %ld 
2278,ii,[ ar_wal_tx_seq.c : 6233 ] tx_seq_trigger_ppdu_start_event_isr: can not switch to MUEDCA %d %d 
2287,iiiiiiiii,[ tx_cong_ctrl.c : 278 ] CONGCTRL FW_CONTROL *OVERRIDE* peer_id:%d tid_num:%d traffic_enq:%d drop:%d deq:%d tot_deq:%d rate_max_allowed:%d old_threshold:%d max_extra:%d 
2286,iiiiiiiii,[ tx_cong_ctrl.c : 291 ] CONGCTRL FW_CONTROL *DISABLED* peer_id:%d tid_num:%d traffic_enq:%d drop:%d deq:%d tot_deq:%d rate_max_allowed:%d old_threshold:%d max_extra:%d 
2285,iIiiiiiii,[ tx_cong_ctrl.c : 307 ] CONGCTRL FW_CONTROL peer_id:%d tid_num__qtype__msduq_masks:0x%08x traffic_enq:%d drop:%d deq:%d tot_deq:%d rate_max_allowed:%d old_threshold:%d max_extra:%d 
2284,iiiiii,[ tx_cong_ctrl.c : 51 ] CONG_CTRL_FD sw_pid:%d tid_num:%d buf_id:%d desc_id:%d bin_idx:%d cur:%d 
2283,iii,[ tx_cong_ctrl.c : 69 ] CONG_CTRL_DiscD sw_pid:%d tid_num:%d buf_id:%d 
2282,iiiiii,[ tx_cong_ctrl.c : 57 ] CONG_CTRL_AD sw_pid:%d tid_num:%d buf_id:%d desc_id:%d bin_idx:%d cur:%d 
2281,iii,[ tx_cong_ctrl.c : 63 ] CONG_CTRL_DropD sw_pid:%d tid_num:%d buf_id:%d 
2299,,[ ar_wal_txbf.c : 1367 ] WAL_POWER_STATE_FULL_SLEEP 
2298,,[ ar_wal_txbf.c : 1394 ] WAL_POWER_STATE_AWAKE 
2297,IIII,[ ar_wal_txbf.c : 1260 ] txbf_peer_setup:Peer_caps VHT:SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2296,IIII,[ ar_wal_txbf.c : 1268 ] txbf_peer_setup:Peer_caps HE :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2295,IIII,[ ar_wal_txbf.c : 1276 ] txbf_peer_setup:Vdev_caps VHT :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2294,IIII,[ ar_wal_txbf.c : 1284 ] txbf_peer_setup:Vdev_caps HE :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2293,II,[ ar_wal_txbf.c : 1303 ] txbf_peer_setup:Txbfer:0x%x and txbfee count:0x%x 
2292,IIII,[ ar_wal_txbf.c : 562 ] txbf_peer_teardown:Peer_caps VHT :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2291,IIII,[ ar_wal_txbf.c : 570 ] txbf_peer_teardown:Peer_caps HE :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2290,II,[ ar_wal_txbf.c : 584 ] txbf_peer_setup:Txbfer:0x%x and txbfee count:0x%x 
2289,iI,[ ar_wal_txbf.c : 1341 ] wal_txbf_update_txbfee_filter:en:%d,txbfee_dis_bitmap:0x%x 
2288,ii,[ ar_wal_txbf.c : 952 ] PHY set gid:%d, pos:%d 
2324,IIIIIIII,[ wmi_svc.c : 363 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
2323,III,[ wmi_svc.c : 374 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 
2322,IIII,[ wmi_svc.c : 377 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 
2321,IIIII,[ wmi_svc.c : 380 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
2320,IIIIII,[ wmi_svc.c : 383 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
2319,IIIIIII,[ wmi_svc.c : 386 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
2318,Ii,[ wmi_svc.c : 556 ] WMI_CMD_RX CmdId = 0x%x Length = %d 
2317,III,[ wmi_svc.c : 563 ] WMI Logging debug stats total_drops = 0x%x resume_cnts = 0x%x, suspend_cnts = 0x%x 
2316,I,[ wmi_svc.c : 368 ] WMI_CMD_PARAMS 0x%08x 
2315,I,[ wmi_svc.c : 577 ] WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x 
2314,iiiI,[ wmi_svc.c : 602 ] WMI_CMD_RX process inline cmd=%d length=%d endPt=%d, pHTCbuf=%x 
2313,I,[ wmi_svc.c : 605 ] start page log CmdId = 0x%x  
2312,I,[ wmi_svc.c : 612 ] stop page log CmdId = 0x%x  
2311,iiiIi,[ wmi_svc.c : 643 ] WMI_CMD_RX send dispatch msg to threads, cmd=%d length=%d endPt=%d, pHTCbuf=%x msg_size=%d 
2310,II,[ wmi_svc.c : 371 ] WMI_CMD_PARAMS 0x%08x 0x%08x 
2309,Ii,[ wmi_svc.c : 879 ] WMI_EVT completion msg to RT pEvt=%p, thread_id=%d 
2308,iiI,[ wmi_svc.c : 1780 ] WMI_EVT msg to HIF EventId=%d length=%d pEvt=%p 
2307,Ii,[ wmi_svc.c : 1918 ] WMI_EVENT_SEND EventId = 0x%x ep = %d 
2306,iiIi,[ wmi_svc.c : 1961 ] RT WMI_EVT EventId=%d length=%d pEvt=%p filterAction:%d 
2305,I,[ wmi_svc.c : 2013 ]  pending EventId = 0x%x 
2304,II,[ wmi_svc.c : 2025 ] WMI_EVENT_SEND drop EventId = 0x%x, action:0x%x 
2303,iiiI,[ wmi_svc.c : 837 ] WMI_CMD_RX cmd comp. handle in hif --free buf cmd=%d length=%d endPt=%d, pHTCbuf=%x 
2302,iiiI,[ wmi_svc.c : 774 ] WMI_CMD_RX handle in BE cmd=%d length=%d endPt=%d, pHTCbuf=%x 
2301,iiiI,[ wmi_svc.c : 740 ] WMI_CMD_RX handle in data offload cmd=%d length=%d endPt=%d, pHTCbuf=%x 
2300,iiiI,[ wmi_svc.c : 808 ] WMI_CMD_RX handle in RT cmd=%d length=%d endPt=%d, pHTCbuf=%x 
2325,i,[ evt_tracer.c : 861 ] suspend_en:%d 
2327,Iii,[ platform_page_log.c : 358 ] PF ADDR:0x%X, THREAD:%d, DSR:%d 
2326,Iii,[ platform_page_log.c : 365 ] PF ADDR:0x%X, THREAD:%d, DSR:%d 
2328,II,[ platform_m3.c : 1730 ] M3 DDR address = %ull, size = 0x%x 
2329,,[ platform_ce.c : 112 ] platform_ce_send_use_hif: Sending msg to HIF thread to do SYNC CE copy 
2330,i,[ platform_gpio.c : 248 ] ERR: setting output for input GPIO %d 
2344,I,[ platform_bdf_and_cal.c : 1087 ] Initiating cal download (halphy)...temp_bin = 0x%x 
2343,i,[ platform_bdf_and_cal.c : 1107 ] Cal download complete...cal file size = %d 
2342,Ii,[ platform_bdf_and_cal.c : 1157 ] Initiating cal update (halphy)...temp_bin = 0x%x | file_size = %d 
2341,,[ platform_bdf_and_cal.c : 1295 ] QMI Platform: Cold Cal done signal received 
2340,,[ platform_bdf_and_cal.c : 1347 ] QMI Platform: Sending FW READY ind... 
2339,,[ platform_bdf_and_cal.c : 1361 ] QMI Platform: Sending FW READY ind... 
2338,i,[ platform_bdf_and_cal.c : 679 ] platorm_idx__download_req= %d, 
2337,i,[ platform_bdf_and_cal.c : 514 ] platorm_idx= %d, 
2336,i,[ platform_bdf_and_cal.c : 643 ] platform_proc_bdf_download_req: BDF download done, current_size = %d, 
2335,i,[ platform_bdf_and_cal.c : 603 ] platform_proc_bdf_download_req: BDF download curr_size = %d, 
2334,I,[ platform_bdf_and_cal.c : 292 ] QMI Platform: Cal download REQ received, seg_id 0x%x 
2333,i,[ platform_bdf_and_cal.c : 199 ] QMI Platform: Cal Update remaining bytes = %d, 
2332,,[ platform_bdf_and_cal.c : 1241 ] sending cal_done indication before changing state 
2331,,[ platform_bdf_and_cal.c : 1283 ] QMI Platform: Sending FW READY ind... 
2354,,[ platform_tsens.c : 1097 ] TSENS_MEMORY_ALLOC_FAILED 
2353,iiiiiiii,[ platform_tsens.c : 1115 ] TSENS_PID_GET_CONFIG temp_thresh_1|2|3 %d %d %d kp = %d, ki = %d, kd = %d, max_temp = %d sensor = %d 
2352,iiiiii,[ platform_tsens.c : 1145 ] TSENS_PID_SET_CONFIG algo = %d, temp_thresh_1|2 %d %d, kp = %d, ki = %d, kd = %d 
2351,,[ platform_tsens.c : 1006 ] TSENS_MEMORY_ALLOC_FAILED 
2350,iIIIIIii,[ platform_tsens.c : 1046 ] TSENS_TEMP_INFO algo = %d, err_info = 0x%x 0x%x 0x%x, num_client|num_sensor = 0x%x, temp_zone|sensor_id = 0x%x, tmr_running = %d last_dc = %d 
2349,iiiiiiii,[ platform_tsens.c : 1056 ] TSENS_TEMP_OFFSET [0-7] %d %d %d %d %d %d %d %d 
2348,iiiiiiii,[ platform_tsens.c : 1024 ] TSENS_PID_DATA temp_thresh_1|2|3 %d %d %d kp = %d, ki = %d, kd = %d, max_temp = %d sensor = %d 
2347,iiiiiiii,[ platform_tsens.c : 1034 ] TSENS_TEMP_DATA_DEGC [0-7] %d %d %d %d %d %d %d %d 
2346,iiiiii,[ platform_tsens.c : 1085 ] TSENS_PID_UPDATE_PARAM algo = %d, temp_thresh_1|2 %d %d, kp = %d, ki = %d, kd = %d 
2345,iiiiiiii,[ platform_tsens.c : 989 ] TSENS_PID_DATA temp_thresh_1|2|3 %d %d %d kp = %d, ki = %d, kd = %d, update_temp_thresh_1|2degC %d %d 
2359,iIIIIIIII,[ txde_thread.c : 101 ] %d [RING_STATS:RING_EMPTY]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
2358,iIIIIIIII,[ txde_thread.c : 140 ] %d [RING_STATS:RING_50_75_PER]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
2357,iIIIIIIII,[ txde_thread.c : 153 ] %d [RING_STATS:(RINGSZ - 12)]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
2356,iIIIIIIII,[ txde_thread.c : 114 ] %d [RING_STATS:RING_FULL]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
2355,iIIIIIIII,[ txde_thread.c : 127 ] %d [RING_STATS:RING_0_50_PER]==> 	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x	0x%08x
 
2361,IIi,[ wal_powersave_sta.c : 336 ] _wal_ps_sta_process_rx_event: frame_control=%0x, qos_control=%0x, thread_id=%d 
2360,,[ wal_powersave_sta.c : 351 ] wal_ps_sta_process_rx_event: leaky AP detected 
2372,iiiiii,[ wal_powersave_ap.c : 1391 ] WAL_AP_PS_DBGID_DETECT_OUT_OF_SYNC_STA: vdev_id=%d, AssocID=%d, Timestamp=%d, OldestTxBufferedWaitingMs=%d, detect_thresh=%d, QDepeth=%d 
2371,iI,[ wal_powersave_ap.c : 645 ] wal_ps_ap_sa_thread_msg_handler: peer=%d, cmd_id:%u 
2370,iiii,[ wal_powersave_ap.c : 1526 ] WAL_AP_PS_DBGID_SLEEP_STA_DEC vdev_id = %d num_sleeping_sta:%d is_tid_paused:%d tid_pause_bitmap:%d 
2369,iiii,[ wal_powersave_ap.c : 1467 ] WAL_AP_PS_DBGID_SLEEP_STA_INC vdev_id = %d num_sleeping_sta:%d is_tid_paused:%d tid_pause_bitmap:%d 
2368,iiii,[ wal_powersave_ap.c : 381 ] WAL_AP_PS_DBGID_PSPOLL_REQ AssocID = %d Aid = %d PeerPSEnabled = %d SendNInProgress = %d 
2367,iii,[ wal_powersave_ap.c : 430 ] WAL_AP_PS_DBGID_DUPLICATE_TRIGGER  AssocID = %d SeqNO = %d Tid = %d 
2366,iii,[ wal_powersave_ap.c : 446 ] WAL_AP_PS_DBGID_NO_TRIGGER  AssocID = %d peer_handle->uapsd_trigger_tids = %d Tid = %d 
2365,iIiI,[ wal_powersave_ap.c : 502 ] wal_ps_buf_peer_rx_event_handler(RX): aid=%d, fc=0x%x, seq=%d, timestamp_us=%u 
2364,iIiII,[ wal_powersave_ap.c : 518 ] wal_ps_buf_peer_rx_event_handler(DATA_PPDU): aid=%d, fc=0x%x, seq=%d, qos=0x%x, timestamp_us=%u 
2363,iiii,[ wal_powersave_ap.c : 1234 ] WAL_AP_PS_DBGIG_SET_PARAM vdev_id = %d AssocID = %d Param = %d Value = %d 
2362,iiII,[ wal_powersave_ap.c : 1296 ] WAL_AP_PS_DBGIG_UAPSD_CFG vdev_id = %d AssocID = %d UAPSDTriggerTids = 0x%x UAPSDDeliveryTids = 0x%x 
2386,iii,[ wal_powersave_buf_peer_sm.c : 1169 ] WAL_AP_PS_DBGID_UPDATE_TIM vdev_id = %d AssocID = %d IsTimSet = %d 
2385,iiiii,[ wal_powersave_buf_peer_sm.c : 970 ] WAL_AP_PS_DBGID_NEXT_RESPONSE vdev_id = %d AssocID = %d USPActive = %d PendingUSP = %d PendingPollResp = %d 
2384,iiI,[ wal_powersave_buf_peer_sm.c : 979 ] WAL_AP_PS_DBGID_START_SP vdev_id = %d AssocID = %d last_rx_trigger_time = %u 
2383,iiII,[ wal_powersave_buf_peer_sm.c : 1010 ] WAL_AP_PS_DBGID_COMPLETED_EOSP vdev_id = %d AssocID = %d tx_comp_ts = %u last_rx_trigger_time = %u 
2382,iii,[ wal_powersave_buf_peer_sm.c : 1029 ] WAL_AP_PS_DBGID_COMPLETED_EOSP vdev_id = %d AssocID = %d retried %d 
2381,iiIIii,[ wal_powersave_buf_peer_sm.c : 1061 ] WAL_AP_PS_DBGID_SEND_COMPLETE vdev_id = %d AssocID = %d FrameCtrl = 0x%x QoSCtrl = 0x%x USPActive = %d PendingPollResp = %d 
2380,iiii,[ wal_powersave_buf_peer_sm.c : 1120 ] WAL_AP_PS_DBGID_SEND_N_COMPLETE vdev_id = %d AssocID = %d USPActive = %d PendingPollResp = %d 
2379,iiIii,[ wal_powersave_buf_peer_sm.c : 746 ] WAL_AP_PS_DBGID_TRIGGER vdev_id = %d AssocID = %d A_MILLISECONDS = %u USPActive = %d SendNInProgress = %d 
2378,iiI,[ wal_powersave_buf_peer_sm.c : 759 ] WAL_AP_PS_DBGID_START_SP vdev_id = %d AssocID = %d A_MILLISECONDS = %u 
2377,iiiIIII,[ wal_powersave_buf_peer_sm.c : 480 ] WAL_AP_PS_DBGID_PSPOLL vdev_id = %d AssocID = %d Tid = %d Flags = 0x%x legacy_tidmask = 0x%x allowed_legacy_tidmask = 0x%x pending_legacy_tidmap = 0x%x 
2376,iiiII,[ wal_powersave_buf_peer_sm.c : 492 ] WAL_AP_PS_DBGID_PSPOLL_ERROR vdev_id = %d AssocID = %d TidPaused = %d AllowdLegacyTidMask = 0x%x LegacyTidMask = 0x%x 
2375,iiiiiIII,[ wal_powersave_buf_peer_sm.c : 693 ] WAL_AP_PS_DBGID_UAPSD_RESPONSE vdev_id = %d AssocID = %d Tid = %d NumMPDUToSend = %d need_extra_qnull = %d Flags = 0x%x allow_n_flags_qnull = 0x%x SPLength = 0x%x 
2374,iiIIII,[ wal_powersave_buf_peer_sm.c : 727 ] WAL_AP_PS_DBGID_UAPSD_RESPONSE_ERROR vdev_id = %d AssocID = %d Tid/Paused = 0x%x AllowedUAPSDTidMask = 0x%x PendingTidMap = 0x%x SPLength = 0x%x 
2373,iiIi,[ wal_powersave_buf_peer_sm.c : 1226 ] WAL_AP_PS_DBGID_SYNC_TIM vdev_id = %d AssocID = %d Tids = 0x%x TimSet = %d 
2390,i,[ twt_protocol.c : 398 ] twt_info unexpected: resp_req(%d)!=0 
2389,i,[ twt_protocol.c : 402 ] twt_info unexpected: next_req(%d)!=0 
2388,I,[ twt_protocol.c : 471 ] twt_parse_teardown_frame(!wake_tbtt_nego): twt_flow=%u 
2387,,[ twt_protocol.c : 67 ] twt_power_2_mantissa wrong parameters  
2423,i,[ twt_ap.c : 1696 ] ap_twt_add_i_session(send_failed): status=%d 
2422,ii,[ twt_ap.c : 869 ] ap_twt_del_all_session: peer=%d, status=%d 
2421,ii,[ twt_ap.c : 1746 ] ap_twt_del_dialog[unknown dialog_id]: peer=%d, dialog_id=%d 
2420,i,[ twt_ap.c : 814 ] twt_ap_twt_session_t == NULL, session_id=%d 
2419,i,[ twt_ap.c : 1220 ] %d: AP TWT not initialized on this MAC 
2418,i,[ twt_ap.c : 1226 ] %d: AP TWT: disable cmd cannot find SOC handle 
2417,i,[ twt_ap.c : 829 ] twt_ap_twt_session_t == NULL, session_id=%d 
2416,i,[ twt_ap.c : 1244 ] %d: AP TWT not initialized on this MAC 
2415,i,[ twt_ap.c : 1250 ] %d: AP TWT: disable cmd cannot find SOC handle 
2414,i,[ twt_ap.c : 846 ] twt_ap_twt_session_t == NULL, session_id=%d 
2413,,[ twt_ap.c : 239 ] POOL ALLOC FAILURE 
2412,i,[ twt_ap.c : 564 ] %d: ap_twt_setup_tx_completion: parse_setup_frame error 
2411,ii,[ twt_ap.c : 568 ] ap_twt_setup_tx_completion: status=%d, comp_ctxt=%d 
2410,i,[ twt_ap.c : 1766 ] %d: AP TWT not enabled on this vdev 
2409,i,[ twt_ap.c : 1780 ] %d: AP TWT not enabled on this peer 
2408,i,[ twt_ap.c : 1906 ] %d: AP TWT not enabled on this vdev 
2407,i,[ twt_ap.c : 1917 ] %d: AP TWT peer memory not available on this vdev 
2406,i,[ twt_ap.c : 2866 ] TWT AP Unexpected frame type %d 
2405,i,[ twt_ap.c : 1832 ] %d: AP TWT not enabled on this vdev 
2404,i,[ twt_ap.c : 1841 ] %d: AP TWT not enabled on this peer 
2403,i,[ twt_ap.c : 1969 ] %d: AP TWT not enabled on this peer 
2402,i,[ twt_ap.c : 1975 ] %d: AP TWT not enabled on this vdev 
2401,i,[ twt_ap.c : 1196 ] %d: AP TWT not initialized on this MAC 
2400,i,[ twt_ap.c : 1202 ] %d: AP TWT: disable cmd cannot find SOC handle 
2399,ii,[ twt_ap.c : 2359 ] %d: session not found: session_id=%d 
2398,i,[ twt_ap.c : 3031 ] %d: AP TWT not initialized on this MAC 
2397,i,[ twt_ap.c : 2278 ] %d: AP TWT not enabled on this peer 
2396,i,[ twt_ap.c : 2307 ] TWT AP Unexpected command %d 
2395,i,[ twt_ap.c : 1157 ] %d: AP TWT not initialized on this MAC 
2394,i,[ twt_ap.c : 1167 ] %d: AP TWT disable 
2393,ii,[ twt_ap.c : 1083 ] %d: AP TWT not initialized on this MAC %d 
2392,ii,[ twt_ap.c : 1093 ] %d: AP TWT enable on MAC %d 
2391,iii,[ twt_ap.c : 1031 ] %d: Mismatch between reported number ofsessions %d and actual number of sessions %d 
2427,i,[ twt_ap_session_sm.c : 847 ] sending teardown frame failed: status=%d 
2426,i,[ twt_ap_session_sm.c : 521 ] sending pause frame failed: status=%d 
2425,i,[ twt_ap_session_sm.c : 414 ] sending renego req frame failed: status=%d 
2424,i,[ twt_ap_session_sm.c : 716 ] sending resume frame failed: status=%d 
2432,I,[ twt_ap_adaptor.c : 716 ] TWT_ADD_TIME_POINT: tsf_cnt(%u) >= arr_len 
2431,I,[ twt_ap_adaptor.c : 719 ] TWT_ADD_TIME_POINT: tsf_cnt(%u) >= arr_len 
2430,I,[ twt_ap_adaptor.c : 872 ] TWT_ADD_TIME_POINT: tsf_cnt(%u) >= arr_len 
2429,I,[ twt_ap_adaptor.c : 878 ] TWT_ADD_TIME_POINT: tsf_cnt(%u) >= arr_len 
2428,I,[ twt_ap_adaptor.c : 877 ] TWT_ADD_TIME_POINT: tsf_cnt(%u) >= arr_len 
2440,I,[ twt_ap_btwt.c : 553 ] ap_btwt_check_persist error: b_twt_persistence(%u) > 254 
2439,II,[ twt_ap_btwt.c : 560 ] ap_btwt_check_persist error: reducing more than 1, cur=%u, new=%u 
2438,ii,[ twt_ap_btwt.c : 757 ] %d: session not found: session_id=%d 
2437,i,[ twt_ap_btwt.c : 577 ] ap_btwt_session == NULL, session_id=%d 
2436,,[ twt_ap_btwt.c : 816 ] btwt get session failure 
2435,,[ twt_ap_btwt.c : 384 ] POOL ALLOC FAILURE 
2434,,[ twt_ap_btwt.c : 613 ] btwt get session failure 
2433,i,[ twt_ap_btwt.c : 1065 ] sending pause frame failed: status=%d 
2448,,[ twt_ap_smartwt.c : 498 ] twt_assign_peer POOL ALLOC FAILURE 
2447,,[ twt_ap_smartwt.c : 522 ] twt_assign_peer POOL ALLOC FAILURE 
2446,,[ twt_ap_smartwt.c : 428 ] twt_slot POOL ALLOC FAILURE 
2445,III,[ twt_ap_smartwt.c : 266 ] ap_smartwt_get_slot_idx_start_time_end_time last_slot_extra_dur_us %llu temp %llu diff_in_time %llu 
2444,IIiI,[ twt_ap_smartwt.c : 34 ] <pdev%u-slot%u>: num_peer=%d, flags=0x%x 
2443,IiiI,[ twt_ap_smartwt.c : 40 ] [slot%u]   peer=%d, session=%d, flags=0x%x 
2442,i,[ twt_ap_smartwt.c : 699 ] ap_smartwt_setup_comp(slot_match failed): slot_id=%d 
2441,i,[ twt_ap_smartwt.c : 1632 ] ap_smartwt_setup_teardown_peers(send_failed): status=%d 
2449,iIii,[ wal_beacon.c : 1035 ] vdev:%d adj tbtt:0x%x d:%d by:%d 
2459,,[ wal_swba.c : 671 ] no vaps to send beacon. swba_map is empty 
2458,II,[ wal_swba.c : 762 ] Staggered beacon drift: next_beacon = %u, next_hw_tbtt = %u 
2457,III,[ wal_swba.c : 772 ] Staggered beacon drift recover: next_beacon = %u, beacon_period = %u, until_next_tbtt = %u 
2456,I,[ wal_swba.c : 792 ] cur_tsf %u 
2455,II,[ wal_swba.c : 873 ] Burst beacon drift: next_beacon = %u, next_hw_tbtt = %u 
2454,III,[ wal_swba.c : 883 ] Burst beacon drift recover: next_beacon = %u,                                         beacon_period = %u, until_next_tbtt = %u 
2453,IIIIII,[ wal_swba.c : 737 ] swba_intr: misc=0x%x,period=%u,tsf=%u,tbtt-curr=%u/next=%u,diff=%u 
2452,,[ wal_swba.c : 275 ] next beacon tsf slot is not proper 
2451,IIII,[ wal_swba.c : 1602 ] _wal_swba_set_and_fire: cur_tsf=0x%x sta_offset=0x%x next_beacon=0x%x next_beacon_slot=%u 
2450,iiii,[ wal_swba.c : 1209 ] Fils is already enabled on some other vdev. fils_period %d vdev_id %d old_fils_period %d old_vdev_id %d 
2463,I,[ wal_chain_mgmt.c : 71 ] WAL_DBGID_GET_HW_CHAINMASK SHIFTED_RF_CM: Rx:0x%x  
2462,I,[ wal_chain_mgmt.c : 54 ] WAL_DBGID_GET_HW_CHAINMASK SHIFTED_RF_CM: Tx:0x%x  
2461,II,[ wal_chain_mgmt.c : 36 ] WAL_DBGID_GET_HW_CHAINMASK  Tx:0x%x Rx:0x%x 
2460,III,[ wal_chain_mgmt.c : 166 ] WAL_DBGID_SET_HW_CHAINMASK 0x%x 0x%x 0x%x 
2464,i,[ wal_channel_change.c : 124 ] _wal_set_home_channel : num home chans = %d 
2470,,[ wal_cold_boot_cal.c : 478 ] cold boot cal start 
2469,iiiii,[ wal_cold_boot_cal.c : 603 ] CBC:: pdev %d phy_mode %d mhz %d freq1 %d freq2 %d 
2468,I,[ wal_cold_boot_cal.c : 666 ] CBC:: Total time taken for CBC = %u us 
2467,iI,[ wal_cold_boot_cal.c : 529 ] CBC:: phy mode %d cal duration so far %u us 
2466,i,[ wal_cold_boot_cal.c : 553 ] Cold Boot Cal, 8 second timeout: actual time taken = %d 
2465,i,[ wal_cold_boot_cal.c : 271 ] cold_boot_cal start time in USecs: %d 
2481,iiiIIII,[ wal_concurrency.c : 526 ] tsf_alloc: pdev_id = %d vdev_id = %d type = %d tsf_id = 0x%x bss_id = 0x%x pdev_tsf_id_map = 0x%x pdev_bss_id_map = 0x%x 
2480,iiIIIiII,[ wal_concurrency.c : 987 ] staid_alloc: pdev_id = %d vdev_id = %d (%x.%x.%x) type = %d sta_id = 0x%x pdev_sta_id_map = 0x%x 
2479,iiIIIiII,[ wal_concurrency.c : 1099 ] staid_free: pdev_id = %d vdev_id = %d (%x.%x.%x) type = %d sta_id = 0x%x pdev_sta_id_map = 0x%x 
2478,ii,[ wal_concurrency.c : 1030 ] wal_concurrency_vdev_attach: vdev_id = %d defer_mac_addr_reg = %d 
2477,iiiIIII,[ wal_concurrency.c : 835 ] tsf_free: pdev_id = %d vdev_id = %d type = %d tsf_id = 0x%x bss_id = 0x%x pdev_tsf_id_map = 0x%x pdev_bss_id_map = 0x%x 
2476,iiIII,[ wal_concurrency.c : 1540 ] wal_vdev_add_random_mac_addr: pdev_id = %d vdev_id = %d spoof_mac=%x.%x.%x 
2475,iiIII,[ wal_concurrency.c : 1582 ] wal_vdev_del_random_mac_addr: pdev_id = %d vdev_id = %d spoof_mac=%x.%x.%x 
2474,IiiiIIII,[ wal_concurrency.c : 617 ] tsf_realloc (flag=0x%x): pdev_id = %d vdev_id = %d type = %d tsf_id = 0x%x bss_id = 0x%x pdev_tsf_id_map = 0x%x pdev_bss_id_map = 0x%x 
2473,iiiII,[ wal_concurrency.c : 1470 ] wal_vdev_restore_mac: pdev_id = %d vdev_id = %d spoof_type = %d sta_id = 0x%x spoof_sta_id=0x%x 
2472,iiIIIIII,[ wal_concurrency.c : 1489 ] wal_vdev_set_mac_addr: pdev_id = %d vdev_id = %d mac=%02x:%02x:%02x:%02x:%02x:%02x 
2471,iiIIIiII,[ wal_concurrency.c : 1390 ] wal_vdev_set_spoofed_mac_addr: pdev_id = %d vdev_id = %d spoof_mac=%x.%x.%x spoof_type=%d sta_id = 0x%x spoof_sta_id=0x%x 
2510,IIIiiI,[ ar_wal_phy_dev.c : 1584 ] _wal_dev_reset: mode=%x,c0=%lx,c1=%lx,inprog=%d,dis=%d,en=%x 
2509,ii,[ ar_wal_phy_dev.c : 4846 ] SMART ANTENNA : config_enable : %d config_mode : %d 
 
2508,,[ ar_wal_phy_dev.c : 526 ] Data stall force reset condition met 
2507,iii,[ ar_wal_phy_dev.c : 567 ] DATA_STALL: Type=%d FAIL_CNT[%d]=%d 
2506,i,[ ar_wal_phy_dev.c : 318 ] DATA_STALL detection: PAUSE, pdev_id:%d 
2505,iii,[ ar_wal_phy_dev.c : 797 ] DATA_STALL monitor: TIMEOUT, pdev_id:%d pause_countdown:%d active_vdev_cnt:%d 
2504,i,[ ar_wal_phy_dev.c : 3029 ] wal_pdev_flush_all_non_pause_tids: send msg to SCHED_ALGO, thread_id =%d
 
2503,IIIIII,[ ar_wal_phy_dev.c : 5753 ] DISPLAY_TPC_STATS: ctl_array_type is %lu ctl_array_len is %lu d1 is %lu d2 is %lu d3 is %lu d4 is %lu 
2502,,[ ar_wal_phy_dev.c : 5782 ] DISPLAY_TPC_STATS: CTL array contents do not match! 
2501,,[ ar_wal_phy_dev.c : 5807 ] DISPLAY_TPC_STATS: CTL array contents do not match! 
2500,II,[ ar_wal_phy_dev.c : 5628 ] DISPLAY_TPC_STATS: rate_array_type is %lu rate_array_len is %lu 
2499,,[ ar_wal_phy_dev.c : 5652 ] DISPLAY_TPC_STATS: Rates array contents do not match! 
2498,I,[ ar_wal_phy_dev.c : 5415 ] DISPLAY_TPC_STATS: wal_pdev_get_ctl_array_len totalSize = %lu 
2497,I,[ ar_wal_phy_dev.c : 5440 ] DISPLAY_TPC_STATS: wal_pdev_get_rates_array_len:  totalSize = %lu 
2496,ii,[ ar_wal_phy_dev.c : 335 ] DATA_STALL: rssi:%d vdev_id:%d 
2495,IIIIII,[ ar_wal_phy_dev.c : 5509 ] DISPLAY_TPC_STATS: reg_power_type is %lu reg_power_array_len is %lu d1 is %lu d2 is %lu d3 is %lu d4 is %lu 
2494,,[ ar_wal_phy_dev.c : 5535 ] DISPLAY_TPC_STATS: Regulatory array contents do not match! 
2493,,[ ar_wal_phy_dev.c : 5550 ] DISPLAY_TPC_STATS: Regulatory array contents do not match! 
2492,,[ ar_wal_phy_dev.c : 5567 ] DISPLAY_TPC_STATS: Regulatory array contents do not match! 
2491,,[ ar_wal_phy_dev.c : 5584 ] DISPLAY_TPC_STATS: Regulatory array contents do not match! 
2490,III,[ ar_wal_phy_dev.c : 5366 ] DISPLAY_TPC_STATS: wmi_tpc_config tlv header is %lu, chanFreq is %lu, phyMode is %lu 
2489,IIiIIIII,[ ar_wal_phy_dev.c : 5368 ] DISPLAY_TPC_STATS: maxAntennaGain is %lu twiceMaxRDPower is %lu userAntennaGain is %d powerLimit is %lu rateMax is %lu numTxChain is %lu cfgctl is %lu flags is %lu 
2488,iiI,[ ar_wal_phy_dev.c : 3134 ] SU PPDU_DURATION %d AMSDU agg_type %d amsdu_factor %f 
2487,iiI,[ ar_wal_phy_dev.c : 3135 ] MU PPDU_DURATION %d AMSDU agg_type %d amsdu_factor %f 
2486,iII,[ ar_wal_phy_dev.c : 2691 ] WAL_DBGID_SET_POWER_STATE pdev = %d current = 0x%x desired = 0x%x 
2485,iiI,[ ar_wal_phy_dev.c : 3279 ] SET_PDEV_PARAM: pdev_id=%d: param=%d value=0x%x 
2484,i,[ ar_wal_phy_dev.c : 3843 ] SET_PDEV_PARAM: DATA_STALL flag param=%d 
2483,ii,[ ar_wal_phy_dev.c : 4856 ] SMART ANTENNA : config_enable : %d rx_antenna : %d 
 
2482,i,[ ar_wal_phy_dev.c : 6049 ] VOW enable %d 
2556,i,[ ar_wal_vdev.c : 907 ] start hwbmiss delay wake tmr, timeout:%d 
2555,III,[ ar_wal_vdev.c : 6699 ] AWGN_INT_DBG bw = 0x%x ed = 0x%x gi = 0x%x
 
2554,ii,[ ar_wal_vdev.c : 214 ] WAL_DBGID_VDEV_ADDR_REGISTER vdev_id = %d pdev_id = %d 
2553,ii,[ ar_wal_vdev.c : 227 ] WAL_DBGID_VDEV_ADDR_UNREGISTER vdev_id = %d pdev_id = %d 
2552,ii,[ ar_wal_vdev.c : 6523 ] wal_vdev_delete_all_peer_msg_hdlr:  thread_id =%d, vdev_id=%d
 
2551,ii,[ ar_wal_vdev.c : 6453 ] wal_vdev_delete_all_peer_resume: vdev = %d, delete_all_peer_in_progress %d 
 
2550,i,[ ar_wal_vdev.c : 6475 ] wal_vdev_delete_all_peer_resume: vdev = %d, set WAL_VDEV_DEL_ALL_PEER_CONF_FROM_LOCAL_FRAME_COMPL 
 
2549,iii,[ ar_wal_vdev.c : 6488 ] wal_vdev_delete_all_peer_resume: vdev = %d, thread_id = %d, msg_id = %d 
 
2548,iii,[ ar_wal_vdev.c : 6494 ] wal_vdev_delete_all_peer_resume: vdev = %d, thread_id = %d, msg_id = %d 
 
2547,iiiIi,[ ar_wal_vdev.c : 2332 ] wal_vdev_down pdev_id %d vdev_id %d vdev_type %d flags 0x%x cnt_per_opmode %d 
2546,,[ ar_wal_vdev.c : 2410 ] AWGN_INT_DBG vdev_down clearing timer handler 
2545,I,[ ar_wal_vdev.c : 4612 ] %s: NULL pointer 
 
2544,II,[ ar_wal_vdev.c : 384 ] flow_config:0x%x 0x%x 
2543,iiI,[ ar_wal_vdev.c : 6624 ] delete_all_peer wal_vdev_free_event_confirmation: vdev_id=%d, flag = %d, vdev_flag_mask = %x
 
2542,iiiiiii,[ ar_wal_vdev.c : 6630 ] delete_all_peer wal_vdev_free_event_confirmation: vdev_id=%d, dbg_rt_del_all_peer_num=%d, dbg_be_del_all_peer_num=%d, dbg_tx_de_del_all_peer_num=%d, dbg_sched_del_all_peer_num=%d, dbg_tqm_del_all_peer_num=%d, dbg_conf_del_all_peer_num = %d
 
2541,iii,[ ar_wal_vdev.c : 6646 ] delete_all_peer wal_vdev_free_event_confirmation DEL_ALL_PEER_DEL_CONF: vdev_id=%d, thread_id = %d, msg_id = %d
 
2540,iii,[ ar_wal_vdev.c : 6657 ] vdev_id:%d, prev_channel:%d, current_channel=%d 
2539,iIiiii,[ ar_wal_vdev.c : 5541 ] wal_vdev_migrate (%d, 0x%x): pdev %d->%d, active=%d/%d 
2538,ii,[ ar_wal_vdev.c : 5362 ] _wal_vdev_migrate_bring_up: vdev_id = %d rssi_beacon = %d 
2537,iIII,[ ar_wal_vdev.c : 5398 ] _wal_vdev_migrate_bring_up: vdev_id = %d cur_tsf_64 = 0x%x sta_bss_tstamp = 0x%x time_at_sta_bss_tstamp = 0x%x 
2536,ii,[ ar_wal_vdev.c : 5277 ] _wal_vdev_migrate_tear_down: vdev_id = %d rssi_beacon = %d 
2535,iII,[ ar_wal_vdev.c : 5292 ] _wal_vdev_migrate_tear_down: vdev_id = %d sta_bss_tstamp = 0x%x time_at_sta_bss_tstamp = 0x%x 
2534,iIi,[ ar_wal_vdev.c : 350 ] wal_vdev_event_handler: vdev_id=%d event_type=0x%x remote_peer_count=%d 
2533,,[ ar_wal_vdev.c : 186 ] peer_bitmap POOL ALLOC FAILURE 
2532,ii,[ ar_wal_vdev.c : 5224 ] wal_vdev_post_migrate - old_pdev is %d, new_pdev is = %d 
2531,ii,[ ar_wal_vdev.c : 5087 ] wal_vdev_pre_migrate - old_pdev is %d, new_pdev is = %d 
2530,ii,[ ar_wal_vdev.c : 1285 ] wal_vdev_reconfig vdev_id %d  tsf_id is %d 
2529,iII,[ ar_wal_vdev.c : 2546 ] [ERP_PROTECTION]: param_val %d default profile 0x%x new profile 0x%x 
2528,ii,[ ar_wal_vdev.c : 2765 ] WAL_VDEV_PARAM_HE_RTS_THRESHOLD_TU: new_rts_thres=%d vdev_id=%d 
2527,Ii,[ ar_wal_vdev.c : 2979 ] #### NEW_STATS MGMT_HDR_dbg monitor vdev %x packet_capture_mode %d #### 
2526,i,[ ar_wal_vdev.c : 2990 ] #### stale_period_sec %d #### 
2525,i,[ ar_wal_vdev.c : 2995 ] #### mcast_dra_enabled %d #### 
2524,iIII,[ ar_wal_vdev.c : 3468 ] WAL_DBGID_SETUP_RSSI_INTERRUPTS vdev_id = %d 0x%x 0x%x 0x%x 
2523,iiii,[ ar_wal_vdev.c : 1728 ] wal_vdev_start vdev_id %d vdev_type %d vdev's mac %dbss_peer %d 
2522,,[ ar_wal_vdev.c : 6131 ] _wal_vdev_state_publish: Entry  
2521,ii,[ ar_wal_vdev.c : 6135 ] _wal_vdev_state_publish: bytes is %d, less than output size = %d  
2520,i,[ ar_wal_vdev.c : 6142 ] _wal_vdev_state_publish: vdev_id_map %d  
2519,i,[ ar_wal_vdev.c : 6147 ] _wal_vdev_state_publish: vdev  %d  
2518,ii,[ ar_wal_vdev.c : 6173 ] _wal_vdev_state_publish: vdev_type_state is %d, vdev_id_state = %d  
2517,iiiiii,[ ar_wal_vdev.c : 6182 ] _wal_vdev_state_publish: mac_address is %d:%d:%d:%d:%d:%d  
2516,,[ ar_wal_vdev.c : 6187 ] _wal_vdev_state_publish: Exit  
2515,i,[ ar_wal_vdev.c : 1854 ] Spectral disabled as vdevs are zero: pdev:%d  
2514,ii,[ ar_wal_vdev.c : 1871 ] wal_vdev_stop vdev_id %d vdev_type %d 
2513,IIIIII,[ ar_wal_vdev.c : 2165 ] pdev(%x)peer %x,vdev-up for tidLen update,refcnt=%x,htc=%x,remap=%x,security=%x 
2512,,[ ar_wal_vdev.c : 2271 ] AWGN_INT_DBG vdev_up: type AWGN Timer initialised
 
2511,iiiIi,[ ar_wal_vdev.c : 2262 ] wal_vdev_up: pdev_id %d vdev_id %d, vdev_type %d flags 0x%x cnt_per_opmode %d 
2566,,[ ar_wal_soc_dev.c : 2065 ] _wal_soc_pkt_info_run_algo: No monitored phy mode or device in sleep mode, enabled pktlog.
 
2565,iiiiii,[ ar_wal_soc_dev.c : 2120 ] pktlog from %d to %d: tx_msdu %d, threshold %d, tx_ppdu %d, threshold %d.
 
2564,iiiiii,[ ar_wal_soc_dev.c : 2129 ] pktlog from %d to %d: rx_msdu %d, threshold %d, rx_ppdu %d, threshold %d.
 
2563,iiiiiii,[ ar_wal_soc_dev.c : 2138 ] pktlog from %d to %d: tx_msdu %d, sum_msdu %d, threshold %d, sum_ppdu %d, threshold %d.
 
2562,IIII,[ ar_wal_soc_dev.c : 2268 ] _wal_soc_register_pkt_info_handler 0x%x, 0x%x, 0x%x, 0x%x 
2561,ii,[ ar_wal_soc_dev.c : 718 ] wal_soc_set_mac_active: nss applied for mac0 -  %d and %d 
2560,iiiii,[ ar_wal_soc_dev.c : 756 ] wal_soc_set_mac_active: mhz=%d mac_id=%d  tx_resumed=%d last_pdev_state=%d dpd_cal=%d 
2559,i,[ ar_wal_soc_dev.c : 1064 ] wal_soc_switch_mode: Start switching to mode = %d 
2558,iiii,[ ar_wal_soc_dev.c : 1088 ] wal_soc_switch_mode: mac_id=%d Tx/Rx chainmask: %d %d pdev_state = %d 
2557,IIII,[ ar_wal_soc_dev.c : 2316 ] _wal_soc_unregister_pkt_info_handler 0x%x, 0x%x, 0x%x, 0x%x 
2611,i,[ wal_dfs.c : 1173 ] Clear NOL list %d 
2610,,[ wal_dfs.c : 1176 ] 2G band : NOL is invalid 
2609,ii,[ wal_dfs.c : 1187 ] removing NOL %d MHz / %d MHz 
2608,i,[ wal_dfs.c : 377 ] DFS Domain=%d  
2607,,[ wal_dfs.c : 928 ]  DFS wal_dfs_disable_nol_tx_timeout_hdlr Blocking all tx activity Timer Triggered for 1 min  
2606,iiiiii,[ wal_dfs.c : 735 ] seg=%d, sidx=%d, offset=%d, chirp=%d, phy_mode=%d, f=%d 
2605,iiii,[ wal_dfs.c : 741 ] su_center_chan =%d ,freq1 = %d, freq2 = %d, offset=%d 
2604,i,[ wal_dfs.c : 753 ] 20MHZ=%d  
2603,i,[ wal_dfs.c : 761 ] 40MHZ=%d  
2602,i,[ wal_dfs.c : 775 ] 80MHZ=%d  
2601,i,[ wal_dfs.c : 778 ] channel phy_mode=%d is invalid 
2600,iii,[ wal_dfs.c : 790 ] offset=%d, chan_freq=%d, f=%d 
2599,I,[ wal_dfs.c : 436 ] b20MHZ=0x%x 
2598,I,[ wal_dfs.c : 477 ] b160MHZ=0x%x 
2597,iiiiiiiii,[ wal_dfs.c : 495 ] 160 MHZ ADFS FW NOL - center freq %d %d %d %d %d %d %d %d %d 
2596,iiiii,[ wal_dfs.c : 513 ] 165 MHz ADFS FW NOL Freq1  %d %d %d %d %d 
2595,iiii,[ wal_dfs.c : 521 ] center_chan =%d ,freq1 = %d, freq2 = %d, phymode = %d 
2594,I,[ wal_dfs.c : 442 ] b40MHZ=0x%x 
2593,I,[ wal_dfs.c : 451 ] b80MHZ=0x%x 
2592,iiii,[ wal_dfs.c : 463 ] NOL - 80_80 MHz %d %d %d %d
 
2591,i,[ wal_dfs.c : 392 ] current Channel in DFS=%d  
2590,,[ wal_dfs.c : 1069 ] dfs is NULL  
2589,,[ wal_dfs.c : 1074 ]  adfs list is empty 
2588,ii,[ wal_dfs.c : 1085 ] update NOL %d MHz / %d MHz 
2587,iiIi,[ wal_dfs.c : 1116 ] new NOL channel %d MHz / %d MHz, %llu, threadid = %d 
2586,,[ wal_dfs.c : 1122 ] failed to allocate memory for nol entry 
2585,ii,[ wal_dfs.c : 1317 ] check NOL %d MHz / %d MHz 
2584,,[ wal_dfs.c : 1330 ] NOL check Failed 
2583,ii,[ wal_dfs.c : 1336 ] wal_dfs_nol_checknol: num %d, status=%d 
2582,ii,[ wal_dfs.c : 1248 ] delete NOL %d MHz / %d MHz 
2581,,[ wal_dfs.c : 1259 ] dfs_nol_count < 0 
2580,i,[ wal_dfs.c : 1208 ] FreeElem %d 
2579,ii,[ wal_dfs.c : 1219 ] removing NOL %d MHz / %d MHz 
2578,,[ wal_dfs.c : 1135 ] DFS_DBG wal_dfs_print_nol dfs is NULL 
2577,iiiII,[ wal_dfs.c : 1151 ] DFS_DBG wal_dfs_print_nol nol:%d channel=%d MHz width=%d MHz time left=%u seconds nol starttick=%llu 
2576,Ii,[ wal_dfs.c : 1153 ] DFS_DBG wal_dfs_print_nol timeout=%llu pdev_id %d 
2575,ii,[ wal_dfs.c : 1635 ] DFS segment Id %d offset %d 
2574,i,[ wal_dfs.c : 1651 ] Invalid num channels: %d 
2573,I,[ wal_dfs.c : 1677 ] ch_freq=0x%x Added to NOL 
2572,i,[ wal_dfs.c : 1797 ] res TX Status=%d 
2571,i,[ wal_dfs.c : 1760 ] res SCHED Status=%d 
2570,ii,[ wal_dfs.c : 326 ] WAL_DFS_SCHED_SUSPEND_HNDLR thrd_id = %d pdev_id = %d 
2569,II,[ wal_dfs.c : 344 ] %s: thread_id=%lx received DFS_SUSPEND msg
 
2568,i,[ wal_dfs.c : 1732 ] sus TX Status=%d 
2567,,[ wal_dfs.c : 846 ]  DFS WAL_PDEV_PARAM_SET_USE_NOL command received, Triggered Timer 
2618,I,[ wal_disa.c : 76 ] crc32_calc: CRC=0x%08x 
2617,I,[ wal_disa.c : 433 ] tx_send_disa_frame: Seq No = 0x%x 
2616,,[ wal_disa.c : 460 ] No MEMORY for DISA frame!!! 
2615,i,[ wal_disa.c : 446 ] DISA HW configuration failed!!! Status=%d 
2614,,[ wal_disa.c : 132 ] disa_frm_buf allocation failed...!!! 
2613,ii,[ wal_disa.c : 135 ] disa_frm_buf allocation success...%d  %d !!! 
2612,,[ wal_disa.c : 368 ] _wal_disa_prepare_80211_frame: QoS frame with order bit set to 1 
2655,Ii,[ ar_wal_connection_pause.c : 1845 ] Tx_Pause: WAL_PEER_EVENT_SEND_N_COMPLETE sent: peer:0X%x, tid_num:%d 
2654,,[ ar_wal_connection_pause.c : 3108 ] POOL ALLOC FAILURE 
2653,,[ ar_wal_connection_pause.c : 3648 ] wal_tx_pause_alloc_handle POOL ALLOC FAILURE 
2652,IiiI,[ ar_wal_connection_pause.c : 3399 ] Tx_Pause: WAL_PEER_SEND_N_REQ rcvd: peer:0X%x, tidno:%d, num_frames:%d, flags:0X%x [No_Resp] 
2651,I,[ ar_wal_connection_pause.c : 3481 ] Tx_Pause: WAL_TX_PAUSE_PEER_RESET rcvd: peer:0X%x [No_Resp] 
2650,i,[ ar_wal_connection_pause.c : 3491 ] Tx_Pause: WAL_TX_PAUSE_HWQ_EMPTY rcvd: tid_num:%d [No_Resp] 
2649,i,[ ar_wal_connection_pause.c : 3501 ] Tx_Pause: WAL_CHECK_PENDING_CMDS_VDEV rcvd: vdev_id:%d [No_Resp] 
2648,i,[ ar_wal_connection_pause.c : 3511 ] Tx_Pause: WAL_CHECK_PENDING_CMDS_PDEV rcvd: pdev_id:%d [No_Resp] 
2647,i,[ ar_wal_connection_pause.c : 3519 ] Tx_Pause: unsupported no-resp request id:%d 
2646,IiiI,[ ar_wal_connection_pause.c : 3440 ] Tx_Pause: WAL_PEER_PS_PRE_REQ rcvd: peer:0X%x, force_ps:%d, pm_ts:%d, paused_tidmask:0X%x  [No_Resp] 
2645,i,[ ar_wal_connection_pause.c : 3450 ] Tx_Pause: WAL_VDEV_TX_PAUSE_RESET_IND rcvd: vdev_id:%d [No_Resp] 
2644,Ii,[ ar_wal_connection_pause.c : 3461 ] Tx_Pause: WAL_TX_PAUSE_TID_CREATE rcvd: peer:0X%x, tid_num:%d [No_Resp] 
2643,i,[ ar_wal_connection_pause.c : 3471 ] Tx_Pause: WAL_TX_PAUSE_VDEV_CREATE rcvd: vdev_id:%d [No_Resp] 
2642,iiii,[ ar_wal_connection_pause.c : 3137 ] Tx_Pause: WAL_PDEV_TX_PAUSE_REQ rcvd: pdev_id:%d, module_id:%d, block:%d, filter:%d 
2641,iii,[ ar_wal_connection_pause.c : 3166 ] Tx_Pause: WAL_PDEV_TX_UNPAUSE_REQ rcvd: pdev_id:%d, module_id:%d, block:%d 
2640,i,[ ar_wal_connection_pause.c : 3186 ] Tx_Pause: unsupported pdev request id:%d 
2639,IiIIi,[ ar_wal_connection_pause.c : 3277 ] Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_REQ rcvd: peer:0X%x, module_id:%d, tids_to_pause:0X%x, tids_to_unpause:0X%x, filter:%d 
2638,IiIIi,[ ar_wal_connection_pause.c : 3330 ] Tx_Pause: WAL_PEER_TX_BLOCK_UNBLOCK_REQ rcvd: peer:0X%x, module_id:%d, tids_to_block:0X%x, tids_to_unblock:0X%x, filter:%d 
2637,i,[ ar_wal_connection_pause.c : 3359 ] Tx_Pause: unsupported peer request id:%d 
2636,IiII,[ ar_wal_connection_pause.c : 2408 ] Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_COMPLETE sent: peer:0X%x, module_id:%d, tids_to_pause:0X%x, tids_to_unpause:0X%x 
2635,IiII,[ ar_wal_connection_pause.c : 2439 ] Tx_Pause: WAL_PEER_TX_BLOCK_UNBLOCK_COMPLETE sent: peer:0X%x, module_id:%d, tids_to_block:0X%x, tids_to_unblock:0X%x 
2634,iii,[ ar_wal_connection_pause.c : 2467 ] Tx_Pause: WAL_VDEV_TX_PAUSE_COMPLETE sent: vdev_id:%d, module_id:%d, block:%d 
2633,iii,[ ar_wal_connection_pause.c : 2494 ] Tx_Pause: WAL_VDEV_TX_UNPAUSE_COMPLETE sent: vdev_id:%d, module_id:%d, block:%d 
2632,iii,[ ar_wal_connection_pause.c : 2521 ] Tx_Pause: WAL_PDEV_TX_PAUSE_COMPLETE sent: pdev_id:%d, module_id:%d, block:%d 
2631,iii,[ ar_wal_connection_pause.c : 2548 ] Tx_Pause: WAL_PDEV_TX_UNPAUSE_COMPLETE sent: pdev_id:%d, module_id:%d, block:%d 
2630,IiII,[ ar_wal_connection_pause.c : 2586 ] Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_REQ comp: peer:0X%x, module_id:%d, tids_to_pause:0X%x, tids_to_unpause:0X%x 
2629,IiII,[ ar_wal_connection_pause.c : 2599 ] Tx_Pause: WAL_PEER_TX_BLOCK_UNBLOCK_REQ comp: peer:0X%x, module_id:%d, tids_to_block:0X%x, tids_to_unblock:0X%x 
2628,iii,[ ar_wal_connection_pause.c : 2610 ] Tx_Pause: WAL_VDEV_TX_PAUSE_REQ comp: vdev_id:%d, module_id:%d, block:%d 
2627,iii,[ ar_wal_connection_pause.c : 2621 ] Tx_Pause: WAL_VDEV_TX_UNPAUSE_REQ comp: vdev_id:%d, module_id:%d, block:%d 
2626,iii,[ ar_wal_connection_pause.c : 2632 ] Tx_Pause: WAL_PDEV_TX_PAUSE_REQ comp: pdev_id:%d, module_id:%d, block:%d 
2625,iii,[ ar_wal_connection_pause.c : 2643 ] Tx_Pause: WAL_PDEV_TX_UNPAUSE_REQ comp: pdev_id:%d, module_id:%d, block:%d 
2624,iiii,[ ar_wal_connection_pause.c : 3209 ] Tx_Pause: WAL_VDEV_TX_PAUSE_REQ rcvd: vdev_id:%d, module_id:%d, block:%d, filter:%d 
2623,iii,[ ar_wal_connection_pause.c : 3229 ] Tx_Pause: WAL_VDEV_TX_UNPAUSE_REQ rcvd: vdev_id:%d, module_id:%d, block:%d 
2622,i,[ ar_wal_connection_pause.c : 3240 ] Tx_Pause: unsupported vdev request id:%d 
2621,iiiI,[ ar_wal_connection_pause.c : 3787 ] tid_pause_data_stall tid_num:%d pause_module_id_map:%d block_module_id_map:%d peer:0X%x 
2620,I,[ ar_wal_connection_pause.c : 2229 ] Tx_Pause: Pdev event PEER_CREATE for peer:0X%x rcvd 
2619,i,[ ar_wal_connection_pause.c : 3564 ] Tx_Pause: unsupported request id:%d 
2663,Iii,[ wal_avg_bmiss.c : 140 ] %p bcn_cnt:%d, bmiss_cnt:%d
 
2662,I,[ wal_avg_bmiss.c : 164 ] %p enter high bmiss mode 
2661,I,[ wal_avg_bmiss.c : 142 ] b:0x%08x
 
2660,I,[ wal_avg_bmiss.c : 158 ] %p can't find vdev
 
2659,Iii,[ wal_avg_bmiss.c : 195 ] %p bcn_cnt:%d, bmiss_cnt:%d
 
2658,I,[ wal_avg_bmiss.c : 197 ] b:0x%08x
 
2657,I,[ wal_avg_bmiss.c : 215 ] %p can't find vdev
 
2656,I,[ wal_avg_bmiss.c : 223 ] %p enter low bmiss mode 
2671,ii,[ wal_rc_peer.c : 2400 ] rx cck Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
2670,ii,[ wal_rc_peer.c : 2231 ] rx mcs 3d Stats publish :: input buffer size = %d 3d stats buffer size = %d 
2669,iiI,[ wal_rc_peer.c : 2327 ] rx mcs Stats publish :: input buffer size = %d mcs stats buffer size = %d, nss:8/bw:8 0x%08x 
2668,ii,[ wal_rc_peer.c : 2364 ] rx ofdm Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
2667,ii,[ wal_rc_peer.c : 2472 ] tx cck Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
2666,ii,[ wal_rc_peer.c : 2189 ] tx mcs 3d Stats publish :: input buffer size = %d 3d stats buffer size = %d 
2665,iiI,[ wal_rc_peer.c : 2280 ] tx mcs Stats publish :: input buffer size = %d mcs stats buffer size = %d, nss:8/bw:8 0x%08x 
2664,ii,[ wal_rc_peer.c : 2436 ] tx ofdm Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
2673,II,[ wal_rc_vdev.c : 600 ] RATECTRL_DBGID_WAL_SET_VDEV_DATA_RX: rc=0x%x data_rc=0x%x 
2672,II,[ wal_rc_vdev.c : 125 ] RATECTRL_DBGID_WAL_SET_VDEV_DATA_RX  rc=0x%x data_rc=0x%x 
2674,iii,[ wal_rc_pdev.c : 723 ] SET tx_chain_mask[%d]: new=%d old=%d 
2721,iii,[ wal_rtt.c : 169 ] Detected Outlier. i: %d rtt: %d bw: %d 
2720,iiii,[ wal_rtt.c : 234 ] chain: %d cumilative_rtt_per_chain: %d, num_samples: %d min_mean_rtt: %d 
2719,ii,[ wal_rtt.c : 2166 ] _wal_collect_report_info: pre %d bw %d 
2718,IIi,[ wal_rtt.c : 1667 ] _wal_report_type2_buffer_done() buff = %p, curr: %p len: %d 
2717,IIii,[ wal_rtt.c : 1650 ] _wal_report_type2_buffer_init buff = %p cur_p = %p chan = %d report_type = %d 
2716,iiiiii,[ wal_rtt.c : 2344 ] _wal_report_type2_collect_report_info:  total_time = %d num_frms = %d info1 = %d info2 = %d info3 = %d start_ts = %d 
2715,IIi,[ wal_rtt.c : 2395 ] RTT_INITR_TSTAMP: t2= 0x%08x%08x fac= %d 
2714,iIiiIIII,[ wal_rtt.c : 2455 ] _wal_report_type2_collect_report_info: rtt_ps: %d rssi=0x%x tx_preamble=%d tx_bw=%d tx_rate_info1 = 0x%x tx_rate_info2= 0x%x rx_rate_info1=0x%x, rx_rate_info2 = 0x%x 
2713,IIiIIiiiI,[ wal_rtt.c : 2485 ] RTT_INITR_TSTAMP: t2=%u, t3=%u  t3_del=%d t1=%u t4=%u t4_del=%d rtt=%d meas_count=%d num_rtt_per_frame_info_saved: %u 
2712,IIII,[ wal_rtt.c : 2507 ] _wal_report_type2_collect_report_info:  tx_rate_info1=0x%x, tx_rate_info2 =0x%x, rx_rate_info1=0x%x, rx_rate_info2=0x%x 
2711,IIiIII,[ wal_rtt.c : 2533 ] RTT_INITR_TSTAMP: t2= 0x%08x%08x fac= %d rx_preamble=%u, rx_bw=%u rssi = 0x%x  
2710,,[ wal_rtt.c : 2377 ] DISCARDING MEASUREMENT!! T3 not captured 
2709,I,[ wal_rtt.c : 1861 ] _wal_report_type2_update_start_ts: start_ts(rtt_ctxt) start_ts(peer_head) %u 
2708,III,[ wal_rtt.c : 1443 ] _wal_rtt_attach() pdev = %p rtt_pdev_ctxt = %p wal_rtt_ctxt = %p 
2707,iiii,[ wal_rtt.c : 339 ] rtt_compute_distance num_meas: %d mean_rtt: %d median_rtt: %d distance_cm: %d 
2706,iiiiiii,[ wal_rtt.c : 1947 ] wal_rtt_ctxt_clean: rxoffld_under_cnt: %d rxoffld_alloc_cnt: %d rxind_under_cnt: %d rxind_alloc_cnt: %d tm_rx_comp_cnt: %d rxoffld_drop_cnt: %d rxind_drop_cnt: %d 
2705,iiiiII,[ wal_rtt.c : 1599 ] _wal_rtt_ctxt_init() :freq: %d is_qca: %d force_legacy_ack: %d enable_ht_vht_ack :%d self_mac: %08x%04x 
2704,IIIIII,[ wal_rtt.c : 502 ] _wal_rtt_get_buffer_ptr:max_len:0x%x rem_len:0x%x reqd_len:0x%x buff:0x%x buf_p:0x%x cur_p:0x%x 
2703,iIIIi,[ wal_rtt.c : 1473 ] _wal_rtt_init() pdev_id = %d rtt_ctxt: %p  alloc_buff = %p buff = %p max_buff_len = %d 
2702,I,[ wal_rtt.c : 1999 ] rtt_local_send() Not a valid rtt frame type, retrun error! txrx_cb_flags: 0x%x 
2701,iIIIi,[ wal_rtt.c : 2052 ] _wal_rtt_local_frame_send_with_rate: acks%d tid_num 0x%x rate_info 0x%08x%08x report %d 
2700,IIiiI,[ wal_rtt.c : 3617 ] _wal_rtt_mt_cb: msg:0x%x id:0x%x s_thr:%d d_thr:%d ticks:0x%x 
2699,,[ wal_rtt.c : 2582 ] TX completion message was dropped. Report failure 
2698,,[ wal_rtt.c : 2588 ] _wal_rtt_null_ack_hdl() is called after RTT session is completed !!! 
2697,II,[ wal_rtt.c : 2595 ] Ignore NULL ack for stale entry: ath_buf: %p: last queued NULL frame ath_buf: %p 
2696,iiiiiiii,[ wal_rtt.c : 375 ] index: %d count: %d rtt_ps: %d sum_rtt: %d tx_bw: %d, rx_bw: %d tx_ch_idx: %d rx_ch_idx: %d 
2695,,[ wal_rtt.c : 2641 ] TX completion message was dropped. Report failure 
2694,,[ wal_rtt.c : 2647 ] _wal_rtt_tm_ack_hdl() is called after RTT session is completed !!! 
2693,II,[ wal_rtt.c : 2654 ] Ignore TM ack for stale entry: ath_buf: %p: last queued TM frame ath_buf: %p 
2692,,[ wal_rtt.c : 2924 ] _wal_rtt_tm_rx_hdl: TM frame not directed to me. Don't process 
2691,,[ wal_rtt.c : 2936 ] _wal_rtt_tm_rx_hdl: Not a valid TM frame. Don't process 
2690,III,[ wal_rtt.c : 3043 ] _wal_rtt_tm_rx_hdl: rx_ts %10u now_ts %10u rx_proc_delay %10u 
2689,i,[ wal_rtt.c : 3117 ] _wal_rtt_tm_rx_hdl: HT_VHT ack enable RTT_TM_FTM1 %d 
2688,iii,[ wal_rtt.c : 3122 ] _wal_rtt_tm_rx_hdl:  expect_token=%d, dia_token=%d, follow_token=%d 
2687,IIII,[ wal_rtt.c : 3222 ] _wal_rtt_tm_rx_hdl:  t1_32=0x%x, t1_0=0x%x, t4_32=0x%x, t4_0=0x%x 
2686,II,[ wal_rtt.c : 3243 ] CFR/CIR report queue full; CFR/CIR data at 0x%04x%04x will be dropped 
2685,i,[ wal_rtt.c : 3247 ] no CFR/CIR pending for report type %d 
2684,iII,[ wal_rtt.c : 3254 ] CFR/CIR pending for report type %d; CFR/CIR data at 0x%04x%04x will be dropped 
2683,,[ wal_rtt.c : 3397 ] wal_rtt_tx_ppdu_done(): rx_location_info is found to be invalid 
2682,IIIIIIIIi,[ wal_rtt.c : 3602 ] _wal_rtt_tx_ppdu_done(%u-sided): abf: 0x0 tx_preamble=%u, retries=%u tod_32=%u tod_0=%u toa_32=%u toa_0=%u fac_valid: %u fac=%d 
2681,II,[ wal_rtt.c : 3449 ] CFR/CIR report queue full; CFR/CIR data at 0x%04x%04x will be dropped 
2680,i,[ wal_rtt.c : 3453 ] no CFR/CIR pending for report type %d 
2679,iII,[ wal_rtt.c : 3460 ] CFR/CIR pending for report type %d; CFR/CIR data at 0x%04x%04x will be dropped 
2678,II,[ wal_rtt.c : 3506 ] CFR/CIR report queue full; CFR/CIR data at 0x%04x%04x will be dropped 
2677,i,[ wal_rtt.c : 3510 ] no CFR/CIR pending for responder report type %d 
2676,iII,[ wal_rtt.c : 3517 ] CFR/CIR pending for responder report type %d; CFR/CIR data at 0x%04x%04x will be dropped 
2675,ii,[ wal_rtt.c : 3745 ] wal_rtt_unit_test: debug_cnt[%d] = %d 
2723,iII,[ wal_rtt_init.c : 83 ] _wal_rtt_psoc_init() wal_rtt_ctxt idx in rtt_psoc_handle: %d rtt_ctxt: %p alloc_buff_p: %p 
2722,Iiii,[ wal_rtt_init.c : 92 ] _wal_rtt_psoc_init() psoc_rtt handle: %p sizes rtt_tx_pool: %d rtt_rx_pool handle: %d, rtt_rx_ofld_pool: %d 
2725,iIIi,[ wal_cfir.c : 44 ] wal_cfir_resolve: pdev %d cfg 0x%08x => 0x%08x status %d 
2724,I,[ wal_cfir.c : 87 ] wal_cfir_req_unregister: req %p already unregistered 
2735,ii,[ wal_spectral.c : 376 ] Pdev id : %d WMI event with reset_delay %d 
2734,iIIi,[ wal_spectral.c : 465 ] <%d>: WMI event called %p with %u buffers for module %d  
2733,ii,[ wal_spectral.c : 523 ] out_ring reap : Before read shadow_tail_idx %d & After read shadow_tail_idx %d 
2732,ii,[ wal_spectral.c : 553 ] SSCAN: cfg.ScanCountCopy %d cfg.ScanCount %d 
2731,i,[ wal_spectral.c : 758 ] pdev_id = %d: spectral sig handler 
2730,i,[ wal_spectral.c : 781 ] pdev_id = %d: spectral sig handler 
2729,i,[ wal_spectral.c : 807 ] pdev_id = %d: spectral sig handler 
2728,i,[ wal_spectral.c : 647 ] Resume SSCAN : pending elements in out_ring %d 
2727,iiii,[ wal_spectral.c : 162 ] SSCAN_DUMP mac_id = %d: trigger = %d enable = %d scan_mode = %d 
2726,I,[ wal_spectral.c : 174 ] SSCAN_DUMP: wal_spectral_scan_get_config  called %p 
2737,i,[ direct_dma_wmi.c : 213 ] pdev_id = %d: DMA is not attached 
2736,i,[ direct_dma_wmi.c : 236 ] pdev_id = %d: DMA is not attached 
2749,Iiii,[ wal_tx_common.c : 648 ] wal_peer_wow_null_per_stats_update: stats_start_time = 0x%x null_success = %d, null_fail = %d, cumulative_wake_time_ps_sta_ms = %d  
2748,Ii,[ wal_tx_common.c : 42 ] WAL_DBGID_STA_KICKOUT:                     peer=0x%x consecutive_null_failure=%d 
2747,iii,[ wal_tx_common.c : 46 ] WAL_DBGID_STA_KICKOUT:                     null_ppdu_fail_time:%dms delta:%dms vdev_type:%d 
2746,iIiIIIIII,[ wal_tx_common.c : 712 ] WAL_DBGID_STA_KICKOUT: KICKOUT_REASON_NULL_PER_CHECK_FAILURE_TH null_per= %d% wake_per= %d% null_fail_count= 0x%x, null_pass_count= 0x%x cumulative_wake_time_ps_sta_ms= 0x%x , null_per_stats_start_time = 0x%x, curr_time= 0x%x  
2745,iiIIIi,[ wal_tx_common.c : 169 ] consecutive_failure_reset : pdev=%d, vdev=%d, peer=0x%x, tid=0x%x (flags=0x%x), failure=%d -> 0 
2744,IIIIII,[ wal_tx_common.c : 382 ] tpc:16/rc_extended_flags:16 =0x%08x sch_cmd_result:0x%x flush_reason:0x%xfes_sched_try:0x%x fes_result:0x%x tsFlags:8/tsAttempts:8 0x%08x
  
2743,IIIIiiIIi,[ wal_tx_common.c : 390 ] pdev_vdev_id=0x%x, peer=0x%x,tid=0x%x (flags=0x%x), consecutive failure=%d, kickout thresh=%d rate_code=0x%x, tsRate flags=0x%x, ppdu_mprot_type:%d 
2742,IIIIIii,[ wal_tx_common.c : 394 ] pdev:8/vdev:8 =0x%08x, peer=0x%x,tid=0x%x (flags=0x%x %x), consecutive failure=%d, kickout thresh=%d  
2741,IIiIIII,[ wal_tx_common.c : 428 ] pdev:8/vdev:8 0x%08x peer=0x%x consecutive_failure:%d cur_time:%x elapsed_ppdu_fail_time:%x tid_retryfailure:%x vdevtype:%x 
2740,II,[ wal_tx_common.c : 518 ] WAL_DBGID_STA_KICKOUT  0x%x 0x%x 
2739,IIII,[ wal_tx_common.c : 522 ] ppdu_fail_time:%x current_time:%x delta:%x type:%x  
2738,III,[ wal_tx_common.c : 289 ] WAL_DBGID_XCESS_FAILURES  %p 0x%x MAC:%x 
2763,III,[ wal_wmm.c : 36 ] WMMAC_PAUSE_CB: peer=0x%x blocked tids=0x%x/0x%x 
2762,Iiii,[ wal_wmm.c : 65 ] WMMAC_Q_REPRIO: peer=0x%x tid=%d qid:%d->%d 
2761,iI,[ wal_wmm.c : 71 ] WMMAC_PAUSE_CB: unblock tid(%d)=0x%x 
2760,Iiii,[ wal_wmm.c : 340 ] WMMAC_Q_DEPRIO: peer=0x%x tid=%d qid:%d->%d 
2759,IiI,[ wal_wmm.c : 350 ] WMMAC_Q_DROP: peer=0x%x tid(%d)=0x%x 
2758,Iiiiii,[ wal_wmm.c : 393 ] WMMAC_STATUS: peer=0x%x, used=%d, admitted=%d, txq_sts=%d/%d, downgrade=%d 
2757,iIiii,[ wal_wmm.c : 424 ] WMMAC_TXQ_STATUS ac=%d txq_status=0x%02x used=%d admitted=%d downgrade=%d 
2756,iiiII,[ wal_wmm.c : 108 ] WMMAC_ADD_DELTS: ac=%d admitted=%d acm=%d block=0x%x downgrade=0x%x 
2755,iii,[ wal_wmm.c : 156 ] WMMAC_UPDATE: used_time=%d admitted_time=%d, downgrade=%d 
2754,IIII,[ wal_wmm.c : 465 ] WMMAC_PERIODIC_UPDATE 0x%x 0x%x 0x%x 0x%x 
2753,I,[ wal_wmm.c : 475 ] WMMAC_NO_DOWNGRADE: unblock tid mask=0x%x 
2752,Iii,[ wal_wmm.c : 496 ] WMMAC_PERIODIC_UPDATE (VO): peer=0x%x, used=%d, admitted=%d 
2751,Iii,[ wal_wmm.c : 506 ] WMMAC_PERIODIC_UPDATE (VI): peer=0x%x, used=%d, admitted=%d 
2750,iii,[ wal_wmm.c : 181 ] WMMAC_USED_TIME_EXCEED: used=%d admitted=%d wmmac_q=%d 
2778,ii,[ wlan_buf.c : 1025 ] MGMT buf get failure: mgmtbufCnt = %d, bsmall = %d 
2777,ii,[ wlan_buf.c : 1053 ] MGMT buf get beacon: mac_id:%d, rsvd:%d 
2776,iii,[ wlan_buf.c : 1086 ] MGMT buf abf failure: smgmtbufCnt = %d, bsmall = %d mgmtBufCnt = %d 
2775,IiiiI,[ wlan_buf.c : 1107 ] MGMT buf get success: abf = 0x%x  mgmtBufCnt =%d smgmtbuffcnt = %d bsmall = %d,flags = 0x%x 
2774,,[ wlan_buf.c : 1196 ] wlan_buf_mac_buffer_dispatcher no buffers available in chain 
2773,i,[ wlan_buf.c : 1209 ] wlan_buf_mac_buffer_dispatcher mac_id=%d
 
2772,,[ wlan_buf.c : 1212 ] wlan_buf_mac_buffer_dispatcher oops 
2771,,[ wlan_buf.c : 1224 ] wlan_buf_mac_buffer_dispatcher oops 
2770,IiI,[ wlan_buf.c : 808 ] buf free: free the reused abf:0x%x, thread:%d, cb flags:0x%x 
2769,iIiiI,[ wlan_buf.c : 883 ] MGMT buf free,small:%d,abf:0x%x,thread:%d,bufCnt:%d,caller:%x 
2768,IiIi,[ wlan_buf.c : 816 ] free beacon abf:0x%x, thread:%d, cb flags:0x%x,rsvd:%d 
2767,iIii,[ wlan_buf.c : 861 ] SMGMT buf free,small:%d,abf:0x%x,thread:%d,bufCnt:%d 
2766,i,[ wlan_buf.c : 1257 ] wlan_buf_rxbuf_requeue mac_id=%d
 
2765,,[ wlan_buf.c : 1262 ] wlan_buf_mac_buffer_dispatcher oops 
2764,,[ wlan_buf.c : 1288 ] wlan_buf_mac_buffer_dispatcher oops 
2779,,[ aes_gcm.c : 318 ] GCM: Tag mismatch 
2780,III,[ cmnos_intmux.c : 97 ] cmnos_intmux_dsr_attach error: handler = %p, pinum = %p, pparg=%p 
2790,IIII,[ cmnos_allocram.c : 503 ] unknown proxy_flag:0x%x, ret:0x%x, ret1:0x%x,ret2:0x%x 
2789,IiII,[ cmnos_allocram.c : 246 ] arena_flags: 0x%x, bytes:%d, call1:0x%x, call2:0x%x
 
2788,,[ cmnos_allocram.c : 633 ] Dumping allocram info into buffer... 
2787,i,[ cmnos_allocram.c : 694 ] Wrote: %d bytes 
2786,,[ cmnos_allocram.c : 713 ] Creating file... 
2785,,[ cmnos_allocram.c : 568 ] BEGIN: cmnos_allocram_info_dump() 
2784,,[ cmnos_allocram.c : 599 ] HEX_DUMP: 
2783,,[ cmnos_allocram.c : 609 ] END: cmnos_allocram_info_dump() 
2782,iIIiii,[ cmnos_allocram.c : 571 ] arena: %d, start: 0x%p, current: 0x%p, used = %d, remaining: %d, num_allocs: %d
 
2781,iiiii,[ cmnos_allocram.c : 597 ] max: %d, idx: %d, total_num: %d, total_bytes: %d, length: %d 
2802,II,[ cmnos_thread.c : 4732 ] assert:r0=0x%x, r1=0x%x
 
2801,III,[ cmnos_thread.c : 3061 ] thread exit exception:r0=0x%x, r1=0x%x, line:0x%x
 
2800,ii,[ cmnos_thread.c : 3954 ] CMNOS_Buf_Alloc_Failure Buffer_Full_thread_id = %d Current_thread_id = %d 
 
2799,Iiiii,[ cmnos_thread.c : 3853 ] LACK ROOM IN %s THREAD'S MSG QUEUE FIFO (need %d, have %d); readIndex=%d writeIndex=%d 
2798,iii,[ cmnos_thread.c : 1958 ] APP THREAD ID %d thread stack: %dB used, %dB unused
 
2797,,[ cmnos_thread.c : 1785 ] cmnos_threads_delete
 
2796,I,[ cmnos_thread.c : 1805 ] cmnos_threads_delete: wait for thread app id 0x%x to exit
 
2795,I,[ cmnos_thread.c : 1808 ] cmnos_threads_delete: thread app id 0x%x is done
 
2794,,[ cmnos_thread.c : 1867 ] cmnos_threads_delete: clean up mutex locks
 
2793,,[ cmnos_thread.c : 1876 ] cmnos_threads_delete: clean up thread barriers
 
2792,,[ cmnos_thread.c : 1887 ] cmnos_threads_delete: do global cleanups
 
2791,I,[ cmnos_thread.c : 1792 ] cmnos_threads_delete: send exit to 0x%x thread app id
 
2806,,[ platform_init.c : 55 ] WLAN Platform: Starting wlan tasks... 
2805,,[ platform_init.c : 249 ] QMI Platform: Sending msg to RT thread to do cold cal init... 
2804,i,[ platform_init.c : 84 ] WLAN Adrastea/MSL HW init, enable_hw_debug =%d 
2803,,[ platform_init.c : 142 ] QMI Platform: Starting wlan tasks... 
2808,,[ platform_deinit.c : 33 ] QMI Platform: Deinit started... 
2807,,[ platform_deinit.c : 80 ] QMI Platform: Threads killed... 
2809,ii,[ platform_common.c : 151 ] plat_set_one_ce_service_map_cfg: ERROR - idx %d > PIPE_TO_CE_MAP_CNT %d 
2813,,[ platform_athdiag.c : 239 ] plat_athdiag_proc_read_req: Sending msg to RT thread to do athdiag read 
2812,,[ platform_athdiag.c : 182 ] plat_athdiag_white_list_add: only support limited security area 
2811,IIi,[ platform_athdiag.c : 377 ] QMI Platform: Athdiag read REQ received...offset = 0x%x | mem_type = 0x%x | data_len = %d 
2810,IIi,[ platform_athdiag.c : 462 ] QMI Platform: Athdiag write REQ received...offset = 0x%x | mem_type = 0x%x | data_len = %d 
2881,II,[ qmi_platform.c : 838 ] Error code 0x%x in msg_id 0x%x 
2880,i,[ qmi_platform.c : 2341 ] qmi_plat_check_state: error - received CFG download REQ at wrong state %d 
2879,i,[ qmi_platform.c : 2306 ] platform_proc_qdss_cfg_download_req: QDSS cfg download curr_size = %d, 
2878,i,[ qmi_platform.c : 2322 ] platform_proc_qdss_cfg_download_req: QDSS cfg download done, current_size = %d, 
2877,IIII,[ qmi_platform.c : 487 ] qmi_event_history_log: msg_id = 0x%x, client_handle = 0x%x, event = 0x%x, tick = 0x%x 
2876,i,[ qmi_platform.c : 152 ] qmi_plat_check_state: error - received HOST_CAP_REQ at wrong state %d 
2875,iI,[ qmi_platform.c : 181 ] qmi_plat_check_state: ERROR: wrong state %d to receive msg_id 0x%x 
2874,i,[ qmi_platform.c : 192 ] qmi_plat_check_state: error - received MSA INFO REQ at wrong state %d 
2873,i,[ qmi_platform.c : 201 ] qmi_plat_check_state: error - received MSA READY REQ at wrong state %d 
2872,i,[ qmi_platform.c : 210 ] qmi_plat_check_state: error - sending MSA READY IND at wrong state %d 
2871,i,[ qmi_platform.c : 220 ] qmi_plat_check_state: error - received CAPABILITY REQ at wrong state %d 
2870,i,[ qmi_platform.c : 244 ] qmi_plat_check_state: error - received CAPABILITY REQ at wrong state %d 
2869,i,[ qmi_platform.c : 277 ] qmi_plat_check_state: error - received BDF DOWNLOAD REQ at wrong state %d 
2868,i,[ qmi_platform.c : 163 ] qmi_plat_check_state: WARNING: wrong state to send remote ddr mem cfg indication, state = %d 
2867,i,[ qmi_platform.c : 288 ] qmi_plat_check_state: error - received CAL_REPORT REQ at wrong state %d 
2866,i,[ qmi_platform.c : 299 ] qmi_plat_check_state: error - received M3_INFO REQ at wrong state %d 
2865,i,[ qmi_platform.c : 309 ] qmi_plat_check_state: error - send FW ready at wrong state %d 
2864,Ii,[ qmi_platform.c : 346 ] qmi_plat_check_state: error - Try to send FW Ready ind at wrong mode 0x%x and wrong state %d 
2863,i,[ qmi_platform.c : 356 ] qmi_plat_check_state: error - received CFG REQ at wrong state %d 
2862,Ii,[ qmi_platform.c : 374 ] qmi_plat_check_state: error - received MODE REQ w/ mode = 0x%x at wrong state %d 
2861,Ii,[ qmi_platform.c : 388 ] qmi_plat_check_state: error - received MODE REQ w/ mode = 0x%x at wrong state %d 
2860,Ii,[ qmi_platform.c : 411 ] qmi_plat_check_state: error - received MODE REQ w/ mode = 0x%x at wrong state %d 
2859,i,[ qmi_platform.c : 425 ] qmi_plat_check_state: error - Try to send CAL Done Ind at wrong state %d 
2858,Ii,[ qmi_platform.c : 433 ] qmi_plat_check_state: error - Try to send Cal Done Ind at wrong mode 0x%x and wrong state %d 
2857,iI,[ qmi_platform.c : 172 ] qmi_plat_check_state: ERROR: wrong state %d to receive msg_id 0x%x 
2856,i,[ qmi_platform.c : 445 ] qmi_plat_check_state: error - Try to send SOC WAKE at wrong state %d 
2855,i,[ qmi_platform.c : 459 ] qmi_plat_check_state: error - Try to send SOC WAKE at wrong state %d 
2854,II,[ qmi_platform.c : 3572 ] M3SSR recipe complete mac_id:%x  ts:%x 
2853,I,[ qmi_platform.c : 687 ] Client with handle 0x%x connected 
2852,I,[ qmi_platform.c : 718 ] Client with handle 0x%x disconnected 
2851,,[ qmi_platform.c : 1849 ] QMI Platform: sending QMI_WLFW_FILE_SAVE_IND_V01 
2850,I,[ qmi_platform.c : 1813 ] QMI Platform: BDF download REQ received, seg_id 0x%x 
2849,,[ qmi_platform.c : 2076 ] QMI Platform: Cal report REQ received 
2848,,[ qmi_platform.c : 2047 ] QMI Platform: Cap REQ received 
2847,ii,[ qmi_platform.c : 1874 ] QMI Platform: QMI_WLFW_FILE_DATA_REQ_V01 received, invalid parameter, req_id %d, cur_seg_id %d 
2846,,[ qmi_platform.c : 1885 ] QMI Platform: QMI_WLFW_FILE_DATA_REQ_V01 received, cur_seg_id 
2845,ii,[ qmi_platform.c : 1913 ] QMI Platform: QMI_WLFW_FILE_DATA_RESP_V01 sent,  data %d, end %d 
2844,II,[ qmi_platform.c : 1008 ] wlfw_handle_host_cap_req: num_clients=%x, nm_modem=%x 
2843,,[ qmi_platform.c : 1131 ] QMI Platform: Ind register REQ received 
2842,I,[ qmi_platform.c : 1165 ] Client with unique ID 0x%x registering 
2841,I,[ qmi_platform.c : 1170 ] Client with unique ID 0x%x found in client_list 
2840,i,[ qmi_platform.c : 1694 ] QMI Platform: INI REQ received, debug mode = %d 
2839,ii,[ qmi_platform.c : 1712 ] QMI Platform: recieved INI REQ, enablefwlog_valid = %d, enablefwlog = %d 
2838,ii,[ qmi_platform.c : 1716 ] QMI Platform: recieved INI REQ, enablefwlog_valid = %d, enablefwlog = %d 
2837,ii,[ qmi_platform.c : 1723 ] QMI Platform: recieved INI REQ, enablefwlog_valid = %d, enablefwlog = %d 
2836,ii,[ qmi_platform.c : 1727 ] QMI Platform: Did not recieve INI REQ, enablefwlog_valid = %d, enablefwlog = %d 
2835,Ii,[ qmi_platform.c : 2035 ] QMI Platform: M3 download REQ received, paddr = %ul, size = %d 
2834,,[ qmi_platform.c : 2097 ] QMI Platform: MAC addr REQ received 
2833,IIIIII,[ qmi_platform.c : 2144 ] Valid mac addr received from modem NV: %x : %x : %x : %x : %x : %x 
2832,,[ qmi_platform.c : 1919 ] I shouldn't have been called F 
2831,,[ qmi_platform.c : 2527 ] QDSS mem info REQ received 
2830,I,[ qmi_platform.c : 2421 ] QDSS mode REQ received, mode = 0x%x 
2829,i,[ qmi_platform.c : 1238 ] wlfw_handle_remote_ddr_mem_req: INFO: num_mem_cfg = %d 
2828,,[ qmi_platform.c : 2221 ] QMI Platform: Shutdown req recvd 
2827,i,[ qmi_platform.c : 2241 ] QMI Platform: platform state %d 
2826,,[ qmi_platform.c : 1552 ] QMI Platform: Wlan Cfg REQ received 
2825,i,[ qmi_platform.c : 1639 ] wlfw_handle_wlan_cfg_req: svc_cfg_len - %d 
2824,I,[ qmi_platform.c : 1304 ] QMI Platform: Wlan mode REQ received, mode = 0x%x 
2823,,[ qmi_platform.c : 1331 ] wlfw_handle_wlan_mode_req: hw_debug_valid = d, hw_debug = d 
2822,,[ qmi_platform.c : 1976 ] WHY DID YOU CALL ME 
2821,,[ qmi_platform.c : 914 ] QMI Platform: sending QMI_WLFW_RESPOND_GET_INFO_IND_V01 
2820,II,[ qmi_platform.c : 578 ] Ind with id 0x%x sent to client handle 0x%x 
2819,II,[ qmi_platform.c : 607 ] Ind with id 0x%x not sent to client handle 0x%x 
2818,II,[ qmi_platform.c : 589 ] Setting fw_status_mask in handle 0x%x with FW READY; new value = 0x%x 
2817,II,[ qmi_platform.c : 596 ] Handle 0x%x, fw_status_mask = 0x%x 
2816,II,[ qmi_platform.c : 602 ] Indication sent failed. Err code = 0x%x id = 0x%x 
2815,,[ qmi_platform.c : 908 ] QMI Platform: sending QMI_WLFW_QDSS_TRACE_FREE_IND_V01 
2814,,[ qmi_platform.c : 886 ] QMI Platform: sending QMI_WLFW_QDSS_TRACE_SAVE_IND_V01 
2882,I,[ pool_mgr_api.c : 406 ] product resulting in buffer overflow: num_of_elem * elem_sz = 0x%x 
2884,i,[ latency_profile.c : 451 ] profile_report: #profiles enabled > WMI limit (=%d) 
2883,i,[ latency_profile.c : 487 ] profile_report: could not alloc, size=%d 
2890,IIIi,[ sm.c : 338 ] SM: %x:%x:%p : allocation from event pool failed for event %d 
2889,IIIi,[ sm.c : 226 ] SM: %x:%x:%p : invalid event %d 
2888,IIIIiIIII,[ sm.c : 246 ] [SM:RcvEvt] CurS:%x <-- Event:%x mod_id=%x instance=%x vapid =%d make_sm = 0x%x extra = 0x%x extra2 = 0x%x extra3 = 0x%x 
2887,IIIii,[ sm.c : 255 ] SM: %x :%x :%p : event %d not handled in state %d 
2886,iiIIiIIII,[ sm.c : 271 ] [SM:RcvEvt] Evt:%d not handled in CurS:%d mod_id=%x instance=%x vapid =%d make_sm = 0x%x extra = 0x%x extra2 = 0x%x extra3 = 0x%x 
2885,IIIIiIIII,[ sm.c : 388 ] [SM:ChgSta] CurS:%x --> NextS:%x mod_id=%x instance=%x vapid =%d make_sm = 0x%x extra = 0x%x extra2 = 0x%x extra3 = 0x%x 
2894,ii,[ mu_gid_mgmt.c : 99 ] 11ac MU-MIMO GID MGMT: user successfully assigned completed: assoc id: %d, mu_user_id: %d 
2893,iii,[ mu_gid_mgmt.c : 116 ] 11ac MU-MIMO GID MGMT: Send GID MGMT failed. AID: %d, mu_user_id: %d, status: %d 
2892,iiIIIIII,[ mu_gid_mgmt.c : 166 ] 11ac MU-MIMO GID MGMT: Sending GID MGMT frame: AID: %d, mu_user_id: %d, grp_status[0]: 0x%08x, grp_status[1]: 0x%08x, user_pos_map[0]: 0x%08x, user_pos_map[1]: 0x%08x, user_pos_map[2]: 0x%08x, user_pos_map[3]: 0x%08x 
2891,ii,[ mu_gid_mgmt.c : 173 ] 11ac MU-MIMO GID MGMT: Send GID MGMT failed. AID: %d, mu_user_id: %d 
2906,II,[ ratectrl.c : 7357 ] rc_get_nondata_rc: %x for peer:%p  
2905,II,[ ratectrl.c : 7410 ] rc_get_ofdm_nondatarc: %x for peer:%p  
2904,iIIII,[ ratectrl.c : 7526 ] pdev_id:%d rc_leg_rate_allowed=0x%x rc_legacy_mask=0x%x temp_cck_rate_bitmap=0x%x module_id=0x%x 
2903,iIIIII,[ ratectrl.c : 7556 ] FINAL: pdev_id:%d rc_leg_rate_allowed=0x%x rc_legacy_mask=0x%x  pdev->rc_legacy_mask: BT=0x%x LTE_COEX=0x%x HE_ASSOC=0x%x
 
2902,,[ ratectrl.c : 5942 ] Set INVALID!!! RTS Rate Index 
2901,ii,[ ratectrl.c : 5952 ] _RATE_SetRtsCtsRate: Def RTS Rate Rix %d Alt RTS Rate Rix %d  
2900,I,[ ratectrl.c : 4722 ] SEC_RETRY skip PER update flags:0x%x 
2899,iii,[ ratectrl.c : 4958 ] _rcUpdate_HT: Xretry Prot failure: After Toggle RTS -- rtsForFirstSeries %d --[RTS Profile %d Toggle %d]
 
2898,IIIII,[ ratectrl.c : 7914 ] rc_update_rts_per: rts_rix 0x%x def_rix 0x%x alt_rix 0x%x curr_rix 0x%x ni_legacy_rate_set 0x%x 
 
2897,II,[ ratectrl.c : 2273 ] rc_validate_rateset/NON_HT:  Before mask update ni_legacy_rate_set 0x%x validTxRateMask 0x%x 
2896,II,[ ratectrl.c : 2316 ] rc_validate_rateset/NON_HT:  After mask update ni_legacy_rate_set 0x%x validTxRateMask 0x%x 
2895,iiIiiI,[ ratectrl.c : 2477 ] NSS Mismatch: 160nss %d, 160_mcs_nss_set %d, 160_mcs_nss_map %x, 80nss %d, 80_mcs_nss_set %d, 80_mcs_nss_map %x 
2913,I,[ ratectrl_if.c : 271 ] is_rc_peer_mem_optimized: peer is invalid vdev:0x%x 
2912,IIi,[ ratectrl_if.c : 2128 ] AUTORATE_RESET_USER_START_RATE: peer  phymode:8/ht:8/vht:8 : 0x%08x ni_flags 0x%x  user_start_rate %d 
2911,,[ ratectrl_if.c : 1870 ] RATE_EnableCCKRatesInHTMode: No vdev's attached to pdev, rejecting WLAN_PDEV_ENABLE_CCK_RATE !
 
2910,IiiIiii,[ ratectrl_if.c : 1932 ] Enabling coex restriction (pdev - 0x%x) enable %d min_rate:%d on wlan_peer:0x%x rc_mode:%d rateMax:%d bestRate:%d 
2909,i,[ ratectrl_if.c : 1942 ] vdev[%d] is NULL, rejecting WLAN_PDEV_ENABLE_CCK_RATE !
 
2908,IiiIiii,[ ratectrl_if.c : 1920 ] Enabling coex restriction (pdev - 0x%x) enable %d min_rate:%d on wlan_peer:0x%x rc_mode:%d rateMax:%d bestRate:%d 
2907,IIiII,[ ratectrl_if.c : 2289 ] 
org_rc_mask_null pdev_rc_mask[0]:%x pdev_rc_mask[1]:%x phymode:%d ni_legacy_rate_set:%x rc_legacy_mask_final:%llx 
2933,,[ ratectrl_debug.c : 425 ] setUnitTestcmd FAILED : SUPPORT_AUTORATE_RESET not implemented 
2932,Ii,[ ratectrl_debug.c : 516 ] RTS_DEBUG: vdev id:8/rts cts type:8/rts cts profile:16 0x%08x rts_rix %d
 
2931,I,[ ratectrl_debug.c : 548 ] RT_UPDATE SU Mode, BW:8/NSS8: %08u. 
2930,I,[ ratectrl_debug.c : 551 ] RT_UPDATE MU Mode,  BW:8/NSS8: %08u. 
2929,I,[ ratectrl_debug.c : 556 ] RT_UPDATE Last Probed  BW:8/NSS:8/MCS:8 : %08u. 
2928,IIIII,[ ratectrl_debug.c : 563 ] RT_UPDATE MCS_%u: PPDU Tried: %u, PPDU ACK Failed: %u, MPDUS Tried: %u, MPDUS Failed: %u. 
2927,I,[ ratectrl_debug.c : 626 ] RA_DBG_CMDID_TEST_PER_CONV_UL_MUMIMO:  ltPer:8/stPer:8/curr_per:8 : 0x%08x 
2926,iiiiiiii,[ ratectrl_debug.c : 718 ] MCAST_RC: vdev_id: %d, Is mcast dra enabled: %d
MCAST_RC: stale_period_sec: %d
MCAST_RC: Number of stale clients: %d
MCAST_RC: Default Mcast rate: %d Mbps, rix: %d
MCAST_RC: Auto Mcast rate: %d Mbps, rix: %d
 
2925,iii,[ ratectrl_debug.c : 453 ] Number of invalid peer assoc capabilities for HT %d, VHT %d, HE %d
 
2924,iiii,[ ratectrl_debug.c : 721 ] MCAST_DBG_RC: RC queries %d, RC updates %d, RIX error: %d, Peer count error: %d
 
2923,iii,[ ratectrl_debug.c : 726 ] MCAST_DBG_RC: Last stale peer id %d, current time %d, stale tx time %d
 
2922,ii,[ ratectrl_debug.c : 733 ] MCAST_DBG_RC: %d Mbps - %d
 
2921,iiiii,[ ratectrl_debug.c : 749 ] MCAST_DBG_RC: peer id: %d, rate kbps: %d, mcast rate kbps: %d, rix:%d, mcast rix:%d
 
2920,,[ ratectrl_debug.c : 877 ] DISABLE_INVALID_RATES: Invalid arg count 
2919,,[ ratectrl_debug.c : 882 ] DISABLE_INVALID_RATES: Invalid arg count 
2918,,[ ratectrl_debug.c : 901 ] DISABLE_INVALID_RATES: Invalid preamble or bw or nss 
2917,,[ ratectrl_debug.c : 907 ] DISABLE_INVALID_RATES: Invalid MCS 
2916,,[ ratectrl_debug.c : 918 ] DISABLE_INVALID_RATES: Exceeded max invalid rate count, Disable and add invalid rate 
2915,,[ ratectrl_debug.c : 936 ] DISABLE_INVALID_RATES: Invalid arg count 
2914,i,[ ratectrl_debug.c : 481 ] g_dbg_enable_he_short_gi: %d 
 
2934,iiiiii,[ ratectrl_ofdma.c : 898 ] OFDMA_RC_DBG: aid: %d, ref_rix: %d, trialBaseRate: %d, complMismatchCnt: %d, ru_cnt: %d, rc_mode: %d 
2948,i,[ ratectrl_ulmumimo.c : 830 ] UL_MUMIMO_DBG_RC, MonoRC forward, nRate %d 
2947,i,[ ratectrl_ulmumimo.c : 841 ] UL_MUMIMO_DBG_RC, MonoRC backward, nRate %d 
2946,iiiiiii,[ ratectrl_ulmumimo.c : 899 ] UL_MUMIMO_DBG_RC, intf_ss_type %d, Update next rate nss %d, mcs %d with PER %d and discount %d to ltPer %d, stPer %d 
2945,iiii,[ ratectrl_ulmumimo.c : 163 ] UL_MUMIMO_DBG_RC, Best rate in backward rates: %d, %d, maxTp: %d %d 
2944,iiii,[ ratectrl_ulmumimo.c : 114 ] UL_MUMIMO_DBG_RC, Best rate in forward rates: %d, %d, maxTp: %d %d 
2943,iiiii,[ ratectrl_ulmumimo.c : 326 ] UL_MUMIMO_DBG_RC, rc_mode %d, forward, BestTput %d, bestRate%d, bestNss %d, nForward %d 
2942,iiiii,[ ratectrl_ulmumimo.c : 398 ] UL_MUMIMO_DBG_RC, not in use rc_mode %d, backward, BestTput %d, bestRate%d, bestNss %d, nBackward %d 
2941,iiiiii,[ ratectrl_ulmumimo.c : 463 ] UL_MUMIMO_DBG_RC, bw %d, rc_mode %d, Best rate : %d, %d, maxTp: %d %d 
2940,iiiii,[ ratectrl_ulmumimo.c : 336 ] UL_MUMIMO_DBG_RC, rc_mode %d, backward, BestTput %d, bestRate%d, bestNss %d, nBackward %d 
2939,iiiiii,[ ratectrl_ulmumimo.c : 386 ] UL_MUMIMO_DBG_RC, not in use rc_mode %d, last_rate %d, forward, BestTput %d, bestRate%d, bestNss %d, nForward %d 
2938,iiiii,[ ratectrl_ulmumimo.c : 1226 ] UL_MUMIMO_DBG_RC, rc_sib_update_state, bw:%d, idx=%d, num_rix=%d, nss_idx=%d, lastSucRate=%d 
2937,iiiiii,[ ratectrl_ulmumimo.c : 1039 ] UL_MUMIMO_DBG_RC, update PER, state_idx %d, ltPer %d, stPer %d, curr_per %d, nTotalMpdu %d, rix %d 
2936,i,[ ratectrl_ulmumimo.c : 1108 ] UL_MUMIMO_DBG_RC, Update lower state %d 
2935,iiii,[ ratectrl_ulmumimo.c : 1132 ] UL_MUMIMO_DBG_RC, Update BW %d, next higher state %d, rix %d with PER %d  
3001,IIIiIII,[ sched_algo.c : 10932 ] AGGR_DBG: aid: %u avg_msdu_bytes: %u, amsdu_estimate: %u, required_bits: %d, required_mpdu: %u, ppdu duration: %u, phy_rate_kbps: %u 
3000,iIIii,[ sched_algo.c : 1957 ] smart_basic_trig : skip_no_ul_data service_interval=%d, time_diff=%lu, last_sched_tsmp=%lu, aid=%d, tid_num=%d 
 
2999,iiIIii,[ sched_algo.c : 1963 ] smart_basic_trig : service_interval=%d, exp_bytes=%d, time_diff=%lu, last_sched_tsmp=%lu, aid=%d, tid_num=%d 
 
2998,I,[ sched_algo.c : 7303 ] BA recovery - mismatch ack type, tid:%x 
2997,I,[ sched_algo.c : 2007 ] ul_dbg_check_eligibility: No UL Trig: is_wmm_txq_ul_trig_disabled=%u 
2996,IiiiIIII,[ sched_algo.c : 2104 ] ul_dbg_check_eligibility: tid_q=%x, tid_num=%d, is_bsr_timeout=%d, num_frms=%d, curr_time = %u, tsf_now=%u, bsr_ts=%u, bsr_timeout_ms=%u 
2995,i,[ sched_algo.c : 2111 ] ul_dbg_check_eligibility: trigger_state=%d 
2994,iiii,[ sched_algo.c : 2157 ] OFDMA_SCHED_DECISION: aid: %d, tid_num: %d, unreliable_basic_trigger: %d, unreliable_metric: %d 
2993,iIi,[ sched_algo.c : 6210 ] MISSING_BSR_DEBUG: aid: %d, trigger in flight=false, updated_ac_bmap: 0x%08x, miss_count: %d 
2992,iIi,[ sched_algo.c : 6226 ] MISSING_BSR_DEBUG2: aid: %d, trigger in flight=false, updated_ac_bmap: 0x%08x, miss_count: %d 
2991,iiii,[ sched_algo.c : 6257 ] MISSING_BSR_DEBUG: aid: %d, trigger in flight=false, ac=%d, orig_timeout: %d, new_timeout: %d 
2990,iiIIiIII,[ sched_algo.c : 6295 ] twt_dbg/ul_dbg: sched_cmd_completion txqid=%d, sched_id=%d, seq_type=%u, peer_id=%u, pending_commands=%d,compl_ts=%u, user_resp=%u, seq_compl_flags=0x%x 
 
2989,IIIII,[ sched_algo.c : 6307 ] twt_dbg: sched_cmd_completion peer_id=%u, tid_num=%u, sched_flags=0x%x, trigger_state=%u, eosp_state=%u 
 
2988,i,[ sched_algo.c : 3246 ] STANDALONE:sched_algo_cmd_update_user_info NDPA FLAG NOT SET $$$tid_num=%d 
2987,IIII,[ sched_algo.c : 4927 ] sched_algo_configure_ul_rts_protection: t_success_rts: %u, t_success_no_rts: %u, t_fail_no_rts: %u, t_fail_rts: %u 
2986,iIIIIII,[ sched_algo.c : 4996 ] sched_algo_configure_ul_rts_protection: ac: %d, num_users: %u, tb_ppdu_duration: %u, trig_rix: %u, mba_rix: %u, min_coll_prob_to_enable_rts_cts: %u, cur_fail_pct: %u 
2985,iII,[ sched_algo.c : 11440 ] sched_algo_disable_sched_mode_bmap_update: IN: txq_id: %d, disabled_sched_mode_bmap_req: 0x%08x, disabled_sched_mode_bmap: 0x%08x 
2984,iII,[ sched_algo.c : 11467 ] sched_algo_disable_sched_mode_bmap_update: OUT: txq_id: %d, disabled_sched_mode_bmap_req: 0x%08x, disabled_sched_mode_bmap: 0x%08x 
2983,IiiiiII,[ sched_algo.c : 5204 ] ul_dbg_sched_dispatch_result: tsf_lsb=%u, sched_mode=%d, tx_mode=%d, seq_type=%d, num_users=%d, tx_time_us=%u, txop_time_us=%u 
2982,i,[ sched_algo.c : 5470 ] MISSING_BSR_DEBUG: aid: %d, trigger in flight=true 
2981,,[ sched_algo.c : 5567 ] MBSSID_CTRL_FRM_DBG MBSSID Ctrl Frame Feature is in use 
2980,,[ sched_algo.c : 5590 ] sched_algo_configure_ul_rts_protection: using shorter RTS duration for non-repeater environment 
2979,iiiIiIII,[ sched_algo.c : 5702 ] twt_dbg_eosp / ul_dbg: sched_dispatch_sched_cmd txqid=%d, sched_id=%d, posted_commands=%d,sched_cmd_flags=0x%x, is_partial=%d, tsf_low=%u, start_time=%u, end_time=%u 
 
2978,IiiIII,[ sched_algo.c : 9942 ] twt_dbg_eosp: sched_algo_dl_eligible_check peer_id=%u, is_announced=%d, is_ul_received=%d,tidq->tid_num=%u, tid_ext_flags=0x%x, eosp_state=%u 
2977,ii,[ sched_algo.c : 4535 ] TTL dropped count:%d, tid:%d 
2976,iii,[ sched_algo.c : 10592 ] UL_FD_RSSI_DBG:sw peer id %d ulmumimo_fd_rssi_100x %d dbg_ulmumimo_fd_rssi_threshold_100x %d 
 
2975,iiiIiii,[ sched_algo.c : 10629 ] UL_MU_MIMO_TX_PARAMS: AID %d: NSS %d: MCS: %d, qdepth bytes: %lu, txtime  %d, num frames: %d tidq_ul_mumimo_eligible %d
 
2974,iiiii,[ sched_algo.c : 10728 ] OFDMA_SCHED_DECISION: top level eligibility: aid: %d, tid_num: %d, sta_is_lowq: %d, avg_txtime_us: %d, average_ul_qdepth_bytes: %d 
2973,III,[ sched_algo.c : 8652 ] migrate peer in delete prog %p, flags:%x, sw_peer_id:%x 
2972,iII,[ sched_algo.c : 8676 ] migrate peer %d, already on MAC(%u %u) 
2971,II,[ sched_algo.c : 11360 ] MBSSID_CTRL_FRM_DBG peer_a RXCFM cap = %u, peer_b RXCFM cap = %u 
2970,,[ sched_algo.c : 11370 ] MBSSID_CTRL_FRM_DBG Using MBSSID Control Frame - Triggering peers on different vdevs 
2969,,[ sched_algo.c : 11388 ] MBSSID_CTRL_FRM_DBG Using MBSSID Control Frame - Triggering peers on different vdevs 
2968,iiiiii,[ sched_algo.c : 3816 ] PPDU Duration debug: sched_id=%d, num_users=%d, txop_us=%d,txtime_us=%d, seq_type=%d, sched_type=%d 
2967,iiI,[ sched_algo.c : 7480 ] soft_msduq_delete: tickle dropped :%d qtype:%d 0x%x 
2966,IIIIII,[ sched_algo.c : 7500 ] sched_algo_process_trigger non_paused_tid enter: tid=0x%x,pdev=0x%x:0x%x,flag=0x%x, paused=0x%0x num_mpdus_in_fq=0x%0x 
2965,IIIII,[ sched_algo.c : 7515 ] discard trigger msg as pdev mismatch peer_id=%x,tid=%x,pdev=%x:%x,flag=%x 
2964,IIIIII,[ sched_algo.c : 7697 ] sched_algo_process_trigger non_paused_tid run_scheduler: tid=0x%x,pdev=0x%x:0x%x,flag=0x%x, paused=0x%0x num_mpdus_in_fq=0x%0x 
2963,i,[ sched_algo.c : 9178 ] sched_algo_req_handler: unsupported msg type:%d 
2962,iiiiii,[ sched_algo.c : 2661 ] twt_dbg: twt_sched_algo_return (slot ended):txqid=%d, tsf_now_msb=%d, lsb=%d, curr_slot_end msb=%d, lsb=%d slot_valid:%d 
2961,iiI,[ sched_algo.c : 2720 ] ul_dbg_sched_new_run: txqid=%d, sched_cmd_space=%d, flags=0x%x 
2960,iiI,[ sched_algo.c : 2795 ] twt_dbg: twt_sched_algo_run_policy: txqid=%d, sched_cmd_space=%d, flags=%x 
2959,iiII,[ sched_algo.c : 6577 ] TTL tid:%d txq_id:%d, flg-clr:%x %x 
2958,ii,[ sched_algo.c : 291 ] STANDALONE : SEND MESSAGE TO SCHEDULER %d thread id %d  
2957,IIIIIIII,[ sched_algo.c : 4640 ] tcp_ul_dbg_sched_dispatch_result: tx_mode=%u, peer_sw_id=%u, sched_id=0x%x, qdepth_adv =%u, qdepth_implicit=%u, qdepth_implicit_final=%u, ru_start=%u, ru_end=%u 
2956,ii,[ sched_algo.c : 1657 ] ul_dbg_sched_algo_tid_register: num_frames=%d, tid_num=%d 
2955,iiiIi,[ sched_algo.c : 1695 ] TID REG:peer %d tidnum %d txqid %d flags %x num active %d
 
2954,ii,[ sched_algo.c : 1761 ] ul_dbg_sched_algo_tid_unregister: num_frames=%d, tid_num=%d 
2953,iiiIii,[ sched_algo.c : 1815 ] TID UNREG:peer %d tidnum %d txq %d flags %x num active %d, pause_tid:%d 
2952,II,[ sched_algo.c : 3075 ] sched_algo_cmd_update_user_info: g_qnull_peer_id%x %x 
2951,,[ sched_algo.c : 3081 ] NEW_STATS: qnull set 
2950,iiiii,[ sched_algo.c : 11018 ] AGGR_DBG: user %d: assigned: %d, rate_kbps: %d, qdepth: %d, target_mpdu: %d
 
2949,Iii,[ sched_algo.c : 3776 ] smart_basic_trig : last_sched_tsmp=%lu aid=%d, tid_num=%d 
 
3002,ii,[ sched_algo_rr.c : 290 ] twt_dbg: sched_algo_run_rr_scheduler_tidq0 skip tid tid:%d elgble: %d 
3019,iiiiiii,[ sched_algo_qos.c : 2707 ] Duration based tx_mode %d, total_psdu_time %d, avg_su_psdu_dur %d, adj_avg_psdu_dur %d, txop_duration %d, max_avg_psdu_dur %d, total_psdu %d
 
3018,iiiii,[ sched_algo_qos.c : 2719 ] Duration based num_txop %d, over_head %d, avg_chan_acc_lat_us %d, gain %d, total_latency %d
 
3017,iiiii,[ sched_algo_qos.c : 2765 ] Duration based selected tx mode %d => tx latency %d : Max users %d candidate_list->num_entries %d chan_access_let %d 
 
3016,iiiiii,[ sched_algo_qos.c : 157 ] OFDMA_SCHED_DECISION: aid: %d, cur_time_ms: %d, use_ul_su_phy_rate: %d, avg_ul_su_phy_rate: %d, rix: %d, phy_rate_kbps: %d 
3015,iiii,[ sched_algo_qos.c : 160 ] OFDMA_SCHED_DECISION: aid: %d, cur_time_ms: %d, ul_su_update_time: %d, ul_ofdma_trig_time: %d 
3014,iiii,[ sched_algo_qos.c : 200 ] OFDMA_SCHED_DECISION: aid: %d, psd_boost_ref_phy_rate: %d, ul_max_nss: %d, ul_max_bw: %d 
3013,iIiii,[ sched_algo_qos.c : 2214 ] ul_dbg_populate_bsr_CTL: tid_num=%d, tidq=0x%x, sch_inp_lsb=%d, last_bsr_lsb=%d, trigger_timeout_ms=%d 
3012,ii,[ sched_algo_qos.c : 2228 ] UL_MUMIMO_DBG: select UL MU-MIMO candidate list. num_frms %d, txtime_us %d 
3011,i,[ sched_algo_qos.c : 239 ] OFDMA_SCHED_DECISION: num_entries: %d 
3010,iiiiI,[ sched_algo_qos.c : 273 ] OFDMA_SCHED_DECISION: aid: %d, avg_txtime_us: %d, avg_ul_qdepth_bytes: %d, txtime_us: %d, qdepth_bytes: %lu 
3009,iii,[ sched_algo_qos.c : 290 ] OFDMA_SCHED_DECISION: num_entries: %d, lowq_users: %d, highq_low_mcs_users: %d 
3008,IIIIII,[ sched_algo_qos.c : 2888 ] twt_dbg: check_eligibility:curr_time_us=%u, txqid=%u, peer_id=%u, tid_num=%u, is_skip_tid=%u, sched_eligible=%u 
3007,ii,[ sched_algo_qos.c : 3027 ] Candidate list: Num entries = %d, TX_MODE = %d 
3006,iiiiii,[ sched_algo_qos.c : 980 ] FORCE_SU_UL_TRIG: peer aid: %d, force_single_user_ul_ofdma: %d, cur_peer_requires_su_trigger: %d, force_2users_in_160_trigger %d, primary peer aid: %d, cur_time: %d 
3005,i,[ sched_algo_qos.c : 1323 ] twt_dbg: twt_sched_algo_qos returned (CL empty): txqid=%d 
3004,Ii,[ sched_algo_qos.c : 4043 ] ul_dbg_tid_unregister_qos: qpeer=0x%x, tid_num=%d 
3003,iii,[ sched_algo_qos.c : 217 ] OFDMA_SCHED_DECISION: aid: %d, psd_boost_phy_rate_max: %d, phy_rate_estimate %d 
3025,iiiiii,[ sched_algo_mu.c : 1555 ] UL_MUMIMO_DBG quit DL delaying for timeout, start_delay_time %d, delay_dur %d, cur_time %d, cur_cnt %d, max_cnt %d, target_cnt %d 
3024,iiiiii,[ sched_algo_mu.c : 1609 ] UL_MUMIMO_DBG quit DL delaying not allowed, start_delay_time %d, delay_dur %d, cur_time %d, cur_cnt %d, max_cnt %d, target_cnt %d 
3023,ii,[ sched_algo_mu.c : 1623 ] UL_MUMIMO_DBG start DL delaying,cur_cnt %d, max_cnt %d 
3022,iiiiii,[ sched_algo_mu.c : 1580 ] UL_MUMIMO_DBG quit DL delaying enough users, start_delay_time %d, delay_dur %d, cur_time %d, cur_cnt %d, max_cnt %d, target_cnt %d 
3021,iiiiii,[ sched_algo_mu.c : 1597 ] UL_MUMIMO_DBG keep on DL delaying, start_delay_time %d, delay_dur %d, cur_time %d, cur_cnt %d, max_cnt %d, target_cnt %d 
3020,II,[ sched_algo_mu.c : 1855 ] mu_sort: sw peer id =%u, qdepth =%u 
3037,iii,[ ru_allocator.c : 4663 ] RU Power imbalance Adjust: pre mcs %d, per_tone_pwr %d, interference_from_pre %d 
3036,iii,[ ru_allocator.c : 4681 ] RU Power imbalance Adjust: next mcs %d, per_tone_pwr %d, interference_from_next %d 
3035,iiiii,[ ru_allocator.c : 4713 ] RU Power imbalance Adjust: mcs %d, per_tone_pwr %d, interference_from_neigbor %d, margin %d, num_notches %d 
3034,iii,[ ru_allocator.c : 4718 ] RU Power imbalance Adjust: pre mcs %d, per_tone_pwr %d, interference_from_pre %d 
3033,ii,[ ru_allocator.c : 182 ] Dropping Static RU Unit Test Cmd - Num Args %d : Max Users: %d 
3032,iii,[ ru_allocator.c : 243 ] RU idx exceeds max idx - ru_idx: %d : ru_size: %d : tx_bw: %d 
3031,iii,[ ru_allocator.c : 249 ] Incorrect Static RU allocation - ru_idx: %d : ru_size: %d : tx_bw: %d 
3030,iIIii,[ ru_allocator.c : 6188 ] RU_ALLOC DBG: id: %d, ru_input: flags: 0x%08x, tx_bw_mask 0x%08x, ppdu_time: %d, input user count: %d 
3029,iiiiIiii,[ ru_allocator.c : 6208 ] RU_ALLOC DBG: id: %d, aid: %d, max_bw: %d, rix: %d, queue_depth: %u, qos_weight: %d, consec_no_mpdu_tried: %d, consec_skip_cnt: %d 
3028,iiiIiii,[ ru_allocator.c : 6232 ] RU_ALLOC DBG: id: %d, ru_result: ret_val: %d, num_users: %d, tx_bw_mask 0x%08x, data_ppdu_dur[0]: %d, data_ppdu_dur[1]: %d, data_ppdu_dur[2]: %d 
3027,iiii,[ ru_allocator.c : 6244 ] RU_ALLOC DBG: id: %d, ru_result: ul_ba_ppdu_duration_us[0]: %d, ul_ba_ppdu_duration_us[1]: %d, ul_ba_ppdu_duration_us[2]: %d 
3026,ii,[ ru_allocator.c : 6252 ] RU_ALLOC DBG: id: %d, DROPPED_USER: aid: %d 
3211,iiiiiiiii,[ sched_algo_dbg.c : 6513 ] AMSDU_DEBUG_CALC: rix=%d preamble=%d nss=%d mcs=%d gi=%d amsdu_64=%d amsdu_128=%d bw=%d rate_kbps=%d
 
3210,iiiiiiiii,[ sched_algo_dbg.c : 6525 ] AMSDU_DEBUG_TBL: rix=%d preamble=%d nss=%d mcs=%d gi=%d amsdu_64=%d amsdu_128=%d bw=%d rate_kbps=%d
 
3209,ii,[ sched_algo_dbg.c : 210 ] STANDALONE : TICKLE SCHEDULER %d thread id %d  
3208,,[ sched_algo_dbg.c : 421 ] ATF stats 
 
3207,ii,[ sched_algo_dbg.c : 1462 ] ULMU_PRINT, ul_bsr_cnt %d, total_cnt %d 
3206,iiiiiiii,[ sched_algo_dbg.c : 1474 ] ULMU_PRINT, dl_cnt[0-3] %d, %d, %d, %d ul_cnt[0-3] %d, %d, %d, %d 
3205,iiiiiiii,[ sched_algo_dbg.c : 1485 ] ULMU_PRINT, dl_cnt[4-7] %d, %d, %d, %d ul_cnt[4-7] %d, %d, %d, %d 
3204,iiiiii,[ sched_algo_dbg.c : 1541 ] ULMU_PRINT, mpdu_ok_per_AID, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d, 6:%d 
3203,iiiiii,[ sched_algo_dbg.c : 1552 ] ULMU_PRINT, mpdu_fail_per_AID, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d, 6:%d 
3202,,[ sched_algo_dbg.c : 454 ] bss  
3201,iiiiiiii,[ sched_algo_dbg.c : 1942 ] mu_mimo_grp_stats:mu_grp_best_grp_size -> (%d, %d, %d, %d, %d, %d, %d, %d )
  
3200,iiii,[ sched_algo_dbg.c : 1968 ] mu_mimo_grp_stats:mu_grp_best_num_users -> (%d, %d, %d, %d)
  
3199,iiiii,[ sched_algo_dbg.c : 1979 ] mu_mimo_grp_stats:mu_mimo_tputs_observed (0-1500Mbps)> (%d, %d, %d, %d, %d )
  
3198,iiiii,[ sched_algo_dbg.c : 1990 ] mu_mimo_grp_stats:mu_mimo_tputs_observed (1500-3000Mbps) (%d, %d, %d, %d, %d)
  
3197,iiiiiiiii,[ sched_algo_dbg.c : 2004 ] mu_mimo_grp_stats:num_mu_mimo_candidate(0-8 users)-> ( %d, %d, %d, %d, %d, %d, %d, %d, %d )
  
3196,iiiiiiii,[ sched_algo_dbg.c : 2017 ] mu_mimo_grp_stats:num_mu_mimo_candidate(9-16 users)-> (%d, %d, %d, %d, %d, %d, %d, %d )
  
3195,iiiiiiii,[ sched_algo_dbg.c : 2030 ] mu_mimo_grp_stats:num_mu_mimo_candidate_nr4 -> (%d, %d, %d, %d, %d, %d, %d, %d )
  
3194,iiiiiiii,[ sched_algo_dbg.c : 2043 ] mu_mimo_grp_stats:num_mu_mimo_candidate_nr8  -> (%d, %d, %d, %d, %d, %d, %d, %d )
  
3193,iiiii,[ sched_algo_dbg.c : 2053 ] mu_mimo_grp_stats:sched_type -> (%d, %d, %d, %d, %d )
  
3192,i,[ sched_algo_dbg.c : 2056 ] mu_mimo_grp_stats:Group_id: %d  
3191,,[ sched_algo_dbg.c : 456 ] self  
3190,iiii,[ sched_algo_dbg.c : 2082 ] mu_mimo_grp_stats:cd_num_entries -> (%d, %d, %d, %d )
  
3189,iiiii,[ sched_algo_dbg.c : 2094 ] mu_mimo_grp_stats:tputs for this group id (0 - 1500 Mbps)-> (%d, %d, %d, %d, %d)  
3188,iiiii,[ sched_algo_dbg.c : 2104 ] mu_mimo_grp_stats:tputs for this group id(1500-3000 Mbps) -> (%d, %d, %d, %d, %d)  
3187,,[ sched_algo_dbg.c : 2107 ] mu_mimo_grp_stats:candidate_rc_mode ->
 
3186,iiiii,[ sched_algo_dbg.c : 2137 ] mu_mimo_grp_stats:user %d -> ( %d, %d, %d, %d) 
 
3185,,[ sched_algo_dbg.c : 2143 ] mu_mimo_grp_stats:candidate_best_nss ->
 
3184,iiiii,[ sched_algo_dbg.c : 2173 ] mu_mimo_grp_stats:user %d -> (%d, %d, %d, %d) 
3183,,[ sched_algo_dbg.c : 2179 ] mu_mimo_grp_stats:candidate_sched_type ->
 
3182,iiiiii,[ sched_algo_dbg.c : 2196 ] mu_mimo_grp_stats:user %d -> ( %d, %d, %d, %d, %d) 
3181,,[ sched_algo_dbg.c : 2200 ] mu_mimo_grp_stats:candidate_sched_compatibility ->
 
3180,iIIIIii,[ sched_algo_dbg.c : 467 ] peer %d, mac %x %x, tx resource consumption %u, rx resource consumption %u, atf units: expected %d actual %d 
 
3179,iiiiiiiii,[ sched_algo_dbg.c : 2223 ] mu_mimo_grp_stats:user %d -> ( %d, %d, %d, %d, %d, %d, %d, %d) 
3178,,[ sched_algo_dbg.c : 2227 ] mu_mimo_grp_stats:candidate_nr_index ->
 
3177,iiiiiiiii,[ sched_algo_dbg.c : 2242 ] mu_mimo_grp_stats:user %d -> ( %d, %d, %d, %d, %d, %d, %d, %d) 
3176,iiii,[ sched_algo_dbg.c : 2270 ] mu_mimo_grp_stats:cd_num_eligible -> (%d, %d, %d, %d ) 
 
3175,,[ sched_algo_dbg.c : 2274 ] mu_mimo_grp_stats:mu_group_eligible_skip ->
 
3174,iiiiiiiii,[ sched_algo_dbg.c : 2297 ] mu_mimo_grp_stats:user %d ->( %d, %d, %d, %d, %d, %d, %d, %d) 
3173,iiiiiiiii,[ sched_algo_dbg.c : 2314 ] mu_mimo_grp_stats: mu_grp_invalid -> (%d, %d, %d, %d, %d, %d, %d, %d %d ) 
 
3172,i,[ sched_algo_dbg.c : 2320 ] mu_mimo_grp_stats:mu_grp_ineligible -> %d 
 
3171,i,[ sched_algo_dbg.c : 2326 ] mu_mimo_grp_stats:mu_grp_eligible -> %d 
 
3170,i,[ sched_algo_dbg.c : 2568 ] SCHED_RU_ALLOC_DBG: g_sched_algo_cfg.dbg.cnt.dl_mode_allocation_failed: %d 
3169,,[ sched_algo_dbg.c : 485 ] Resetting ATF stats 
 
3168,i,[ sched_algo_dbg.c : 2572 ] SCHED_RU_ALLOC_DBG: g_sched_algo_cfg.dbg.cnt.ul_mode_allocation_failed: %d 
3167,ii,[ sched_algo_dbg.c : 2581 ] SCHED_RU_ALLOC_DBG: g_sched_algo_cfg.dbg.cnt.sched_mode_disabled[%d]: %d 
3166,i,[ sched_algo_dbg.c : 2588 ] SCHED_RU_ALLOC_DBG: g_dbg_ul_ofdma_160mhz_ru_war.peers_ineligible: %d 
3165,i,[ sched_algo_dbg.c : 2592 ] SCHED_RU_ALLOC_DBG: g_dbg_ul_ofdma_160mhz_ru_war.peers_ineligible_ul_ofdma: %d 
3164,i,[ sched_algo_dbg.c : 2596 ] SCHED_RU_ALLOC_DBG: g_dbg_ul_ofdma_160mhz_ru_war.peers_eligible_ul_ofdma: %d 
3163,i,[ sched_algo_dbg.c : 2860 ] pdev %d not initialized 
 
3162,ii,[ sched_algo_dbg.c : 2864 ] pdev %d rx_ps_fifo_drop %d 
 
3161,iiii,[ sched_algo_dbg.c : 3045 ] ULMU_PRINT, FDRSSI_per_usr_nss_bin, %d, %d, %d: %d 
3160,iiiiii,[ sched_algo_dbg.c : 3146 ] ULMU_PRINT, mcs_0_5_per_AID, 1, 0:%d, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d 
3159,iiiiii,[ sched_algo_dbg.c : 3156 ] ULMU_PRINT, mcs_6_11_per_AID, 1, 6:%d, 7:%d, 8:%d, 9:%d, 10:%d, 11:%d 
3158,iiiii,[ sched_algo_dbg.c : 533 ] SCHED_LOGS: Num active tids in txq %d %d, %d, %d, %d 
 
3157,iiiiii,[ sched_algo_dbg.c : 3166 ] ULMU_PRINT, mcs_0_5_per_AID, 2, 0:%d, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d 
3156,iiiiii,[ sched_algo_dbg.c : 3176 ] ULMU_PRINT, mcs_6_11_per_AID, 2, 6:%d, 7:%d, 8:%d, 9:%d, 10:%d, 11:%d 
3155,iiiiii,[ sched_algo_dbg.c : 3186 ] ULMU_PRINT, mcs_0_5_per_AID, 3, 0:%d, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d 
3154,iiiiii,[ sched_algo_dbg.c : 3196 ] ULMU_PRINT, mcs_6_11_per_AID, 3, 6:%d, 7:%d, 8:%d, 9:%d, 10:%d, 11:%d 
3153,iiiiii,[ sched_algo_dbg.c : 3206 ] ULMU_PRINT, mcs_0_5_per_AID, 4, 0:%d, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d 
3152,iiiiii,[ sched_algo_dbg.c : 3216 ] ULMU_PRINT, mcs_6_11_per_AID, 4, 6:%d, 7:%d, 8:%d, 9:%d, 10:%d, 11:%d 
3151,iiiiii,[ sched_algo_dbg.c : 3226 ] ULMU_PRINT, mcs_0_5_per_AID, 5, 0:%d, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d 
3150,iiiiii,[ sched_algo_dbg.c : 3236 ] ULMU_PRINT, mcs_6_11_per_AID, 5, 6:%d, 7:%d, 8:%d, 9:%d, 10:%d, 11:%d 
3149,iiiiii,[ sched_algo_dbg.c : 3246 ] ULMU_PRINT, mcs_0_5_per_AID, 6, 0:%d, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d 
3148,iiiiii,[ sched_algo_dbg.c : 3256 ] ULMU_PRINT, mcs_6_11_per_AID, 6, 6:%d, 7:%d, 8:%d, 9:%d, 10:%d, 11:%d 
3147,ii,[ sched_algo_dbg.c : 537 ] SCHED_LOGS: Registered tids in txq %d list %d 
 
3146,iiii,[ sched_algo_dbg.c : 3280 ] ULMU_PRINT, FDRSSI_per_AID_nss_bin, %d, %d, %d: %d 
3145,iii,[ sched_algo_dbg.c : 3306 ] ULMU_PRINT, Target_RSSI_per_AID_bin, %d, %d: %d 
3144,iiiiiii,[ sched_algo_dbg.c : 3660 ] ATM: group_id %d, group_units %d, flags %d, wmm_be_units %d, wmm_bk_units %d, wmm_vo_units %d, wmm_vi_units %d 
3143,iiii,[ sched_algo_dbg.c : 3666 ] ATM: ERR_STATS Ivalid grp_id %d, Invalid group %d, Invalid group units %d, Invalid peer %d 
3142,iiii,[ sched_algo_dbg.c : 3673 ] ATM: Eligibility counters 0: %d, 1: %d, 2: %d, 3: %d 
3141,iii,[ sched_algo_dbg.c : 3714 ] STANDALONE INVALID SW PEER ID cmd num %d pdev id %d sw peer id %d 
3140,iii,[ sched_algo_dbg.c : 3717 ] STANDALONE  cmd num %d pdev id %d sw peer id %d  
3139,I,[ sched_algo_dbg.c : 3780 ] effective_tput_gain_factor: %u. 
3138,IIIII,[ sched_algo_dbg.c : 3845 ] UL_SCHED_DEC_STATS: ac: %u, count: %u, latency_sensitive: %u, psd_boost: %u, collision_reduction: %u 
3137,II,[ sched_algo_dbg.c : 3875 ] PARTIAL_SND_STATS: : MU2  1:%u 2:%u  
3136,i,[ sched_algo_dbg.c : 541 ] SCHED_LOGS: peer id %d 
 
3135,III,[ sched_algo_dbg.c : 3880 ] PARTIAL_SND_STATS: : MU3  1:%u 2:%u 3:%u 
3134,IIII,[ sched_algo_dbg.c : 3886 ] PARTIAL_SND_STATS: : MU4  1:%u 2:%u 3:%u 4:%u 
3133,II,[ sched_algo_dbg.c : 4016 ] dl_mu_mimo_my_cv_sync g_dbg_mu_cv_sync_counter: %u, g_dbg_mu_cv_sync_counter_invalid_idx: %u. 
3132,iiiiii,[ sched_algo_dbg.c : 4160 ] SCHED_CMD_DBG: AVG Tx: %d, AVG legacy Rx %d, AVG HE Rx: %d                      rx < tx | rx < ax_rx: %d, rx > tx -> 1. With pending sched cmds %d 2. No sched cmd %d 
3131,,[ sched_algo_dbg.c : 4192 ] SU_STATS_DBG: usage: wifitool athX setUnitTestCmd 0x47 3 258 < 0 / 1 > 
3130,,[ sched_algo_dbg.c : 4216 ] SU_STATS_DBG: ---Cleared all SU Multi Destination and SU Only stats--- 
3129,iiii,[ sched_algo_dbg.c : 4222 ] SU_STATS_DBG: num_su_multi_dest_scheduled: BK: %d | BE = %d | VI = %d | VO = %d 
3128,iiii,[ sched_algo_dbg.c : 4228 ] SU_STATS_DBG:       num_su_only_scheduled: BK: %d | BE = %d | VI = %d | VO = %d 
3127,i,[ sched_algo_dbg.c : 4290 ] STANDALONE INVALID SW PEER ID %d 
3126,,[ sched_algo_dbg.c : 4296 ] STANDALONE SEND MSG SUCCESSFUL 
3125,iii,[ sched_algo_dbg.c : 428 ] atf pdev %d tx resource consumption %d, rx resource consumption %d 
 
3124,iii,[ sched_algo_dbg.c : 547 ] SCHED_LOGS: Pdev id %d, txq %d, last sched order idx %d 
 
3123,,[ sched_algo_dbg.c : 4298 ] STANDALONE SEND MSG FAILED  
3122,iiii,[ sched_algo_dbg.c : 4320 ] AC_DBG: Requests BE: %d, BK: %d, VI: %d, VO: %d 
3121,iiii,[ sched_algo_dbg.c : 4321 ] AC_DBG: Counters Data Txq : %d, Other Txq: %d, i/p max_sched_cmd < pending sched_cmds: %d, default %d 
3120,I,[ sched_algo_dbg.c : 4430 ] CV_UPLOAD cv_fcs_err          : %u 
3119,I,[ sched_algo_dbg.c : 4433 ] CV_UPLOAD cv_frag_idx_mimatch : %u 
3118,I,[ sched_algo_dbg.c : 4436 ] CV_UPLOAD cv_invalid_peer_id  : %u 
3117,I,[ sched_algo_dbg.c : 4439 ] CV_UPLOAD cv_dma_not_done_err : %u 
3116,I,[ sched_algo_dbg.c : 4442 ] CV_UPLOAD cv_dma_timeout_err  : %u 
3115,I,[ sched_algo_dbg.c : 4445 ] CV_UPLOAD cv_nc_idx_mismatch  : %u 
3114,I,[ sched_algo_dbg.c : 4448 ] CV_UPLOAD cv_expiry_in_update : %u 
3113,iiiii,[ sched_algo_dbg.c : 556 ] SCHED_LOGS: last scheduled peer ids %d, %d, %d, %d, %d 
3112,I,[ sched_algo_dbg.c : 4451 ] CV_UPLOAD cv_update_failed    : %u 
3111,I,[ sched_algo_dbg.c : 4454 ] CV_UPLOAD cv_pkt_bw_exceed    : %u 
3110,I,[ sched_algo_dbg.c : 4505 ] DYN_MIMO_PS num_seq_posted: %u 
3109,II,[ sched_algo_dbg.c : 4510 ] DYN_MIMO_PS num_dyn_mimo_ps_users [%u]: %u 
3108,II,[ sched_algo_dbg.c : 4516 ] DYN_MIMO_PS num_users_posted [%u]: %u 
3107,II,[ sched_algo_dbg.c : 4575 ] ULMU_PRINT: Num Triggers %u: %u 
3106,II,[ sched_algo_dbg.c : 4578 ] ULMU_PRINT: Total Txop %u: %u 
3105,iiiiiiii,[ sched_algo_dbg.c : 4683 ] ULMU_PRINT: ulmu_mimo_grp_stats:mu_grp_best_grp_size -> (%d, %d, %d, %d, %d, %d, %d, %d )
  
3104,iiii,[ sched_algo_dbg.c : 4709 ] ULMU_PRINT: ulmu_mimo_grp_stats:mu_grp_best_num_users -> (%d, %d, %d, %d )
  
3103,iiiii,[ sched_algo_dbg.c : 4720 ] ULMU_PRINT: ulmu_mimo_grp_stats:mu_mimo_tputs_observed (0-1500Mbps)> (%d, %d, %d, %d, %d )
  
3102,iiiii,[ sched_algo_dbg.c : 1053 ] ac_mu_mimo : Num_users %d Per user txtime user%d_bin_%d - %d : %d 
3101,iiiii,[ sched_algo_dbg.c : 4730 ] ULMU_PRINT: ulmu_mimo_grp_stats:mu_mimo_tputs_observed (1500-3000Mbps) (%d, %d, %d, %d, %d)
  
3100,iiiiiiiii,[ sched_algo_dbg.c : 4744 ] ULMU_PRINT : ulmu_mimo_grp_stats:num_mu_mimo_candidate(0-8 users)-> ( %d, %d, %d, %d, %d, %d, %d, %d, %d )
  
3099,iiiiiiii,[ sched_algo_dbg.c : 4756 ] ULMU_PRINT: ulmu_mimo_grp_stats:num_mu_mimo_candidate(9-16 users)-> (%d, %d, %d, %d, %d, %d, %d, %d )
  
3098,i,[ sched_algo_dbg.c : 4759 ] ULMU_PRINT: ulmu_mimo_grp_stats:Group_id: %d  
3097,iiii,[ sched_algo_dbg.c : 4785 ] ULMU_PRINT: ulmu_mimo_grp_stats:cd_num_entries -> (%d, %d, %d, %d )
  
3096,iiiii,[ sched_algo_dbg.c : 4797 ] ULMU_PRINT: ulmu_mimo_grp_stats:tputs for this group id (0 - 1500 Mbps)-> (%d, %d, %d, %d, %d)  
3095,iiiii,[ sched_algo_dbg.c : 4807 ] ULMU_PRINT: ulmu_mimo_grp_stats:tputs for this group id(1500-3000 Mbps) -> (%d, %d, %d, %d, %d)  
3094,,[ sched_algo_dbg.c : 4810 ] ULMU_PRINT: ulmu_mimo_grp_stats:candidate_rc_mode ->
 
3093,iiiii,[ sched_algo_dbg.c : 4840 ] ULMU_PRINT: ulmu_mimo_grp_stats:user %d -> (%d, %d, %d ,%d) 
 
3092,,[ sched_algo_dbg.c : 4846 ] ULMU_PRINT: ulmu_mimo_grp_stats:candidate_best_nss ->
 
3091,ii,[ sched_algo_dbg.c : 1063 ] ac_mu_mimo : Num schedules with num_users as %d : %d 
3090,iiiiiiiii,[ sched_algo_dbg.c : 4876 ] ULMU_PRINT: ulmu_mimo_grp_stats:user %d -> (%d, %d, %d, %d, %d, %d, %d, %d) 
3089,,[ sched_algo_dbg.c : 4881 ] ULMU_PRINT: ulmu_mimo_grp_stats:candidate_sched_compatibility ->
 
3088,iiiiiiiii,[ sched_algo_dbg.c : 4904 ] ULMU_PRINT: ulmu_mimo_grp_stats:user %d -> ( %d, %d, %d, %d, %d, %d, %d, %d) 
3087,,[ sched_algo_dbg.c : 4908 ] ULMU_PRINT: ulmu_mimo_grp_stats:candidate_nr_index ->
 
3086,iiiiiiiii,[ sched_algo_dbg.c : 4923 ] ULMU_PRINT: ulmu_mimo_grp_stats:user %d -> ( %d, %d, %d, %d, %d, %d, %d, %d) 
3085,iiii,[ sched_algo_dbg.c : 4952 ] ULMU_PRINT: ulmu_mimo_grp_stats:cd_num_eligible -> (%d, %d, %d, %d ) 
 
3084,,[ sched_algo_dbg.c : 4956 ] ULMU_PRINT: ulmu_mimo_grp_stats:mu_group_eligible_skip ->
 
3083,iiiiiiiii,[ sched_algo_dbg.c : 4979 ] ULMU_PRINT: ulmu_mimo_grp_stats:user %d ->( %d, %d, %d, %d, %d, %d, %d, %d) 
3082,iiiiiiii,[ sched_algo_dbg.c : 4994 ] ULMU_PRINT: ulmu_mimo_grp_stats: mu_grp_invalid -> (%d, %d, %d, %d, %d, %d, %d, %d ) 
 
3081,i,[ sched_algo_dbg.c : 5000 ] ULMU_PRINT: ulmu_mimo_grp_stats:mu_grp_ineligible -> %d 
 
3080,iiiii,[ sched_algo_dbg.c : 1117 ] SCHED_LOGS: Peer AID %d: num_schedules = %d, ppdus_queued = %d, mpdus_enqueued = %d, mpdus_failed = %d
 
3079,i,[ sched_algo_dbg.c : 5006 ] ULMU_PRINT: ulmu_mimo_grp_stats:mu_grp_eligible -> %d 
 
3078,II,[ sched_algo_dbg.c : 5143 ] DYN_MIMO_PS sw_peer_id: %u, dyn_mimo_ps_enabled: %u. 
3077,,[ sched_algo_dbg.c : 5238 ] punc stats 
 
3076,i,[ sched_algo_dbg.c : 5241 ] punc vdev %d 
 
3075,,[ sched_algo_dbg.c : 5254 ] punc bss  
3074,,[ sched_algo_dbg.c : 5256 ] punc self  
3073,iIIII,[ sched_algo_dbg.c : 5266 ] peer %d, mac %x %x, punc capability %x, host config %x
 
3072,i,[ sched_algo_dbg.c : 5286 ] punc case 242 %d
 
3071,i,[ sched_algo_dbg.c : 5287 ] punc empty case 242 %d
 
3070,i,[ sched_algo_dbg.c : 5288 ] punc case 484 0 %d
 
3069,I,[ sched_algo_dbg.c : 1171 ] SCHED_LOGS: Tx_SCHEDULE_CMD Tx mode = %u 
 
3068,i,[ sched_algo_dbg.c : 5289 ] punc case 484 1 %d
 
3067,i,[ sched_algo_dbg.c : 5290 ] punc case 996 0 %d
 
3066,i,[ sched_algo_dbg.c : 5291 ] punc case 996 1 %d
 
3065,i,[ sched_algo_dbg.c : 5292 ] punc patt 1  %d
 
3064,i,[ sched_algo_dbg.c : 5293 ] punc patt 2  %d
 
3063,i,[ sched_algo_dbg.c : 5294 ] punc patt 3  %d
 
3062,i,[ sched_algo_dbg.c : 5295 ] punc patt 4  %d
 
3061,i,[ sched_algo_dbg.c : 5296 ] punc patt   %d
 
3060,i,[ sched_algo_dbg.c : 5297 ] punc legal_ru dl %d
 
3059,i,[ sched_algo_dbg.c : 5298 ] punc legal_ru ul %d
 
3058,IIiI,[ sched_algo_dbg.c : 1180 ] SCHED_LOGS: peer_aid = %u, weight = %u, OFDMA_status = %d, ru_width = %u 
 
3057,i,[ sched_algo_dbg.c : 5299 ] punc TLVs %d
 
3056,i,[ sched_algo_dbg.c : 5300 ] punc BW 20 %d
 
3055,i,[ sched_algo_dbg.c : 5301 ] punc BW 40 %d
 
3054,i,[ sched_algo_dbg.c : 5302 ] punc BW 80 %d
 
3053,i,[ sched_algo_dbg.c : 5303 ] punc BW 160 %d
 
3052,i,[ sched_algo_dbg.c : 5306 ] punc ru242_idx  %d
 
3051,I,[ sched_algo_dbg.c : 5406 ] twt_dbg: g_dbg_disable_triggers_from_wmm_txq = %u 
3050,I,[ sched_algo_dbg.c : 5470 ] dbg: g_dbg_disable_timeout_based_bsr_trigger = %u 
3049,i,[ sched_algo_dbg.c : 5521 ] MBO txmode current AC : %d 
 
3048,ii,[ sched_algo_dbg.c : 5523 ] MBO txmode %d : %d
 
3047,,[ sched_algo_dbg.c : 1185 ] SCHED_LOGS: PPDU_COMPLETION 
 
3046,I,[ sched_algo_dbg.c : 5548 ] Updated Idle condition trigger count as value = %u 
3045,IIIIII,[ sched_algo_dbg.c : 1194 ] SCHED_LOGS: peer_aid = %u, ru_width = %u, rtxop = %u, ppdu_duration = %u, nss_usr = %u, BW = %u 
 
3044,II,[ sched_algo_dbg.c : 1201 ] SCHED_LOGS: Last populated index TxScheduleCmd = %u, PPDUCompletion = %u 
  
3043,i,[ sched_algo_dbg.c : 431 ] atf vdev %d 
 
3042,iiiiiiii,[ sched_algo_dbg.c : 1393 ] ULMU_PRINT, Avg_FDRSSI  NSS:0 - 0:%d, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d, 6:%d, 7:%d 
3041,iiiiiiii,[ sched_algo_dbg.c : 1401 ] ULMU_PRINT, Avg_FDRSSI  NSS:1 - 0:%d, 1:%d, 2:%d, 3:%d, 4:%d, 5:%d, 6:%d, 7:%d 
3040,iiiiiiii,[ sched_algo_dbg.c : 1425 ] ULMU_PRINT, Avg_FDRSSI_AID NSS:0 - 1:%d, 2:%d, 3:%d, 4:%d, 5:%d, 6:%d, 7:%d, 8:%d 
3039,iiiiiiii,[ sched_algo_dbg.c : 1432 ] ULMU_PRINT, Avg_FDRSSI_AID NSS:1 - 1:%d, 2:%d, 3:%d, 4:%d, 5:%d, 6:%d, 7:%d, 8:%d 
3038,iiiiiiii,[ sched_algo_dbg.c : 1456 ] ULMU_PRINT, Avg_Target_RSSI AID - 1:%d, 2:%d, 3:%d, 4:%d, 5:%d, 6:%d, 7:%d, 8:%d 
3223,IIIII,[ sched_algo_twt.c : 230 ] twt_dbg: twt_construct_cl_super_cycle:peer_id=%u, START_TSF msb=%u, lsb=%u, peer_end_tsf msb=%u, lsb=%u 
3222,I,[ sched_algo_twt.c : 239 ] twt_dbg: twt_construct_cl_super_cycle peer_id=%u 
3221,IIIIIIII,[ sched_algo_twt.c : 949 ] twt_dbg_eosp: check_eosp_eligibility:tid_num=%u, inactivity_time_us=%u, last_activity_ts=%u, frms_swq=%u, frms_hwq=%u, is_eosp_eligible=%u,elapsed_time=%u, remaining_time=%u
 
3220,II,[ sched_algo_twt.c : 638 ] twt_dbg: twt_peer_register peer_id=%u, twt_peer_count=%u 
3219,II,[ sched_algo_twt.c : 642 ] twt_dbg: twt_peer_register g_dbg_disable_triggers_from_wmm_txq = %u; peer->is_wmm_txq_ul_trig_disabled = %u 
3218,III,[ sched_algo_twt.c : 687 ] twt_dbg: twt_peer_unregister peer_id=%u, twt_peer_count=%u, peer_twt_state=0x%x 
3217,IIiII,[ sched_algo_twt.c : 56 ] twt_dbg: twt_scheduler_timer1: tsf_now_msb=%u, lsb=%u, curr_slot_idx=%d, curr_slot_start msb=%u, lsb=%u 
3216,iiII,[ sched_algo_twt.c : 63 ] twt_dbg: twt_scheduler_timer1: 5ghz=%d, next_slot_idx=%d, next_slot_start msb=%u, lsb=%u 
3215,IIIi,[ sched_algo_twt.c : 98 ] twt_dbg: twt_scheduler_timer:peer_id=%u, peer_end_tsf msb=%u, lsb=%u, twt_qid=%d 
3214,Iii,[ sched_algo_twt.c : 530 ] twt_dbg: sched_algo_twt_sp_info_update peer_id=%u, is_announced=%d, is_ul_received=%d 
3213,I,[ sched_algo_twt.c : 557 ] twt_dbg: sched_algo_twt_sp_info_update_triggered_super_cycle peer_id=%u 
3212,IIIII,[ sched_algo_twt.c : 479 ] twt_dbg: twt_update_start_end_time peer_id=%u, start_time=%u, end_time=%u, flags=0x%x, valid=%u 
3225,IiIiii,[ sched_algo_ul_mumimo.c : 1022 ] UL_MUMIMO_DBG allocate1: peer=0x%x, tid_num=%d, tx_bw_mask=0x%x, ru_start_20=%d, ru_end_20=%d, stream_offset_20=%d 
3224,iiiiii,[ sched_algo_ul_mumimo.c : 1033 ] UL_MUMIMO_DBG allocate2: ru_start_40=%d, ru_end_40=%d, ru_start_80=%d, ru_end_80=%d, stream_offset_40=%d, stream_offset_80=%d 
3229,i,[ sched_algo_ulmu_grouping.c : 905 ] UL_MUMIMO_DBG: truncate UL MU-MIMO candidate list. num_entries %d 
3228,i,[ sched_algo_ulmu_grouping.c : 941 ] UL_MUMIMO_DBG: max_mu_grp_sz: %d 
3227,iii,[ sched_algo_ulmu_grouping.c : 493 ] UL_MUMIMO_DBG: sched_algo_construct_ulmu_candidate_table. group size %d, max_intf_nss %d, rc_mode_max %d 
3226,i,[ sched_algo_ulmu_grouping.c : 586 ] UL_MUMIMO_DBG: sched_algo_construct_ulmu_candidate_table. number of entries added %d 
3234,iiiii,[ sched_algo_qos_result.c : 719 ] ofdma_user_cap: tx_mode: %d, num_users: %d, sta_count_having_short_payload: %d, ul_sta_count_having_low_mcs: %d, truncate_candidate_list: %d 
3233,IiIii,[ sched_algo_qos_result.c : 1109 ] ul_dbg_passed_ru_alloc: peer=0x%x, tid_num=%d, tx_bw_mask=0x%x, ru_start_20=%d, ru_end_20=%d 
3232,iiii,[ sched_algo_qos_result.c : 1118 ] ul_dbg_passed_ru_alloc_2: ru_start_40=%d, ru_end_40=%d, ru_start_80=%d, ru_end_80=%d 
3231,ii,[ sched_algo_qos_result.c : 1388 ] Per user txtime user%d : %d 
3230,i,[ sched_algo_qos_result.c : 1314 ]  ul_ppdu_count %d
 
3245,IIIIIIIII,[ sched_algo_txbf.c : 830 ] SW Peer ID: %x cbf_mimo_ctrl VHT_HE: %x, NR: %x, NC: %x, FB: %x, BW: %x, NG: %x, CB: %x, BUF_IDX: %u. 
3244,IIII,[ sched_algo_txbf.c : 851 ] cbf_mimo_ctrl NC index mismatch. SW_PEER_ID: %u, PEER_NC: %u, CV_NC: %u, Total Mismatch: %u. 
3243,IIII,[ sched_algo_txbf.c : 1843 ] tone out of index: is_he:%x,cbf_bw:%x,pkt_bw:%x, ng:%x 
3242,IIII,[ sched_algo_txbf.c : 1852 ] tone out of index: is_he:%x,cbf_bw:%x,pkt_bw:%x, ng:%x 
3241,IIII,[ sched_algo_txbf.c : 1887 ] tone out of index: is_he:%x,cbf_bw:%x,pkt_bw:%x, ng:%x 
3240,IIII,[ sched_algo_txbf.c : 1896 ] tone out of index: is_he:%x,cbf_bw:%x,pkt_bw:%x, ng:%x 
3239,II,[ sched_algo_txbf.c : 1559 ] cbf nss mis-match cv_flags=%x cv_Nc=%x
 
3238,II,[ sched_algo_txbf.c : 1585 ] OFDMA cbf bw mis-match cv_flags=%x cv_bw=%x
 
3237,II,[ sched_algo_txbf.c : 1601 ] cbf bw mis-match cv_flags=%x cv_bw=%x
 
3236,II,[ sched_algo_txbf.c : 1610 ] cbf nr mis-match cv_flags=%x cv_Nr=%x
 
3235,Ii,[ sched_algo_txbf.c : 3493 ] cv_upload_dma invalid SW peer ID cv_buf->sw_peer_id 0x%x pdev_id %d 
3259,i,[ sched_algo_txbf_ofdma.c : 560 ] ru_to_start_and_end_tone (bw > BW_CNT) bw = %d 
3258,ii,[ sched_algo_txbf_ofdma.c : 565 ] ru_to_start_and_end_tone invalid ru_end (ru_end > MAX_RU_PER_BW[%d]) ru_end =%d 
3257,ii,[ sched_algo_txbf_ofdma.c : 570 ] ru_to_start_and_end_tone invalid ru_start (ru_start > MAX_RU_PER_BW[%d]) ru_start =%d 
3256,ii,[ sched_algo_txbf_ofdma.c : 576 ] ru_to_start_and_end_tone invalid ru_start/ru_end (ru_end < ru_start) ru_start = %d, ru_end = %d 
3255,i,[ sched_algo_txbf_ofdma.c : 581 ] ru_to_start_and_end_tone invalid (NG > WAL_TXBF_HE_NG_MAX) ng = %d 
3254,,[ sched_algo_txbf_ofdma.c : 586 ] ru_to_start_and_end_tone start_tone is NULL 
3253,,[ sched_algo_txbf_ofdma.c : 591 ] ru_to_start_and_end_tone end_tone is NULL 
3252,i,[ sched_algo_txbf_ofdma.c : 491 ] ru_to_tone_offset_size (bw > BW_CNT) bw = %d 
3251,ii,[ sched_algo_txbf_ofdma.c : 496 ] ru_to_tone_offset_size invalid ru_end (ru_end > MAX_RU_PER_BW[%d]) ru_end =%d 
3250,ii,[ sched_algo_txbf_ofdma.c : 501 ] ru_to_tone_offset_size invalid ru_start (ru_start > MAX_RU_PER_BW[%d]) ru_start =%d 
3249,ii,[ sched_algo_txbf_ofdma.c : 507 ] ru_to_tone_offset_size invalid ru_start/ru_end (ru_end < ru_start) ru_start = %d, ru_end = %d 
3248,i,[ sched_algo_txbf_ofdma.c : 512 ] ru_to_tone_offset_size invalid ng  ( ng  >= WAL_TXBF_HE_NG_MAX ), ng  = %d 
3247,,[ sched_algo_txbf_ofdma.c : 517 ] ru_to_tone_offset_size tone_offset is NULL 
3246,,[ sched_algo_txbf_ofdma.c : 522 ] ru_to_tone_offset_size num_tones is NULL 
3271,iiiiiiii,[ sched_algo_muedca.c : 406 ] MU_EDCA_DEBUG: compute_mu_edca_params: ac: %d, trig_capable_user_count: %d, non_trig_capable_user_count: %d, num_ulmu_non_cap_ax_sta: %d, rx_loading_pct: %d, num_mumimo_txop %d, ul_ppdu: %d, ul_tcp_ppdu: %d 
3270,IIII,[ sched_algo_muedca.c : 104 ] MU_EDCA_DEBUG: AIFS for BE = %u, CWMIN = %u, num_ax_sta: %u, num_legacy_sta: %u 
3269,II,[ sched_algo_muedca.c : 122 ] MU_EDCA_DEBUG: AIFS for VI = %u, CWMIN = %u 
3268,IIIII,[ sched_algo_muedca.c : 57 ] MU_EDCA_DEBUG: ULMU- AIFS for BE = %u, CWMIN = %u, num_ax_sta: %u, num_legacy_sta: %u, num_non_ulmu_cap_sta: %u 
3267,II,[ sched_algo_muedca.c : 75 ] MU_EDCA_DEBUG: ULMU- AIFS for VI = %u, CWMIN = %u 
3266,iiiiii,[ sched_algo_muedca.c : 598 ] MU_EDCA_DEBUG: ac: %d, wal_txq_num: %d, qnum: %d, aifs_n: %d, cw_min: %d, cw_max: %d 
3265,,[ sched_algo_muedca.c : 725 ] MU_EDCA_DEBUG: Running Dynamic MU EDCA update 
3264,iiiiii,[ sched_algo_muedca.c : 206 ] MU_EDCA_DEBUG: tune_edca_parameters: trig_capable_user_count: %d, non_trig_capable_user_count: %d, non_ulmu_trig_capable_user_count: %d, rx_loading_pct: %d, curr_state: %d, new_state: %d 
3263,iiiii,[ sched_algo_muedca.c : 238 ] MU_EDCA_DEBUG: tune_edca_parameters: applying config to ac %d, old aifs: %d, new aifs: %d, old cwmin: %d, new cwmin: %d 
3262,II,[ sched_algo_muedca.c : 666 ] MU_EDCA_DEBUG: Current OFDMA Trigger Status = %u for AC = %u 
3261,,[ sched_algo_muedca.c : 564 ] MU_EDCA_DEBUG: Sending WMI MESSAGE 
3260,IIII,[ sched_algo_muedca.c : 566 ] MU_EDCA_DEBUG: aifsn be = %u, bk = %u, vi = %u, vo = %u 
3274,,[ hca_HwComponentBbLithium_debug.cpp : 231 ] PHYDBG::Dump::Capture enable clear-Timeout
 
3273,,[ hca_HwComponentBbLithium_debug.cpp : 932 ] PHYDBG DISABLE: HcaHwComponentBbLithium_debug::PHYDBG_disable 
3272,,[ hca_HwComponentBbLithium_debug.cpp : 934 ] PHYDBG disabled
 
3275,i,[ hca_HwComponentBbLithium_pcss_ipc.cpp : 530 ] PcssIpcRingIRQHandler: PS Mode, ignoring IPC Ring IRQ! phyId:%d 
3276,I,[ hca_HwComponentBbLithium_phy.cpp : 139 ] %s
 
3285,III,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 316 ] DFS_DUMPS Rejecting Radar since delta peak values are invalid : dl_delta_peak_match_count=%lu, dl_psidx_diff_match_count=%lu, rf_threshold=%lu
 
3284,IIi,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 321 ] DFS_DUMPS %s: Rejecting Radar since duration diff %ld is more than %d
 
3283,i,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 576 ] DFS_DUMPS Rejecteing as radar injected in non-DFS channel, freq offset=%d 
3282,i,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 587 ] DFS_DUMPS Rejecteing as radar injected in non-DFS channel in 165MHZ. fre offset=%d 
3281,,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1009 ] DFS_DUMPS found bin5 radar
 
3280,ii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1051 ] DFS_DUMPS Rejecting pulses on rssi rssi=%d, thresh=%d
 
3279,iiii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1306 ] DFS_DUMPS Radar Found with Filter Id = %d min dur=%d sidx=%d freq_offset=%d
 
3278,ii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1313 ] CHANNEL_CLOSE radarevent g_dfs_test_mode=%d  event_data.detection_mode=%d
 
3277,i,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1414 ] DFS_DEBUGS false_radar dfs->dfs_seq_num =%d
 
3299,I,[ hca_HwComponentBbLithium_debug_core.cpp : 520 ] PHYDBG LWod 0x%lx
 
3298,I,[ hca_HwComponentBbLithium_debug_core.cpp : 521 ] PHYDBG UWod 0x%lx
 
3297,Ii,[ hca_HwComponentBbLithium_debug_core.cpp : 273 ] %s skipping bank %d
 
3296,I,[ hca_HwComponentBbLithium_debug_core.cpp : 471 ] PHYDBG_CAPTURE_U 0x%lx
 
3295,I,[ hca_HwComponentBbLithium_debug_core.cpp : 472 ] PHYDBG_CAPTURE_L 0x%lx
 
3294,I,[ hca_HwComponentBbLithium_debug_core.cpp : 473 ] PHYDBG_PLAYBACK_U 0x%lx
 
3293,I,[ hca_HwComponentBbLithium_debug_core.cpp : 474 ] PHYDBG_PLAYBACK_L 0x%lx
 
3292,I,[ hca_HwComponentBbLithium_debug_core.cpp : 475 ] PHYDBG_PHYRF_TX_PRE_DESC_WR_1_L 0x%lx
 
3291,I,[ hca_HwComponentBbLithium_debug_core.cpp : 476 ] PHYDBG_WFAX_PHYRF_PHYRF_ACTIVATION_CTRL_L 0x%lx
 
3290,I,[ hca_HwComponentBbLithium_debug_core.cpp : 477 ] PHYDBG_MODE_L 0x%lx
 
3289,I,[ hca_HwComponentBbLithium_debug_core.cpp : 478 ] PHYDBG_TRIGGER_0_L 0x%lx
 
3288,I,[ hca_HwComponentBbLithium_debug_core.cpp : 479 ] PHYDBG_TRIGGER_0_U 0x%lx
 
3287,I,[ hca_HwComponentBbLithium_debug_core.cpp : 480 ] PHYDBG_TRIGGER_1_L 0x%lx
 
3286,Ii,[ hca_HwComponentBbLithium_debug_core.cpp : 377 ] %s skipping bank %d
 
3303,iiIiiiiii,[ hca_HwComponentBbLithium_dfs_phyerr_tlv.cpp : 294 ] DFS_DUMPS ts=%d diff_ts=%d sidx=%i dur=%d chirp=%d det=%d radar_check=%d agc_event=%d rssi=%d  
3302,iiiii,[ hca_HwComponentBbLithium_dfs_phyerr_tlv.cpp : 300 ] DFS_DUMPS ts=%d delta_peak=%d delta_diff=%d total_gain=%d is_max_pw=%d  
3301,iiiii,[ hca_HwComponentBbLithium_dfs_phyerr_tlv.cpp : 324 ] DFS_DUMP radar summary detection_mode=%d  timestamp=%d pulse_rssi=%d is_chirp=%d sidx=%d
 
3300,iiiiiIiii,[ hca_HwComponentBbLithium_dfs_phyerr_tlv.cpp : 191 ] DFS_DUMPS ts=%d fft_num=%d radar_check=%d total_gain=%d base_pwr=%d peak_sidx=%i relpwr=%d peak_mag=%d num_str_bins_ib=%d
 
3313,ii,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 477 ] DFS_DUMP Dfs0Sighandler pHandle=%d ipc_ring_id=%d
 
3312,ii,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 485 ] DFS_DUMP Dfs1Sighandler pHandle=%d ipc_ring_id=%d
 
3311,ii,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 495 ] DFS_DUMP Dfs2Sighandler pHandle=%d ipc_ring_id=%d
 
3310,,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 268 ] FFT_RAW START 
 
3309,II,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 272 ] FFT_RAW %p 0x%x 
 
3308,II,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 276 ] FFT_RAW %p 0x%x 
 
3307,II,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 278 ] FFT_RAW %p 0x%x 
 
3306,II,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 279 ] FFT_RAW %p 0x%x 
 
3305,,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 284 ] FFT_RAW END 
 
3304,iii,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 458 ] DFS_DUMP pcss_ipc_sig_handler_process_multiple_ring_element pHandle=%d ipc_ring_id=%d num_bufs=%d
 
3314,ii,[ hca_HwComponentBbQcn9000_spectral.cpp : 483 ] SSCAN: BinIndices scanMode %d isChan165 %d 
3336,I,[ hca_HwComponentBbQcn9000_reset.cpp : 511 ] PCSS_VR: Indicate ucode on channel/band change UCODE_MODE_MAP writen value %x
 
3335,ii,[ hca_HwComponentBbQcn9000_reset.cpp : 360 ] DFS_DUMPS Post Prog Init phyDfsEnMask=%d, synthSelMask=%d
 
3334,iii,[ hca_HwComponentBbQcn9000_reset.cpp : 364 ] ASSCAN: Post Prog Init phySscanEnMask=%d, synthSelMask=%d aDfsSynthFreq=%d 
3333,ii,[ hca_HwComponentBbQcn9000_reset.cpp : 779 ] PerformPhyOff::BuildId=%d BranchId=%d is not supported
 
3332,ii,[ hca_HwComponentBbQcn9000_reset.cpp : 785 ] PerformPhyOff::BuildId=%d BranchId=%d is supported 
 
3331,Ii,[ hca_HwComponentBbQcn9000_reset.cpp : 797 ] PerformPhyOff:: q6_to_m3_ipc_address=0x%x q6_to_m3_ipc=%d 
 
3330,Ii,[ hca_HwComponentBbQcn9000_reset.cpp : 809 ] PerformPhyOff::(VR_Q6_TO_M3_10_L) failure status : 0x%x, loopCount=%d
 
3329,i,[ hca_HwComponentBbQcn9000_reset.cpp : 838 ] M3_SSR::CheckIfPhyIsOff CF_active: %d 
3328,,[ hca_HwComponentBbQcn9000_reset.cpp : 843 ] M3_SSR::CheckIfPhyIsOff:: Forcing CF_ACTIVE LOW 
3327,ii,[ hca_HwComponentBbQcn9000_reset.cpp : 848 ] M3_SSR::CheckIfPhyIsOff CF_active: %d readStatus: %d  
3326,,[ hca_HwComponentBbQcn9000_reset.cpp : 864 ] CheckIfPhyIsOff::phyOff was not received by uCode, forcing phyOff via Interrupt
 
3325,,[ hca_HwComponentBbQcn9000_reset.cpp : 870 ] CheckIfPhyIsOff::phyOff was received by uCode via TLV
 
3324,i,[ hca_HwComponentBbQcn9000_reset.cpp : 602 ] ANI_DUMP_PHYID%d SAVE ANI DEFAULTS 
 
3323,ii,[ hca_HwComponentBbQcn9000_reset.cpp : 186 ] ADFS_DUMPS / ASSCAN SetHwChainMasks phyDfsEnMask=%d phySscanEnMask=%d  
3322,iiiIi,[ hca_HwComponentBbQcn9000_reset.cpp : 958 ] ADFS_DUMPS / ASSCAN PostSetChannelAgile phyDfsEnMask=%d, phySscanEnMask=%d, synthSelMask=%d, rxchainmsk=%, txchainmsk=%d  
3321,i,[ hca_HwComponentBbQcn9000_reset.cpp : 221 ] Tx_Gain Overrided - %d
 
3320,,[ hca_HwComponentBbQcn9000_reset.cpp : 239 ] Tx_Gain Removed
 
3319,ii,[ hca_HwComponentBbQcn9000_reset.cpp : 1516 ] Before ShiftChainMask: tx:%d rx:%d 
3318,ii,[ hca_HwComponentBbQcn9000_reset.cpp : 1544 ] After ShiftChainMask: tx:%d rx:%d 
3317,,[ hca_HwComponentBbQcn9000_reset.cpp : 592 ] CV_UPLOAD_SIGNED Enabled
 
3316,,[ hca_HwComponentBbQcn9000_reset.cpp : 595 ] uCode does not advertised CV_UPLOAD_SIGNED Enabled
 
3315,,[ hca_HwComponentBbQcn9000_reset.cpp : 732 ] M3_SSR::WarmReset calling CheckIfPhyIsOff 
3338,,[ hca_HwComponentBbQcn9000_preInit.cpp : 236 ] No BDF merge since one of the pointer is NULL or invalid length 
3337,i,[ hca_HwComponentBbQcn9000_preInit.cpp : 241 ] golden bdf_calversion  : %d 
3339,ii,[ hca_HwComponentBbQcn9000_pcss.cpp : 133 ] PCSS Version : Branch = %d, Build ID = %d  
3340,iiiII,[ hca_HwComponentBbQcn9000_dfs_phyerr_tlv.cpp : 83 ] DFS_DUMP pcss_ipc_sig_handler_process_multiple_ring_element pHandle=%d ipc_ring_id=%d num_bufs=%d read_address=%p readaddressvalue=%p
 
3347,iI,[ hca_HwComponentBbQcn9000_ani.cpp : 282 ] ANI_EDCCA_PHYID%d MAX_ED_CCA=0x%x 
 
3346,iIII,[ hca_HwComponentBbQcn9000_ani.cpp : 300 ] ANI_EDCCA_PHYID%d ED_A_VAL=0x%x ED_B_VAL=0x%x ED_C_VAL=0x%x 
 
3345,iII,[ hca_HwComponentBbQcn9000_ani.cpp : 177 ] ANI_DUMP_PHYID%d DISABLED ANI rxtd_rssi_thr_l=%x rxtd_rssi_thr_u=%x 
 
3344,iI,[ hca_HwComponentBbQcn9000_ani.cpp : 118 ] ANI_DUMP OFDM DL=%d RSSI_THR_L =%x 
 
3343,iii,[ hca_HwComponentBbQcn9000_ani.cpp : 202 ] STR_DET_WAR ERROR RATE %d < %d THR %d
 
3342,iii,[ hca_HwComponentBbQcn9000_ani.cpp : 238 ] STR_DET_WAR ERROR RATE %d > %d THR %d
 
3341,i,[ hca_HwComponentBbQcn9000_ani.cpp : 258 ] STR_DET_WAR ERROR RATE CONSECUTIVE LESS ERROR Reset Regs THR %d
 
3352,,[ hca_HwComponentBbQcn9000_spurMit.cpp : 134 ] SpurMitigation: No 2G Spur freq available 
 
3351,,[ hca_HwComponentBbQcn9000_spurMit.cpp : 141 ] SpurMitigation: No 6G spur freq available 
 
3350,,[ hca_HwComponentBbQcn9000_spurMit.cpp : 143 ] SpurMitigation: No 5G spur freq available 
 
3349,IIII,[ hca_HwComponentBbQcn9000_spurMit.cpp : 498 ] %s PriCount : 0x%lx , 1stPriSpur : 0x%lx , 2ndPriSpur : 0x%lx 
 
3348,IIII,[ hca_HwComponentBbQcn9000_spurMit.cpp : 499 ] %s ExtCount : 0x%lx , 1stExtSpur : 0x%lx , 2ndExtSpur : 0x%lx 
 
3357,i,[ phyDevLibCommon.c : 67 ] Error: Invalid PHY ID [=%d] 
3356,II,[ phyDevLibCommon.c : 125 ] Dumping PDMEM: [0x%08lx : 0x%08lx] 
3355,,[ phyDevLibCommon.c : 130 ] Dumping PDMEM Done 
3354,I,[ phyDevLibCommon.c : 88 ] Switch WCSS ENV to %s 
3353,,[ phyDevLibCommon.c : 44 ] register polling disabled 
3359,,[ phyIniAg.c : 411 ] Error: cannot commit NULL table! 
3358,iI,[ phyIniAg.c : 438 ] Note: table filtered out. table[%d].filter = %c 
3362,I,[ phy_dev_init.c : 281 ] Fatal Error! Invalid PHY ID[=%lu]. 
3361,I,[ phy_dev_init.c : 89 ] wlan base: 0x%x 
3360,III,[ phy_dev_init.c : 99 ] CHIP: %s ENV: %s VER: %s 
3375,Ii,[ m3_init.c : 98 ] %s: phy%d 
3374,,[ m3_init.c : 119 ] M3 Reset de-asserted [Running @640MHz] 
3373,i,[ m3_init.c : 120 ] Polling for boot completion ... [max_poll_count = %d] 
3372,,[ m3_init.c : 136 ] Warning: Max Poll Count Exceeded 
3371,,[ m3_init.c : 143 ] M3 is idle 
3370,,[ m3_init.c : 148 ] Alert: M3 has reported boot failure 
3369,,[ m3_init.c : 156 ] Error: Could not detect M3 Boot completion 
3368,,[ m3_init.c : 105 ] M3 is already Running. Asserting Reset 
3367,,[ m3_init.c : 230 ] Recipe Complete 
3366,,[ m3_init.c : 197 ] invalid phym3 binary, skip loading 
3365,,[ m3_init.c : 201 ] Loading PDMEM (may take few minutes)... 
3364,iIIII,[ m3_init.c : 207 ] seg%d: buf: %p dsize: %x msize: %x offset: %x 
3363,,[ m3_init.c : 211 ] Loading PDMEM done 
3382,ii,[ m3Config.c : 353 ] [uCode] Branch=%d Ver=%d 
3381,i,[ m3Config.c : 357 ] Warning: uCode version mismatch detected [Expected Ver >= %d] 
3380,i,[ m3Config.c : 114 ] Fatal Error: Invalid PHYID[=%d] 
3379,I,[ m3Config.c : 239 ] forceCrashMask=0x%0.08x 
3378,,[ m3Config.c : 269 ] DFS INI programmed 
3377,i,[ m3Config.c : 126 ] phyM3Ini: phyId = %d 
3376,,[ m3Config.c : 293 ] SPECTRAL SCAN INI programmed 
3386,i,[ phy_dev_setChainMask.c : 130 ] phySetChainMask: setting chain mask for phyId = %d ... 
3385,,[ phy_dev_setChainMask.c : 134 ]          RXCHMASK will be forced to 0x1 
3384,i,[ phy_dev_setChainMask.c : 188 ] phySetChainMask: chain mask for phyId = %d completed 
3383,iiI,[ phy_dev_setChainMask.c : 133 ] Warning: [PHYID=%d isSBS=%d RXCHMASK=0x%X] is not supported. 
3388,i,[ phy_dev_setXbar.c : 75 ] phySetXbar: setting xbar for phyId = %d ... 
3387,i,[ phy_dev_setXbar.c : 88 ] phySetXbar: xbar for phyId = %d completed 
3390,iiii,[ phyHeavyClip.c : 219 ] isHcEn_qcn90xx : mcs[%d] nss[%d] pktType[%d] hcEn [%d] 
3389,iii,[ phyHeavyClip.c : 259 ] heavyClipPerMcs:%d, heavyClipEnablePktType:%d, heavyClipNssThreshold:%d 
3393,IIII,[ phyInitCfoCsr.c : 114 ] fc=%f fcPri20=%f shft_pri80in160=%f cfoCorrFracFloat=%f 
3392,III,[ phyInitCfoCsr.c : 147 ] cfoCorrFracPri80=%hhd cfoCorrFracSec80=%hhd cfoCorrFrac_80in160=%hhd 
3391,II,[ phyInitCfoCsr.c : 159 ] vsrc_ppm_fc_factor(%uMHz) = %u 
3395,,[ phyRegIni.c : 336 ] DFS INI programmed 
3394,,[ phyRegIni.c : 383 ] Sscan INI programmed 
3415,,[ phyReset.c : 867 ] RxDco Cal complete.
 
3414,i,[ phyReset.c : 93 ] [phyId=%d] 
3413,i,[ phyReset.c : 96 ] [bandCode=%d] 
3412,I,[ phyReset.c : 97 ] [rxChMask=0x%x] 
3411,i,[ phyReset.c : 98 ] [dynPriChn=%d] 
3410,i,[ phyReset.c : 99 ] [band_center_freq1=%dMHz] 
3409,i,[ phyReset.c : 100 ] [band_center_freq2=%dMHz] 
3408,I,[ phyReset.c : 101 ] [loadIniMask=0x%x] 
3407,I,[ phyReset.c : 94 ] [phyBase=0x%0.08x] 
3406,i,[ phyReset.c : 95 ] [bwCode=%d] 
3405,,[ phyReset.c : 822 ] Recipe Complete phyChannelSwitch_qcn90xx 
3404,,[ phyReset.c : 136 ] (Start) 
3403,,[ phyReset.c : 153 ] (End) 
3402,,[ phyReset.c : 848 ] Recipe Complete 
3401,,[ phyReset.c : 111 ] phyRegAccessPass 
3400,,[ phyReset.c : 707 ] Error: Skipping phyReset since reset_input is NULL!!  
3399,I,[ phyReset.c : 712 ] [phyResetCtrl=0x%x] 
3398,,[ phyReset.c : 717 ] Error: phyRegAccess Failed 
3397,I,[ phyReset.c : 718 ] Skipping phyReset for [phyBase = 0x%0.08X] 
3396,,[ phyReset.c : 781 ] Recipe Complete phyReset_qcn90xx  
3417,i,[ phySetRx11bDetThr.c : 67 ] phySetRx11bDetCorrThr: Warning: numRxChain = %d was unexpected! 
3416,,[ phySetRx11bDetThr.c : 78 ] Recipe Complete 
3418,I,[ phySetRxfePerNrx.c : 139 ] numChains = %lu 
3422,i,[ phyCfrCirCap.c : 41 ] Enable CFR ini programming phyId=%d 
3421,i,[ phyCfrCirCap.c : 52 ] Restoring Enable CFR ini programed phyId=%d 
3420,i,[ phyCfrCirCap.c : 63 ] Enable CFR ini programming phyId=%d 
3419,i,[ phyCfrCirCap.c : 74 ] Restoring Enable CFR ini programed phyId=%d 
3424,i,[ phyRtt.c : 41 ] RTT per busrt ini programming phyId=%d 
3423,i,[ phyRtt.c : 53 ] Restoring RTT per burst ini programed phyId=%d 
3426,iii,[ phySpurMitigation.c : 147 ]  numberOfSpurs = %d 
 spur1Offset = %d 
 spur2Offset = %d 
3425,I,[ phySpurMitigation.c : 248 ] WFAX_RXTD_NOTCH_CNTL_1_L = 0x%lx 
3428,,[ phyWarmRst.c : 43 ] Executing Warm Reset on PHYA 
3427,,[ phyWarmRst.c : 49 ] RECIPE COMPLETE 
3429,iiiI,[ phyVersion.c : 18 ] HDL Version %d.%d.%d (Released On %s) 
3504,iiiiii,[ phyrf_ani.c : 114 ] NFREAD%d PHYID=%d NFInDBr=%d NFToDBm=%d maxNumChain=%d maxNFInDBm=%d 
 
3503,ii,[ phyrf_ani.c : 125 ] ANI_LOG: ETSI Domain - maxNFInDBm=%d, DL_MAX value =%d 
3502,i,[ phyrf_ani.c : 130 ] ANI_LOG - DL_MAX value =%d 
3501,iiii,[ phyrf_ani.c : 163 ] ANI_EDCCA_PHYID%d CHAIN%d NFBDF=%d NFRUNTIME=%d 
3500,iiiiii,[ phyrf_ani.c : 170 ] ANI_EDCCA_PHYID%d NFBDF=%d NFRUNTIME=%d DELTA=%d txChainMask=%d rxChainMask=%d 
3499,i,[ phyrf_ani.c : 176 ] ANI_API_PHYID%d API: ANI CONFIGURE 
 
3498,iiiii,[ phyrf_ani.c : 241 ] ANI_DUMP_PHYID%d DL_OFDM %d DL_CCK %d DL_MIN %d DL_MAX %d 
 
3497,iiii,[ phyrf_ani.c : 244 ] ANI_DUMP_PHYID%d DL_OFDM %d DL_MIN %d DL_MAX %d 
 
3496,i,[ phyrf_ani.c : 373 ] ANI_LOG PHY%d ANI_RESET 
 
3495,i,[ phyrf_ani.c : 375 ] ANI_LOG PHY%d ANI_RESET 
 
3494,I,[ phyrf_ani.c : 380 ] ANI_CHANNEL_CHANGE - resetCause=%x 
 
3493,ii,[ phyrf_ani.c : 386 ] ANI_CHANNEL_CHANGE - clear ANI histogram counters phyID=%d ,size=%d 
 
3492,iiiii,[ phyrf_ani.c : 448 ] ANI_DUMP_PHYID%d ofdmPhyErrCnt %d lsigPhyErrCnt %d cckPhyErrCnt %d sizing1 %d 
 
3491,iiiiiii,[ phyrf_ani.c : 582 ] ANI_LOG PHYA POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL -%d
 
3490,iiiiiii,[ phyrf_ani.c : 584 ] ANI_LOG PHYA POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL %d
 
3489,ii,[ phyrf_ani.c : 593 ] ANI_DUMP_PHYID%d ERROR RATE < %d PERCENT 
 
3488,ii,[ phyrf_ani.c : 608 ] ANI_DUMP_PHYID%d ERROR RATE > %d PERCENT 
 
3487,i,[ phyrf_ani.c : 629 ] ANI_DUMP_PHYID%d CONSECUTIVE ERROR, INCREMENTING DESENSE LEVEL 
 
3486,i,[ phyrf_ani.c : 647 ] ANI_DUMP_PHYID%d CONSECUTIVE LESS ERROR, DECREMENTING DESENSE LEVEL 
 
3485,ii,[ phyrf_ani.c : 687 ] ANI_DUMP PHYID%d ramp_up_time %dms
 
3484,ii,[ phyrf_ani.c : 703 ] ANI_DUMP PHYID%d ramp_down_time %dms
 
3483,iiii,[ phyrf_ani.c : 454 ] ANI_LOW_POWER_CNTR_PHYID%d rxClearCnt %d ccaCntr0 %d time %d 
 
3482,iii,[ phyrf_ani.c : 455 ] ANI_DUMP_PHYID%d CYCLE_CNT %d time %d 
 
3481,iiiiii,[ phyrf_ani.c : 493 ] ANI_LOW_POWER_CNTR_PHYID%d cycleCnt %d txFrameCnt %d rxframecnt %d rxClearCnt %d time %d 
 
3480,iii,[ phyrf_ani.c : 495 ] ANI_EDCCA_PHYID%d raw_nfdelta=%d pedccaParam->curr_delta=%d 
 
3479,ii,[ phyrf_ani.c : 524 ] ANI_DUMP LISTEN_TIME=%d , log_cnt=%d 
 
3478,i,[ phyrf_ani.c : 542 ] ANI_DUMP Log_cnt=%d 
 
3477,ii,[ phyrf_ani.c : 548 ] ANI_DUMP 2GHZ bo=%d, bc=%d 
 
3476,iiiiiiii,[ phyrf_ani.c : 550 ] ANI_LOG PHYB POLL %dms LISTEN %dms: OFDM %d LSIG %d CCK %d SIZ1 %d M %d OFDM_DL -%d 
 
3475,iiiiiiii,[ phyrf_ani.c : 552 ] ANI_LOG PHYB POLL %dms LISTEN %dms: OFDM %d LSIG %d CCK %d SIZ1 %d M %d OFDM_DL %d 
 
3474,iiiiiiii,[ phyrf_ani.c : 554 ] ANI_LOG PHYB POLL %dms LISTEN %dms: OFDM %d LSIG %d CCK %d SIZ1 %d M %d OFDM_DL -%d 
 
3473,iiiiiiii,[ phyrf_ani.c : 556 ] ANI_LOG PHYB POLL %dms LISTEN %dms: OFDM %d LSIG %d CCK %d SIZ1 %d M %d OFDM_DL %d 
 
3472,,[ phyrf_ani.c : 561 ] ANI_DUMP 5GHZ 
 
3471,iiiiiii,[ phyrf_ani.c : 567 ] ANI_LOG PHYA1 POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL -%d
 
3470,iiiiiii,[ phyrf_ani.c : 569 ] ANI_LOG PHYA1 POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL %d
 
3469,iiiiiii,[ phyrf_ani.c : 574 ] ANI_LOG PHYA0 POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL -%d
 
3468,iiiiiii,[ phyrf_ani.c : 576 ] ANI_LOG PHYA0 POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL %d
 
3467,i,[ phyrf_ani.c : 805 ] ANI_LOG - phyrf_ani_EnableAni - g_ani_enable=%d 
 
3466,ii,[ phyrf_ani.c : 811 ] ANI_DUMP_PHYID%d ANI API ENABLED %d 
 
3465,ii,[ phyrf_ani.c : 837 ] ANI_DUMP_PHYID%d ENABLED %d 
 
3464,ii,[ phyrf_ani.c : 852 ] ANI_DUMP_PHYID%d DISABLED %d 
 
3463,ii,[ phyrf_ani.c : 949 ] ANI_DUMP_PHYID%d GET ANI STATE %d 
 
3462,i,[ phyrf_ani.c : 1539 ] phyrf_ani_GetCckLevel (Invalid PHY_ID) phyID=%d 
3461,iii,[ phyrf_ani.c : 1551 ] phyrf_ani_GetCckLevel (ANI not enabled) phyID=%d, g_ani_enable[%d]=%d 
3460,i,[ phyrf_ani.c : 358 ] ANI_LOG GetListenTime=%d 
3459,i,[ phyrf_ani.c : 1515 ] phyrf_ani_GetOfdmLevel (Invalid PHY_ID) phyID=%d 
3458,iii,[ phyrf_ani.c : 1527 ] phyrf_ani_GetOfdmLevel (ANI not enabled) phyID=%d, g_ani_enable[%d]=%d 
3457,iii,[ phyrf_ani.c : 1140 ] ANI_LOG - OverrideAniDlMinMax aniMode=%d, DL_min=%d, DL_max=%d 
3456,ii,[ phyrf_ani.c : 1081 ] ANI_LOG - SetAniCckImmunLevel - g_ani_trigger=%d, pAniParam->dl_cck=%d 
3455,ii,[ phyrf_ani.c : 943 ] ANI_LOG PHYID%d SetAniListenPeriod %d 
 
3454,i,[ phyrf_ani.c : 1029 ] ANI_LOG PHYID%d SetAniOfdmImmunLevel error : ANI Disabled.Cannot set OFDM level 
 
3453,ii,[ phyrf_ani.c : 1053 ] ANI_LOG - SetAniOfdmImmunLevel - g_ani_trigger=%d, pAniParam->dl_ofdm=%d 
3452,iiii,[ phyrf_ani.c : 1231 ] ANI_LOG - SetAniPollListenDesenseStepSize - PHYID=%d aniMode=%d SetAniPollPeriod=%d SetAniListenPeriod=%d 
3451,ii,[ phyrf_ani.c : 936 ] ANI_LOG PHYID%d SetAniPollPeriod %d 
 
3450,iii,[ phyrf_ani.c : 1193 ] ANI_LOG - SetMinAniDl -MinAniDl_input=%d, DL_min=%d, DL_max=%d 
3449,i,[ phyrf_ani.c : 1366 ] 
 ANI-VREG-ERR Invalid ANI hist types =%d 
3448,,[ phyrf_ani.c : 1375 ] 
ANI-VREG-ERR LIST 
3447,i,[ phyrf_ani.c : 1376 ] 
ANI-VREG-ERR phyId=%d 
3446,i,[ phyrf_ani.c : 1377 ] 
ANI-VREG-ERR Latest index in histogram =%d 
3445,,[ phyrf_ani.c : 1380 ] 
ANI-VREG-ERR collection_interval = 10ms
 
3444,,[ phyrf_ani.c : 1382 ] 
ANI-VREG-ERR collection_interval = 1second
 
3443,i,[ phyrf_ani.c : 1384 ] 
ANI-VREG-ERR Channel-frequency (Mhz) =%d 
3442,,[ phyrf_ani.c : 1390 ] ANI-VREG-ERR |rx_ofdma_timing_err | rx_cck_fail |mac_tx_abort | mac_rx_abort |phy_tx_abort | phy_rx_abort | phyrf_defer_abort| sizing1_evt | sizing2_evt 
 
3441,IIIIIIIII,[ phyrf_ani.c : 1405 ] ANI-VREG-ERR |%20u|%13u|%13u|%14u|%13u|%14u|%18u|%13u|%13u 
 
3440,,[ phyrf_ani.c : 1414 ] ANI-VREG-ERR |RX_PKT_CNT_11A |RX_PKT_CNT_11B |RX_PKT_CNT_11N |RX_PKT_CNT_11AC |RX_PKT_CNT_11AX |RX_PKT_CNT_GF 
 
3439,IIIIII,[ phyrf_ani.c : 1426 ] ANI-VREG-ERR |%15u|%15u|%15u|%16u|%16u|%14u 
 
3438,,[ phyrf_ani.c : 1435 ] ANI-VREG-ERR |RX_PKT_CRC_PASS_CNT_11A |RX_PKT_CRC_PASS_CNT_11B |RX_PKT_CRC_PASS_CNT_11N |RX_PKT_CRC_PASS_CNT_11AC |RX_PKT_CRC_PASS_CNT_11AX |RX_PKT_CRC_PASS_CNT_GF 
 
3437,IIIIII,[ phyrf_ani.c : 1447 ] ANI-VREG-ERR |%24u|%24u|%24u|%25u|%25u|%23u 
 
3436,,[ phyrf_ani.c : 1456 ] ANI-VREG-ERR |LSIG_ERROR | HTSIG_ERROR |VHTSIG_ERROR |HESIG_ERROR |RXTD_OTA |RXTD_FATAL |TXFD |TXTD |PHYRF 
 
3435,IIIIIIIII,[ phyrf_ani.c : 1471 ] ANI-VREG-ERR |%11u|%13u|%13u|%12u|%9u|%11u|%5u|%5u|%5u 
 
3434,,[ phyrf_ani.c : 1480 ] ANI-VREG-ERR |VOTING_FAIL |WEAK_DET_FAIL |STRONG_SIG_FAIL |CCK_FAIL |POWER_SURGE |BTCF_TIMING |BTCF_PACKET_DETECT |COARSE_TIMEOUT 
 
3433,IIIIIIII,[ phyrf_ani.c : 1494 ] ANI-VREG-ERR |%12u|%14u|%16u|%9u|%12u|%12u|%19u|%14u 
 
3432,I,[ phyrf_ani.c : 1503 ] ANI-VREG-ERR - Invalid Error TYPE = %x 
 
3431,i,[ phyrf_ani.c : 396 ] ANI_DUMP_PHYID%d READ AND CACHE VREG VALUES 
 
3430,i,[ phyrf_ani.c : 271 ] ANI_DUMP_PHYID%d RESTORE DL 
 
3541,,[ phyrf_bdf.c : 4587 ] Functionality unavailable now  
3540,,[ phyrf_bdf.c : 4623 ] phyrf_Set_BDFVersion: Feature support unavailable 
3539,ii,[ phyrf_bdf.c : 4593 ] phyrf_Get_BDFVersion: SW major : %d , SW minor: %d 
3538,I,[ phyrf_bdf.c : 4599 ] phyrf_Get_BDFVersion: setting meta no.: %u 
3537,I,[ phyrf_bdf.c : 4611 ] phyrf_Get_BDFVersion: ProjectID: 0x%x 
3536,,[ phyrf_bdf.c : 4616 ] phyrf_Get_BDFVersion:OPERATION UNALLOWED  
3535,,[ phyrf_bdf.c : 4537 ] phyrf_Set_BDFVersion: setting BDF tpl ver. 
3534,ii,[ phyrf_bdf.c : 4542 ] phyrf_Set_BDFVersion: major: %d, minor : %d 
3533,I,[ phyrf_bdf.c : 4546 ] phyrf_Set_BDFVersion: meta: %u 
3532,I,[ phyrf_bdf.c : 4557 ] phyrf_Set_BDFVersion: projectID: 0x%x 
3531,I,[ phyrf_bdf.c : 4561 ] phyrf_Set_BDFVersion: ProjectID: 0x%x 
3530,,[ phyrf_bdf.c : 4563 ] phyrf_Get_BDFVersion: ProjectID:ERROR! OTP WRITE UNALLOWED 
3529,I,[ phyrf_bdf.c : 4566 ] phyrf_Set_BDFVersion:WARNING: OTP fused: projectID: 0x%x 
3528,,[ phyrf_bdf.c : 4574 ] phyrf_Set_BDFVersion: Feature support unavailable 
3527,II,[ phyrf_bdf.c : 4251 ] %s:EEPROM i2cResult - %ld 
3526,I,[ phyrf_bdf.c : 4256 ] %s:EEPROM Init failed 
3525,,[ phyrf_bdf.c : 2558 ] TPC: isFbin is TRUE 
3524,i,[ phyrf_bdf.c : 2571 ] TPC: pTpcCalFreq=%d 
3523,i,[ phyrf_bdf.c : 2579 ] TPC: chans5G=%d 
3522,i,[ phyrf_bdf.c : 2591 ] TPC: chans5G=%d 
3521,i,[ phyrf_bdf.c : 2624 ] TPC: chans6G=%d 
3520,i,[ phyrf_bdf.c : 1074 ] TPC_DLOFDMA: Target power is %d
 
3519,iiii,[ phyrf_bdf.c : 1418 ] DumpTpcPerPacket: rtIdx = %d numStreams %d numChains %d rateCode %d
 
3518,iii,[ phyrf_bdf.c : 1489 ] DumpTpcPerPacket: Get Rate CTL pwr TPC pwr = ch0=%d ch1=%d phy: %d
 
3517,iii,[ phyrf_bdf.c : 1539 ] DumpTpcPerPacket: Get Rate regulatory pwr TPC pwr = ch0=%d ch1=%d phy: %d
 
3516,iii,[ phyrf_bdf.c : 1604 ] DumpTpcPerPacket: Get Rate regulatory pwr TPC pwr = ch0=%d ch1=%d phy: %d
 
3515,iii,[ phyrf_bdf.c : 1479 ] DumpTpcPerPacket: Get Rate target pwr TPC pwr = ch0=%d ch1=%d phy: %d
 
3514,,[ phyrf_bdf.c : 1848 ] phyrf_bdf_GetTpcMaxTxPwr :: Invalid Channel Frequency 
3513,iiIi,[ phyrf_bdf.c : 1869 ] GetTpcMaxTxPwr: phyId %d txCM %d rcFlags 0x%x tpc_max_tx_power %d 
3512,i,[ phyrf_bdf.c : 1877 ] MaxPwr tpc_max_tx %d
 
3511,II,[ phyrf_bdf.c : 4391 ] %s: eeprom addr - %lx 
3510,III,[ phyrf_bdf.c : 4392 ] %s: read failed expected - %ld retrived - %ld 
3509,i,[ phyrf_bdf.c : 2845 ] phyrf_bdf_SetBoardCalVersion: New CalVersion %d is programmed 
3508,,[ phyrf_bdf.c : 2848 ] phyrf_bdf_SetBoardCalVersion: SwCalVersion is zero, if MergeBDF() not executed due to NO-caldata in the board. 
3507,II,[ phyrf_bdf.c : 4458 ] %s: eeprom addr - %lx 
3506,III,[ phyrf_bdf.c : 4459 ] %s: write failed expected - %ld retrived - %ld 
3505,,[ phyrf_bdf.c : 4779 ] DumpTpcPerPacket: Set regulatory Info Hal-phy call 
 
3549,IIIIIII,[ phyrf_cal.c : 791 ] phyid %u, mhz %4u, f1 %4u, f2 %4u, phyMode %2u, calType %2u, calResult %3u 
3548,i,[ phyrf_cal.c : 104 ] Skip Periodic NFCAL for phyId %d 
3547,i,[ phyrf_cal.c : 705 ] in phyrf_cal_RunDPDCalibration : %d
 
3546,iiiI,[ phyrf_cal.c : 1087 ] cp_stats : total_num_cals %d num_pdev_ids_processed %d buf_length %d buf_ptr 0x%x 
3545,iii,[ phyrf_cal.c : 1096 ] cp_stats param_tlv->pdev_ids %d mac_id %d phy_id %d 
3544,iiiiii,[ phyrf_cal.c : 909 ] phyrf_cal_log_calibration_stats : CAL_STATS calProfile %d calType %d cal_triggered_cnt: %d cal_fail_cnt: %d cal_fcs_cnt: %d cal_fcs_fail_cnt: %d 
3543,iii,[ phyrf_cal.c : 949 ] phyrf_cal_log_calibration_stats : CAL_STATS periodicCalType %d cal_triggered_cnt: %d cal_fail_cnt: %d 
3542,IIiI,[ phyrf_cal.c : 1001 ] cp_stats cal_type 0x%x cal_profile 0x%x isPeriodic %d cal_info 0x%x 
3561,IIII,[ phyrf_cal_sm.c : 853 ] CC::: inside cal_SM_Main, 0x%x, (pHandle=0x%x, smInput=0x%x, pCalSmTable=0x%x) 
3560,iIII,[ phyrf_cal_sm.c : 934 ] CAL SM::: cal type idx=%d, ptrStandalone=%x, pIn=%x, pOut=%x  
3559,Iii,[ phyrf_cal_sm.c : 551 ] CC::: generateCalSmTable=0x%x, callingContext=%d, curCalTypeIdx=%d 
3558,iiiiiIIi,[ phyrf_cal_sm.c : 598 ] CALSM: 	globalCallingContext[%d]=%d, 	mhz=%d, 	freq1=%d, 	freq2=%d, 	phy_mode=%3d, 	chainMask=%2X, 	Total_cal_time=%d us 
3557,ii,[ phyrf_cal_sm.c : 600 ] Summary starts: calibration with globalCallingContext[%d]=%d 
3556,iiiii,[ phyrf_cal_sm.c : 612 ] :::::::: %d	%d	%d	%d	%d 
3555,iI,[ phyrf_cal_sm.c : 657 ] CAL SM::: genCalTable calType=%d hwCalMask 0x%x 
3554,iii,[ phyrf_cal_sm.c : 1032 ] CAL SM::: Phy mode=%d, IsTrue160supported=%d, bwcode=%d 
3553,Iiiii,[ phyrf_cal_sm.c : 175 ] CALSM: %x,  callingContext=%d, dB size = %d, masterCalDbExist()=%d, isSBS=%d 
3552,iiiii,[ phyrf_cal_sm.c : 465 ] :::: shortenPhyId=%d, callingContext = %d, Final doCalFlag = %d, docalFlagRxDCO = %d doCalFlagCombIQ = %d 
3551,iiiii,[ phyrf_cal_sm.c : 183 ] CALSM:  final 	calDBEnableSetting=%d, 	final CalTimeOutSetting = %d, 	final PersistentEnable = %d, 	masterCalDbExist()=%d, ColdBootDfsCalEnable=%d 
3550,iiii,[ phyrf_cal_sm.c : 322 ] :::: shortenPhyId=%d, callingContext = %d, Final doCalFlag = %d, doCalFlagCombIQ = %d 
3615,,[ phyrf_caldb.c : 4469 ] CALDB ::: CheckCombCalForFCS  [PREVIOUS_RECORD == PRESENT_RECORD] 
3614,,[ phyrf_caldb.c : 4474 ] CALDB ::: CheckCombCalForFCS  [PREVIOUS_RECORD != PRESENT_RECORD] 
3613,,[ phyrf_caldb.c : 4479 ] CALDB ::: CheckCombCalForFCS  [PRESENT_RECORD = INVALID] 
3612,iiiiii,[ phyrf_caldb.c : 4538 ] CheckDpdMemForFCS() : maxChainIdx %d rfChainMask %d cur_tbl_idx %d subModeIndxFor80p80 %d phyId %d, chainIdx %d  
3611,IIii,[ phyrf_caldb.c : 4543 ]  previous hw tracking table %x , curremt tracking table %x tableValid %d CALDB_STATUS_VALID %d 
3610,I,[ phyrf_caldb.c : 4555 ] CB::: CheckDpdMemForFCS() : %x,   
3609,,[ phyrf_caldb.c : 4384 ] CALDB ::: CheckRXDCOForFCS  [PREVIOUS_RECORD == PRESENT_RECORD] 
3608,,[ phyrf_caldb.c : 4389 ] CALDB ::: CheckRXDCOForFCS  [PREVIOUS_RECORD != PRESENT_RECORD] 
3607,,[ phyrf_caldb.c : 4394 ] CALDB ::: CheckRXDCOForFCS  [PRESENT_RECORD = INVALID] 
3606,iiiiiIii,[ phyrf_caldb.c : 5908 ] TEMPSEN:::   phyId = %d, chainIdx = %d, CBNormalizedOffset=%d, CBTempInC=%d, LastTempInC=%d, getTime=%u, curTempID=%d, CBtempeID=%d 
3605,iiii,[ phyrf_caldb.c : 7078 ]  chain %d MemDPDValidateCurChSwForFCS %d channel %d rssult %d 
3604,iiiiii,[ phyrf_caldb.c : 2404 ] CALDB TEMPSEN:::  phyId=%d, calType=%d rfChainMask = %d, chainIdx=%d, globalCallingContext=%d, UseAltTableAllowed=%d  
3603,I,[ phyrf_caldb.c : 4598 ] CALDB::: IS_FTM_MODE() : %x, DISALBE_RESTORE_FOR_FTM is defined 
3602,i,[ phyrf_caldb.c : 6574 ] dualband_enable_phyb = %d 
 
3601,i,[ phyrf_caldb.c : 1280 ] dual_lo_needed = %d 
 
3600,IIIII,[ phyrf_caldb.c : 6553 ] CALDB_DEBUG: Frequency table dump  Start Freq %u | End freq %u | Sequential Index %u | Master Index %u | TPC mapped freq %u 
3599,iiiiiii,[ phyrf_caldb.c : 6300 ] caldB_synopsis: [%d], 	phyID=%d, 	mHz=%d, 	f1=%d, 	f2=%d, 	phyMode=%d, 	fullResetTime(us)=%d 
3598,i,[ phyrf_caldb.c : 6396 ] caldB_synopsis: No of coldboot channels : %d  
3597,IIII,[ phyrf_caldb.c : 6324 ] caldB_synopsis: RXDCO Addr :	0x%08x 	0x%08x,	0x%08x, 	0x%08x 
3596,IIII,[ phyrf_caldb.c : 6327 ] caldB_synopsis: RXDCO Valid:	0x%08x 	0x%08x,	;0x%08x, 	0x%08x 
3595,IIII,[ phyrf_caldb.c : 6335 ] caldB_synopsis: RXDCO Addr :	0x%08x 	0x%08x,	0x%08x, 	0x%08x 
3594,IIII,[ phyrf_caldb.c : 6338 ] caldB_synopsis: RXDCO Valid:	0x%08x 	0x%08x,	0x%08x, 	0x%08x 
3593,II,[ phyrf_caldb.c : 6343 ] caldB_synopsis: RXDCO Addr :	0x%08x 	0x%08x 
3592,II,[ phyrf_caldb.c : 6345 ] caldB_synopsis: RXDCO Valid:	0x%08x 	0x%08x 
3591,IIII,[ phyrf_caldb.c : 6370 ] caldB_synopsis: COMIQ Addr :	0x%08x 	0x%08x,	0x%08x, 	0x%08x 
3590,IIII,[ phyrf_caldb.c : 6373 ] caldB_synopsis: COMIQ Valid:	0x%08x 	0x%08x,	0x%08x, 	0x%08x 
3589,IIII,[ phyrf_caldb.c : 6381 ] caldB_synopsis: COMIQ Addr :	0x%08x 	0x%08x,	0x%08x, 	0x%08x 
3588,IIII,[ phyrf_caldb.c : 6384 ] caldB_synopsis: COMIQ Valid:	0x%08x 	0x%08x,	0x%08x, 	0x%08x 
3587,II,[ phyrf_caldb.c : 6389 ] caldB_synopsis: COMIQ Addr :	0x%08x 	0x%08x 
3586,II,[ phyrf_caldb.c : 6391 ] caldB_synopsis: COMIQ Valid:	0x%08x 	0x%08x 
3585,iII,[ phyrf_caldb.c : 6502 ] caldB_synopsis: 	phyId=%d 	calFileVersionID=0x%08x 	calFileRevisionID=0x%08x 
3584,,[ phyrf_caldb.c : 273 ] Secondary effrfchnmask: Invalid chainmask config!!! 
3583,,[ phyrf_caldb.c : 311 ] Listen effrfchnmask-  Invalid chainmask config!!! 
3582,i,[ phyrf_caldb.c : 1805 ] CALDB ERROR: invalid band of %d
 
3581,iiiiii,[ phyrf_caldb.c : 1966 ] CALDB :::: frequency=%d, bandw:%d calTypeIdx=%d,  *mapToCalGroupIdx=%d, *rfsub =%d, *sequentialSubBandIdx=%d 
3580,,[ phyrf_caldb.c : 1988 ] CALDB ERROR: illegal channel access detected! asserting here
 
3579,,[ phyrf_caldb.c : 1822 ] CALDB ERROR: illegal band access detected! asserting here
 
3578,III,[ phyrf_caldb.c : 3576 ] CC::: rxiqStart: %x, txiqStart: %x, txloStart: %x 
3577,iiIi,[ phyrf_caldb.c : 3757 ] dpdStart address for cur_tbl_idx [%d] chainIdx %d is 0x%x channel %d 
3576,,[ phyrf_caldb.c : 3343 ] error: phyId not matched to system supported number of PHYs. 
3575,iii,[ phyrf_caldb.c : 6709 ]  invalid  Cal attemps %d chain index %d freq %d 
3574,iii,[ phyrf_caldb.c : 6679 ]  update  Cal attemps %d chain index %d freq %d 
3573,,[ phyrf_caldb.c : 2212 ] error: phyId not matched to system supported number of PHYs. 
3572,iii,[ phyrf_caldb.c : 1426 ] Wow mode status operation : %d wow_mode_status (0: master calDB can be access) %d, wow entry cnt=%d  
3571,,[ phyrf_caldb.c : 5377 ] ERROR: CalDB checksum failure 
3570,,[ phyrf_caldb.c : 5185 ] error: phyId not matched to system supported number of PHYs. 
3569,,[ phyrf_caldb.c : 158 ] ERROR: supported phy not match to phyId 
3568,I,[ phyrf_caldb.c : 6539 ] eDPD ptr %p 
3567,i,[ phyrf_caldb.c : 1355 ] isDFS = %d 
3566,iiiiiii,[ phyrf_caldb.c : 6228 ] updating_caldB_synopsis: [%d], 	phyID=%d, 	mHz=%d, 	f1=%d, 	f2=%d, 	phyMode=%d, 	fullResetTime(us)=%d 
3565,iII,[ phyrf_caldb.c : 6241 ] updating_caldB_synopsis: RXDCO, 	chainIdx=%d, 	Addr=0x%08x, 	Valid=0x%08x 
3564,iiII,[ phyrf_caldb.c : 6256 ] updating_caldB_synopsis: COMBIQ, 	tableIdx=%d, 	chainIdx=%d, 	Addr=0x%08x, 	Valid=0x%08x 
3563,II,[ phyrf_caldb.c : 7097 ] in fn updateCurChSwMemDpdCal address1 %x = address0 %x 
 
3562,,[ phyrf_caldb.c : 3450 ] error: phyId not matched to system supported number of PHYs. 
3617,i,[ phyrf_cbc.c : 885 ] cbc: ENABLE_CHANNEL_LIST_IN_BDF not defined: repeatLimit=%d 
3616,i,[ phyrf_cbc.c : 308 ] CALDB_DEBUG: skipping the wrong channel for the radio : %d 
 
3635,,[ phyrf_caldb_aging.c : 186 ] REGEN_CALDB: starting 
3634,,[ phyrf_caldb_aging.c : 191 ] REGEN_CALDB: Invalid phy Handle. Exiting Caldb regen 
3633,,[ phyrf_caldb_aging.c : 197 ] REGEN_CALDB: Invalid phyId. Exiting Caldb regen 
3632,,[ phyrf_caldb_aging.c : 204 ] REGEN_CALDB: Software configuration to skip CalDb Regen 
3631,,[ phyrf_caldb_aging.c : 220 ] REGEN_CALDB: Invalid Mac Handle. Exiting Caldb regen 
3630,,[ phyrf_caldb_aging.c : 232 ] REGEN_CALDB: CALBD CLEARED: 
3629,,[ phyrf_caldb_aging.c : 235 ] REGEN_CALDB: INVALID PHYID OR CALDB NOT CLEARED 
3628,,[ phyrf_caldb_aging.c : 239 ] REGEN_CALDB: Save the pre regen channel 
3627,,[ phyrf_caldb_aging.c : 256 ] REGEN_CALDB: Turning off phy pre regen 
3626,II,[ phyrf_caldb_aging.c : 323 ] REGEN_CALDB: Skipping due to invalid PHYID groupMapping[%u][1] is %u 
3625,iiii,[ phyrf_caldb_aging.c : 419 ] gurug REGEN_CALDB: calChEntry[%d][%d] %d chIdx %d 
3624,,[ phyrf_caldb_aging.c : 471 ] REGEN_CALDB: Restore pre regen channel 
3623,,[ phyrf_caldb_aging.c : 482 ] REGEN_CALDB: Turning on phy post regen 
3622,I,[ phyrf_caldb_aging.c : 490 ] REGEN_CALDB: completed in %u uSec 
3621,,[ phyrf_caldb_aging.c : 95 ] REGEN_CALDB: Invalid Phy Handle 
3620,I,[ phyrf_caldb_aging.c : 117 ] REGEN_CALDB: Skipping cal as freq %u is not supported 
3619,,[ phyrf_caldb_aging.c : 103 ] REGEN_CALDB: Invalid pdev Handle 
3618,,[ phyrf_caldb_aging.c : 109 ] REGEN_CALDB: Invalid Mac Handle 
3637,i,[ phyrf_debug.c : 759 ] HALPHY DUMP: WIFITOOL issued with subcommand ID %d 
3636,i,[ phyrf_debug.c : 770 ] Invalid or Unsupported halphy debug sub command: %d 
3648,ii,[ phyrf_debug_prdd.c : 559 ] PRDD - Invalid number of args (should be %d..%d) 
3647,i,[ phyrf_debug_prdd.c : 730 ] PRDD - Invalid PRDD command (should be 0..%d) 
3646,,[ phyrf_debug_prdd.c : 735 ] PRDD - Invalid number of args in PRDD command (should be >= 2 args) 
3645,I,[ phyrf_debug_prdd.c : 742 ] PRDD - Invalid phyId - should be 0..%lu 
3644,,[ phyrf_debug_prdd.c : 701 ] PRDD - Not enough memory to support fixed mode 
3643,II,[ phyrf_debug_prdd.c : 454 ] PRDD - No report for phy%u at %u MHz 
3642,iii,[ phyrf_debug_prdd.c : 311 ] PRDD - %d MHz, phy%d, 1swT %d ms 
3641,iI,[ phyrf_debug_prdd.c : 400 ] PRDD -   module%d 0x%08lx 
3640,,[ phyrf_debug_prdd.c : 469 ] No PRDD report 
3639,i,[ phyrf_debug_prdd.c : 121 ] PRDD - Could not find idx for freq %d 
3638,ii,[ phyrf_debug_prdd.c : 964 ] PRDD - channel %d is not found in phy%d 
3876,I,[ phyrf_debug_cmd.c : 2921 ] CAL_STATS: CAL PROFILE - COLD_BOOT_CAL (0x%x) 
3875,I,[ phyrf_debug_cmd.c : 2924 ] CAL_STATS: CAL PROFILE - FULL_CHAN_SWITCH (0x%x) 
3874,I,[ phyrf_debug_cmd.c : 2927 ] CAL_STATS: CAL PROFILE - SCAN_CHAN_SWITCH (0x%x) 
3873,I,[ phyrf_debug_cmd.c : 2930 ] CAL_STATS: CAL PROFILE - DPD_SPLIT_CAL (0x%x) 
3872,I,[ phyrf_debug_cmd.c : 2933 ] CAL_STATS: CAL PROFILE - TEMP_TRIGEER_CAL (0x%x) 
3871,I,[ phyrf_debug_cmd.c : 2936 ] CAL_STATS: CAL PROFILE - POWER_SAVE_WAKE_UP (0x%x) 
3870,I,[ phyrf_debug_cmd.c : 2939 ] CAL_STATS: CAL PROFILE - TIMER_TRIGGER_CAL (0x%x) 
3869,I,[ phyrf_debug_cmd.c : 2942 ] CAL_STATS: CAL PROFILE - FTM_TRIGGER_CAL (0x%x) 
3868,I,[ phyrf_debug_cmd.c : 2945 ] CAL_STATS: CAL PROFILE - POWER_DOWN_DTIM (0x%x) 
3867,I,[ phyrf_debug_cmd.c : 2948 ] CAL_STATS: CAL PROFILE - NOISY_ENV_RXDO (0x%x) 
3866,I,[ phyrf_debug_cmd.c : 2951 ] CAL_STATS: CAL PROFILE - UNKNOWN_PROFILE (0x%x) 
3865,I,[ phyrf_debug_cmd.c : 2961 ] CAL_STATS: CAL TYPE - ADC (0x%x) 
3864,I,[ phyrf_debug_cmd.c : 2964 ] CAL_STATS: CAL TYPE - DAC (0x%x) 
3863,I,[ phyrf_debug_cmd.c : 2967 ] CAL_STATS: CAL TYPE - NOISE_FLOOR (0x%x) 
3862,I,[ phyrf_debug_cmd.c : 2970 ] CAL_STATS: CAL TYPE - RXDCO (0x%x) 
3861,I,[ phyrf_debug_cmd.c : 2973 ] CAL_STATS: CAL TYPE - COMB_TXLO_TXIQ_RXIQ (0x%x) 
3860,I,[ phyrf_debug_cmd.c : 2976 ] CAL_STATS: CAL TYPE - DPD_MEMORYLESS (0x%x) 
3859,I,[ phyrf_debug_cmd.c : 2979 ] CAL_STATS: CAL TYPE - DPD_MEMORY (0x%x) 
3858,I,[ phyrf_debug_cmd.c : 2982 ] CAL_STATS: CAL TYPE - IBF (0x%x) 
3857,I,[ phyrf_debug_cmd.c : 2985 ] CAL_STATS: CAL TYPE - PDET_AND_PAL (0x%x) 
3856,I,[ phyrf_debug_cmd.c : 2988 ] CAL_STATS: CAL TYPE - RXDCO_DTIM (0x%x) 
3855,I,[ phyrf_debug_cmd.c : 2991 ] CAL_STATS: CAL TYPE - RXDCO_IQ (0x%x) 
3854,I,[ phyrf_debug_cmd.c : 2994 ] CAL_STATS: CAL TYPE - BWFILTER (0x%x) 
3853,I,[ phyrf_debug_cmd.c : 2997 ] CAL_STATS: CAL TYPE - PADROOP (0x%x) 
3852,I,[ phyrf_debug_cmd.c : 3000 ] CAL_STATS: CAL TYPE - INVALID_CAL_ID (0x%x) 
3851,I,[ phyrf_debug_cmd.c : 3010 ] CAL_STATS: CAL TYPE - PERIODIC_NOISE_FLOOR (0x%x) 
3850,I,[ phyrf_debug_cmd.c : 3013 ] CAL_STATS: CAL TYPE - PERIODIC_DPD_MEMORYLESS (0x%x) 
3849,I,[ phyrf_debug_cmd.c : 3016 ] CAL_STATS: CAL TYPE - PERIODIC_INVALID_CAL (0x%x) 
3848,,[ phyrf_debug_cmd.c : 933 ] WIFITOOL: PHYID is not active 
 
3847,iiii,[ phyrf_debug_cmd.c : 975 ] ANI_LOG PHYID%d ani_dl_min %d, ani_dl_max %d, error_threshold %d 
3846,ii,[ phyrf_debug_cmd.c : 987 ] ANI_LOG PHYID%d ani_ramp_down %d 
 
3845,i,[ phyrf_debug_cmd.c : 996 ] ANI_LOG_ERR - Before- value of ANI histogram=%d 
3844,i,[ phyrf_debug_cmd.c : 998 ] ANI_LOG_ERR - After - value of ANI histogram=%d 
3843,,[ phyrf_debug_cmd.c : 1001 ] ANI_LOG_ERR VREG ERR COUNTER VALUES 
3842,iiii,[ phyrf_debug_cmd.c : 3304 ] MMHostCmdAvgCFO : num_args %d cmd_id %d phy_id %d sub_cmd_id %d 
3841,I,[ phyrf_debug_cmd.c : 3311 ] MMHostCmdAvgCFO : Invalid phyId %u 
3840,I,[ phyrf_debug_cmd.c : 3319 ] MMHostCmdAvgCFO : Invalid pHandle for phyId %u 
3839,i,[ phyrf_debug_cmd.c : 2141 ] BT_CLOCK_ENABLE: %d 
3838,I,[ phyrf_debug_cmd.c : 3033 ] MMHostCmdCalStats : Invalid phyId %u 
3837,I,[ phyrf_debug_cmd.c : 3041 ] MMHostCmdCalStats : Invalid pHandle for phyId %u 
3836,iiii,[ phyrf_debug_cmd.c : 3052 ] MMHostCmdCalStats : num_args %d cmd_id %d phy_id %d sub_cmd_id %d 
3835,,[ phyrf_debug_cmd.c : 3062 ] CAL_STATS : Reset calibration stats 
3834,,[ phyrf_debug_cmd.c : 3068 ] CAL_STATS : Valid Cal profiles and cal types 
3833,I,[ phyrf_debug_cmd.c : 3076 ] CAL_STATS : Number of cal types in this profile = %u 
3832,,[ phyrf_debug_cmd.c : 3091 ] CAL_STATS : Calibration stats for valid Cal profiles and cal types 
3831,,[ phyrf_debug_cmd.c : 3099 ] ************************************************ 
3830,IIIII,[ phyrf_debug_cmd.c : 3113 ] CAL_STATS : cal_type = %u | cal_triggered_cnt = %u | cal_fail_cnt = %u | cal_fcs_cnt = %u | cal_fcs_fail_cnt = %u 
3829,,[ phyrf_debug_cmd.c : 3117 ] ************************************************** 
3828,,[ phyrf_debug_cmd.c : 3124 ] CAL_STATS : Calibration stats for valid Periodic Cal profiles and cal types 
3827,I,[ phyrf_debug_cmd.c : 3128 ] CAL_STATS : PERIODIC CAL cal_profile = %u 
3826,III,[ phyrf_debug_cmd.c : 3138 ] CAL_STATS : cal_type = %u | cal_triggered_cnt = %u | cal_fail_cnt = %u  
3825,,[ phyrf_debug_cmd.c : 2633 ] Coldboot Calibration Feature Not Supported 
3824,,[ phyrf_debug_cmd.c : 2638 ] Coldboot Calibration Feature: Invalid test arguments 
3823,i,[ phyrf_debug_cmd.c : 1710 ] WIFITOOL: PHYID %d is not active 
 
3822,ii,[ phyrf_debug_cmd.c : 1715 ] EnableDssWarCFO: enable=%d FOR PHYID %d 
 
3821,iiII,[ phyrf_debug_cmd.c : 2204 ] CHAINMASKOVERRIDE %d - phy[%d]: txChMask 0x%x; rxChMask 0x%x 
3820,,[ phyrf_debug_cmd.c : 609 ] CTL_DISABLE: Invalid test arguments 
3819,,[ phyrf_debug_cmd.c : 615 ] CTL_DISABLE: Invalid phyId 
3818,,[ phyrf_debug_cmd.c : 627 ] CTL_DISABLE: Disabling CTL power limits! 
3817,,[ phyrf_debug_cmd.c : 632 ] CTL_DISABLE: Enabling back CTL power limits! 
3816,,[ phyrf_debug_cmd.c : 2360 ] DFS_ENABLE: Invalid test arguments  
3815,,[ phyrf_debug_cmd.c : 2366 ] DFS_ENABLE: Invalid phyId 
3814,,[ phyrf_debug_cmd.c : 2576 ] PHYRF_DEBUG_MM_HOST_CMD_SET_DPD_EDPD_ENABLE Invalid Command 
3813,Ii,[ phyrf_debug_cmd.c : 2583 ] PHYRF_DEBUG_MM_HOST_CMD_SET_DPD_EDPD_ENABLE: Invalid PHY ID = %u, phyrf_init_GetNumPhys()=%d 
3812,i,[ phyrf_debug_cmd.c : 2591 ] PHYRF_DEBUG_MM_HOST_CMD_SET_DPD_EDPD_ENABLE: Invalid pHandle for phyId=%d 
3811,iI,[ phyrf_debug_cmd.c : 2598 ] Set g_halphy_dpd_enable[%d] =0x%x
 
3810,,[ phyrf_debug_cmd.c : 850 ] DO_NFCAL_ACTION Invalid Command 
3809,I,[ phyrf_debug_cmd.c : 857 ] DO_NFCAL_ACTION: Invalid PHY ID = %u 
3808,II,[ phyrf_debug_cmd.c : 876 ] DO_NFCAL_ACTION: Setting NF home channl IterCount to %u for phyId = %u 
3807,II,[ phyrf_debug_cmd.c : 883 ] DO_NFCAL_ACTION: Setting pResetStruct->nfPeriodicCalControl to %u for phyId %u 
3806,II,[ phyrf_debug_cmd.c : 890 ] DO_NFCAL_ACTION: Setting pResetStruct->nfPeriodicCalWithPhyOffPhyOnControl to %u for phyId %u 
3805,II,[ phyrf_debug_cmd.c : 897 ] DO_NFCAL_ACTION: Setting pResetStruct->nfResetCalControl to %u for phyId %u 
3804,II,[ phyrf_debug_cmd.c : 907 ] DO_NFCAL_ACTION: Triggering NFCAL with flags %x for phyId %u 
3803,i,[ phyrf_debug_cmd.c : 1478 ] DSS: WIFITOOL ISSUED TO ENABLE/DISABLE DSS %d
 
3802,i,[ phyrf_debug_cmd.c : 1489 ] DSS: G_SYNTH_CONTROL_FTM=%d FOR PHYID 0 
 
3801,i,[ phyrf_debug_cmd.c : 1501 ] DSS: G_SYNTH_CONTROL=%d FOR PHYID 0 
 
3800,i,[ phyrf_debug_cmd.c : 1690 ] WIFITOOL: PHYID %d is not active 
 
3799,ii,[ phyrf_debug_cmd.c : 1695 ] SetDssWarCFODeltaThreshold: cfo_threshold=%d FOR PHYID %d 
 
3798,i,[ phyrf_debug_cmd.c : 2673 ] DUMP_TPC_GLUT_WAKEUP_SLEEP: WIFITOOL ISSUED TO ENABLE TPC GLUT DUMP %d
 
3797,,[ phyrf_debug_cmd.c : 2677 ] DUMP_TPC_GLUT_WAKEUP_SLEEP: wifitool : Invalid test arguments 
3796,i,[ phyrf_debug_cmd.c : 2682 ] DUMP_TPC_GLUT_WAKEUP_SLEEP: WIFITOOL ISSUED TO DISABLE TPC GLUT DUMP %d
 
3795,i,[ phyrf_debug_cmd.c : 2656 ] DUMP_TPC_REGS_ENABLE: WIFITOOL ISSUED TO ENABLE TPC REG DUMP %d
 
3794,,[ phyrf_debug_cmd.c : 2660 ] DUMP_TPC_REGS_ENABLE: wifitool : Invalid test arguments 
3793,I,[ phyrf_debug_cmd.c : 1057 ] pResetStruct->enable_ldocal_otp = %u 
3792,i,[ phyrf_debug_cmd.c : 1144 ] PAPRD: Invalid PHY ID = %d 
3791,ii,[ phyrf_debug_cmd.c : 1148 ] PAPRD: Phy ID %d | Enable for MM = %d 
3790,ii,[ phyrf_debug_cmd.c : 1131 ] ANI_LOG PHYID%d error_threshold %d 
 
3789,,[ phyrf_debug_cmd.c : 2861 ] wrong no of arguments from unit test command 
3788,ii,[ phyrf_debug_cmd.c : 1857 ] DSS: WIFITOOL ISSUED TO FORCED SYNTH phyId %d, Synth %d
 
3787,i,[ phyrf_debug_cmd.c : 1860 ] FORCED_SYNTH: Invalid PHY ID = %d 
3786,ii,[ phyrf_debug_cmd.c : 1876 ] FORCED SYNTH: G_SYNTH_CONTROL=%d FOR PHYID %d 
 
3785,ii,[ phyrf_debug_cmd.c : 1881 ] FORCED SYNTH: G_SYNTH_CONTROL=%d FOR PHYID %d 
 
3784,,[ phyrf_debug_cmd.c : 2820 ] CWOFFSET : wifitool : Invalid test arguments 
3783,Ii,[ phyrf_debug_cmd.c : 2826 ] phyrf_debug_MMHostCmdGenerateCWToneAtOffset: Invalid PHY ID = %u, phyrf_init_GetNumPhys()=%d 
3782,i,[ phyrf_debug_cmd.c : 2832 ] phyrf_debug_MMHostCmdGenerateCWToneAtOffset: Invalid pHandle for phyId=%d 
3781,,[ phyrf_debug_cmd.c : 2848 ] phyrf_debug_MMHostCmdGenerateCWToneAtOffset: Invalid command 
3780,,[ phyrf_debug_cmd.c : 3201 ] GET_BDF_FEATURE_FLAGS: wifitool : Invalid test arguments 
3779,I,[ phyrf_debug_cmd.c : 3209 ] GET_BDF_FEATURE_FLAGS: Invalid PHY ID = %u 
3778,iiII,[ phyrf_debug_cmd.c : 3236 ] GET_BDF_FEATURE_FLAGS: wifitool : nvCaldbEnable=%d calDbPersistentEnable=%d tpc_flag=0x%x commonBoardFlags=0x%x 
3777,Iiii,[ phyrf_debug_cmd.c : 3237 ] GET_BDF_FEATURE_FLAGS: wifitool : projectId = 0x%x boardCalVersion=%d, bdfVersion=%d, iniVersion=%d 
3776,ii,[ phyrf_debug_cmd.c : 3238 ] GET_BDF_FEATURE_FLAGS: wifitool :templateVersionMajor=%d templateVersionMinor=%d 
3775,iii,[ phyrf_debug_cmd.c : 3240 ] GET_BDF_FEATURE_FLAGS: wifitool : dpdEnable =%d regMismatchFeatureEnable=%d antenna_gain_feature_enabled=%d 
3774,,[ phyrf_debug_cmd.c : 2693 ] GET BOARD CAL DETAILS : wifitool : Invalid test arguments 
3773,ii,[ phyrf_debug_cmd.c : 2697 ] GET BOARD CAL DETAILS : wifitool : SW version : %d.%d 
3772,i,[ phyrf_debug_cmd.c : 2699 ] GET BOARD CAL DETAILS : wifitool : Meta version : %d 
3771,I,[ phyrf_debug_cmd.c : 2702 ] GET BOARD CAL DETAILS : wifitool : ProjectID in OTP : 0x%x 
3770,II,[ phyrf_debug_cmd.c : 1294 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( Internal Error ) 
3769,II,[ phyrf_debug_cmd.c : 1298 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( No Entry ) 
3768,II,[ phyrf_debug_cmd.c : 1302 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( No Memory) 
3767,III,[ phyrf_debug_cmd.c : 1306 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( Success ), chanGradeInfoCount %u 
3766,IIIi,[ phyrf_debug_cmd.c : 1315 ] %u. Freq %u, BW %u, ChanPerfMetric %d 
3765,II,[ phyrf_debug_cmd.c : 1320 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( Unknown Error ) 
3764,i,[ phyrf_debug_cmd.c : 1241 ] PCSS: Invalid PHY ID = %d 
3763,iiii,[ phyrf_debug_cmd.c : 1228 ] PDL Version : %d.%d - RDL Version : %d.%d 
3762,,[ phyrf_debug_cmd.c : 1332 ] GetSignalLevel : Invalid test arguments  
3761,,[ phyrf_debug_cmd.c : 1348 ] GetSignalLevel : pHandle not found 
3760,IIIII,[ phyrf_debug_cmd.c : 1356 ] GetSignalLevel phyId %u, snrInput %u, chainMask %x, bandwidth %u, combRssi %u 
3759,I,[ phyrf_debug_cmd.c : 1360 ] GetSignalLevel : SNR Input %u 
3758,III,[ phyrf_debug_cmd.c : 1375 ] GetSignalLevel : SNR BW Segment Input %8x%8x for Chain %u 
3757,I,[ phyrf_debug_cmd.c : 1383 ] GetSignalLevel : Returns %u (WHAL_EINVAL) 
3756,Ii,[ phyrf_debug_cmd.c : 1392 ] GetSignalLevel : SNR=%u RSSI=%d 
3755,IIIIIi,[ phyrf_debug_cmd.c : 1406 ] GetSignalLevel : SNR[%u][%u]=%u RSSI[%u][%u]=%d 
3754,I,[ phyrf_debug_cmd.c : 3157 ] GET_START_END_FREQ: Invalid PHY ID = %u 
3753,,[ phyrf_debug_cmd.c : 3170 ] GET_START_END_FREQ: wifitool : Invalid test arguments 
3752,iiii,[ phyrf_debug_cmd.c : 3174 ] GET_START_END_FREQ : wifitool : low_2ghz_chan = %d high_2ghz_chan=%d low_5ghz_chan=%d high_5ghz_chan=%d 
3751,i,[ phyrf_debug_cmd.c : 2278 ] GTXENABLE: Invalid PHY ID = %d 
3750,ii,[ phyrf_debug_cmd.c : 2284 ] GreenTx Enable[%d]=%d 
3749,i,[ phyrf_debug_cmd.c : 2297 ] ImpsBmpsControl: Invalid PHY ID = %d 
3748,ii,[ phyrf_debug_cmd.c : 2308 ] ImpsBmpsControl: enable=%d, phyId=%d 
3747,iii,[ phyrf_debug_cmd.c : 2322 ] ImpsBmpsControl: imps=%d, enable=%d, phyId=%d 
3746,iiii,[ phyrf_debug_cmd.c : 2341 ] ImpsBmpsControl: imps=%d, w2s=%d, enable=%d, phyId=%d 
3745,I,[ phyrf_debug_cmd.c : 3256 ] MMHostCmdLMConfig :: LM_DBG: Invalid phyId %u 
3744,I,[ phyrf_debug_cmd.c : 3264 ] MMHostCmdLMConfig :: LM_DBG: Invalid pHandle for phyId %u 
3743,,[ phyrf_debug_cmd.c : 2110 ] LP_SYNTH: Invalid test arguments  
3742,ii,[ phyrf_debug_cmd.c : 2127 ] LPSYNTHFORLEGACY: WIFITOOL ISSUED TO ENABLE LP SYNTH: legacy rate: %d, dtim: %d
 
3741,I,[ phyrf_debug_cmd.c : 1076 ] ANI_LOG g_max_edcca=%x 
3740,ii,[ phyrf_debug_cmd.c : 1090 ] ANI_LOG PHYID%d g_ani_cca %d 
 
3739,iii,[ phyrf_debug_cmd.c : 1110 ] ANI_LOG PHYID%d ani_dl_min %d, ani_dl_max %d 
 
3738,I,[ phyrf_debug_cmd.c : 1813 ] NFCAL_READ_TEST : phyId %u not available for test 
3737,IIIIIi,[ phyrf_debug_cmd.c : 1831 ] NFCAL_READ_TEST : phyId %u, nfType 0x%x, bufferSize %u, validBuffer %u, bufferPointer 0x%x, returns %d 
3736,IIIi,[ phyrf_debug_cmd.c : 1839 ] NFCAL_READ_TEST : phyId %u, nfType 0x%x, Chain %u, NFValue %d 
3735,,[ phyrf_debug_cmd.c : 2406 ] IpcHandler_Enable: Invalid test arguments  
3734,,[ phyrf_debug_cmd.c : 2412 ] IpcHandler_Enable: Invalid phyId 
3733,ii,[ phyrf_debug_cmd.c : 2419 ] IpcHandler_Enable: enable=%d, phyId=%d 
3732,ii,[ phyrf_debug_cmd.c : 1429 ] PHYDBG: g_phydbg_phy_disable[%d] = %d 
3731,,[ phyrf_debug_cmd.c : 1446 ] phydbg_reconfigure : Invalid test arguments  
3730,i,[ phyrf_debug_cmd.c : 1454 ] phydbg_reconfigure : Invalid PHY ID = %d
 
3729,ii,[ phyrf_debug_cmd.c : 1458 ] phydbg_reconfigure : PHYID = %d ,Event = %d
 
3728,,[ phyrf_debug_cmd.c : 2721 ] DebugCmdPhyOnOffSeq : Invalid test arguments 
3727,I,[ phyrf_debug_cmd.c : 2728 ] DebugCmdPhyOnOffSeq : Invalid phyId %u 
3726,I,[ phyrf_debug_cmd.c : 2736 ] DebugCmdPhyOnOffSeq : Invalid pHandle for phyId %u 
3725,I,[ phyrf_debug_cmd.c : 2744 ] DebugCmdPhyOnOffSeq : Invalid pResetStruct for phyId %u 
3724,IIII,[ phyrf_debug_cmd.c : 2753 ] DebugCmdPhyOnOffSeq : Pretest Counter phyId %u, cfActiveLow_Fail_cnt %04u, cfActiveLow_Pass_cnt %04u, phyOffThroughVregCnt %04u 
3723,I,[ phyrf_debug_cmd.c : 2764 ] DebugCmdPhyOnOffSeq : Validating vreg based phyOff for phyId %u 
3722,I,[ phyrf_debug_cmd.c : 2768 ] DebugCmdPhyOnOffSeq : Validating tlv based phyOff followed by vreg based phyOff for phyId %u 
3721,I,[ phyrf_debug_cmd.c : 2773 ] DebugCmdPhyOnOffSeq : Validating calling vreg based phyOff twice for phyId %u 
3720,I,[ phyrf_debug_cmd.c : 2779 ] DebugCmdPhyOnOffSeq : Validating tlv based phyOff for phyId %u 
3719,IIII,[ phyrf_debug_cmd.c : 2792 ] DebugCmdPhyOnOffSeq : Posttest Counter phyId %u, cfActiveLow_Fail_cnt %04u, cfActiveLow_Pass_cnt %04u, phyOffThroughVregCnt %04u 
3718,i,[ phyrf_debug_cmd.c : 680 ] BDF DUMP: Invalid NV Section  %d 
3717,i,[ phyrf_debug_cmd.c : 685 ] BDF DUMP: NV Section Size: %d 
3716,ii,[ phyrf_debug_cmd.c : 696 ] BDF DUMP: sub-section size: %d sub-section id: 0x%d 
3715,iI,[ phyrf_debug_cmd.c : 702 ] BDF DUMP: index: %d d: 0x%x 
3714,iI,[ phyrf_debug_cmd.c : 711 ] BDF DUMP: index: %d d:0x%x 
3713,I,[ phyrf_debug_cmd.c : 245 ] RegDumpId %u :: NFCAL_BDF_PER_CHAIN :: Exceptions :: Value = 1 : Chain Unsupported 
3712,,[ phyrf_debug_cmd.c : 515 ] REGEN_CALDB: wal_pdev is NULL. Skipping 
3711,ii,[ phyrf_debug_cmd.c : 583 ] TT-Chain=%d, Temperature=%d 
 
3710,II,[ phyrf_debug_cmd.c : 591 ] Avg temp across %u chains=%u 
3709,IIIii,[ phyrf_debug_cmd.c : 281 ] RegDumpId %u :: NFCAL_RUNTIME_PER_CHAIN :: phyId %u :: Chain %u :: %d dBr :: %d dBm 
3708,III,[ phyrf_debug_cmd.c : 291 ] RegDumpId %u :: XTAL CAPIN=%u 	 CAPOUT=%u
 
3707,IIi,[ phyrf_debug_cmd.c : 295 ] BdfDump :: XTAL CAPIN=%u 	 CAPOUT=%u 	 PPM=%d 
 
3706,IIi,[ phyrf_debug_cmd.c : 298 ] BdfDump :: XTAL CAPIN=%u 	 CAPOUT=%u 	 PPM=-%d 
 
3705,II,[ phyrf_debug_cmd.c : 318 ] RegDumpId %u :: TPC_DUMP MASK %u 
3704,iii,[ phyrf_debug_cmd.c : 341 ] RxGainCalResult phyId:%d channel_idx:%d, channel_freq:%d 
3703,iiiii,[ phyrf_debug_cmd.c : 347 ] RxGainCalResult phyId:%d channel_idx:%d, chain_idx:%d, DBr_value:%d, DBm_value:%d 
3702,IIIii,[ phyrf_debug_cmd.c : 252 ] RegDumpId %u :: NFCAL_BDF_PER_CHAIN :: phyId %u :: Chain %u :: %d dBr :: %d dBm 
3701,iI,[ phyrf_debug_cmd.c : 365 ] FTM_DEBUG: g_ftm_ctxt[%d] addr = %p 
3700,iIIII,[ phyrf_debug_cmd.c : 376 ] FTM_DEBUG: g_ftm_ctxt[%d]: pdev = %p, vdev = %p, peer = %p, ftm_mode = 0x%x 
3699,iIIII,[ phyrf_debug_cmd.c : 378 ] FTM_DEBUG: g_ftm_ctxt[%d]: send_mgmt = 0x%x, send_data = 0x%x, encap_cfg = %p, ctrl = %p 
3698,,[ phyrf_debug_cmd.c : 382 ] FTM_DEBUG: encap_cfg pointer is NULL in g_ftm_ctxt !!  
3697,iiiI,[ phyrf_debug_cmd.c : 390 ] FTM_DEBUG: g_ftm_ctxt[%d].encap_cfg: pkt_len = %d, pkt_type = %d, vdev = %p 
3696,iIIIIII,[ phyrf_debug_cmd.c : 397 ] FTM_DEBUG: g_ftm_ctxt[%d].encap_cfg->sa_addr = 0x%02x:%02x:%02x:%02x:%02x:%02x 
3695,iIIIIII,[ phyrf_debug_cmd.c : 405 ] FTM_DEBUG: g_ftm_ctxt[%d].encap_cfg->da_addr = 0x%02x:%02x:%02x:%02x:%02x:%02x 
3694,iIIIIII,[ phyrf_debug_cmd.c : 413 ] FTM_DEBUG: g_ftm_ctxt[%d].encap_cfg->bss_addr = 0x%02x:%02x:%02x:%02x:%02x:%02x 
3693,,[ phyrf_debug_cmd.c : 418 ] FTM_DEBUG: ctrl pointer is NULL in g_ftm_ctxt !! 
3692,iii,[ phyrf_debug_cmd.c : 425 ] FTM_DEBUG: g_ftm_ctxt[%d].ctrl: num_pkts_to_send = %d, is_aggr_ok = %d 
3691,I,[ phyrf_debug_cmd.c : 274 ] RegDumpId %u :: NFCAL_RUNTIME_PER_CHAIN :: Exceptions :: Value = 1 : Chain Unsupported, Value = 0 : NFCAL Convergence Failed 
3690,iii,[ phyrf_debug_cmd.c : 432 ] FTM_DEBUG: g_dbg_overwrite_ppdu_dur_us = %d, g_dbg_gi_override = %d, g_dbg_he_ltf_override = %d 
3689,iiii,[ phyrf_debug_cmd.c : 463 ] CALDB_DEBUG:   	calDBEnableSetting=%d, 	 CalTimeOutSetting = %d, 	PersistentEnable = %d, 	masterCalDbExist()=%d 
3688,Ii,[ phyrf_debug_cmd.c : 464 ] CALDB_DEBUG: CALDB_ADDRE= %x dB size = %d 
3687,,[ phyrf_debug_cmd.c : 465 ] CALDB_DEBUG: Version info and CALDB Synopsis follows: 
3686,,[ phyrf_debug_cmd.c : 499 ] REGEN_CALDB: Re-generating cold boot calibration over debug - Command - wait for 60seconds ...
 
3685,iIIi,[ phyrf_debug_cmd.c : 1186 ] ADDRVAL: indx = %d addr = 0x%X val = 0x%X en=%d 
3684,iIIi,[ phyrf_debug_cmd.c : 1196 ] ADDRVAL: indx = %d addr = 0x%X val = 0x%X en=%d 
3683,iIIi,[ phyrf_debug_cmd.c : 1202 ] ADDRVAL: indx = %d addr = 0x%X val = 0x%X en=%d 
3682,,[ phyrf_debug_cmd.c : 2541 ] phyrf_debug_MMHostCmdSetCalMask Invalid Command 
3681,Ii,[ phyrf_debug_cmd.c : 2548 ] phyrf_debug_MMHostCmdSetCalMask: Invalid PHY ID = %u, phyrf_init_GetNumPhys()=%d 
3680,i,[ phyrf_debug_cmd.c : 2556 ] phyrf_debug_MMHostCmdSetCalMask: Invalid pHandle for phyId=%d 
3679,I,[ phyrf_debug_cmd.c : 2563 ] Set g_halphy_debug_cal_mask =0x%x
 
3678,,[ phyrf_debug_cmd.c : 2427 ] SetCcaThreshold: Invalid test arguments  
3677,,[ phyrf_debug_cmd.c : 2433 ] SetCcaThreshold: Invalid phyId 
3676,I,[ phyrf_debug_cmd.c : 2088 ] Set g_halphy_debug_mask =0x%x
 
3675,I,[ phyrf_debug_cmd.c : 2094 ] Set phyDebugMask =0x%x
 
3674,,[ phyrf_debug_cmd.c : 1894 ] PAPRD: Invalid test arguments  
3673,i,[ phyrf_debug_cmd.c : 1902 ] PAPRD: Invalid PHY ID = %d
 
3672,ii,[ phyrf_debug_cmd.c : 1906 ] PAPRD: PHYID = %d ,Event = %d
 
3671,i,[ phyrf_debug_cmd.c : 2017 ] Setting PBS Mode to %d
 
3670,,[ phyrf_debug_cmd.c : 2802 ] FUSE BOARD ID VALUE TO OTP : wifitool : Invalid test arguments 
3669,,[ phyrf_debug_cmd.c : 2808 ] FUSE BOARD ID VALUE TO OTP : wifitool :Completed  
3668,,[ phyrf_debug_cmd.c : 2228 ] SPECTRAL_ENABLE: Invalid test arguments  
3667,,[ phyrf_debug_cmd.c : 2234 ] SPECTRAL_ENABLE: Invalid phyId 
3666,,[ phyrf_debug_cmd.c : 2240 ] SPECTRAL_ENABLE: Invalid scanMode 
3665,i,[ phyrf_debug_cmd.c : 2882 ] phyrf_debug_MMHostCmdTPCDebug g_clpc_corr_thr %d  
3664,ii,[ phyrf_debug_cmd.c : 2897 ] phyrf_debug_MMHostCmdTPCDebug pdadc_read %d meas_pwr %d 
3663,ii,[ phyrf_debug_cmd.c : 2902 ] phyrf_debug_MMHostCmdTPCDebug PLUT[%d] = %d 
3662,,[ phyrf_debug_cmd.c : 2909 ] phyrf_debug_MMHostCmdTPCDebug Invalid commands 
3661,i,[ phyrf_debug_cmd.c : 1034 ] THERMAL: Invalid PHY ID = %d 
3660,ii,[ phyrf_debug_cmd.c : 1041 ] g_ThermalEnable[%d]=%d 
3659,,[ phyrf_debug_cmd.c : 2512 ] TPC CLPC SWITCH: Invalid test arguments  
3658,,[ phyrf_debug_cmd.c : 2518 ] TPC CLPC: Invalid phyId 
3657,,[ phyrf_debug_cmd.c : 2525 ] TPC CLPC: TO BE IMPLEMENTED 
3656,,[ phyrf_debug_cmd.c : 2465 ] TpcPowerOverride: Invalid test arguments  
3655,,[ phyrf_debug_cmd.c : 2471 ] TpcPowerOverride: Invalid phy ID 
3654,,[ phyrf_debug_cmd.c : 2489 ] TpcPowerOverride: Invalid test arguments  
3653,ii,[ phyrf_debug_cmd.c : 2497 ] TpcPowerOverride: chain %d: power: %d 
3652,i,[ phyrf_debug_cmd.c : 1015 ] XTAL: Invalid PHY ID = %d 
3651,ii,[ phyrf_debug_cmd.c : 1020 ] g_XtalCalPPM[%d]=%d 
3650,i,[ phyrf_debug_cmd.c : 3288 ] WIFITOOL ISSUED TO ENABLE/DISABLE PER-PACKET CHAINMASK SUPPORT = %d
 
3649,i,[ phyrf_debug_cmd.c : 3292 ] ENABLE/DISABLE PER-PACKET CHAINMASK SUPPORT: INVALID INPUT %d
 
3877,i,[ dfs_fcc_bin5.c : 110 ] DFS_DUMPS Rejecting pulses as they are not chirp %d
 
3910,,[ phyrf_dfs.c : 678 ] Invalid Channel Number 
3909,i,[ phyrf_dfs.c : 711 ] Invalid frequency : %d 
3908,I,[ phyrf_dfs.c : 761 ] %s: DFS ic is Invalid 
3907,II,[ phyrf_dfs.c : 768 ] %s: allocation of dfs_ic->ic_curchan failed %zu 
3906,iiiii,[ phyrf_dfs.c : 788 ] ADFS_DUMPS : req_chan=%d, ic_ieee_chan=%d, center_freq1=%d, center_freq2=%d, chan_wodth=%d
 
3905,I,[ phyrf_dfs.c : 802 ] %s: ADFS- CHANNEL CONFIGURED 
3904,iii,[ phyrf_dfs.c : 407 ] DFS_DUMPS regdomain %d phyId=%d g_DfsConfiguration=%d
 
3903,,[ phyrf_dfs.c : 234 ] DFS_DUMPS set 0x8000 
 
3902,,[ phyrf_dfs.c : 257 ] DFS_DUMP set g_dfs_test_mode 
 
3901,,[ phyrf_dfs.c : 262 ] DFS_DUMP clear g_dfs_test_mode 
 
3900,,[ phyrf_dfs.c : 267 ] DFS_DUMP Send Radar summary pulse to host 
 
3899,,[ phyrf_dfs.c : 271 ] DFS_DUMP stop Sending Radar summary pulse to host 
 
3898,,[ phyrf_dfs.c : 276 ] DFS_DUMPS Print all the pulse information
 
3897,,[ phyrf_dfs.c : 281 ] DFS_DUMPS Stop printing pulse information
 
3896,i,[ phyrf_dfs.c : 286 ] DFS_DUMPS RAW_FFT Data Dump set to %d
 
3895,iiiiiiiii,[ phyrf_dfs.c : 247 ] DFS_DUMPS timestamp=%d diff_ts=%d pulse_rssi=%d pulse_duration=%d is_chirp=%d sidx=%d detector_id=%d
 false_radar=%d radar_check=%d 
3894,,[ phyrf_dfs.c : 252 ] DFS_DUMPS set 0x8001 
 
3893,II,[ phyrf_dfs.c : 972 ] %s:Allocation of g_dfs_ic[dfs_detector_id] failed %zu 
3892,I,[ phyrf_dfs.c : 525 ] %s: DFS ic is Invalid 
3891,I,[ phyrf_dfs.c : 541 ] %s: DFS-FCC domain 
3890,I,[ phyrf_dfs.c : 549 ] %s: DFS-ETSI domain 
3889,I,[ phyrf_dfs.c : 564 ] %s:DFS-MKKN domain 
3888,I,[ phyrf_dfs.c : 582 ] %s: DFS-MKK domain 
3887,I,[ phyrf_dfs.c : 598 ] %s:  DFS_CN_DOMAIN 
3886,I,[ phyrf_dfs.c : 612 ] %s:  DFS_KR_DOMAIN 
3885,I,[ phyrf_dfs.c : 630 ] %s: DFS-UNINT domain 
3884,,[ phyrf_dfs.c : 653 ] PRDD_Test_Radar_Enable 
3883,Ii,[ phyrf_dfs.c : 656 ] %s[%d]: DFS- Radar Detection Enabling Failed 
3882,I,[ phyrf_dfs.c : 850 ] %s: DFS ic is Invalid 
3881,I,[ phyrf_dfs.c : 953 ] %s: DFS- CHANNEL CONFIGURED 
3880,II,[ phyrf_dfs.c : 861 ] %s: allocation of dfs_ic->ic_curchan failed %zu 
3879,iiiii,[ phyrf_dfs.c : 883 ] DFS_DUMPS : req_chan=%d, ic_ieee_chan=%d, center_freq1=%d, center_freq2=%d, chan_wodth=%d
 
3878,Ii,[ phyrf_dfs.c : 933 ] %s: Recieved a wrong channel width %d 
3911,III,[ wma_dfs_interface.c : 63 ] %s: called; ptr=%p, radar_info=%p
 
3913,,[ hca_rf_ftmIf_api.cpp : 140 ] ftmIf_SetRxDeaf 
3912,,[ hca_rf_ftmIf_api.cpp : 154 ] ftmIf_SetRxListen 
3914,i,[ hca_HwComponentTrx.cpp : 78 ] Error: processCmd ID of %d, unknown state. 
3915,i,[ hca_config.cpp : 85 ] Invalid HW component type %d
 
3988,i,[ phyrf_mc_paprd.c : 2113 ] PAPRD:Tx stats : hw_queued %d 
3987,i,[ phyrf_mc_paprd.c : 2114 ] PAPRD:Tx stats : hw_reaped %d 
3986,i,[ phyrf_mc_paprd.c : 2115 ] PAPRD:Tx stats : tx_done %d 
3985,i,[ phyrf_mc_paprd.c : 2116 ] PAPRD:Tx stats : tx_abort %d 
3984,i,[ phyrf_mc_paprd.c : 2117 ] PAPRD:Tx stats : tx_abort_compl_err_status %d 
3983,i,[ phyrf_mc_paprd.c : 2118 ] PAPRD:Tx stats : tx_abort_pdev_suspend %d 
3982,i,[ phyrf_mc_paprd.c : 2119 ] PAPRD:Tx stats : tx_async_enqueue %d 
3981,i,[ phyrf_mc_paprd.c : 2120 ] PAPRD:Tx stats : tx_async_dequeue %d 
3980,i,[ phyrf_mc_paprd.c : 2121 ] PAPRD:Tx stats : tx_fail %d 
3979,,[ phyrf_mc_paprd.c : 786 ] PAPRD: pHandle NULL 
3978,i,[ phyrf_mc_paprd.c : 796 ] PAPRD: PhyId %d Inactive, returning without CAL 
3977,i,[ phyrf_mc_paprd.c : 802 ] PAPRD: Start Calibration : %d ms Timer expired  
3976,,[ phyrf_mc_paprd.c : 2607 ] PAPRD: pHandle NULL 
3975,i,[ phyrf_mc_paprd.c : 2614 ] PAPRD: PhyId %d dpd_cal_sync_timer_handler_0, releasing the wal_lock 
3974,iiiiii,[ phyrf_mc_paprd.c : 1949 ] PAPRD: Abort TempRecal phy %d, curr time %d, currTemp %d, last calTemp  %d curr Channel %d thermal channel %d 
3973,iiii,[ phyrf_mc_paprd.c : 1963 ] PAPRD : FTM PHY id %d currTemp %d cal temp %d tempDiff_scale %d 
3972,iiiiii,[ phyrf_mc_paprd.c : 1974 ] PAPRD : TempRecal triggered phy %d, curr time %d, currTemp %d, last calTemp  %d channel %d tempDiff %d 
3971,iiii,[ phyrf_mc_paprd.c : 1991 ] PAPRD : PHY id %d currTemp %d cal temp %d tempDiff_scale %d 
3970,iiiiii,[ phyrf_mc_paprd.c : 2446 ]  (chan %d ,cm %d halphyMemDPDValidateCalDB , result [%d %d], cal_attempts[%d %d] 
3969,iiiii,[ phyrf_mc_paprd.c : 2450 ]  (chan %d ,cm %d halphyMemDPDValidateCalDB , max attemps %d temp [%d %d] 
3968,iiii,[ phyrf_mc_paprd.c : 2416 ]  halphyPaprdValidateMemCalibration calattempts %d %d, validBits %d %d 
3967,,[ phyrf_mc_paprd.c : 2421 ]  CALIBRATION COMPLETE  chain 0, result 1 
3966,,[ phyrf_mc_paprd.c : 2425 ]  CALIBRATION COMPLETE  chain 1, result 1 
3965,,[ phyrf_mc_paprd.c : 2522 ] Do not have access to masterCalDb or localCalDb, failed to restore DPD 
3964,ii,[ phyrf_mc_paprd.c : 2526 ] DPD Memory : paprd_restore : finalCase %d channel %d 
3963,,[ phyrf_mc_paprd.c : 2588 ] PAPRD: pHandle NULL 
3962,iiii,[ phyrf_mc_paprd.c : 1612 ] PAPRD: cur_channel %d, wal_channel %d, scan_channel %d, phyReset %d 
3961,iiiii,[ phyrf_mc_paprd.c : 1187 ] PAPRD: DPD calibration aborted on chain %d, tableIdx %d, channel %d, state %d, new_channel_change_request %d 
3960,i,[ phyrf_mc_paprd.c : 1204 ] PAPRD: DPD calibration aborted on channel %d 
3959,i,[ phyrf_mc_paprd.c : 238 ] PAPRD:SM state %d 
3958,ii,[ phyrf_mc_paprd.c : 330 ] PAPRD: MEM DPD Aborting Excess Retries. retry_dpd %d, Tx_Err %d 
3957,,[ phyrf_mc_paprd.c : 331 ] PAPRD: Enabling DPD because eDPD failed 
3956,ii,[ phyrf_mc_paprd.c : 334 ] PAPRD: Aborting Excess Retries. retry_dpd %d, Tx_Err %d 
3955,ii,[ phyrf_mc_paprd.c : 434 ] PAPRD: incrementing retry_dpd %d, Tx_Err %d 
3954,ii,[ phyrf_mc_paprd.c : 440 ] 2: PAPRD: incrementing retry_dpd %d, Tx_Err %d 
3953,i,[ phyrf_mc_paprd.c : 444 ] PAPRD: PAPRD_CAL_SM_DPD_TRAINING_PROCESS_DATA hwPaPrdStatus(fail) retry_dpd %d 
3952,iii,[ phyrf_mc_paprd.c : 506 ] PAPRD: TRAINING_PROCESS_DATA chain %d tableIdx %d processing_time %d 
3951,,[ phyrf_mc_paprd.c : 282 ] PAPRD: UCODE VREG WAR enabled 
3950,i,[ phyrf_mc_paprd.c : 542 ]  DPD Aborted due to BG thread activated in FTM mode : smState %d 
3949,,[ phyrf_mc_paprd.c : 603 ] PAPRD: PAPRD_CAL_SM_TEARDOWN_TRAINING : DPD ABORT 
3948,iii,[ phyrf_mc_paprd.c : 624 ] PAPRD: is160mode %d secondary %d primary_done %d 
3947,iii,[ phyrf_mc_paprd.c : 642 ] PAPRD: phy_a0_done %d phy_a1_done %d phy_a1_secondary_done %d 
3946,ii,[ phyrf_mc_paprd.c : 654 ] PAPRD: PAPRDTUNING DONE. total_caltime  %d, phyOff_cnt  %d 
3945,,[ phyrf_mc_paprd.c : 664 ] ----- PAPRDTUNING SECONDARY started----- 
3944,ii,[ phyrf_mc_paprd.c : 674 ] PAPRD: PAPRDTUNING DONE. total_caltime %d, phyOff_cnt %d 
3943,iii,[ phyrf_mc_paprd.c : 679 ] PAPRD: is160mode %d, secondary %d, isExtn %d 
3942,ii,[ phyrf_mc_paprd.c : 680 ] PAPRD: lastcalTime %d, current_time %d 
3941,iiii,[ phyrf_mc_paprd.c : 302 ] PAPRD: State m/c : channel %d, txchain %d, table %d, state %d 
3940,ii,[ phyrf_mc_paprd.c : 1134 ] PAPRD: Channel = %d, dpd_enable = %d 
3939,iii,[ phyrf_mc_paprd.c : 1153 ] PAPRD: Chain = %d, txgainIdx = %d, dacgain = %d 
3938,,[ phyrf_mc_paprd.c : 927 ] PAPRD : phyrf_mc_PaprdStartTimer: 
3937,iiiiiii,[ phyrf_mc_paprd.c : 1717 ] PAPRD: phyrf_mc_SendTxCompletion : channel %d, txchain %d, table %d, new_channel_change_request %d, cal abort_ppdu %d, status %d, retry_cnt %d 
3936,iiiiiii,[ phyrf_mc_paprd.c : 1731 ] PAPRD: new_channel_change_request : channel %d, txchain %d, table %d, new_channel_change_request %d, cal abort_ppdu %d, status %d, retry_cnt %d 
3935,iiiii,[ phyrf_mc_paprd.c : 1756 ] PAPRD: Status %d, whal_tx_err_status_t %d, Flush_req_reason %d, tx_ctxt_flags %d, pdev_paused %d 
3934,i,[ phyrf_mc_paprd.c : 1773 ] PAPRD: HALPHY_TX_TBTT_FLUSH : condition hit , flush_req_reason = %d 
3933,iiii,[ phyrf_mc_paprd.c : 1792 ] PAPRD: Tx Completion Status(HALPHY_TX_ERROR) %d, whal_tx_err_status_t = %d , retrying (chain %d table %d) 
3932,iiiiii,[ phyrf_mc_paprd.c : 1642 ] PAPRD: TxChain %d, tableIdx %d, channel %d, state %d, new_channel_change_request %d, startEvtLatency %d 
3931,,[ phyrf_mc_paprd.c : 1681 ]  PAPRD: phyrf_paprd_TrainingStatus fail 
3930,,[ phyrf_mc_paprd.c : 1657 ] PAPRD: PPDU Start Event Delayed - skip further processing and retry DPD 
3929,iii,[ phyrf_mc_paprd.c : 1671 ] PAPRD: Aborted. Status %d abort_ppdu %d cur_tbl_idx %d 
3928,,[ phyrf_mc_paprd.c : 1677 ]  PAPRD: phyrf_paprd_TrainingStatus success 
3927,i,[ phyrf_mc_paprd.c : 153 ] PAPRD: Paprd Done status is %d
 
3926,iiii,[ phyrf_mc_paprd.c : 1851 ]  PAPRD: phyId %d, txchainmask %d chain %d, degC %d 
3925,iiii,[ phyrf_mc_paprd.c : 1856 ]  PAPRD: phyId %d, txchainmask %d currtime %d, degC %d 
3924,iiii,[ phyrf_mc_paprd.c : 2144 ] PAPRD ApplyTempScaling: PhyId %d slope %d temp delta %d scaling %d 
3923,iiii,[ phyrf_mc_paprd.c : 2667 ] PAPRD: last_valid_chain_idx %d last_valid_table_index %d pPaprdStruct->txChain %d pPaprdStruct->tableIndex %d
 
3922,ii,[ phyrf_mc_paprd.c : 2677 ] PAPRD: phyrf_paprd_HandleMaxRetry pPaprdStruct->training_fail_table %d and calAttempts %d
 
3921,iiiiiii,[ phyrf_mc_paprd.c : 2366 ]  phyId %d thread context : workingChannel %d txChainMask  %d bHomeChan %d phyrfMode %d  WoW Mode %d curr Channel %d 
3920,ii,[ phyrf_mc_paprd.c : 2384 ]  MEM_DPD THREAD (START the new table) : UPDATING CALDB POST PROCESSING DATA :  %d %d 
3919,iiii,[ phyrf_mc_paprd.c : 2397 ]  BG THREAD CONTEXT is DIFFERENT :  %d %d, curr channel %d  bChannelContext %d 
3918,ii,[ phyrf_mc_paprd.c : 2084 ] thermal scaling value is %d and thermal slope is %d 
3917,iii,[ phyrf_mc_paprd.c : 2101 ] PAPRD: temp_recal_timer started. tempRecalcount %d, phyId %d, calTemp %d 
3916,iiiiii,[ phyrf_mc_paprd.c : 2577 ]  phyId %d  thread context : workingChannel %d txChainMask  %d bHomeChan %d phyrfMode %d  WoW Mode %d 
3989,I,[ phyrf_phy.c : 79 ] MAC FW Vreg update RU26 Tx disable = %x 
4033,iii,[ phyrf_regulatory.c : 264 ] RegDB-6G MaxBW AP SP - %d, LPI - %d, VLP - %d
 
4032,iii,[ phyrf_regulatory.c : 270 ] RegDB-6G MaxBW CLIENT SP - %d, LPI - %d, VLP - %d
 
4031,,[ phyrf_regulatory.c : 277 ] RegDB - phyrf_regulatory_FillMinBW_6g
 
4030,iii,[ phyrf_regulatory.c : 281 ] RegDB-6G MinBW AP SP - %d, LPI - %d, VLP - %d
 
4029,iii,[ phyrf_regulatory.c : 287 ] RegDB-6G MinBW CLIENT SP - %d, LPI - %d, VLP - %d
 
4028,iii,[ phyrf_regulatory.c : 297 ] RegDB-6G NumRules AP SP - %d, LPI - %d, VLP - %d
 
4027,iii,[ phyrf_regulatory.c : 303 ] RegDB-6G NumRules CLIENT SP - %d, LPI - %d, VLP - %d
 
4026,Ii,[ phyrf_regulatory.c : 1899 ] RegDB-Test_Super Domain 6G %x %d
 
4025,iii,[ phyrf_regulatory.c : 924 ] RegDB-BDF CC %d BDF RD %d CC Type %d
 
4024,i,[ phyrf_regulatory.c : 1123 ] RegDB-Status %d
 
4023,iiiiiiii,[ phyrf_regulatory.c : 1124 ] RegDB-Final Result alpha0 %d alpha1 %d alpha_size %d max_rules %d get_type %d cc_type %d ctryID %d dmnCode %d
 
4022,iiiiiiii,[ phyrf_regulatory.c : 1125 ] RegDB-Final Result num_2g_rules %d num_5g_rules %d phybitmap %d dfsregion %d min_bw_2g %d min_bw_5g %d max_bw_2g %d max_bw_5g %d
 
4021,i,[ phyrf_regulatory.c : 956 ] RegDB-No Reg_Dmn diff with BDF %d
 
4020,,[ phyrf_regulatory.c : 962 ] RegDB-Has a 6G domain ID
 
4019,,[ phyrf_regulatory.c : 967 ] RegDB-Valid 6G super dmn and 5G2G reg pair Combo
 
4018,,[ phyrf_regulatory.c : 974 ] RegDB-Invlid Combo
 
4017,ii,[ phyrf_regulatory.c : 1055 ] RegDB-6G Super Dmn %d Max BW %d
 
4016,ii,[ phyrf_regulatory.c : 1060 ] RegDB-Valid country ID %d Correspondig RegDmn %d
 
4015,ii,[ phyrf_regulatory.c : 1107 ] RegDB-6G Super Dmn %d Max BW %d
 
4014,ii,[ phyrf_regulatory.c : 1112 ] RegDB-Valid country ID %d Correspondig RegDmn %d
 
4013,,[ phyrf_regulatory.c : 612 ] RegDB-New Extended Event Invoked
 
4012,iii,[ phyrf_regulatory.c : 648 ] RegDB-Super Dmn Id %d validity %d Idx %d
 
4011,iii,[ phyrf_regulatory.c : 693 ] RegDB-Super Dmn Id %d validity %d Idx %d
 
4010,iii,[ phyrf_regulatory.c : 739 ] RegDB - Ext Event Status - 2G5G %d 6G %d Overall %d
 
4009,iiiiiiii,[ phyrf_regulatory.c : 740 ] RegDB-Final Result_Ext alpha0 %d alpha1 %d alpha_size %d max_rules %d get_type %d cc_type %d ctryID %d dmnCode %d
 
4008,iiiiiiii,[ phyrf_regulatory.c : 741 ] RegDB-Final Result_Ext num_2g_rules %d num_5g_rules %d phybitmap %d dfsregion %d min_bw_2g %d min_bw_5g %d max_bw_2g %d max_bw_5g %d
 
4007,Ii,[ phyrf_regulatory.c : 1748 ] RegDB-Test_Super Domain 6G %x %d
 
4006,ii,[ phyrf_regulatory.c : 451 ] RegDB-Getting 6G_AP_LPI Rules dmn_id %d num_rules %d
 
4005,ii,[ phyrf_regulatory.c : 454 ] RegDB-Getting 6G_AP_SP Rules dmn_id %d num_rules %d
 
4004,ii,[ phyrf_regulatory.c : 457 ] RegDB-Getting 6G_AP_VLP Rules dmn_id %d num_rules %d
 
4003,ii,[ phyrf_regulatory.c : 462 ] RegDB-Getting 6G_CLIENT_LPI Rules dmn_id %d num_rules %d
 
4002,ii,[ phyrf_regulatory.c : 469 ] RegDB-Getting 6G_CLIENT_SP Rules dmn_id %d num_rules %d
 
4001,ii,[ phyrf_regulatory.c : 476 ] RegDB-Getting 6G_CLIENT_VLP Rules dmn_id %d num_rules %d
 
4000,i,[ phyrf_regulatory.c : 1149 ] RegDB-Valid reg dmn pair id %d
 
3999,ii,[ phyrf_regulatory.c : 1163 ] RegDB-Valid domain 2g rules %d 5g rules %d
  
3998,,[ phyrf_regulatory.c : 1264 ] Invalid country code. Setting to "US". 
3997,,[ phyrf_regulatory.c : 1338 ] Invalid country_code/domain_code. No currentRD or ctl value change. 
3996,ii,[ phyrf_regulatory.c : 1572 ] REGDB isG=%d dmncode=%d 
3995,ii,[ phyrf_regulatory.c : 1529 ] REGDB isG=%d dmncode=%d 
3994,ii,[ phyrf_regulatory.c : 1551 ] REGDB isG=%d dmncode=%d 
3993,iiiiii,[ phyrf_regulatory.c : 209 ] RegDB 2G-Rule%d start %d end %d max_bw %d reg_power %d flags %d
 
3992,iiiiii,[ phyrf_regulatory.c : 237 ] RegDB 5G-Rule%d start %d end %d max_bw %d reg_power %d flags %d
 
3991,ii,[ phyrf_regulatory.c : 310 ] RegDB 6G Getting Rules dmn_id %d num_rules %d
 
3990,iiiiiii,[ phyrf_regulatory.c : 321 ] RegDB 6G-Rule%d start %d end %d max_bw %d tx_power_eirp %d max_psd_eirp %d flags %d
 
4062,iii,[ phyrf_reset.c : 673 ] DumpTpc-3: set trasmit chan power: %d, forced: %d, max tx: %d 
4061,i,[ phyrf_reset.c : 674 ] phyrf_reset_ForceTxPower: homeChanFlag: %d  
4060,i,[ phyrf_reset.c : 3293 ] Invalid number of chains %d. Resetting PPET to all 0s 
4059,iI,[ phyrf_reset.c : 3336 ] ppet16_8ru0_3[%d] = 0x%x 
4058,iI,[ phyrf_reset.c : 3338 ] update_ppet->numNss_m1 %d, update_ppet->ruMask 0x%x 
4057,i,[ phyrf_reset.c : 3265 ] Invalid ChainIndex %d. Returning the input chainIndex without translating 
4056,i,[ phyrf_reset.c : 3272 ] Invalid ChainIndex %d. Returning the input chainIndex without translating 
4055,i,[ phyrf_reset.c : 3277 ] Translated ChainIndex %d 
4054,I,[ phyrf_reset.c : 3222 ] Translated chainmask 0x%x  
4053,I,[ phyrf_reset.c : 1194 ] HALPHY_RESET_SETUP: Reset cause is %lu
 
4052,I,[ phyrf_reset.c : 1201 ] HALPHY_RESET_SETUP: Scan to home channel change & reset cause is %lu
 
4051,I,[ phyrf_reset.c : 1206 ] HALPHY_RESET_SETUP: Returning to a different home channel and resetCause is %lu
 
4050,,[ phyrf_reset.c : 1210 ] HALPHY_RESET_SETUP: Home to scan channel change!
 
4049,,[ phyrf_reset.c : 1214 ] HALPHY_RESET_SETUP: Home channel change!
 
4048,iiii,[ phyrf_reset.c : 1249 ] DumpTpc-5: set trasmit chan power: %d, 2g limit: %d, 5g limit: %d, max tx: %d 
4047,II,[ phyrf_reset.c : 3122 ] PowerMode setting for phyId : 0x%x, value : 0x%x 
4046,ii,[ phyrf_reset.c : 1658 ] SetChainMasks: tx:%d rx:%d 
4045,ii,[ phyrf_reset.c : 746 ] Not a 160 channel chan->band_center_freq1 %d, chan->band_center_freq2 %d 
4044,iiii,[ phyrf_reset.c : 479 ] DumpTpc-1: set trasmit chan power: %d, 2g limit: %d, 5g limit: %d, max tx: %d 
4043,i,[ phyrf_reset.c : 506 ] halphySetTxChannelPowerLimit homeChanFlag: %d  
4042,iiii,[ phyrf_reset.c : 505 ] halphySetTxChannelPowerLimit phyId %d limit %d maxTxPower %d curChan->mhz %d 
4041,iiii,[ phyrf_reset.c : 428 ] DumpTpc-4: set trasmit chan power: %d, 2g limit: %d, 5g limit: %d, max tx: %d 
4040,i,[ phyrf_reset.c : 429 ] phyrf_reset_SetTxPowerLimit: homeChanFlag: %d  
4039,iiii,[ phyrf_reset.c : 929 ] DumpTpc-4: set trasmit chan power: %d, 2g limit: %d, 5g limit: %d, max tx: %d 
4038,i,[ phyrf_reset.c : 930 ] phyrf_reset_SetTxPowerScale: homeChanFlag: %d  
4037,iiii,[ phyrf_reset.c : 1135 ] UpdateResetParms : homeChannel[0] %d homeChannel[1] %d curChan freq1 %d curChan freq2 %d 
4036,iiIi,[ phyrf_reset.c : 3360 ] PPET  numNss_m1 %d, nss_2g %d, chainmask %x, numchains %d 
4035,iiIi,[ phyrf_reset.c : 3376 ] PPET  numNss_m1 %d, nss_5g %d, chainmask %x, numchains %d 
4034,iii,[ phyrf_reset.c : 3386 ] PPET updated = %d (1=YES,0=NO) phyId %d rf_mode %d 
4067,,[ phyrf_spectral.c : 306 ] SSCAN: Activating spectral scan  
4066,,[ phyrf_spectral.c : 326 ] SSCAN: Deactivating spectral scan  
4065,,[ phyrf_spectral.c : 457 ] SSCAN: Disabling spectral scan  
4064,,[ phyrf_spectral.c : 228 ] SSCAN: Enabling spectral scan  
4063,,[ phyrf_spectral.c : 350 ] SSCAN: Resetting spectral scan  
4071,III,[ phyrf_tpc.c : 347 ] %s:chan 0x%x  flag:0x%x
 
4070,i,[ phyrf_tpc.c : 416 ] TPC_ED WarmReset %d 
 
4069,i,[ phyrf_tpc.c : 419 ] TPC_ED WarmReset %d 
 
4068,ii,[ phyrf_tpc.c : 494 ] setting plut and alut for 160 chan1 %d chan2 %d 
4078,iii,[ phyrf_bdf_tpc.c : 1194 ]  phyrf_tpc_device_ClpcPlutAlutUpdate tpcPowerOffset[%d] %d twoPtOffset[cmask] %d 
4077,iiiii,[ phyrf_bdf_tpc.c : 231 ] return from phyrf_tpc_device_AlutGeneration as pdadc meas seems to be zero %d %d %d %d %d 
4076,ii,[ phyrf_bdf_tpc.c : 802 ] ##TPC_DBG: GVC Chan %d CalDB %d
 
4075,i,[ phyrf_bdf_tpc.c : 907 ] GLUT_PROG_ERROR: pRawCalPerPointOlpcGtxExt was unexpectedly NULL, last 2 entries of GLUT NOT BEING PROGRAMMED maxGlutIdx = %d 
4074,Iiiiii,[ phyrf_bdf_tpc.c : 1014 ] ##GVC0 chIDX %lu, pwr %d, dGain %d, gIdx %d, paCfg %d, maxGlutIdx %d 
 
4073,ii,[ phyrf_bdf_tpc.c : 807 ] ##TPC_DBG: sec80 Chan %d sec80 CalDB %d
 
4072,i,[ phyrf_bdf_tpc.c : 820 ] Zero TPC FreqPiers for the band %d 
 
4099,,[ wlan_stats.c : 2024 ] PS_STA_AVG_CHANNEL_CONGESTION(ERROR0):total_awake_period == 0 
4098,II,[ wlan_stats.c : 2043 ] PS_STA_AVG_CHANNEL_CONGESTION(ERROR1):diff_all(%u) < diff_tx(%u) 
4097,I,[ wlan_stats.c : 2061 ] PS_STA_AVG_CHANNEL_CONGESTION(ERROR2): chan_activity(%u) > 100 
4096,IIIIIII,[ wlan_stats.c : 2084 ] PS_STA_AVG_CHANNEL_CONGESTION: vdev_id=%u, running_avg=%u, chan_activity=%u, total_period=%u, busy_activity=%u, diff_all=%u, diff_tx=%u 
4095,,[ wlan_stats.c : 1839 ] chan_init POOL ALLOC FAILURE 
4094,iii,[ wlan_stats.c : 529 ] wlan_stats_processor:vdev_id:%d ch%d_snr:%d 
4093,,[ wlan_stats.c : 4138 ] _wlan_iface_link_stats_process: vdev is NULL 
4092,iii,[ wlan_stats.c : 4248 ] total_num_peers:%d num_peer_stats_events:%d num_peer_in_event: %d 
4091,,[ wlan_stats.c : 4081 ] radio_link_stats_process no buffer 
4090,ii,[ wlan_stats.c : 4108 ] radio_link_stats_process cur_pwr_state:%d next_pwr_state:%d 
4089,,[ wlan_stats.c : 4941 ] WMI_VDEV_SEND_BIG_DATA_EVENTID Err mem alloc failed  
4088,ii,[ wlan_stats.c : 4981 ] wlan_send_big_data_to_host : VDEV EVT:WMI_VDEV_SEND_BIG_DATA_EVENTID vdevId=%d time=%d 
4087,ii,[ wlan_stats.c : 428 ]  PS_STA_AVG_CHANNEL_CONGESTION BusyChanRunningAvg = %d %d 
4086,ii,[ wlan_stats.c : 1144 ] wlan_stats_processor:vdev_id:%d mac_snr:%d 
4085,iii,[ wlan_stats.c : 1320 ] wlan_stats_processor: peer_stats->peer_tx_rate = %d rx_rate = %d rssi = %d 
4084,,[ wlan_stats.c : 1626 ] wlan_stats_processor: Ran out of buffers; Aborting Report generation;		       Sending Report to Host  
4083,ii,[ wlan_stats.c : 1168 ] wlan_stats_processor:vdev_id:%d invalid_snr:%d 
4082,ii,[ wlan_stats.c : 1179 ] wlan_stats_processor:vdev_id:%d bcn_snr:%d 
4081,,[ wlan_stats.c : 4776 ] _wlan_wlm_stats_process: vdev is NULL 
4080,,[ wlan_stats.c : 4784 ] _wlan_wlm_stats_process: wal_vdev is NULL 
4079,i,[ wlan_stats.c : 4789 ] _wlan_wlm_stats_process: cmd->vdev_id:%d is not up or sta 
4105,I,[ wlan_wmi_ctrl_path_stats.c : 419 ] cp_stats print stats for pdev_id =0x%X 
4104,I,[ wlan_wmi_ctrl_path_stats.c : 108 ] cp_stats event_send_complete & released buffer= 0x%X  
4103,II,[ wlan_wmi_ctrl_path_stats.c : 695 ] cp_stats Reeived cp stats_req with stats_id_mask =0x%X  action =0x%X 
4102,,[ wlan_wmi_ctrl_path_stats.c : 136 ] cp_stats calling send event 
4101,II,[ wlan_wmi_ctrl_path_stats.c : 166 ] cp_stats send wmi event with more data = 0x%X  event_status = 0x%X 
4100,I,[ wlan_wmi_ctrl_path_stats.c : 672 ] cp_stats call send event with more data = 0x%X  
4123,iIIiiII,[ wlan_rssi_monitor.c : 250 ] RSSI_MONITOR_ARBITER: vdevid=%d, client=%u, rssi_threshold_type=%u, low_rssi_threshold=%d, high_rssi_threshold=%d, configure_low_rssi_thresh=%u, configure_high_rssi_thresh=%u 
4122,iIiIiIii,[ wlan_rssi_monitor.c : 311 ] RSSI_MONITOR_ARBITER_CONFIG_HW: vdevid=%d, configure_low_rssi_thresh=%u, final_low_rssi_thresh=%d, configure_high_rssi_thresh=%u, final_high_rssi_thresh=%d, rssi_weight=%u low client:%d high client:%d 
4121,ii,[ wlan_rssi_monitor.c : 163 ] RSSI_MONITOR_CHECK_AND_DELIVER_EVENT: vdevid=%d, current_rssi=%d 
4120,iIII,[ wlan_rssi_monitor.c : 145 ] RSSI_MONITOR_DELIVER_EVENT: vdevid=%d, client=%u, evt_type=%u, cb_fn=%#x 
4119,iII,[ wlan_rssi_monitor.c : 419 ] RSSI_MONITOR_DISABLE_THRESHOLDS_CLIENT_REQ: vdevid=%d, client=%u, rssi_threshold_type=%u 
4118,iI,[ wlan_rssi_monitor.c : 424 ] RSSI_MONITOR_DISABLE_THRESHOLDS_CLIENT_REQ_ERR(!vdev_rssi_monitor): vdevid=%d, client=%u 
4117,iIIii,[ wlan_rssi_monitor.c : 343 ] RSSI_MONITOR_ENABLE_THRESHOLDS_CLIENT_REQ: vdevid=%d, client=%u, rssi_threshold_type=%u, low_rssi_threshold=%d, high_rssi_threshold=%d 
4116,iI,[ wlan_rssi_monitor.c : 348 ] RSSI_MONITOR_ENABLE_THRESHOLDS_CLIENT_REQ_ERR(!vdev_rssi_monitor): vdevid=%d, client=%u 
4115,iI,[ wlan_rssi_monitor.c : 391 ] RSSI_MONITOR_ENABLE_THRESHOLDS_CLIENT_REQ_ERR(!client_data): vdevid=%d, client=%u 
4114,iii,[ wlan_rssi_monitor.c : 52 ] RSSI_MONITOR_GET_BEACON_RSSI_AVG: vdevid=%d, rssi_avg=%d, mac_id=%d 
4113,iI,[ wlan_rssi_monitor.c : 461 ] RSSI_MONITOR_HW_EVENT: vdevid=%d, event_type=%x 
4112,i,[ wlan_rssi_monitor.c : 475 ] RSSI_MONITOR_HW_EVENT(!low_rssi_threshold_configured): vdevid=%d 
4111,i,[ wlan_rssi_monitor.c : 492 ] RSSI_MONITOR_HW_EVENT(!high_rssi_threshold_configured): vdevid=%d 
4110,iIIiii,[ wlan_rssi_monitor.c : 119 ] RSSI_MONITOR_UPDATE_BEACON_RSSI: vdevid=%d, mac_id=%u, rssi_last=%u, rssi_avg_last=%d rssi_new=%d rssi_avg_new=%d 
4109,iIIiii,[ wlan_rssi_monitor.c : 123 ] RSSI_MONITOR_UPDATE_BEACON_RSSI: vdevid=%d, mac_id=%u, rssi_last=%u, rssi_avg_last=%d rssi_new=%d rssi_avg_new=%d 
4108,iI,[ wlan_rssi_monitor.c : 512 ] RSSI_MONITOR_VDEV_EVENT: vdevid=%d, notif=%u 
4107,i,[ wlan_rssi_monitor.c : 596 ] RSSI_MONITOR_VDEV_FREE: vdevid=%d 
4106,i,[ wlan_rssi_monitor.c : 584 ] RSSI_MONITOR_VDEV_INIT: vdevid=%d 
4131,ii,[ wlan_opmode.c : 76 ] WLAN_OPMODE_SET_PMAC_LATENCY: mac_id=%d, opmode_latency=%d 
4130,ii,[ wlan_opmode.c : 85 ] WLAN_OPMODE_SET_PMAC_LATENCY: mac_id=%d, opmode_latency=%d [!WAL_EOK returned] 
4129,iiii,[ wlan_opmode.c : 142 ] WLAN_OPMODE_UPDATE_PMAC_LATENCY: mac_id=%d, final_latency=%d, power_state=%d, is_pmac_idle=%d 
4128,i,[ wlan_opmode.c : 259 ] WLAN_OPMODE_VDEV_FREE: vdev_id=%d 
4127,i,[ wlan_opmode.c : 243 ] WLAN_OPMODE_VDEV_INIT: vdev_id=%d 
4126,i,[ wlan_opmode.c : 250 ] WLAN_OPMODE_VDEV_INIT: vdev_id=%d [!A_OK returned] 
4125,iI,[ wlan_opmode.c : 157 ] WLAN_OPMODE_WAL_PDEV_EVT: pmac_id=%d, event=0x%x 
4124,ii,[ wlan_opmode.c : 182 ] WLAN_OPMODE_VDEV_EVT: vdev_id=%d, event=%d 
4140,ii,[ wlan_pm_arbiter.c : 486 ] wlan_pm_arbiter_dump_wake_stats: mac_id=%d, ModuleID=%d 
4139,iii,[ wlan_pm_arbiter.c : 471 ] wlan_pm_arbiter_req_migration: vdevid=%d, old_mac_id=%d, new_mac_id=%d 
4138,iiiIiiI,[ wlan_pm_arbiter.c : 763 ] PS_STA_PM_ARB_REQUEST: vdev_id=%d, mac_id=%d, ModuleID=%d, Flags=0x%x, LastRequestTime=%d, Request=%d pm_arb_req_handle = 0x%x 
4137,IIII,[ wlan_pm_arbiter.c : 770 ] Updated wake lock module bitmask, bitmask[0]=0x%x, bitmask[1]=0x%x, bitmask[2]=0x%x, bitmask[3]=0x%x 
4136,ii,[ wlan_pm_arbiter.c : 334 ] PS_STA_PM_ARB_RESOLVE: macid=%d, power_state=%d 
4135,ii,[ wlan_pm_arbiter.c : 638 ] wake_monitor mac:%d win_len:%dms 
4134,iiiiii,[ wlan_pm_arbiter.c : 682 ] wake_monitor mac:%d s_list mod:%d vdev:%d total_time:%dms total_cnt:%d max_time:%dms 
4133,iiiiii,[ wlan_pm_arbiter.c : 661 ] wake_monitor mac:%d w_list mod:%d vdev:%d total_time:%dms total_cnt:%d max_time:%dms 
4132,iii,[ wlan_pm_arbiter.c : 422 ] wlan_pm_arbiter_vdev_migration: vdevid=%d, old_mac_id=%d, new_mac_id=%d 
4145,iiiIi,[ wlan_powersave_ap.c : 2320 ] AP_PS_DBGID_DELIVER_CAB vdev_id = %d Tid = %d NumMPDU = %d Flags = 0x%x RetryOther = %d 
4144,i,[ wlan_powersave_ap.c : 2258 ] AP_PS_DBGID_CAB_FINISH vdev_id = %d 
4143,i,[ wlan_powersave_ap.c : 2414 ] AP_PS_DBGID_START_CAB vdev_id = %d 
4142,i,[ wlan_powersave_ap.c : 3136 ] AP_PS_DBGID_VDEV_CREATION_FAILURE AP PS:vdev_id = %d vdev alloc failed 
4141,Ii,[ wlan_powersave_ap.c : 3343 ] AP_PS_DBGID_HOST_TX_PAUSE vdev_map = %0x, pause: %d 
4162,iiiiiI,[ wlan_powersave_sta.c : 2729 ] PS_STA_PSPOLL_SEQ_DONE vdev_id = %d QueueTime = %d CompleteTime = %d ResponseTime = %d ResponseDuration = %d ResponseFrameCtrl/QosCtrl = 0x%x 
4161,,[ wlan_powersave_sta.c : 1454 ] sta_handle POOL ALLOC FAILURE 
4160,iii,[ wlan_powersave_sta.c : 1861 ] PS_STA_DELIVER_EVENT vdev_id = %d EventType = %d Statue = %d 
4159,ii,[ wlan_powersave_sta.c : 3337 ] wlan_ps_sta_enable_disable_dbg_logs vdev_id = %d, enable = %d 
4158,iI,[ wlan_powersave_sta.c : 2991 ] STA PS: wlan_ps_sta_health_monitor_timeout: vdev_id=%d sta_flags=0x%X 
4157,iI,[ wlan_powersave_sta.c : 1702 ] wlan_ps_sta_pause: vdev_id=%d, timeout_us=%u 
4156,iiIi,[ wlan_powersave_sta.c : 1780 ] PS_STA_PSPOLL_ALLOW vdev_id = %d Allow = %d Flags = 0x%x Time = %d 
4155,iiIIII,[ wlan_powersave_sta.c : 1009 ] PS_STA_RESYNC vdev_id = %d VDevUpCnt = %d IsBTConnected = 0x%x Flags = 0x%x VDevSubMode = 0x%x BitMap = 0x%x 
4154,ii,[ wlan_powersave_sta.c : 2599 ] PS_STA_COEX_MODE vdev_id = %d Enable = %d 
4153,ii,[ wlan_powersave_sta.c : 2610 ] PS_STA_WOW_MODE vdev_id = %d Enable = %d 
4152,iII,[ wlan_powersave_sta.c : 1936 ] PS_STA_SET_PARAM vdev_id = %d param = 0x%x value = 0x%x 
4151,i,[ wlan_powersave_sta.c : 736 ] STA PS vdev_id = %d, No buffers available for null frames 
4150,ii,[ wlan_powersave_sta.c : 871 ] PS_STA_INACTIVITY_INFO ITO picked = %d us, current ITO = %d,  
4149,i,[ wlan_powersave_sta.c : 1750 ] wlan_ps_sta_unpause: vdev_id=%d 
4148,Iiii,[ wlan_powersave_sta.c : 2913 ] STA PS: VOWiFi: voip_notify: vdev_id=%u, vo_call_start=%d, intvl_ms=%d media_quality=%d 
4147,ii,[ wlan_powersave_sta.c : 2447 ] PS_STA_UAPSD_AUTO_TRIG VdevID = %d NumAC = %d 
4146,iiiiii,[ wlan_powersave_sta.c : 2468 ] PS_STA_UAPSD_AUTO_TRIG_PER_AC vdev_id = %d WMM_AC = %d UserPriority = %d SrvIntl = %d SuspIntl = %d DelayIntl = %d 
4171,ii,[ wlan_powersave_sta_sm.c : 668 ] wlan_ps_sta_data_activity_pending: vdev_id=%d, inactive_time_us=%d 
4170,ii,[ wlan_powersave_sta_sm.c : 1342 ] wlan_ps_sta_state_pause_event: vdev id = %d, pause_stat_rx_frms_leaked = %d 
4169,iii,[ wlan_powersave_sta_sm.c : 3361 ] SPEC_PSPOLL_TIMEOUT: vdevid=%d, spec=%d, timeout=%d 
4168,iiii,[ wlan_powersave_sta_sm.c : 2823 ] sleep_awake_event_rx: MD=%d, pspoll_count=%d, is_qos_null:%d, nodata_count=%d 
4167,iiii,[ wlan_powersave_sta_sm.c : 2828 ] sleep_awake_event_rx: is_qos_null:%d, wakeup_dur=%d, nodata_count=%d, max_count=%d 
4166,,[ wlan_powersave_sta_sm.c : 3072 ] total_spec_pspoll_count reaches MAX: reset it 
4165,iIIiI,[ wlan_powersave_sta_sm.c : 378 ] wlan_ps_sta_tx_sent_send_nullfunc: vdevid=%d, force_ps=0X%x, sta_handle=%p, peer_type=%d, blocked_tids=0X%x 
4164,ii,[ wlan_powersave_sta_sm.c : 1824 ] PS_STA_SPECPOLL_TIMER_STARTED vdev_id = %d SpecPsPollNoDataCnt = %d 
4163,i,[ wlan_powersave_sta_sm.c : 1837 ] PS_STA_SPECPOLL_TIMER_STOPPED: vdev_id = %d 
4224,iiiiiii,[ wlan_smps.c : 2412 ] STA_SMPS_VHT_OP_MODE_NOTIF_PEER_COMPLETE : vdevid = %d peerid = %d completion_status = %d peer_smps_frames_sent_mask = %d vedevNotif = %dsm_power_control = %d, vcLastSMpwrCntrl = %d 
4223,i,[ wlan_smps.c : 2481 ] SMPS Action TX frame not sent, attemps:%d 
4222,ii,[ wlan_smps.c : 2488 ] SMPS action frame attempt mask %d smps_power_control %d 
4221,,[ wlan_smps.c : 2654 ] SMPS_AP Action frame could not send BW OMN notification connection is not VHT 
4220,i,[ wlan_smps.c : 2695 ] SMPS Action TX frame not sent, attemps:%d 
4219,iii,[ wlan_smps.c : 2542 ] STA_SMPS_SEND_VHT_OPMODE_NOTIF_FRAME_TO_PEER vdevid = %d peerid = %d ret_value = %d 
4218,i,[ wlan_smps.c : 4323 ] SMPS Build Operation mode notification IE: enable = %d 
4217,,[ wlan_smps.c : 3462 ] wlan_smps_cfg_change_timeout 
 
4216,iii,[ wlan_smps.c : 3604 ] wlan_smps_cfg_notify_done: status:%d, stage:%d->0 smps_cfg_notify_compl_args.ctxt=%d  
4215,iiiIi,[ wlan_smps.c : 3638 ] wlan_smps_chainmask_change_handle_done: status:%d, stage:%d->0,smps_cfg_notify_compl_args.ctxt=%d cur_chain_h16/next_chain=0x%x,smstate:%d 
4214,,[ wlan_smps.c : 3293 ] wlan_smps_vc_cfg_notify queued cfg 
 
4213,iI,[ wlan_smps.c : 4347 ] SMPS get Operation mode notification IE length %d %p 
4212,ii,[ wlan_smps.c : 1299 ] wlan_smps_get_peer_bandwidth channel_width = %d, peer_bw = %d 
4211,ii,[ wlan_smps.c : 2783 ] STA_SMPS_CREATE_NON_STA_INSTANCE vdevid = %d smps_handle = %d 
4210,ii,[ wlan_smps.c : 2794 ] STA_SMPS_DELETE_NON_STA_INSTANCE : vdevid = %d smps_handle = %d  
4209,iii,[ wlan_smps.c : 2052 ] STA_SMPS_DTIM_CHMASK_UPDATE_AWAKE : tx_chainmask = %d rx_chainmask = %d orig_rx_chainmask = %d 
4208,ii,[ wlan_smps.c : 2057 ] DTIM_UPDATE_CHAIN_ON_AWAKE: update chain in single chain, hwchain=%d, new=%d 
4207,i,[ wlan_smps.c : 2024 ] wlan_smps_pdev_update_dtim_chmask_on_sleep RSSI_INDICATION = %d 
4206,I,[ wlan_smps.c : 3563 ] wlan_smps_set_current_cfg vdev level notification hence no update vdev_map = 0x%x 
4205,i,[ wlan_smps.c : 2312 ] STA_SMPS_CREATE_STA_INSTANCE : sta_handle = %d 
4204,i,[ wlan_smps.c : 2335 ] STA_SMPS_DELETE_STA_INSTANCE : sta_handle = %d 
4203,,[ wlan_smps.c : 1451 ] SMPS_STA Action frame could not send BW OMN/OMI notification connection is not VHT 
4202,,[ wlan_smps.c : 1496 ] SMPS_STA Action frame could not send BW OMN/OMI notification wrong rx NSS 
4201,,[ wlan_smps.c : 1506 ] SMPS_STA Action frame could not send BW OMN/OMI notification wrong tx NSS 
4200,,[ wlan_smps.c : 1511 ] wlan_smps_sta_send_action_frame IEEE80211_NODE_HE 
4199,ii,[ wlan_smps.c : 1549 ] SMPS_STA Action frame send power_control: %d ret_value:%d 
4198,iIIiIi,[ wlan_smps.c : 4049 ] wlan_smps_vc_cfg_notify : arg %d req rx_chainmask = 0x%x currVCrxnss = 0x%xnew_channel_width = %d , updatecfg= 0x%x, is_vdev_notif = %d 
4197,I,[ wlan_smps.c : 4063 ] SMPS not supported on current channel 0x%x 
4196,iIi,[ wlan_smps.c : 4071 ] wlan_smps_vc_cfg_notify vc_handle->cfg_change_stage=%d, new_cfg.update_cf=%x, new_cfg.vdev_map = %d 
4195,,[ wlan_smps.c : 4085 ] wlan_smps_rejecting_queuing, something is already queued 
 
4194,Ii,[ wlan_smps.c : 4108 ] wlan_smps_vc_cfg_notify queued cb = 0x%x, ret = %d 
4193,i,[ wlan_smps.c : 4118 ] invalid smps cfg notification value new_cfg.channel_width = %d 
4192,,[ wlan_smps.c : 4158 ] SMPS_CFG_CHANGE_NOTIFY: rejected due to duplicate request 
4191,IiI,[ wlan_smps.c : 4243 ] SMPS_CFG_CHANGE_NOTIFY: ONLY CFG PARAM CHANGE mhz: 0x%x, ret = %d, Notification mask = 0x%x 
4190,Iiiii,[ wlan_smps.c : 4254 ] SMPS_CFG_CHANGE_NOTIFY:  mhz: 0x%x, ret = %d, prev_vc_rx_chain_mode: %d, next_vc_rx_chain_mode: %d, chain_mask_change_stage: %d  
4189,I,[ wlan_smps.c : 4256 ] SMPS_CFG_CHANGE_NOTIFY: Invalid VC handle %p 
4188,iiIIII,[ wlan_smps.c : 3894 ] invalid smps cfg notification requested ul_disablemu = %d, channel_width = %d rx_chainmask = 0x%x, tx_chainmask = 0x%x, update cfg = %x, vdev map = %x 
4187,I,[ wlan_smps.c : 3973 ] vdev level notification is requested  = 0x%x 
4186,iiiii,[ wlan_smps.c : 891 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL_OLD_DBG : power control = %d vc_handle->last_frame_sm_pwr_ctrl = %d completion status = %d current_state = %d vc_handle->cfg_change_stage = %d  
4185,iI,[ wlan_smps.c : 895 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL Additional params: prev_forced_mode = %d channel mhz = 0x%x 
4184,,[ wlan_smps.c : 993 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL : incorrect state readjustment 
 
4183,,[ wlan_smps.c : 1024 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL : fallback on legacy SMPS configuration 
 
4182,i,[ wlan_smps.c : 1086 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL : action_valid = %d 
 
4181,,[ wlan_smps.c : 1098 ] wlan_smps_vc_cfg_notify queued cfg 
 
4180,i,[ wlan_smps.c : 2877 ] STA_SMPS_CREATE_VIRTUAL_CHAN_INSTANCE : vc_handle = %d 
4179,i,[ wlan_smps.c : 2953 ] STA_SMPS_DELETE_VIRTUAL_CHAN_INSTANCE : vc_handle = %d 
4178,ii,[ wlan_smps.c : 340 ]  STA_SMPS_VIRTUAL_CHAN_SMPS_START : vc_handle = %d, vc_handle->enabled = %d 
4177,ii,[ wlan_smps.c : 357 ] SMPSVC CHNL START : STA_SMPS_INVALID_SM_EVENT event = %d dynamicSMPSSupported = %d 
4176,ii,[ wlan_smps.c : 387 ] STA_SMPS_VIRTUAL_CHAN_SMPS_STOP : vc_handle = %d, vc_handle->enabled = %d  
4175,iiiiii,[ wlan_smps.c : 415 ] wlan_smps_virtual_chan_update : vc_handle = %d, vc_handle->enabled = %d,vc_handle->cfg_notification_mode = %d, vc_handle->fw_forced_mode =%d , vc_handle->host_forced_mode = %d, smps_cur_state = %d   
4174,,[ wlan_smps.c : 449 ] wlan_smps_virtual_chan_update : smps action frame sent  
4173,,[ wlan_smps.c : 444 ] wlan_smps_virtual_chan_update : smps restarted  
4172,i,[ wlan_smps.c : 1704 ] wlan_smps_virtual_chan_update_dtim_chmask WAL_PM_MAC_PARAM_RSSI_INDICATION = %d 
4225,ii,[ wlan_smps_sm.c : 186 ] SMPS_STATE_STATIC_EVENT: chain: %d, dropped ev:%d 
4245,ii,[ wlan_twt.c : 334 ] wlan_twt_wmi_add_dialog: vdev_id=%d, id=%d 
4244,iii,[ wlan_twt.c : 428 ] wlan_twt_wmi_add_dialog_complete_event: vdev=%d, id=%d, status=%d 
4243,ii,[ wlan_twt.c : 745 ] wmi_twt_btwt_invite_sta: vdev_id=%d, id=%d 
4242,III,[ wlan_twt.c : 752 ] AP TWT: Cant find peer: lsb_mac=%x:%x:%x 
4241,III,[ wlan_twt.c : 760 ] wlan_twt_wmi_btwt_invite_sta: WMI_PEER_TYPE_SELF: lsb_mac=%x:%x:%x 
4240,iii,[ wlan_twt.c : 785 ] wlan_twt_wmi_btwt_invite_sta_complete_event: vdev=%d, id=%d, status=%d 
4239,ii,[ wlan_twt.c : 828 ] wmi_twt_btwt_remove_sta: vdev_id=%d, id=%d 
4238,III,[ wlan_twt.c : 835 ] AP TWT: Cant find peer: lsb_mac=%x:%x:%x 
4237,III,[ wlan_twt.c : 843 ] wlan_twt_wmi_btwt_remove_sta: WMI_PEER_TYPE_SELF: lsb_mac=%x:%x:%x 
4236,iii,[ wlan_twt.c : 868 ] wlan_twt_wmi_btwt_remove_sta_complete_event: vdev=%d, id=%d, status=%d 
4235,iii,[ wlan_twt.c : 502 ] wlan_twt_wmi_del_dialog: vdev_id=%d, id=%d, b_twt_persistence=%d 
4234,iii,[ wlan_twt.c : 540 ] wlan_twt_wmi_del_dialog_complete_event: vdev=%d, id=%d, status=%d 
4233,iI,[ wlan_twt.c : 235 ] wlan_twt_wmi_disable: pdev_id=%d, flags=0x%x 
4232,i,[ wlan_twt.c : 280 ] wlan_twt_wmi_disable_complete_event: pdev_id=%d 
4231,iiI,[ wlan_twt.c : 120 ] wlan_twt_wmi_enable: pdev_id=%d, sta_cong_timer_ms=%d, pdev-flags=0x%x 
4230,ii,[ wlan_twt.c : 163 ] wlan_twt_wmi_enable_complete_event: pdev_id=%d, status=%d 
4229,ii,[ wlan_twt.c : 581 ] wlan_twt_wmi_pause_dialog: vdev_id=%d, id=%d 
4228,iii,[ wlan_twt.c : 614 ] wlan_twt_wmi_pause_dialog_complete_event: vdev=%d, id=%d, status=%d 
4227,iii,[ wlan_twt.c : 655 ] wlan_twt_wmi_resume_dialog: vdev_id=%d, id=%d, next_twt_size=%d 
4226,iii,[ wlan_twt.c : 700 ] wlan_twt_wmi_resume_dialog_complete_event: vdev=%d, id=%d, status=%d 
4246,iii,[ wlan_twt_protocol.c : 236 ] wlan_twt_action_frame_handler: cat=%d, act=%d, len=%d 
4251,III,[ wlan_twt_ap.c : 259 ] AP TWT: Cant find peer lsb_mac=%x:%x:%x 
4250,i,[ wlan_twt_ap.c : 491 ] AP TWT: Vdev id = %d not TWT enabled 
4249,i,[ wlan_twt_ap.c : 889 ] AP TWT: Vdev id = %d not TWT enabled 
4248,i,[ wlan_twt_ap.c : 647 ] AP TWT: peer id = %d not TWT enabled 
4247,i,[ wlan_twt_ap.c : 824 ] AP TWT: Vdev id = %d not TWT enabled 
4255,iiiiiiii,[ wlan_twt_unit_test.c : 745 ] wlan_twt_unit_test: vdev_id=%d, num_args=%d, type=%d, args:%d-%d-%d-%d-%d 
4254,i,[ wlan_twt_unit_test.c : 748 ] vdev == NULL: %d 
4253,i,[ wlan_twt_unit_test.c : 749 ] !vdev->ifUp, %d 
4252,III,[ wlan_twt_unit_test.c : 492 ] AP TWT: Cant find peer: lsb_mac=%x:%x:%x 
4367,I,[ hca_HwComponentRf_bdf_v1.cpp : 88 ] %s NOT available
 
4366,I,[ hca_HwComponentRf_bdf_v1.cpp : 38 ] %s NOT available
 
4365,I,[ hca_HwComponentRf_bdf_v1.cpp : 96 ] %s NOT available
 
4364,I,[ hca_HwComponentRf_bdf_v1.cpp : 79 ] %s NOT available
 
4363,I,[ hca_HwComponentRf_bdf_v1.cpp : 115 ] %s NOT available
 
4362,I,[ hca_HwComponentRf_bdf_v1.cpp : 70 ] %s NOT available
 
4361,I,[ hca_HwComponentRf_bdf_v1.cpp : 60 ] %s NOT available
 
4360,I,[ hca_HwComponentRf_bdf_v1.cpp : 77 ] %s NOT available
 
4359,I,[ hca_HwComponentRf_bdf_v1.cpp : 64 ] %s NOT available
 
4358,I,[ hca_HwComponentRf_bdf_v1.cpp : 71 ] %s NOT available
 
4357,I,[ hca_HwComponentRf_bdf_v1.cpp : 89 ] %s NOT available
 
4356,I,[ hca_HwComponentRf_bdf_v1.cpp : 76 ] %s NOT available
 
4355,I,[ hca_HwComponentRf_bdf_v1.cpp : 105 ] %s NOT available
 
4354,I,[ hca_HwComponentRf_bdf_v1.cpp : 129 ] %s NOT available
 
4353,I,[ hca_HwComponentRf_bdf_v1.cpp : 91 ] %s NOT available
 
4352,I,[ hca_HwComponentRf_bdf_v1.cpp : 75 ] %s NOT available
 
4351,I,[ hca_HwComponentRf_bdf_v1.cpp : 45 ] %s NOT available
 
4350,I,[ hca_HwComponentRf_bdf_v1.cpp : 95 ] %s NOT available
 
4349,I,[ hca_HwComponentRf_bdf_v1.cpp : 51 ] %s NOT available
 
4348,I,[ hca_HwComponentRf_bdf_v1.cpp : 40 ] %s NOT available
 
4347,I,[ hca_HwComponentRf_bdf_v1.cpp : 65 ] %s NOT available
 
4346,I,[ hca_HwComponentRf_bdf_v1.cpp : 81 ] %s NOT available
 
4345,I,[ hca_HwComponentRf_bdf_v1.cpp : 78 ] %s NOT available
 
4344,I,[ hca_HwComponentRf_bdf_v1.cpp : 92 ] %s NOT available
 
4343,I,[ hca_HwComponentRf_bdf_v1.cpp : 101 ] %s NOT available
 
4342,I,[ hca_HwComponentRf_bdf_v1.cpp : 69 ] %s NOT available
 
4341,I,[ hca_HwComponentRf_bdf_v1.cpp : 100 ] %s NOT available
 
4340,I,[ hca_HwComponentRf_bdf_v1.cpp : 99 ] %s NOT available
 
4339,I,[ hca_HwComponentRf_bdf_v1.cpp : 116 ] %s NOT available
 
4338,I,[ hca_HwComponentRf_bdf_v1.cpp : 128 ] %s NOT available
 
4337,I,[ hca_HwComponentRf_bdf_v1.cpp : 73 ] %s NOT available
 
4336,I,[ hca_HwComponentRf_bdf_v1.cpp : 39 ] %s NOT available
 
4335,I,[ hca_HwComponentRf_bdf_v1.cpp : 50 ] %s NOT available
 
4334,I,[ hca_HwComponentRf_bdf_v1.cpp : 80 ] %s NOT available
 
4333,I,[ hca_HwComponentRf_bdf_v1.cpp : 63 ] %s NOT available
 
4332,I,[ hca_HwComponentRf_bdf_v1.cpp : 55 ] %s NOT available
 
4331,I,[ hca_HwComponentRf_bdf_v1.cpp : 46 ] %s NOT available
 
4330,I,[ hca_HwComponentRf_bdf_v1.cpp : 67 ] %s NOT available
 
4329,I,[ hca_HwComponentRf_bdf_v1.cpp : 74 ] %s NOT available
 
4328,I,[ hca_HwComponentRf_bdf_v1.cpp : 44 ] %s NOT available
 
4327,I,[ hca_HwComponentRf_bdf_v1.cpp : 68 ] %s NOT available
 
4326,I,[ hca_HwComponentRf_bdf_v1.cpp : 42 ] %s NOT available
 
4325,I,[ hca_HwComponentRf_bdf_v1.cpp : 58 ] %s NOT available
 
4324,I,[ hca_HwComponentRf_bdf_v1.cpp : 102 ] %s NOT available
 
4323,I,[ hca_HwComponentRf_bdf_v1.cpp : 41 ] %s NOT available
 
4322,I,[ hca_HwComponentRf_bdf_v1.cpp : 90 ] %s NOT available
 
4321,I,[ hca_HwComponentRf_bdf_v1.cpp : 57 ] %s NOT available
 
4320,I,[ hca_HwComponentRf_bdf_v1.cpp : 56 ] %s NOT available
 
4319,I,[ hca_HwComponentRf_bdf_v1.cpp : 110 ] %s NOT available
 
4318,I,[ hca_HwComponentRf_bdf_v1.cpp : 103 ] %s NOT available
 
4317,I,[ hca_HwComponentRf_bdf_v1.cpp : 61 ] %s NOT available
 
4316,I,[ hca_HwComponentRf_bdf_v1.cpp : 93 ] %s NOT available
 
4315,I,[ hca_HwComponentRf_bdf_v1.cpp : 43 ] %s NOT available
 
4314,I,[ hca_HwComponentRf_bdf_v1.cpp : 107 ] %s NOT available
 
4313,I,[ hca_HwComponentRf_bdf_v1.cpp : 114 ] %s NOT available
 
4312,I,[ hca_HwComponentRf_bdf_v1.cpp : 111 ] %s NOT available
 
4311,I,[ hca_HwComponentRf_bdf_v1.cpp : 106 ] %s NOT available
 
4310,I,[ hca_HwComponentRf_bdf_v1.cpp : 47 ] %s NOT available
 
4309,I,[ hca_HwComponentRf_bdf_v1.cpp : 48 ] %s NOT available
 
4308,I,[ hca_HwComponentRf_bdf_v1.cpp : 109 ] %s NOT available
 
4307,I,[ hca_HwComponentRf_bdf_v1.cpp : 82 ] %s NOT available
 
4306,I,[ hca_HwComponentRf_bdf_v1.cpp : 83 ] %s NOT available
 
4289,I,[ hca_HwComponentRf_bdf_v1.cpp : 118 ] %s NOT available
 
4305,I,[ hca_HwComponentRf_bdf_v1.cpp : 126 ] %s NOT available
 
4304,I,[ hca_HwComponentRf_bdf_v1.cpp : 72 ] %s NOT available
 
4303,I,[ hca_HwComponentRf_bdf_v1.cpp : 104 ] %s NOT available
 
4290,I,[ hca_HwComponentRf_bdf_v1.cpp : 119 ] %s NOT available
 
4302,I,[ hca_HwComponentRf_bdf_v1.cpp : 85 ] %s NOT available
 
4301,I,[ hca_HwComponentRf_bdf_v1.cpp : 112 ] %s NOT available
 
4300,I,[ hca_HwComponentRf_bdf_v1.cpp : 113 ] %s NOT available
 
4299,I,[ hca_HwComponentRf_bdf_v1.cpp : 66 ] %s NOT available
 
4298,I,[ hca_HwComponentRf_bdf_v1.cpp : 62 ] %s NOT available
 
4297,I,[ hca_HwComponentRf_bdf_v1.cpp : 84 ] %s NOT available
 
4296,I,[ hca_HwComponentRf_bdf_v1.cpp : 94 ] %s NOT available
 
4295,I,[ hca_HwComponentRf_bdf_v1.cpp : 108 ] %s NOT available
 
4294,I,[ hca_HwComponentRf_bdf_v1.cpp : 52 ] %s NOT available
 
4293,I,[ hca_HwComponentRf_bdf_v1.cpp : 86 ] %s NOT available
 
4292,I,[ hca_HwComponentRf_bdf_v1.cpp : 59 ] %s NOT available
 
4291,I,[ hca_HwComponentRf_bdf_v1.cpp : 37 ] %s NOT available
 
4287,i,[ hca_HwComponentRf_bdf_v1.cpp : 2540 ] RTT - Invalid preamble: %d; return 0 delays 
4286,iiiiiiii,[ hca_HwComponentRf_bdf_v1.cpp : 2553 ] RTT - phy%d chainNum: %d txRxIdx: %d, dynBw: %d, preamble: %d, heLtf: %d, pktBw: %d, whalRate: %d 
4285,i,[ hca_HwComponentRf_bdf_v1.cpp : 2564 ] RTT - base=%d 
4284,ii,[ hca_HwComponentRf_bdf_v1.cpp : 2568 ] RTT - freq %d, delta=%d 
4283,i,[ hca_HwComponentRf_bdf_v1.cpp : 2574 ] RTT - pri20, delta=%d 
4282,ii,[ hca_HwComponentRf_bdf_v1.cpp : 2582 ] RTT - chain %d delta=%d 
4281,i,[ hca_HwComponentRf_bdf_v1.cpp : 2589 ] RTT - IQ, delta=%d 
4280,i,[ hca_HwComponentRf_bdf_v1.cpp : 2594 ] RTT - LCP, delta=%d 
4279,i,[ hca_HwComponentRf_bdf_v1.cpp : 2605 ] RTT - heavyclip, delta=%d 
4278,i,[ hca_HwComponentRf_bdf_v1.cpp : 2610 ] RTT - DPD PEF, delta=%d 
4277,i,[ hca_HwComponentRf_bdf_v1.cpp : 2615 ] RTT - Tx DAC, delta=%d 
4276,i,[ hca_HwComponentRf_bdf_v1.cpp : 2624 ] RTT - Ti ADC, delta=%d 
4275,i,[ hca_HwComponentRf_bdf_v1.cpp : 2629 ] RTT - VSRC, delta=%d 
4274,i,[ hca_HwComponentRf_bdf_v1.cpp : 2634 ] RTT - spur mit, delta=%d 
4273,,[ hca_HwComponentRf_bdf_v1.cpp : 2643 ] RTT - apply 2G 6us offset
 
4272,i,[ hca_HwComponentRf_bdf_v1.cpp : 2648 ] RTT - delayPs=%d ps 
4271,,[ hca_HwComponentRf_bdf_v1.cpp : 2723 ] NEED to implement GetTpcCalFreq in chip specific class 
4270,iiI,[ hca_HwComponentRf_bdf_v1.cpp : 565 ]  ccaThresh:%d deltaNF:%d reg:%x 
4269,,[ hca_HwComponentRf_bdf_v1.cpp : 3666 ] FTM CALDB: Skipping regeneration of CALDB:
 
4268,,[ hca_HwComponentRf_bdf_v1.cpp : 3668 ] FTM CALDB: NOT Skipping regeneration of CALDB:
 
4267,,[ hca_HwComponentRf_bdf_v1.cpp : 2802 ] TPC_CTL: STBC type and NSS was 1 for NTx >= 2 so setting NSS 2
 
4266,,[ hca_HwComponentRf_bdf_v1.cpp : 2808 ] TPC_CTL: STBC type but NSS was not 1
 
4265,ii,[ hca_HwComponentRf_bdf_v1.cpp : 2511 ] RTT - pktBw %d is not valid in dynamicBw %d 
4264,III,[ hca_HwComponentRf_bdf_v1.cpp : 1922 ] sticky - add 0x%08lx, flag 0x%08lx, val 0x%08lx 
4263,iii,[ hca_HwComponentRf_bdf_v1.cpp : 2384 ] GetCalVersionDetails:: SWCAL DEBUG swCalVersion =%d, boardCalVersion=%d, calStatus=%d 
4262,i,[ hca_HwComponentRf_bdf_v1.cpp : 2091 ] returning from phyrf_bdf_GetRxGainCalCfgLocalByBand: %d
 
4261,iiii,[ hca_HwComponentRf_bdf_v1.cpp : 3164 ] DumpTpcPerPacket: Get regulatory pwr EIRP: %d, is PSD: %d, New regdb WMI call: %d, curr_BW:%d 
 
4260,iii,[ hca_HwComponentRf_bdf_v1.cpp : 3240 ] DumpTpcPerPacket: Get regulatory Final combined power : %d CurrBW: %d, isValidTxPwr: %d
 
4259,I,[ hca_HwComponentRf_bdf_v1.cpp : 346 ] WHAL_ERROR_EEPROM_MACADDR - sum = %lx
 
4258,iiii,[ hca_HwComponentRf_bdf_v1.cpp : 2484 ] tempCode ch%d = %d, calTemp %d, tempSlope %d
 
4257,ii,[ hca_HwComponentRf_bdf_v1.cpp : 2488 ] ##########bdf thermCode %d, calTemp %d
 
4256,i,[ hca_HwComponentRf_bdf_v1.cpp : 2492 ] ##########bdf temp slope %d
 
4290,I,[ hca_HwComponentRf_bdf_v1.cpp : 119 ] %s NOT available
 
4289,I,[ hca_HwComponentRf_bdf_v1.cpp : 118 ] %s NOT available
 
4288,I,[ hca_HwComponentRf_bdf_v1.cpp : 142 ] %s NOT available
 
4371,I,[ phy_dev_calUtils.c : 259 ] otpRead: otp_read_en = 0x%08x 
4370,i,[ phy_dev_calUtils.c : 264 ] Invalid OTP_WORD[=%d]. 
4369,,[ phy_dev_calUtils.c : 319 ] Recipe failure 
4368,I,[ phy_dev_calUtils.c : 320 ] [trigger_cal Recipe failure=%x] 
4385,i,[ phy_dev_fdmtCombCal.c : 958 ] FDMT: CAL_INFO_MEM_0: RUN %d: START 
4384,i,[ phy_dev_fdmtCombCal.c : 961 ] FDMT: CAL_INFO_MEM_0: RUN %d: END 
4383,i,[ phy_dev_fdmtCombCal.c : 963 ] FDMT: CAL_INFO_MEM_1: RUN %d: START 
4382,i,[ phy_dev_fdmtCombCal.c : 966 ] FDMT: CAL_INFO_MEM_1: RUN %d: END 
4381,II,[ phy_dev_fdmtCombCal.c : 82 ] FDMT: ADDR: 0x%08x VAL: 0x%08x 
4380,i,[ phy_dev_fdmtCombCal.c : 168 ] FDMT: RXIQ: CHAIN%d-PRI: 
4379,i,[ phy_dev_fdmtCombCal.c : 171 ] FDMT: RXIQ: CHAIN%d-SEC: 
4378,i,[ phy_dev_fdmtCombCal.c : 174 ] FDMT: RXIQ: CHAIN%d-FCS: 
4377,i,[ phy_dev_fdmtCombCal.c : 132 ] FDMT: TXCL: CHAIN%d-PRI: 
4376,i,[ phy_dev_fdmtCombCal.c : 135 ] FDMT: TXCL: CHAIN%d-FCS: 
4375,i,[ phy_dev_fdmtCombCal.c : 105 ] FDMT: TXDCOC: CHAIN%d-PRI-PRISYN: 
4374,i,[ phy_dev_fdmtCombCal.c : 108 ] FDMT: TXDCOC: CHAIN%d-FCS-PRISYN: 
4373,i,[ phy_dev_fdmtCombCal.c : 150 ] FDMT: TXIQ: CHAIN%d-PRI: 
4372,i,[ phy_dev_fdmtCombCal.c : 153 ] FDMT: TXIQ: CHAIN%d-FCS: 
4392,,[ phy_dev_NFCal.c : 753 ] NFCAL: Enter NFCAL Mode 
4391,,[ phy_dev_NFCal.c : 767 ] NFCAL: Exit NFCAL Mode 
4390,ii,[ phy_dev_NFCal.c : 741 ] NFCAL: Forcing Chain%d MINCCAPWR_PRI80_DB2 with %ddBm 
4389,ii,[ phy_dev_NFCal.c : 742 ] NFCAL: Forcing Chain%d MINCCAPWR_SEC80_DB2 with %ddBm 
4388,ii,[ phy_dev_NFCal.c : 579 ] NFCAL: Converged value for Chain%d MINCCAPWR_OUT_DB2 is %ddBm 
4387,,[ phy_dev_NFCal.c : 68 ] NFCAL: Running Noise Floor CAL 
4386,,[ phy_dev_NFCal.c : 72 ] NFCAL: Noise Floor CAL completed 
4483,,[ phy_dev_paprd_device.c : 128 ] eDPD SendDpdTrainPktFtpg: Invaild PHY BW!!!!
 
4482,III,[ phy_dev_paprd_device.c : 139 ] DPD SendDpdTrainPktFtpg: mcs %u, mpduLen, %u, pktBWCode, %u
 
4481,i,[ phy_dev_paprd_device.c : 3949 ] -Q5-PAPRD-:channel freq %d
 
4480,ii,[ phy_dev_paprd_device.c : 3950 ] -Q5-PAPRD-:txChain %d tableIndex %d
 
4479,i,[ phy_dev_paprd_device.c : 3951 ] -Q5-PAPRD-:forced_sq_idx %d 
4478,ii,[ phy_dev_paprd_device.c : 3952 ] -Q5-PAPRD-:sq_idx_sw %d sq_idx_hw %d
 
4477,,[ phy_dev_paprd_device.c : 1447 ]  Stopping phyDBG capture enable  
4476,I,[ phy_dev_paprd_device.c : 1469 ] -Q5-PAPRDTUNING-:DPD training AGC2 size %lx 
 
4475,I,[ phy_dev_paprd_device.c : 1472 ] -Q5-PAPRDTUNING-:DPD training AGC2 pwr 0x%8lx 
 
4474,I,[ phy_dev_paprd_device.c : 1474 ] -Q5-PAPRDTUNING-:DPD training rx gain idx 0x%lx 
 
4473,I,[ phy_dev_paprd_device.c : 1478 ] -Q5-PAPRD-:DPD training active %lu 
 
4472,I,[ phy_dev_paprd_device.c : 1481 ] -Q5-PAPRD-:DPD training incomplete %lu 
 
4471,I,[ phy_dev_paprd_device.c : 1484 ] -Q5-PAPRDTUNING-:SQ index HW is %lu 
 
4470,i,[ phy_dev_paprd_device.c : 1496 ] -Q5-PAPRD-:DC estimate I %d 
 
4469,i,[ phy_dev_paprd_device.c : 1497 ] -Q5-PAPRD-:DC estimate Q %d 
 
4468,I,[ phy_dev_paprd_device.c : 1503 ] -Q5-PAPRD-:HW calculated stage2 min dispersion = %lu 
 
4467,I,[ phy_dev_paprd_device.c : 1504 ] -Q5-PAPRD-:Dispersion value at SQ Stage2 (minimum index - 1) = %lu 
 
4466,I,[ phy_dev_paprd_device.c : 1505 ] -Q5-PAPRD-:Dispersion value at SQ Stage2 (minimum index + 1) = %lu 
 
4465,II,[ phy_dev_paprd_device.c : 4035 ] --Q5--PAPRD: validmask 0x%lx phyInput->validChainMask 0x%x
 
4464,,[ phy_dev_paprd_device.c : 523 ] PAPRD: HWDISABLE ALL
 
4463,i,[ phy_dev_paprd_device.c : 510 ] PAPRD: HWDISABLE CHAIN : %d
 
4462,i,[ phy_dev_paprd_device.c : 291 ] --Q5-PAPRD : For DPD Cal - Choosing GLUT %d
 
4461,i,[ phy_dev_paprd_device.c : 301 ] --Q5-PAPRD : txMaskImprFlag %d
 
4460,i,[ phy_dev_paprd_device.c : 448 ] eDPD SendDpdTrainPkt: %d
 
4459,i,[ phy_dev_paprd_device.c : 806 ] -Q5-PAPRDTUNING-:DynBW = %d 
 
4458,,[ phy_dev_paprd_device.c : 978 ] force SQ 
 
4457,iI,[ phy_dev_paprd_device.c : 981 ] -Q5-PAPRDTUNING-:Forcing sq index hw for table %d with %lu 
 
4456,iii,[ phy_dev_paprd_device.c : 828 ] TxCount = %d table index = %d, txChina = %d 
 
4455,iiii,[ phy_dev_paprd_device.c : 860 ] -Q5-PAPRD : TxCount = %d table index = %d, txChina = %d, dacGain = %d 
 
4454,i,[ phy_dev_paprd_device.c : 875 ] -Q5 - PAPRDTUNING - :min loopback delay = %d 
 
4453,ii,[ phy_dev_paprd_device.c : 885 ] ADC OVRD VAL is %d with j as  %d 
4452,ii,[ phy_dev_paprd_device.c : 891 ] ADC OVRD VAL is %d with j as  %d 
4451,,[ phy_dev_paprd_device.c : 951 ]  Enabling PHY DBG capture  
4450,,[ phy_dev_paprd_device.c : 959 ] force SQ 
 
4449,,[ phy_dev_paprd_device.c : 966 ] NOT force SQ 
 
4448,ii,[ phy_dev_paprd_device.c : 973 ] Table Index = %d  TxCount = %d
 
4447,iI,[ phy_dev_paprd_device.c : 597 ] -Q5-PAPRD-:Chain = %d, Tx Cal Sub Mode = %lu 
 
4446,iiI,[ phy_dev_paprd_device.c : 602 ] -Q5-PAPRD-:Chain = %d, dpd Rx loop chian %d Rx Cal Sub Mode = %lu 
 
4445,ii,[ phy_dev_paprd_device.c : 606 ] -Q5-PAPRD-: HWIO : Tx Chain %d Attenuation value %d 
 
4444,ii,[ phy_dev_paprd_device.c : 611 ] -Q5-PAPRD-: HWIO : Rx Chain %d Attenuation value %d 
 
4443,,[ phy_dev_paprd_device.c : 748 ] -Q5-PAPRD-: phy_paprd_device_Iron_programming 
 
4442,II,[ phy_dev_paprd_device.c : 3329 ] Populate DPD LUT of Chain %hhu at table_idx %hhu 
 
4441,,[ phy_dev_paprd_device.c : 3383 ] Invalid tableOffset 
 
4440,,[ phy_dev_paprd_device.c : 3436 ] Invalid tableOffset 
 
4439,,[ phy_dev_paprd_device.c : 3442 ] Invalid tableType 
 
4438,iiiI,[ phy_dev_paprd_device.c : 3455 ]  PAPRD:tableType: %d tableIdx: %d at even entry: %d from is : %lx
 
4437,iiiI,[ phy_dev_paprd_device.c : 3457 ]  PAPRD:tableType: %d tableIdx: %d at odd entry: %d from is : %lx
 
4436,,[ phy_dev_paprd_device.c : 3465 ] Start Populated MemoryDPD Table! 
 
4435,i,[ phy_dev_paprd_device.c : 3470 ] int delay ddr x1 = %d
 
4434,i,[ phy_dev_paprd_device.c : 3471 ] int delay ddr x2 = %d
 
4433,i,[ phy_dev_paprd_device.c : 3472 ] int delay ddr x3 = %d
 
4432,i,[ phy_dev_paprd_device.c : 3473 ] int delay ddr x4 = %d
 
4431,i,[ phy_dev_paprd_device.c : 3474 ] int delay ddr x5 = %d
 
4430,i,[ phy_dev_paprd_device.c : 3475 ] int delay ddr x6 = %d
 
4429,,[ phy_dev_paprd_device.c : 3659 ] Invalid tableOffset 
 
4428,,[ phy_dev_paprd_device.c : 3683 ] Invalid tableOffset 
 
4427,,[ phy_dev_paprd_device.c : 3692 ] Finished populating DPD LUT into memory!  
4426,,[ phy_dev_paprd_device.c : 1672 ] -Q5-PAPRD-:Read back DPD training data from memory:
 
4425,ii,[ phy_dev_paprd_device.c : 1673 ] -Q5-PAPRD-:Raw Data: chain %d table %d
 
4424,,[ phy_dev_paprd_device.c : 1674 ] -Q5-PAPRD-:DpdTrainData0	  DpdTrainData1	 DpdTrainData2	 DpdTrainData3 
 
4423,IIII,[ phy_dev_paprd_device.c : 1677 ] -Q5-PAPRD-:%lu	 %lu	 %lu	 %lu 
 
4422,iii,[ phy_dev_paprd_device.c : 472 ] PAPRD: Current Temp is %d Temp Threshold is %d dynGlutEn %d
 
4421,iiIIii,[ phy_dev_paprd_device.c : 500 ] PAPRD:Chain = %d, tpc_index = %d, table_offset = %lu, glut_idx_offset = %lx, txgain_index = %d Power=%d 
 
4420,IIIII,[ phy_dev_paprd_device.c : 3883 ] -Q5-PAPRD- : RestorePreCalSettings savePreCalSettings[0] 0x%x [1] 0x%x [3] 0x%x [4] 0x%x [2] 0x%x 
4419,IIIIi,[ phy_dev_paprd_device.c : 3890 ] -Q5-PAPRD- : RestorePreCalSettings TPC_FORCE_CTRL 0x%x PHYDBG_MODE 0x%x PHYDBG_CAPTURE_L 0x%x PHYDBG_CAPTURE_U 0x%x PHYDBG_TRIGGER_1_L 0x%d 
4418,iI,[ phy_dev_paprd_device.c : 3894 ] -Q5-PAPRD- : RestorePreCalSettings RXBB-EN0 for Chain %d 0x%x  
4417,ii,[ phy_dev_paprd_device.c : 3897 ] -Q5-PAPRD- : RestorePreCalSettings PHYRF_CAL_SEQ_CTRL_19_L %d PHYRF_CAL_MEAS_CTRL_4_U %d 
4416,IIIIi,[ phy_dev_paprd_device.c : 3833 ] -Q5-PAPRD- : SavePreCalSettings TPC_FORCE_CTRL 0x%x PHYDBG_MODE 0x%x PHYDBG_CAPTURE_L 0x%x PHYDBG_CAPTURE_U 0x%x PHYDBG_TRIGGER_1_L 0x%d 
4415,iI,[ phy_dev_paprd_device.c : 3837 ] -Q5-PAPRD- : SavePreCalSettings RXBB-EN0 for Chain %d 0x%x  
4414,ii,[ phy_dev_paprd_device.c : 3841 ] -Q5-PAPRD- : savePreCalSettings PHYRF_CAL_SEQ_CTRL_19_L %d PHYRF_CAL_MEAS_CTRL_4_U %d 
4413,i,[ phy_dev_paprd_device.c : 1038 ] agc2pwr = %d 
4412,i,[ phy_dev_paprd_device.c : 1192 ] -Q5-PAPRD : StopTraining for Chain = %d 
 
4411,iiii,[ phy_dev_paprd_device.c : 1594 ] -Q5-PAPRD-: In training signal quality --- Bin idx %d -- accum count = %d, X value = %d, Average X = %d
 
4410,i,[ phy_dev_paprd_device.c : 1602 ] -Q5-PAPRD-:Max value of Averaged X = %d
 
4409,iiii,[ phy_dev_paprd_device.c : 1620 ] -Q5-PAPRD-:Bin %d chk_acc = %d, cnt = %d, diffn = %d 
4408,i,[ phy_dev_paprd_device.c : 1634 ] -Q5-PAPRD-: Averaged SQ value is %d
 
4407,i,[ phy_dev_paprd_device.c : 1323 ] -Q5-PAPRD : TRAINING DONE value is %d 
 
4406,i,[ phy_dev_paprd_device.c : 1331 ]  SQ value is %d 
 
4405,I,[ phy_dev_paprd_device.c : 1355 ] -Q5-PAPRDTUNING-:TABLE 0 1 SQ index HW is %lu 
 
4404,iIi,[ phy_dev_paprd_device.c : 1371 ] -Q5-PAPRDTUNING-:sq PASS: sq_idx_sw %d sq_idx_hw %ld force_sq_idx %d
 
4403,iiIi,[ phy_dev_paprd_device.c : 1379 ] -Q5-PAPRDTUNING-:sq FAIL : %d sq_idx_sw %d sq_idx_hw %ld force_sq_idx %d
 
4402,,[ phy_dev_paprd_device.c : 1386 ] -Q5-PAPRD-:DPD training Failed. Paprd Done bit is not set in HW!
 
4401,,[ phy_dev_paprd_device.c : 1126 ] -Q5-PAPRD-: phy_paprd_device_XmitTrainningFrame 
 
4400,iI,[ phy_dev_paprd_device.c : 3764 ] -Q5-PAPRD-:Exit Cal function - Chain = %d, Tx Cal Sub Mode = %lu 
 
4399,iiI,[ phy_dev_paprd_device.c : 3769 ] -Q5-PAPRD-:Exit Cal function - Chain = %d, dpd Rx loop chain %d Rx Cal Sub Mode = %lu 
 
4398,,[ phy_dev_paprd_device.c : 535 ] PAPRD: Force enable tlv 
 
4397,i,[ phy_dev_paprd_device.c : 767 ] PAPRD: txgain_index = %d 
 
4396,i,[ phy_dev_paprd_device.c : 780 ] PAPRD: dpdDacGain = %d 
 
4395,I,[ phy_dev_paprd_device.c : 1207 ] --Q5--PAPRDPHYDBG Base = 0x%lx
 
4394,iIIII,[ phy_dev_paprd_device.c : 1244 ] --Q5--PAPRDPHYDBG-IQ %d %05d %05d %05d %05d
 
4393,,[ phy_dev_paprd_device.c : 1248 ] --Q5--PAPRDPHYDBG-IQ delay 1ms 
4504,iI,[ phy_dev_paprd_core.c : 642 ] phy_core_PaprdCalcGainFxp : max bins %d X[GfxpIdx] %lu
 
4503,Ii,[ phy_dev_paprd_core.c : 647 ] -Q5-PAPRD : small signal gain is %ld, max_bins %d
 
4502,ii,[ phy_dev_paprd_core.c : 46 ] phy_core_PaprdChangeTrainingIndex(): Change training position to chain index %d and dpd table index %d 
 
4501,ii,[ phy_dev_paprd_core.c : 441 ] -Q5-PAPRD : Max_index = %d, lssCount = %d  
4500,I,[ phy_dev_paprd_core.c : 612 ] small signal gain is %ld
 
4499,iI,[ phy_dev_paprd_core.c : 619 ] -Q5-PAPRD : PA_in[%d] = 0x%lx
 
4498,i,[ phy_dev_paprd_core.c : 98 ] Channel %d is not in valid range
 
4497,i,[ phy_dev_paprd_core.c : 69 ] Invalid channel %d
 
4496,ii,[ phy_dev_paprd_core.c : 145 ] pPaprdStruct->tableIndex = %d, pPaprdStruct->txChain = %d
 
4495,,[ phy_dev_paprd_core.c : 160 ] ******Memless DPD 
4494,I,[ phy_dev_paprd_core.c : 197 ] SQ is %lu and update DPD table 
 
4493,ii,[ phy_dev_paprd_core.c : 210 ]  SQ > SQ limit, DPD cal failed at chain %d and table index %d
 
4492,I,[ phy_dev_paprd_core.c : 211 ]  SQ = %lu
 
4491,i,[ phy_dev_paprd_core.c : 148 ] training_done_for_curr_table_idx %d 
 
4490,i,[ phy_dev_paprd_core.c : 335 ] -Q5-PAPRD-:max_idx = %d (before adding bin#1) 
 
4489,,[ phy_dev_paprd_core.c : 340 ] -Q5-PAPRD-:X	Y	theta	accCount
 
4488,IIii,[ phy_dev_paprd_core.c : 344 ] -Q5-PAPRD-:%lu	%lu	%d	%d
 
4487,i,[ phy_dev_paprd_core.c : 256 ] Channel %d is not in valid range
 
4486,i,[ phy_dev_paprd_core.c : 839 ] -Q5-PAPRDTUNING-: max_bin  %d 
4485,i,[ phy_dev_paprd_core.c : 840 ] -Q5-PAPRDTUNING-: base_bin %d 
4484,i,[ phy_dev_paprd_core.c : 867 ]  -Q5-PAPRD : Compression Ratio is %d  
4520,i,[ phy_dev_DPDCal.c : 85 ] phyId : %d 
 
4519,i,[ phy_dev_DPDCal.c : 87 ] txmask = %d
 
4518,i,[ phy_dev_DPDCal.c : 88 ] rxmask = %d
 
4517,i,[ phy_dev_DPDCal.c : 89 ] gi = %d
 
4516,,[ phy_dev_DPDCal.c : 102 ] Start to setup DPD cal: phy_DPDCal_InitTrainingData()
 
4515,i,[ phy_dev_DPDCal.c : 103 ] phyId = %d
 
4514,i,[ phy_dev_DPDCal.c : 104 ] txmask = %d
 
4513,i,[ phy_dev_DPDCal.c : 105 ] gi = %d
 
4512,,[ phy_dev_DPDCal.c : 115 ] Start to transmit training packet: phy_paprd_device_TransmitTrainingPacket() 
4511,iIII,[ phy_dev_DPDCal.c : 131 ] %d 	 0x%08x 	 0x%05x%08x 
4510,,[ phy_dev_DPDCal.c : 139 ] Training Done, Start post-processing
 
4509,,[ phy_dev_DPDCal.c : 146 ] Finished post-processing
 
4508,I,[ phy_dev_DPDCal.c : 86 ] phyBase = 0x%lx
 
4507,,[ phy_dev_DPDCal.c : 151 ] Training data not valid poor SQ 
 
4506,,[ phy_dev_DPDCal.c : 157 ] train_done flag cannot be set by HW, DPD Cal hits an critical error and abort
 
4505,,[ phy_dev_DPDCal.c : 301 ] DPDCal Recipe Start!!!
 
4529,iI,[ phy_dev_DACCal.c : 139 ] Q5-DACcal: calibration completed for chain%d, result = 0x%x 
4528,iI,[ phy_dev_DACCal.c : 144 ] Q5-DACcal: calibration failed for chain%d, result = 0x%x 
4527,,[ phy_dev_DACCal.c : 166 ] Disabling TxBBF before DAC Cal for every chain 
4526,i,[ phy_dev_DACCal.c : 192 ] DAC Cal time: = %d us
 
4525,,[ phy_dev_DACCal.c : 182 ] Restoring TxBBF settings 
4524,,[ phy_dev_DACCal.c : 230 ] DAC Cal Restore 
4523,,[ phy_dev_DACCal.c : 205 ] DAC Cal Save 
4522,i,[ phy_dev_DACCal.c : 70 ] running dac_cal_setup for chain%d 
4521,ii,[ phy_dev_DACCal.c : 94 ] running enable_dac_cal for chain%d in mode %d 
4540,,[ phy_dev_PkDetCal.c : 100 ] Enter Peak Detector CAL 
4539,Iii,[ phy_dev_PkDetCal.c : 189 ] remainingChains = %x DCOC_RES_Chain%d= 'd%d  
4538,Iii,[ phy_dev_PkDetCal.c : 193 ] calStatus check failed,  remainingChains = %x chain = %d calStatus=%d 
4537,I,[ phy_dev_PkDetCal.c : 216 ] D_AGC_PKDET_GAIN is set to %x 
4536,iiii,[ phy_dev_PkDetCal.c : 218 ] PKDET_DCOC_RES_OVD for chain %d  is = 'd%d is_sbs=%d PKDET_THRES_5G = %d 
4535,I,[ phy_dev_PkDetCal.c : 224 ] D_AGC_PKDET_GAIN is set to %x 
4534,iiii,[ phy_dev_PkDetCal.c : 226 ] PKDET_DCOC_RES_OVD for chain %d  is = 'd%d is_sbs=%d PKDET_THRES_2G = %d 
4533,II,[ phy_dev_PkDetCal.c : 113 ] rxChMask=%x,counter:%x 
4532,IIII,[ phy_dev_PkDetCal.c : 182 ] PKdet cal check result, RO_AGC_CAL=%x , current chain=%x , remain chain=%x , counter=%x 
4531,IIIii,[ phy_dev_PkDetCal.c : 345 ] pkdet_restore :: regCalResult = 0x%x regParameters[0] = 0x%x regParameters[1] = 0x%x chain = %d is_sbs=%d 
4530,IIIii,[ phy_dev_PkDetCal.c : 302 ] pkdet_save :: regCalResult = 0x%x regParameters[0] = 0x%x regParameters[1] = 0x%x chain = %d is_sbs=%d 
4586,i,[ phy_dev_RxDCOCal.c : 1841 ] RxDCO: Cal failed on chain%d! Writing zeros to DCO LUT... 
4585,iii,[ phy_dev_RxDCOCal.c : 1847 ] RXDCO: Using forced value:Ch[%d] (I,Q)=(%d, %d) 
4584,,[ phy_dev_RxDCOCal.c : 2049 ] phyRxDCOCal_qcn90xx 
4583,,[ phy_dev_RxDCOCal.c : 1871 ] restore_rxdco_calResult 
4582,,[ phy_dev_RxDCOCal.c : 1887 ] RXDCO: Allocating memory for DcoLut 
4581,I,[ phy_dev_RxDCOCal.c : 1410 ] RXDCO: A_DELAY_USECS cal_done time out calDoneCount=%u 
4580,i,[ phy_dev_RxDCOCal.c : 1414 ] RXDCO: A_DELAY_USECS cal_done early calDoneCount=%d 
4579,I,[ phy_dev_RxDCOCal.c : 1417 ] do cal after triggered=0x%X 
4578,,[ phy_dev_RxDCOCal.c : 1423 ] RXDCO: cal_done failure and reset DO_CALIBRATE bit and CF_RESET_CORE !!!!! 
4577,I,[ phy_dev_RxDCOCal.c : 1426 ] WFAX_PHYRF_CAL_SEQ_CTRL_16_L.DO_CALIBRATE= %lu 
4576,,[ phy_dev_RxDCOCal.c : 2034 ] rxdco_disable 
4575,,[ phy_dev_RxDCOCal.c : 155 ] rxdco_docal 
4574,,[ phy_dev_RxDCOCal.c : 271 ] RXDCO: Allocating memory for DcoLut 
4573,i,[ phy_dev_RxDCOCal.c : 278 ] rxdco_docal, RXDCO TIMER1: %d
 
4572,i,[ phy_dev_RxDCOCal.c : 290 ] rxdco_docal, RXDCO TIMER2: %d 
4571,,[ phy_dev_RxDCOCal.c : 298 ] RXDCO: Allocating memory for CalResult 
4570,I,[ phy_dev_RxDCOCal.c : 156 ] RxDCO CAL DEBUG VERSION - 0x%x
 
4569,i,[ phy_dev_RxDCOCal.c : 263 ] rxdco_docal, RXDCO TIMER0: %d 
4568,,[ phy_dev_RxDCOCal.c : 2024 ] rxdco_enable 
4567,,[ phy_dev_RxDCOCal.c : 1598 ] index out of range 
4566,I,[ phy_dev_RxDCOCal.c : 1284 ] xfem_gpo_cfg= 0x%x 
4565,,[ phy_dev_RxDCOCal.c : 999 ] RESULT>>> ch_idx, odac_range, cal_gain, Success, ODAC_I, ODAC_Q, Res_I, Res_Q, interf_pwr, interf_var 
4564,II,[ phy_dev_RxDCOCal.c : 1002 ] ch_idx = [0x%x] rxChMask = 0x%x 
4563,,[ phy_dev_RxDCOCal.c : 2000 ] rxdco_restore 
4562,,[ phy_dev_RxDCOCal.c : 528 ] RXDCO: Cal for MIn Gain 
4561,i,[ phy_dev_RxDCOCal.c : 567 ] RxDCO: Cal failed on chain%d! Writing zeros to DCO LUT... 
4560,iii,[ phy_dev_RxDCOCal.c : 573 ] RXDCO: Using forced value:Ch[%d] (I,Q)=(%d, %d) 
4559,,[ phy_dev_RxDCOCal.c : 533 ] RXDCO: Cal for MAx Gain 
4558,,[ phy_dev_RxDCOCal.c : 556 ] RXDCO: Cal for MIn Gain 
4557,,[ phy_dev_RxDCOCal.c : 362 ] RXDCO: *************************************** HW cal timeout 
4556,i,[ phy_dev_RxDCOCal.c : 371 ] RXDCO: cal done successful, range_iter=%d 
4555,i,[ phy_dev_RxDCOCal.c : 390 ] Condition for Cal Success: cal_success= %d 
4554,i,[ phy_dev_RxDCOCal.c : 396 ] rxdco_run_rxdco_hw_cal: range_iter= %d 
4553,,[ phy_dev_RxDCOCal.c : 444 ] RXDCO: Failed in all tries! 
4552,,[ phy_dev_RxDCOCal.c : 1976 ] rxdco_save 
4551,,[ phy_dev_RxDCOCal.c : 1991 ] RxDCO: Invalid selection. CAL_SAVE is not supported for raw Cal Results 
4550,,[ phy_dev_RxDCOCal.c : 1179 ] RXDCO Cal: rxdco_validate_hw_results 
4549,iiiii,[ phy_dev_RxDCOCal.c : 1224 ] ch_idx=%d i=%d Overall_Success=%d RangeOK=%d ResidualOK=%d 
4548,ii,[ phy_dev_RxDCOCal.c : 1225 ] RC_CH[%d]= %d 
4547,i,[ phy_dev_RxDCOCal.c : 1230 ] RXDCO Cal: rxdco_validate_hw_results: dcoc_range= %d 
4546,i,[ phy_dev_RxDCOCal.c : 1242 ] skip_forceTRSW= %d 
4545,i,[ phy_dev_RxDCOCal.c : 1253 ] forceTRSW= %d 
4544,II,[ phy_dev_RxDCOCal.c : 761 ] mode = [0x%x] rxChMask = 0x%x 
4543,i,[ phy_dev_RxDCOCal.c : 771 ] Def_GainTbl_Max = %d 
4542,,[ phy_dev_RxDCOCal.c : 1638 ] save_restore_rxdco_DcoLut 
4541,I,[ phy_dev_RxDCOCal.c : 1680 ] save_restore_rxdco_DcoLut:::Override mode is not restored for table mode: Value = %x 
4592,,[ phy_dev_RxDCOCal_SWPP.c : 540 ] 2G 20MHz
 
4591,,[ phy_dev_RxDCOCal_SWPP.c : 586 ] 5G Set0
 
4590,,[ phy_dev_RxDCOCal_SWPP.c : 608 ] 5G Set1
 
4589,,[ phy_dev_RxDCOCal_SWPP.c : 635 ] 6G Set0
 
4588,,[ phy_dev_RxDCOCal_SWPP.c : 657 ] 6G Set1
 
4587,,[ phy_dev_RxDCOCal_SWPP.c : 560 ] 2G 40MHz
 
4673,I,[ phy_dev_TPCcal.c : 1074 ] GLUT - Chain %u
 
4672,I,[ phy_dev_TPCcal.c : 2587 ] In CLPCModeICOUPLER_IS: txChainMask = 0x%x
 
4671,I,[ phy_dev_TPCcal.c : 2640 ] In CLPCModeICOUPLER_PO: txChainMask = 0x%x
 
4670,I,[ phy_dev_TPCcal.c : 2705 ] In CLPCModePdet: txChainMask = 0x%x
 
4669,I,[ phy_dev_TPCcal.c : 2685 ] In CLPCModeVdet: txChainMask = 0x%x
 
4668,,[ phy_dev_TPCcal.c : 1032 ] In clearalut routine, Clearing ALUT indices 
4667,,[ phy_dev_TPCcal.c : 999 ] In clearglut routine, Clearing GLUT indices 
4666,i,[ phy_dev_TPCcal.c : 2055 ] Q5-TPC: HW_PDET_CAL: Count is %d
 
4665,,[ phy_dev_TPCcal.c : 2059 ] Q5-TPC: HW_PDET_CAL: LG CAL PAILED !!!!!!!!! 
 
4664,i,[ phy_dev_TPCcal.c : 2083 ] Q5-TPC: HW_PDET_CAL: Count is %d
 
4663,,[ phy_dev_TPCcal.c : 2087 ] Q5-TPC: HW_PDET_CAL: HG CAL PAILED !!!!!!!!! 
 
4662,II,[ phy_dev_TPCcal.c : 752 ] PDL_TPC: EnableTPCMode input->tgtPwrClpcThrDb4 %x with shift %x 
4661,,[ phy_dev_TPCcal.c : 1228 ] Invalid GLUT numEntries!
 
4660,I,[ phy_dev_TPCcal.c : 1248 ] GLUT - Chain %u
 
4659,i,[ phy_dev_TPCcal.c : 176 ] HeavyClippingOffsetSetup %d 
4658,,[ phy_dev_TPCcal.c : 2296 ] OverrideHwPdetCalValues 
4657,I,[ phy_dev_TPCcal.c : 1148 ] PLUT - Chain %u
 
4656,IIIIIII,[ phy_dev_TPCcal.c : 502 ] TPC_PHYDEVLIB maxQAM[0..6] %x %x %x %x %x %x %x 
4655,IIIIIII,[ phy_dev_TPCcal.c : 504 ] TPC_PHYDEVLIB minQAM[0..6] %x %x %x %x %x %x %x 
4654,IIIIIII,[ phy_dev_TPCcal.c : 506 ] TPC_PHYDEVLIB maxQAM MU[0..6] %x %x %x %x %x %x %x 
4653,IIIIIII,[ phy_dev_TPCcal.c : 508 ] TPC_PHYDEVLIB minQAM MU[0..6] %x %x %x %x %x %x %x 
4652,i,[ phy_dev_TPCcal.c : 389 ] In ProgramGLUTIndicesByRange: powerRange = %d
 
4651,,[ phy_dev_TPCcal.c : 393 ] Programming GLUT Indices Range 0
 
4650,,[ phy_dev_TPCcal.c : 411 ] Programming GLUT Indices Range 1
 
4649,,[ phy_dev_TPCcal.c : 424 ] Programming GLUT Indices Range 2
 
4648,,[ phy_dev_TPCcal.c : 437 ] Programming GLUT Indices Range 3
 
4647,i,[ phy_dev_TPCcal.c : 326 ] pktMCSType = %d 
 
4646,IiI,[ phy_dev_TPCcal.c : 961 ] programGLUT: Address of the GLUt base  = 0x%x: GLUT_Idx = %d; Measured power = %hx
 
4645,I,[ phy_dev_TPCcal.c : 600 ] TPC_PHYDEVLIB: TPC_GLUT_TARGET_PWR_LEVEL %x 
4644,I,[ phy_dev_TPCcal.c : 608 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_4_L %x 
4643,I,[ phy_dev_TPCcal.c : 616 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_5_L %x 
4642,I,[ phy_dev_TPCcal.c : 624 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_2_L %x 
4641,I,[ phy_dev_TPCcal.c : 632 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_3_L %x 
4640,I,[ phy_dev_TPCcal.c : 640 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_0_L %x 
4639,I,[ phy_dev_TPCcal.c : 648 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_1_L %x 
4638,I,[ phy_dev_TPCcal.c : 656 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_6_L %x 
4637,I,[ phy_dev_TPCcal.c : 664 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_7_L %x 
4636,IIII,[ phy_dev_TPCcal.c : 3202 ] tpcOnepointCal:: thermCalValue %u alphaTherm %u thermGainErrMax %u for chain %u 
4635,ii,[ phy_dev_TPCcal.c : 1615 ] TX_CONV: Invalid chain_idx:%d for phy_idx:%d  
4634,iii,[ phy_dev_TPCcal.c : 1658 ] TX_CONV: TxConvergenceRegRead phy_idx:%d for chain_idx:%d state:%d 
4633,i,[ phy_dev_TPCcal.c : 1659 ] TX_CONV: txgain_count:%d 
4632,i,[ phy_dev_TPCcal.c : 1660 ] TX_CONV: stat_latest_fwd:%d 
4631,i,[ phy_dev_TPCcal.c : 1661 ] TX_CONV: stat_latest_lb:%d 
4630,iii,[ phy_dev_TPCcal.c : 1704 ] TX_CONV: TX_CONVERGENCE_VALIDATION_RETRY_SUCCESS  phy_idx:%d chain_idx:%d retry_cnt:%d 
4629,iii,[ phy_dev_TPCcal.c : 1709 ] TX_CONV: TX_CONVERGENCE_VALIDATION_RETRY  phy_idx:%d chain_idx:%d retry_cnt:%d 
4628,iii,[ phy_dev_TPCcal.c : 1712 ] TX_CONV: TX_CONVERGENCE_VALIDATION_FAILURE  phy_idx:%d chain_idx:%d retry_cnt:%d 
4627,iiii,[ phy_dev_TPCcal.c : 1721 ] TX_CONV: mhz:%d phy_idx:%d chain_idx:%d state:%d 
4626,,[ phy_dev_TPCcal.c : 1726 ] TX_CONV: TX_CONVERGENCE_CLEAR 
4625,,[ phy_dev_TPCcal.c : 1732 ] TX_CONV: TX_CONVERGENCE_INIT 
4624,,[ phy_dev_TPCcal.c : 1737 ] TX_CONV: TX_CONVERGENCE_UPDATE 
4623,,[ phy_dev_TPCcal.c : 1745 ] TX_CONV: TX_CONVERGENCE_UPDATE_RETRY 
4622,i,[ phy_dev_TPCcal.c : 1758 ] TX_CONV: Invalid state: %d 
4621,iiii,[ phy_dev_TPCcal.c : 1683 ] TX_CONV: phy_idx:%d chain_idx:%d txgain_count_delta:%d latest_pwr_delta:%d 
4620,,[ phy_dev_TPCcal.c : 1687 ] TX_CONV: TX_CONVERGENCE_VALIDATION_SUCCESS 
4619,i,[ phy_dev_TPCcal.c : 2527 ] ov_rel1:%d 
4618,,[ phy_dev_TPCcal.c : 1421 ] Printing all the input paramters
 
4617,iI,[ phy_dev_TPCcal.c : 1429 ] ForcedDacGain[%d] = 0x%x
 
4616,iI,[ phy_dev_TPCcal.c : 1430 ] ForcedTxGainIdx[%d] = 0x%x
 
4615,iI,[ phy_dev_TPCcal.c : 1431 ] ForcedGLUTIdx[%d] = 0x%x
 
4614,I,[ phy_dev_TPCcal.c : 1439 ] Force target Power = 0x%x
 
4613,i,[ phy_dev_TPCcal.c : 1422 ] bandCode - %d
 
4612,I,[ phy_dev_TPCcal.c : 1423 ] ForcedTargetPower - 0x%x
 
4611,I,[ phy_dev_TPCcal.c : 1424 ] ForceDacGain - 0x%x
 
4610,I,[ phy_dev_TPCcal.c : 1425 ] ForceTxGainIdx - 0x%x
 
4609,,[ phy_dev_TPCcal.c : 1833 ] -Q5-TPC:- phyLatestAccumulatedCLPCError_qcn90xx was passed NULL Ptr 
4608,iII,[ phy_dev_TPCcal.c : 1847 ] -Q5-TPC:- tpcOnepointCal::bandCode %d Chain %u latestAccumulatedClpcError %u 
4607,ii,[ phy_dev_TPCcal.c : 1878 ] temp %d = %d 
4606,,[ phy_dev_TPCcal.c : 1886 ] phyLatestThermValue_qcn90xx was passed NULL Ptr 
4605,iII,[ phy_dev_TPCcal.c : 1892 ] -Q5-TPC :- tpcOnepointCal::phyId %d Chain %u thermalVal %u 
4604,,[ phy_dev_TPCcal.c : 3218 ] phyOLPCTempComp_qcn90xx 
4603,,[ phy_dev_TPCcal.c : 3231 ] phyOLPCTempUpdate_qcn90xx 
4602,IIII,[ phy_dev_TPCcal.c : 100 ] Get the Modes - CLPCMode - 0x%x readTPCStatus - 0x%x Force Mode - 0x%x Forced gain - 0x%x 
4601,,[ phy_dev_TPCcal.c : 127 ] Incorrect Test Selection ... 
4600,II,[ phy_dev_TPCcal.c : 161 ] set ch %x TPC_OVERRIDE_3 to %x
 
4599,iii,[ phy_dev_TPCcal.c : 1799 ] TX_CONV: TX_CONVERGENCE_VALIDATION_FAILURE invalid phy_base_addr:%d phy_idx:%d chain_idx:%d 
4598,iii,[ phy_dev_TPCcal.c : 1804 ] TX_CONV: phyInput->bandCode:%d, phyInput->txChMask:%d, tx_active_chain_mask:%d 
4597,i,[ phy_dev_TPCcal.c : 1816 ] TX_CONV: End: tx_converged:%d  
4596,i,[ phy_dev_TPCcal.c : 229 ] -Q5-TPC : In setupTPC: fcsEnabled = %d
 
4595,i,[ phy_dev_TPCcal.c : 235 ] -Q5-TPC : Configuring TPC Mode on PHY with BandCode - %d
 
4594,,[ phy_dev_TPCcal.c : 275 ] -Q5-TPC : Completed the Setup TPC settings... 
4593,iiii,[ phy_dev_TPCcal.c : 2478 ] PDL_TPC_DBG: pdadc[0] %d dcVal[0] %d pdadc[1] %d dcVal[1] %d 
4682,II,[ phy_dev_TxBBFCal.c : 167 ] beol: 0x%x pw: 0x%x
 
4681,,[ phy_dev_TxBBFCal.c : 189 ] Beol and/or pw came back as zero - OTP is likely not programmed 
4680,iii,[ phy_dev_TxBBFCal.c : 203 ] rSkew: %d rc3Skew: %d rc4Skew: %d 
4679,iiiii,[ phy_dev_TxBBFCal.c : 204 ] beol40: %d beol75: %d beol120: %d beol150: %d beol270: %d 
4678,IIIII,[ phy_dev_TxBBFCal.c : 238 ] tiaRtuneTarget: %u lvlRtuneTarget: %u bqRtune1Target: %u bqRtune2Target: %u bqRtune3Target: %u 
4677,IIIII,[ phy_dev_TxBBFCal.c : 239 ] tiaCcompTarget: %u tiaCfwrdTarget: %u tiaCtuneTarget: %u bqC1CtuneTarget: %u bqC2CtuneTarget: %u 
4676,IIIII,[ phy_dev_TxBBFCal.c : 292 ] tiaRtuneTarget: %u lvlRtuneTarget: %u bqRtune1Target: %u bqRtune2Target: %u bqRtune3Target: %u 
4675,IIIII,[ phy_dev_TxBBFCal.c : 293 ] tiaCcompTarget: %u tiaCfwrdTarget: %u tiaCtuneTarget: %u bqC1CtuneTarget: %u bqC2CtuneTarget: %u 
4674,II,[ phy_dev_TxBBFCal.c : 181 ] beol_1.25: 0x%x pw_1.25: 0x%x
 
4695,I,[ phy_dev_RxBBFCal.c : 247 ] rfa_otp_address_base= 0x%08x  
4694,,[ phy_dev_RxBBFCal.c : 267 ] Beol came back as Zero - OTP is likely not programmed 
4693,,[ phy_dev_RxBBFCal.c : 268 ] no action taken 
4692,ii,[ phy_dev_RxBBFCal.c : 273 ] rTune: %d rInt: %d 
4691,,[ phy_dev_RxBBFCal.c : 288 ] RXBBFCAL: bw code too large!!! Defaulting to 0 
4690,,[ phy_dev_RxBBFCal.c : 294 ] RXBBFCAL: bw code 80P80 or 160 or 165 
4689,III,[ phy_dev_RxBBFCal.c : 303 ] rc_corner_scale : %u r_corner_scale: %u c_corner_scale: %u 
4688,IIII,[ phy_dev_RxBBFCal.c : 392 ] Reg_TIA_Gain: %u	tia_Gain_Factor[Reg_TIA_Gain]: %u	chainIdx: %u	ch_factor[chainIdx] = %u 
4687,I,[ phy_dev_RxBBFCal.c : 251 ] hirc 0x%x
 
4686,III,[ phy_dev_RxBBFCal.c : 401 ] bq_cfb_total_ref: %u	bq_cfb_fixed: %u	bq_cfb_tuned = %u 
4685,II,[ phy_dev_RxBBFCal.c : 405 ] chainIdx: %u	ch_factor_BQ_2G[chainIdx] = %u 
4684,II,[ phy_dev_RxBBFCal.c : 410 ] chainIdx: %u	ch_factor_BQ_5G[chainIdx] = %u 
4683,I,[ phy_dev_RxBBFCal.c : 263 ] hirc_1.25 0x%x
 
4715,I,[ rfaConfig.c : 199 ] INVALID FREQUENCY1 %u 
4714,III,[ rfaConfig.c : 229 ] NfNbna: LOFrequency=%0.2fMHz NBNA=0x%x NF=0x%x 
4713,,[ rfaConfig.c : 1065 ] ironInit 
4712,,[ rfaConfig.c : 1087 ]  
4711,,[ rfaConfig.c : 785 ] phyRfaIni 
4710,,[ rfaConfig.c : 790 ] ERROR! UNKNOWN WCSS ENVIRONMENT 
4709,,[ rfaConfig.c : 856 ] RfaIni Done 
4708,,[ rfaConfig.c : 1042 ] set channel Agile Recipe Start 
4707,,[ rfaConfig.c : 1054 ] set channel Agile Recipe Complete 
4706,,[ rfaConfig.c : 1020 ] set channel Recipe Start 
4705,,[ rfaConfig.c : 1032 ] set channel Recipe Complete 
4704,,[ rfaConfig.c : 369 ] Error! : Synth frequency is out of range from defined list 
4703,iii,[ rfaConfig.c : 947 ] freq=%dMHz chanIdx=%d sBandCode=%d 
4702,,[ rfaConfig.c : 905 ] aDFS Configuration not supported 
4701,,[ rfaConfig.c : 323 ] Error! : Synth frequency is out of range from defined list 
4700,I,[ rfaConfig.c : 326 ] da_ctune = 0x%x 
4699,I,[ rfaConfig.c : 329 ] da_ctune = 0x%x 
4698,,[ rfaConfig.c : 283 ] Error! : Synth frequency is out of range from defined list 
4697,III,[ rfaConfig.c : 286 ] ctune[1, 3, 5] = [0x%x, 0x%x, 0x%x] 
4696,III,[ rfaConfig.c : 289 ] ctune[1, 3, 5] = [0x%x, 0x%x, 0x%x] 
4726,III,[ hca_HwComponentTrxPine_tpc.cpp : 140 ] TPC_DBG:EnableCLPC clpc thresh from BDF %x clpc thresh in alutGen %x out %x 
4725,i,[ hca_HwComponentTrxPine_tpc.cpp : 248 ] HcaHwComponentTrxPine_tpc::EnableCLPC=%d PDET Cal executed 
4724,i,[ hca_HwComponentTrxPine_tpc.cpp : 377 ] ov_rel0:%d 
4723,iii,[ hca_HwComponentTrxPine_tpc.cpp : 324 ] force glut: chain%d, gainindex%d: dacgain=%d
 
4722,i,[ hca_HwComponentTrxPine_tpc.cpp : 393 ] OPC: phyId:%d state 
4721,,[ hca_HwComponentTrxPine_tpc.cpp : 639 ] OLPC_TEMP_COMP: Invalid latestThermValue!
 
4720,I,[ hca_HwComponentTrxPine_tpc.cpp : 650 ] OLPC_TEMP_COMP: latestThermValue = %u
 
4719,II,[ hca_HwComponentTrxPine_tpc.cpp : 678 ] TPC_DUMP: PrimaryChan %u, SecondaryChan %u 
 
4718,IIIIIIII,[ hca_HwComponentTrxPine_tpc.cpp : 717 ] TPC_DUMP_GLUT: tpcTblIdx %3u |  tpcChainIdx %3u | tpcGainIdx %3u | pwrMeas %3d | minDacGain %3d | txGainIdx %3d | clpcError %3d | tpcClPktCnt %3d 
4717,IIIIIIIII,[ hca_HwComponentTrxPine_tpc.cpp : 749 ] TPC_DUMP_PLUT: tpcTblIdx %3u |  tpcChainIdx %3u | tpcPlutIdx %3u | pdadc[%3u-%3u] HEX:%8x | pdadc[%3u-%3u] HEX:%8x | 
4716,IIIIIIIII,[ hca_HwComponentTrxPine_tpc.cpp : 781 ] TPC_DUMP_ALUT: tpcTblIdx %3u |  tpcChainIdx %3u | tpcAlutIdx %3u | Alut tgtPwr Step [%3u-%3u] HEX:%8x | Alut tgtPwr Step [%3u-%3u]  HEX:%8x 
4736,II,[ hca_HwComponentTrxPine_cal.cpp : 159 ] RY: RestoreSetHwChainMasks: forceTxChainMask=%x, forceRxChainMask=%x 
4735,i,[ hca_HwComponentTrxPine_cal.cpp : 775 ] VK_NF minNfLimit=%d 
4734,Iii,[ hca_HwComponentTrxPine_cal.cpp : 817 ] DBG_NF per chain : rxChainMask 0x%x nfPerChain[%d] = %d 
4733,i,[ hca_HwComponentTrxPine_cal.cpp : 245 ] NFCAL, itercount : %d 
4732,iii,[ hca_HwComponentTrxPine_cal.cpp : 720 ] AoA - phy%d, numChains %d, freq %d 
4731,iiiiii,[ hca_HwComponentTrxPine_cal.cpp : 732 ] AoA - ch%d, gnIdx %d, dataSz %d, bdfVal %d calVal %d, AoAphase %d 
4730,IIIII,[ hca_HwComponentTrxPine_cal.cpp : 532 ] NFCAL backed up phyId %u, rssiThr1aDb %x, rssiThr1bDb %x, rssiThr1cDb %x, rssiThr1dDb %x 
4729,IIIII,[ hca_HwComponentTrxPine_cal.cpp : 688 ] NFCAL phyId %u, Result %u, ccaCountMax %u, firPwrThrdB2 %u, relPwrThrdB2 %u 
4728,IIIIIIIi,[ hca_HwComponentTrxPine_cal.cpp : 692 ] NFCAL phyId %u, Chan %u, Chain %u, curCCaCnt %u, firpwrCnt %u, relPwrCnt %u, nf_cal_gtc_mask %u, nf %d 
4727,i,[ hca_HwComponentTrxPine_cal.cpp : 618 ] VK_NF minNfLimit=%d 
4741,I,[ hca_HwComponentTrxPine_xtalCal.cpp : 165 ] XTAL_CAL_PINE - Enable flag =0x%x
 
4740,i,[ hca_HwComponentTrxPine_xtalCal.cpp : 183 ] XTAL_CAL- CWgain_index=%d 
4739,i,[ hca_HwComponentTrxPine_xtalCal.cpp : 189 ] XTAL_CAL clear - gainIdx4XtalCal=%d 
4738,iiI,[ hca_HwComponentTrxPine_xtalCal.cpp : 240 ] XTAL_CAL_PINE :SET -Reg_values, chain=%d, idx=%d , value=0x%x
 
4737,iiI,[ hca_HwComponentTrxPine_xtalCal.cpp : 304 ] XTAL_CAL_PINE :Clear - Reg_values, chain=%d, idx=%d , value=0x%x
 
4816,,[ hca_HwComponentTrxPine_bdf.cpp : 2633 ] TPC_DBG: using 2G data 
4815,,[ hca_HwComponentTrxPine_bdf.cpp : 2648 ] TPC_DBG: using 6G data 
4814,,[ hca_HwComponentTrxPine_bdf.cpp : 2661 ] TPC_DBG: using 5G2 data 
4813,i,[ hca_HwComponentTrxPine_bdf.cpp : 6483 ] TLMM::::  GPIO config Success for freq: %d 
4812,,[ hca_HwComponentTrxPine_bdf.cpp : 2811 ] SetCtlTable halphy api called. Access to BDF CTL data temporarily disabled. 
4811,,[ hca_HwComponentTrxPine_bdf.cpp : 2816 ] CTL DATA push failed. 
4810,iiiiiii,[ hca_HwComponentTrxPine_bdf.cpp : 2827 ] Variables: isG: %d, seq: %d, endflag: %d, totalLen: %d, ctl_ptr: %d, beginning actual address: %d, BDF beginning: %d 
4809,i,[ hca_HwComponentTrxPine_bdf.cpp : 2829 ] CTL 2G DATA push under process at seq %d 
4808,i,[ hca_HwComponentTrxPine_bdf.cpp : 2830 ] Size being copied in this iteration: %d 
4807,ii,[ hca_HwComponentTrxPine_bdf.cpp : 2831 ] Value at address %d before copy: %d 
4806,,[ hca_HwComponentTrxPine_bdf.cpp : 2834 ] Invalid CTL data size. Access denied to copy this fragment. Please copy CTL blob from beginning with right size. 
4805,ii,[ hca_HwComponentTrxPine_bdf.cpp : 2840 ] Value at address %d after copy: %d 
4804,i,[ hca_HwComponentTrxPine_bdf.cpp : 2841 ] Size copied: %d 
4803,iiiiiii,[ hca_HwComponentTrxPine_bdf.cpp : 2849 ] Variables: isG: %d, seq: %d, endflag: %d, totalLen: %d, ctl_ptr: %d, beginning actual address: %d, BDF beginning: %d 
4802,i,[ hca_HwComponentTrxPine_bdf.cpp : 2851 ] CTL 6G DATA push under process at seq %d 
4801,i,[ hca_HwComponentTrxPine_bdf.cpp : 2852 ] Size being copied in this iteration: %d 
4800,ii,[ hca_HwComponentTrxPine_bdf.cpp : 2853 ] Value at address %d before copy: %d 
4799,,[ hca_HwComponentTrxPine_bdf.cpp : 2856 ] Invalid CTL data size. Access denied to copy this fragment. Please copy CTL blob from beginning with right size. 
4798,ii,[ hca_HwComponentTrxPine_bdf.cpp : 2862 ] Value at address %d after copy: %d 
4797,i,[ hca_HwComponentTrxPine_bdf.cpp : 2863 ] Size copied: %d 
4796,iiiiiii,[ hca_HwComponentTrxPine_bdf.cpp : 2872 ] Variables: isG: %d, seq: %d, endflag: %d, totalLen: %d, ctl_ptr: %d, beginning actual address: %d, BDF beginning: %d 
4795,i,[ hca_HwComponentTrxPine_bdf.cpp : 2874 ] CTL 5G DATA push under process at seq %d 
4794,i,[ hca_HwComponentTrxPine_bdf.cpp : 2875 ] Size being copied in this iteration: %d 
4793,ii,[ hca_HwComponentTrxPine_bdf.cpp : 2876 ] Value at address %d before copy: %d 
4792,,[ hca_HwComponentTrxPine_bdf.cpp : 2879 ] Invalid CTL data size. Access denied to copy this fragment. Please copy CTL blob from beginning with right size. 
4791,ii,[ hca_HwComponentTrxPine_bdf.cpp : 2885 ] Value at address %d after copy: %d 
4790,i,[ hca_HwComponentTrxPine_bdf.cpp : 2886 ] Size copied: %d 
4789,,[ hca_HwComponentTrxPine_bdf.cpp : 2891 ] CTL DATA push successful. CTL parsing will be allowed. 
4788,i,[ hca_HwComponentTrxPine_bdf.cpp : 6498 ] TLMM:::: DAL_DeviceAttach TLMM: Failed due to Dal result %d
 
4787,,[ hca_HwComponentTrxPine_bdf.cpp : 6506 ] TLMM:::: Null pointer exception on gpiointConfig 
4786,i,[ hca_HwComponentTrxPine_bdf.cpp : 6512 ] TLMM:::: DalTlmm_ConfigGpio: Failed due to Dal result %d
 
4785,i,[ hca_HwComponentTrxPine_bdf.cpp : 6519 ] TLMM:::: DalTlmm_GpioOut: Failed due to Dal result %d
 
4784,iii,[ hca_HwComponentTrxPine_bdf.cpp : 5508 ] ACR : cfgCtl2G=%d, isG[2G=1,5G=0,6G=2]=%d, acrSetting=%d 
 
4783,IIIIIII,[ hca_HwComponentTrxPine_bdf.cpp : 4644 ] tpcOnepointCal:: chosen phyId %u alphaThermFreq[%u] %u curChan %u curChain %u tempIdx %u alphaThermValue %u 
4782,i,[ hca_HwComponentTrxPine_bdf.cpp : 2677 ] TPC_DBG: precaldata band %d 
4781,,[ hca_HwComponentTrxPine_bdf.cpp : 1192 ] TPC_CTL: Unable to find channel and power index for RD!!!Hence setting max power
 
4780,iiiiii,[ hca_HwComponentTrxPine_bdf.cpp : 6970 ] perPacketCMFeatureEnable rcFlag=%d ctlPwr=%d tmpPwr=%d finCtlPwr=%d numChRes=%d finChMsk=%d 
4779,iiiiiiii,[ hca_HwComponentTrxPine_bdf.cpp : 2901 ] RegModeFlags part1 %d %d %d %d %d %d %d %d 
4778,iiiiiiii,[ hca_HwComponentTrxPine_bdf.cpp : 2902 ] RegModeFlags part2 %d %d %d %d %d %d %d %d 
4777,,[ hca_HwComponentTrxPine_bdf.cpp : 2765 ] Board data address pointer is NULL !! 
4776,,[ hca_HwComponentTrxPine_bdf.cpp : 7014 ] DFS_DUMP :: radar det thresh programming 
4775,,[ hca_HwComponentTrxPine_bdf.cpp : 7083 ] DFS_DUMP :: radar det thresh programming 
4774,ii,[ hca_HwComponentTrxPine_bdf.cpp : 3274 ] phyrf_tpc_device_GetOnePointTpcOffset channel %d chosen_chanid = %d 
4773,iiii,[ hca_HwComponentTrxPine_bdf.cpp : 3296 ] tpcOnepointCal::channel:%d cmask:%d is2GHz:%d tpcPowerOffset:%d
 
4772,ii,[ hca_HwComponentTrxPine_bdf.cpp : 259 ] RTT - pri20 %d is not valid in dynamicBw %d 
4771,i,[ hca_HwComponentTrxPine_bdf.cpp : 294 ] RTT - Invalid dynamicBw %d 
4770,i,[ hca_HwComponentTrxPine_bdf.cpp : 108 ] RTT - Error: unsupported pktBw %d 
4769,,[ hca_HwComponentTrxPine_bdf.cpp : 2934 ] Board data address pointer is NULL !! 
4768,,[ hca_HwComponentTrxPine_bdf.cpp : 1446 ] CTL table under update process. CTL table will not be parsed/updated at this time. 
4767,i,[ hca_HwComponentTrxPine_bdf.cpp : 1504 ] CTL6G Value %d
 
4766,i,[ hca_HwComponentTrxPine_bdf.cpp : 169 ] RTT - Error: unsupported pktBw %d 
4765,ii,[ hca_HwComponentTrxPine_bdf.cpp : 2480 ] ProgramGIcorrGICCAThr is6Ghz:%d and is6gFCC:%d GICorr and GI CCA Thr settings 
4764,iii,[ hca_HwComponentTrxPine_bdf.cpp : 5355 ] HC: band: %d, chan %d, hcliteThr %d 
4763,IIIIIi,[ hca_HwComponentTrxPine_bdf.cpp : 4431 ] tpcOnepointCal:: chosen phyId %u calFreq[%u] %u curChan %u curChain %u onePointThermOffset %d 
4762,i,[ hca_HwComponentTrxPine_bdf.cpp : 213 ] RTT - Invalid dynamicBw %d for 2G 
4761,iI,[ hca_HwComponentTrxPine_bdf.cpp : 2510 ] wmi ccaThres programming for phyId:%d reg:0x%x  
4760,i,[ hca_HwComponentTrxPine_bdf.cpp : 194 ] RTT - Invalid dynamicBw %d for 5G 
4759,IIII,[ hca_HwComponentTrxPine_bdf.cpp : 5847 ] PhyId: %lu, Mode : %lu, Rate : %lu, Target Power: %lu 
4758,IIIIIi,[ hca_HwComponentTrxPine_bdf.cpp : 4319 ] tpcOnepointCal:: chosen phyId %u calFreq[%u] %u curChan %u curChain %u onePointTpcGLUTOffset %d 
4757,,[ hca_HwComponentTrxPine_bdf.cpp : 2974 ] Board data address pointer is NULL !! 
4756,,[ hca_HwComponentTrxPine_bdf.cpp : 3025 ] Board data address pointer is NULL !! 
4755,iIIII,[ hca_HwComponentTrxPine_bdf.cpp : 3064 ] tpcOnepointCal::Saving to BDF txPwrOffset_db8 %d for Band %u, Chain %u,Chan %u, calAttempts %u 
4754,iIIII,[ hca_HwComponentTrxPine_bdf.cpp : 3073 ] tpcOnepointCal::Saving to BDF glutOffset %d for Band %u, Chain %u,Chan %u, calAttempts %u 
4753,IIIII,[ hca_HwComponentTrxPine_bdf.cpp : 3083 ] tpcOnepointCal:: Saving to BDF thermalOffset %u for Band %u, Chain %u,Chan %u, calAttempts %u 
4752,iIIII,[ hca_HwComponentTrxPine_bdf.cpp : 3095 ] tpcOnepointCal::Saving to BDF txPwrOffset_db8 %d for Band %u, Chain %u,Chan %u, calAttempts %u 
4751,iIIII,[ hca_HwComponentTrxPine_bdf.cpp : 3104 ] tpcOnepointCal::Saving to BDF glutOffset %d for Band %u, Chain %u,Chan %u, calAttempts %u 
4750,IIIII,[ hca_HwComponentTrxPine_bdf.cpp : 3114 ] tpcOnepointCal:: Saving to BDF thermalOffset %u for Band %u, Chain %u,Chan %u, calAttempts %u 
4749,iIIII,[ hca_HwComponentTrxPine_bdf.cpp : 3128 ] tpcOnepointCal::Saving to BDF txPwrOffset_db8 %d for Band %u, Chain %u,Chan %u, calAttempts %u 
4748,iIIII,[ hca_HwComponentTrxPine_bdf.cpp : 3137 ] tpcOnepointCal::Saving to BDF glutOffset %d for Band %u, Chain %u,Chan %u, calAttempts %u 
4747,IIIII,[ hca_HwComponentTrxPine_bdf.cpp : 3147 ] tpcOnepointCal:: Saving to BDF thermalOffset %u for Band %u, Chain %u,Chan %u, calAttempts %u 
4746,i,[ hca_HwComponentTrxPine_bdf.cpp : 6985 ] Per-Packet Chainmask support is Disabled. perPacketCMFeatureEnable = %d 
4745,i,[ hca_HwComponentTrxPine_bdf.cpp : 6988 ] Per-Packet Chainmask support is Enabled. perPacketCMFeatureEnable = %d 
4744,ii,[ hca_HwComponentTrxPine_bdf.cpp : 6990 ] Per-Packet Chainmask support: perPacketCMFeatureEnable = %d, Debug Log = %d  
4743,ii,[ hca_HwComponentTrxPine_bdf.cpp : 6993 ] Per-Packet Chainmask support: perPacketCMFeatureEnable = %d, DebugLogEnabled = %d 
4742,ii,[ hca_HwComponentTrxPine_bdf.cpp : 6996 ] Per-Packet Chainmask support: perPacketCMFeatureEnable = %d, DebugLogDisabled = %d  
4826,,[ hca_HwComponentTrxPine_efuse.cpp : 290 ] HcaHwComponentTrxPine_efuse::ReadPerRfa apply_xo_param bit is enabled 
4825,ii,[ hca_HwComponentTrxPine_efuse.cpp : 295 ] HcaHwComponentTrxPine_efuse::ReadPerRfa %d, %d 
4824,iii,[ hca_HwComponentTrxPine_efuse.cpp : 331 ] HcaHwComponentTrxPine_efuse::WritePerRfa::XO cdacin %d, cdacout %d rc %d  
4823,II,[ hca_HwComponentTrxPine_efuse.cpp : 37 ] Error: buffer is out of bounds. offset = %lu, numBytes = %lu
 
4822,iII,[ hca_HwComponentTrxPine_efuse.cpp : 44 ] efuseR[%d] ->address [%lu] Value 0x%lx
 
4821,II,[ hca_HwComponentTrxPine_efuse.cpp : 58 ] Error: buffer is out of bounds. offset = %lu, numBytes = %lu
 
4820,I,[ hca_HwComponentTrxPine_efuse.cpp : 64 ] Error; numBytes not a mulpile of 4,  numBytes = %lu
 
4819,iII,[ hca_HwComponentTrxPine_efuse.cpp : 88 ] efuseW[%d] ->address [%lu] Value 0x%lx
 
4818,III,[ hca_HwComponentTrxPine_efuse.cpp : 111 ] efuseR[%lu] = 0x%lx != 0x%lx
 
4817,II,[ hca_HwComponentTrxPine_efuse.cpp : 117 ] Error: %lu/%lu bytes were not written to eFuse correctly.
 
4829,i,[ hca_HwComponentTrxPine_config.cpp : 185 ] PRDD-DFS ADFS SynthFreq - %d 
4828,,[ hca_HwComponentTrxPine_config.cpp : 259 ] Agile DFS Channel in Secondary 80 of 165 MHz 
4827,,[ hca_HwComponentTrxPine_config.cpp : 266 ] Agile Non DFS Channel in Secondary 80 of 165 MHz 
4836,I,[ hca_HwComponentTrxPine_calDb.cpp : 890 ] CALDB_DEBUG: channel list table dump 2G 20 %u 
4835,I,[ hca_HwComponentTrxPine_calDb.cpp : 894 ] CALDB_DEBUG: channel list table dump 2G 40 %u 
4834,I,[ hca_HwComponentTrxPine_calDb.cpp : 898 ] CALDB_DEBUG: channel list table dump 5G 20 %u 
4833,I,[ hca_HwComponentTrxPine_calDb.cpp : 902 ] CALDB_DEBUG: channel list table dump 5G 40 %u 
4832,I,[ hca_HwComponentTrxPine_calDb.cpp : 906 ] CALDB_DEBUG: channel list table dump 5G 80 %u 
4831,I,[ hca_HwComponentTrxPine_calDb.cpp : 910 ] CALDB_DEBUG: channel list table dump 5G 160 %u 
4830,i,[ hca_HwComponentTrxPine_calDb.cpp : 914 ] CALDB_DEBUG: groupMapping[i][1]=%d  
4850,ii,[ hca_HwComponentTrxPine_paprd.cpp : 669 ] PAPRD HcaHwComponentTrxPine_paprd::FtmControl : channel %d dpd_enable %d 
4849,iii,[ hca_HwComponentTrxPine_paprd.cpp : 694 ] PAPRD ResetParams phyExtn = %d phyId %d enable %d 
4848,i,[ hca_HwComponentTrxPine_paprd.cpp : 784 ] PAPRD: Unknown PHY Id %d 
4847,I,[ hca_HwComponentTrxPine_paprd.cpp : 83 ] PAPRD: Debugflag entered %x 
4846,iii,[ hca_HwComponentTrxPine_paprd.cpp : 656 ] PAPRD SetPaprdEnable : enable %d paprdEnable2G %d paprdEnable5G %d 
4845,iiiiii,[ hca_HwComponentTrxPine_paprd.cpp : 739 ] PAPRD: GetDPDChannelRange PHY ID %d isG %d start %d end %d chan start %d chan end %d 
4844,iiII,[ hca_HwComponentTrxPine_paprd.cpp : 319 ] PAPRD PDL secondary %d cur cal Temperature %d phyInput->txChMask 0x%x tx mask 0x%x 
4843,ii,[ hca_HwComponentTrxPine_paprd.cpp : 153 ] PAPRDTUNING: SETTING - LoopBack Attn | Glut %d Value %d 
4842,ii,[ hca_HwComponentTrxPine_paprd.cpp : 158 ] PAPRDTUNING: SETTING - Timing Delay | Glut %d Value %d 
4841,iiii,[ hca_HwComponentTrxPine_paprd.cpp : 560 ] PAPRDTUNING: Channel %d chainIdx %d glutIdx %d gainIdx %d
 
4840,iiii,[ hca_HwComponentTrxPine_paprd.cpp : 562 ] PAPRDTUNING: Channel %d chainIdx %d glutIdx %d gainIdx %d
 
4839,i,[ hca_HwComponentTrxPine_paprd.cpp : 386 ] PAPRD: XmitTrainingFrame failed. Status %d 
 
4838,iIi,[ hca_HwComponentTrxPine_paprd.cpp : 388 ] PAPRD: XmitTrainingFrame tx_count %d, tx_ctxt_flags 0x%x cal type %d 
4837,Ii,[ hca_HwComponentTrxPine_paprd.cpp : 47 ] PAPRD:HcaHwComponentTrxPine_paprd::HwDisable all : PhyBase %8x channel %d 
4857,iiIII,[ hca_HwComponentTrxPine_calSmBwFilter.cpp : 78 ] phyInput->homeCh %d 
				 phyInput->bandCode %d 
				 phyInput->phyBase 0x%x 
				 phyInput->txChMask 0x%x 
				 phyInput->rxChMask 0x%x 
 
4856,i,[ hca_HwComponentTrxPine_calSmBwFilter.cpp : 79 ] phyInput->bwCode %d 
 
4855,i,[ hca_HwComponentTrxPine_calSmBwFilter.cpp : 80 ] ACR : rx_bbf_cal_input->acrSetting %d 
 
4854,i,[ hca_HwComponentTrxPine_calSmBwFilter.cpp : 128 ]  TxBBF and RxBBF cals loadIniMask %d 
4853,i,[ hca_HwComponentTrxPine_calSmBwFilter.cpp : 131 ]  Skipping TxBBF and RxBBF cals. Reason: No BW/Band change loadIniMask %d 
4852,i,[ hca_HwComponentTrxPine_calSmBwFilter.cpp : 145 ]  TxBBF cal completed result=%d
 
4851,i,[ hca_HwComponentTrxPine_calSmBwFilter.cpp : 155 ]  RxBBF cal completed result=%d
 
4862,ii,[ hca_HwComponentTrxPine_calSmDpdMemoryLess.cpp : 95 ] DPD Cal State m/c ::: new_channel_change_request(%d) on channel %d 
4861,,[ hca_HwComponentTrxPine_calSmDpdMemoryLess.cpp : 126 ] PAPRD: DPD disabled for this range of frequency 
4860,Iiiiiii,[ hca_HwComponentTrxPine_calSmDpdMemoryLess.cpp : 151 ] Run DPD Calibration ::: pHdl=%x, phyMode=%d, phyID=%d, channel %d, bwCode %d, txCM=%d, rxCM=%d  
4859,iiii,[ hca_HwComponentTrxPine_calSmDpdMemoryLess.cpp : 155 ] DPD Cal State m/c ::: Channel %d= State %d, DPD Queue %d, tx pkt cnt %d 
4858,,[ hca_HwComponentTrxPine_calSmDpdMemoryLess.cpp : 162 ] PAPRD: DPD not triggered. 
 
4976,iI,[ hca_HwComponentTrxPine_calSmComb.cpp : 970 ] combCal_SM_save: RXIQ: chainIdx=%d,  pStartRxIq=%x 
4975,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1018 ] cannot update RxIq table in caldb for chainIdx = %d! 
4974,iI,[ hca_HwComponentTrxPine_calSmComb.cpp : 1068 ] combCal_SM_save: TXIQ: chainIdx=%d,  pStartTxIq=%x 
4973,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1088 ] cannot update TxIq table in caldb for chainIdx = %d! 
4972,iIi,[ hca_HwComponentTrxPine_calSmComb.cpp : 1132 ] combCal_SM_save: TXLO: chainIdx=%d,  pStartTxLo=%x, 4 * NUM_GAINS_PER_MODE_DIG_ANA_CL=%d 
4971,Iii,[ hca_HwComponentTrxPine_calSmComb.cpp : 1141 ] #### SAVE rxChainMask=%x, maxChain=%d, fdmtCombCalInput->chainIdx = %d 
4970,ii,[ hca_HwComponentTrxPine_calSmComb.cpp : 1142 ] #### SAVE fdmtCombCalInput->combCalType = %d (COMB_CAL_TYPE_CL=%d) 
4969,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1143 ] #### SAVE fdmtCombCalInput->calCmdId=%d 
4968,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1144 ] #### ADDR SAVE:pStartTxLo=%x 
4967,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1205 ] cannot update txlo table in caldb for chainIdx = %d! 
4966,,[ hca_HwComponentTrxPine_calSmComb.cpp : 286 ] APPLICALBE_RESUBMISSION_ONLY:: failure on not getting pStart (= NULL) from caldb! 
4965,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1617 ] CAL_COMMON_PARAM pHandle 	=%x 
4964,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1618 ] CAL_COMMON_PARAM calType 	=%d 
4963,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1619 ] CAL_COMMON_PARAM cmdGroupId 	=%d 
4962,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1620 ] CAL_COMMON_PARAM isRestoreOnly 	=%d 
4961,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1621 ] CAL_COMMON_PARAM calTypeVarianceId 	=%d 
4960,iii,[ hca_HwComponentTrxPine_calSmComb.cpp : 1622 ] CAL_COMMON_PARAM reserved 	=%d %d %d 
4959,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1623 ] CAL_COMMON_PARAM (pIn->pHandle).phyId 	=%x 
4958,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1624 ] CAL_COMMON_PARAM halphyBW 	=%x 
4957,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1625 ] PHYDEVLIB_PHY_INPUT phyId 		=%d 
4956,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1626 ] PHYDEVLIB_PHY_INPUT bandCode	=%d 
4955,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1627 ] PHYDEVLIB_PHY_INPUT bwCode 	=%d 
4954,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1628 ] PHYDEVLIB_PHY_INPUT phyMode 	=%d 
4953,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1629 ] PHYDEVLIB_PHY_INPUT band_center_freq1 	=%d 
4952,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1630 ] PHYDEVLIB_PHY_INPUT band_center_freq2 	=%d 
4951,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1631 ] PHYDEVLIB_PHY_INPUT txChMask 	=%x 
4950,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1632 ] PHYDEVLIB_PHY_INPUT rxChMask 	=%x 
4949,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1633 ] PHYDEVLIB_PHY_INPUT phyBase 	=%x 
4948,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1634 ] PHYDEVLIB_PHY_INPUT phyBaseExt 	=%x 
4947,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1635 ] PHYDEVLIB_PHY_INPUT concMode 	=%d 
4946,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1636 ] PHYDEVLIB_PHY_INPUT dynPriChan 	=%d 
4945,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1637 ] PHYDEVLIB_PHY_INPUT homeCh		=%d 
4944,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1638 ] PHYDEVLIB_PHY_INPUT dtim 		=%d 
4943,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1639 ] PHYDEVLIB_PHY_INPUT extLNA 		=%d 
4942,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1640 ] PHYDEVLIB_PHY_INPUT extPA 		=%d 
4941,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1641 ] PHYDEVLIB_PHY_INPUT phyrf_init_GetPhyRfMode 		=%x 
4940,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1642 ] PHYDEVLIB_PHY_INPUT isSBSmode 	=%d 
4939,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1643 ] PHYDEVLIB_PHY_INPUT loType 		=%d 
4938,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1644 ] PHYDEVLIB_PHY_INPUT dpdMode 	=%d 
4937,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1645 ] PHYDEVLIB_PHY_INPUT loadIniMask 	=%d 
4936,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1646 ] PHYDEVLIB_PHY_INPUT calMask 	=%d 
4935,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1647 ] PHYDEVLIB_PHY_INPUT cal_mode_ctrl 	=%d 
4934,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1649 ] CCAL_INPUT calCmdId		=%d 
4933,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1650 ] CCAL_INPUT cal_chain_mask		=%x 
4932,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1651 ] CCAL_INPUT cal_mode		=%d 
4931,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1652 ] CCAL_INPUT mode (80p80 mode)		=%d 
4930,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1653 ] CCAL_INPUT fixed_gain		=%d 
4929,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1654 ] CCAL_INPUT engineSharing		=%d 
4928,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1655 ] CCAL_INPUT driveTxGLUTIdx		=%d 
4927,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1656 ] CCAL_INPUT enableBlockAccAvg		=%d 
4926,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1657 ] CCAL_INPUT blockSize		=%d 
4925,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1658 ] CCAL_INPUT dcEstWindowSize		=%d 
4924,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1659 ] CCAL_INPUT numOfBlocks		=%d 
4923,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1660 ] CCAL_INPUT numSamplesToReadback[0]	=%d 
4922,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1661 ] CCAL_INPUT numSamplesToReadback[1]	=%d 
4921,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1662 ] CCAL_INPUT numSamplesToReadback[2]	=%d 
4920,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1663 ] CCAL_INPUT rxGainSettlingTime		=%d 
4919,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1664 ] CCAL_INPUT txGainSettlingTime		=%d 
4918,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1665 ] CCAL_INPUT txShiftSettlingTime		=%d 
4917,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1666 ] CCAL_INPUT calModeSettlingTime	=%d 
4916,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1667 ] CCAL_INPUT loopbackSettlingTime	=%d 
4915,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1668 ] CCAL_INPUT txResidueSettlingTime	=%d 
4914,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1669 ] CCAL_INPUT numTaps[0] 		=%d 
4913,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1670 ] CCAL_INPUT numTaps[1] 		=%d 
4912,iI,[ hca_HwComponentTrxPine_calSmComb.cpp : 677 ] combCal_SM_restore: RXIQ: chainIdx=%d,  pStartRxIq=%x 
4911,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 721 ] cannot update RxIq table in caldb for chainIdx = %d! 
4910,iI,[ hca_HwComponentTrxPine_calSmComb.cpp : 800 ] combCal_SM_restore: TXIQ: chainIdx=%d,  pStartTxIq=%x 
4909,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 814 ] cannot update TxIq table in caldb for chainIdx = %d! 
4908,iI,[ hca_HwComponentTrxPine_calSmComb.cpp : 866 ] combCal_SM_restore: TXLO: chainIdx=%d,  pStartTxLo=%x 
4907,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 885 ] cannot update txlo table in caldb for chainIdx = %d! 
4906,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1311 ] MODE2CALID in  *calMode		=%d 
4905,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1312 ] MODE2CALID in  *calId		=%d 
4904,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1313 ] MODE2CALID in  retValue		=%d 
4903,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1371 ] OVERRIDE FINALCASE pHandle 		=%x 
4902,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1372 ] OVERRIDE FINALCASE callingContext 	=%d 
4901,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1373 ] OVERRIDE FINALCASE calId 		=%d 
4900,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1374 ] OVERRIDE FINALCASE in finalCase 	=%d 
4899,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1390 ] OVERRIDE FINALCASE out finalCase 	=%d 
4898,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1470 ] FC_HANDLE  pHandle 		=%x 
4897,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1471 ] FC_HANDLE  phyInput 		=%x 
4896,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1472 ] FC_HANDLE  fdmtCombCalInput 	=%x 
4895,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1473 ] FC_HANDLE  fdmtCombCalOutput 	=%x 
4894,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1474 ] FC_HANDLE  finalCase 		=%d 
4893,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1475 ] FC_HANDLE  rfChainMask 		=%x 
4892,,[ hca_HwComponentTrxPine_calSmComb.cpp : 1551 ] #### reset current associated table only 
4891,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1562 ] path to call docal due to NEED_TO_DO_CAL,  calCmdId 		=%d 
4890,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1398 ] ITER2CMDIDX  iterIdx 		=%d 
4889,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1423 ] ITER2CMDIDX  cmdIdx 		=%d 
4888,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1435 ] UPDATE_COMBC_TRACKING  pHandle 	=%x 
4887,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1436 ] UPDATE_COMBC_TRACKING  calMode 	=%d 
4886,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1437 ] UPDATE_COMBC_TRACKING  rfChainMask 	=%x 
4885,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1438 ] UPDATE_COMBC_TRACKING  subMode80p80 	=%d 
4884,,[ hca_HwComponentTrxPine_calSmComb.cpp : 1443 ] UPDATE_COMBC_TRACKING  		COMB_TXLO_TXIQ_RXIQ 
4883,,[ hca_HwComponentTrxPine_calSmComb.cpp : 1448 ] UPDATE_COMBC_TRACKING  		COMB_CAL_MODE_DPD_LP_RXIQ 
4882,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1225 ] COMPOSE CMBIQ INPUT pIn 		=%x 
4881,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1226 ] COMPOSE CMBIQ INPUT phyInput 	=%x 
4880,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1227 ] COMPOSE CMBIQ INPUT rxdcoInput 	=%x 
4879,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1228 ] COMPOSE CMBIQ INPUT in *calId 	=%x 
4878,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1287 ] COMPOSE CMBIQ INPUT out *calId 	=%x 
4877,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1329 ] FINALCASE pHandle 		=%x 
4876,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1330 ] FINALCASE callingContext 		=%d 
4875,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1331 ] FINALCASE calMode 		=%x 
4874,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1332 ] FINALCASE calId 			=%d 
4873,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1333 ] FINALCASE rfChainMask 		=%x 
4872,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1334 ] FINALCASE in finalCase		=%x 
4871,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1335 ] FINALCASE statusChainMask 		=%x 
4870,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1336 ] FINALCASE subMode80p80 		=%x 
4869,I,[ hca_HwComponentTrxPine_calSmComb.cpp : 1359 ] FINALCASE out finalCase		=%x 
4868,,[ hca_HwComponentTrxPine_calSmComb.cpp : 1730 ] skipping comb I and Q on DFS channel in cold boot time 
4867,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1821 ] CalSM: scan cal end 	phyId=%d 
4866,i,[ hca_HwComponentTrxPine_calSmComb.cpp : 1857 ] CalSM: cal end 	phyId=%d 
4865,,[ hca_HwComponentTrxPine_calSmComb.cpp : 1866 ] :::: phyrf_turn_on is called 
4864,,[ hca_HwComponentTrxPine_calSmComb.cpp : 1868 ] :::: phyrf_turn_off is called 
4863,,[ hca_HwComponentTrxPine_calSmComb.cpp : 1680 ] Welcome, cal SM for Comb Cal will be created..
 
4984,,[ hca_HwComponentTrxPine_calSmDac.cpp : 161 ] DACCAL_SM ::: SKIP for Scan Radio  
4983,I,[ hca_HwComponentTrxPine_calSmDac.cpp : 165 ] DACCAL_SM ::: START resetCause: %x 
4982,i,[ hca_HwComponentTrxPine_calSmDac.cpp : 192 ] DACCAL_SM: RECIPE : %d 
4981,iiI,[ hca_HwComponentTrxPine_calSmDac.cpp : 205 ] DACCAL_SM: save invoked on chainIdx = %d bandcode= %d pDACData:0x%x 
4980,iiI,[ hca_HwComponentTrxPine_calSmDac.cpp : 227 ] DACCAL_SM: restore invoked cal on chainIdx = %d bandcode=%d pDACData:0x%x 
4979,,[ hca_HwComponentTrxPine_calSmDac.cpp : 241 ] CalSM: DAC cal end 
4978,,[ hca_HwComponentTrxPine_calSmDac.cpp : 249 ] :::: phyrf_turn_on is called 
4977,,[ hca_HwComponentTrxPine_calSmDac.cpp : 251 ] :::: phyrf_turn_off is called 
4985,,[ hca_HwComponentTrxPine_calSmPadroop.cpp : 31 ] Welcome, cal SM for Dadroop Cal will be created..
 
4989,,[ hca_HwComponentTrxPine_calSmIbf.cpp : 115 ] HcaHwComponentTrxPine_calSmIbf enter
 
4988,,[ hca_HwComponentTrxPine_calSmIbf.cpp : 137 ] :::: phyrf_turn_on is called 
4987,,[ hca_HwComponentTrxPine_calSmIbf.cpp : 139 ] :::: phyrf_turn_off is called 
4986,,[ hca_HwComponentTrxPine_calSmIbf.cpp : 34 ] Welcome, cal SM for IBF will be created..
 
5011,,[ hca_HwComponentTrxPine_calSmPdet.cpp : 427 ] PALCAL STARTED 
5010,i,[ hca_HwComponentTrxPine_calSmPdet.cpp : 438 ] PALCAL CONF final pal_cal_input->pcalMethod=%d 
5009,,[ hca_HwComponentTrxPine_calSmPdet.cpp : 439 ] PALCAL COMPLETED 
5008,,[ hca_HwComponentTrxPine_calSmPdet.cpp : 446 ] :::: phyrf_turn_on is called 
5007,,[ hca_HwComponentTrxPine_calSmPdet.cpp : 448 ] :::: phyrf_turn_off is called 
5006,i,[ hca_HwComponentTrxPine_calSmPdet.cpp : 212 ] PALCAL_INPUT calCmdId			=%d 
5005,I,[ hca_HwComponentTrxPine_calSmPdet.cpp : 213 ] PALCAL_INPUT pPalDlyVals			=%x 
5004,i,[ hca_HwComponentTrxPine_calSmPdet.cpp : 214 ] PALCAL_INPUT pcalMethod			=%d 
5003,i,[ hca_HwComponentTrxPine_calSmPdet.cpp : 215 ] PALCAL_INPUT pcalOptDoSetEDandDM		=%d 
5002,iii,[ hca_HwComponentTrxPine_calSmPdet.cpp : 218 ] PALCAL CONF ModeStatus[phyId=%d][ConfMode=%d][0]	=%d 
5001,iii,[ hca_HwComponentTrxPine_calSmPdet.cpp : 219 ] PALCAL CONF ModeStatus[phyId=%d][ConfMode=%d][1]	=%d 
5000,iii,[ hca_HwComponentTrxPine_calSmPdet.cpp : 220 ] PALCAL CONF ModeStatus[phyId=%d][ConfMode=%d][2]	=%d 
4999,iii,[ hca_HwComponentTrxPine_calSmPdet.cpp : 221 ] PALCAL STORE palCalDlyVals[phyId=%d][%d][0]		=%d 
4998,iii,[ hca_HwComponentTrxPine_calSmPdet.cpp : 222 ] PALCAL STORE palCalDlyVals[phyId=%d]{%d][1]		=%d 
4997,iii,[ hca_HwComponentTrxPine_calSmPdet.cpp : 223 ] PALCAL STORE palCalDlyVals[phyId=%d][%d][2]		=%d 
4996,iii,[ hca_HwComponentTrxPine_calSmPdet.cpp : 224 ] PALCAL STORE palCalDlyVals[phyId=%d][%d][3]		=%d 
4995,iii,[ hca_HwComponentTrxPine_calSmPdet.cpp : 225 ] PALCAL STORE palCalDlyVals[phyId=%d][%d][4]		=%d 
4994,iii,[ hca_HwComponentTrxPine_calSmPdet.cpp : 226 ] PALCAL STORE palCalDlyVals[phyId=%d][%d][5]		=%d 
4993,,[ hca_HwComponentTrxPine_calSmPdet.cpp : 493 ] PAL cal is disabled by BDF cal mask flag 
4992,,[ hca_HwComponentTrxPine_calSmPdet.cpp : 498 ] PAL cal is disabled for HW SBS specific board for now 
4991,,[ hca_HwComponentTrxPine_calSmPdet.cpp : 504 ] PAL cal Option control parameter is not equal to desired PAL CAL OPTION, PAL is skipped 
4990,,[ hca_HwComponentTrxPine_calSmPdet.cpp : 347 ] Welcome, cal SM for Pdet Cal will be created 
5113,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 345 ] CAL_COMMON_PARAM pHandle 	=%x 
5112,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 346 ] CAL_COMMON_PARAM calType 	=%d 
5111,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 347 ] CAL_COMMON_PARAM cmdGroupId 	=%d 
5110,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 348 ] CAL_COMMON_PARAM isRestoreOnly 	=%d 
5109,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 349 ] CAL_COMMON_PARAM calTypeVarianceId 	=%d 
5108,iii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 350 ] CAL_COMMON_PARAM reserved 	=%d %d %d 
5107,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 351 ] CAL_COMMON_PARAM (pIn->pHandle).phyId 	=%x 
5106,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 352 ] CAL_COMMON_PARAM halphyBW 	=%x 
5105,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 353 ] PHYDEVLIB_PHY_INPUT phyId 		=%d 
5104,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 354 ] PHYDEVLIB_PHY_INPUT bandCode	=%d 
5103,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 355 ] PHYDEVLIB_PHY_INPUT bwCode 	=%d 
5102,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 356 ] PHYDEVLIB_PHY_INPUT phyMode 	=%d 
5101,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 357 ] PHYDEVLIB_PHY_INPUT band_center_freq1 	=%d 
5100,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 358 ] PHYDEVLIB_PHY_INPUT band_center_freq2 	=%d 
5099,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 359 ] PHYDEVLIB_PHY_INPUT txChMask 	=%x 
5098,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 360 ] PHYDEVLIB_PHY_INPUT rxChMask 	=%x 
5097,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 361 ] PHYDEVLIB_PHY_INPUT phyBase 	=%x 
5096,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 362 ] PHYDEVLIB_PHY_INPUT phyBaseExt 	=%x 
5095,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 363 ] PHYDEVLIB_PHY_INPUT concMode 	=%d 
5094,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 364 ] PHYDEVLIB_PHY_INPUT dynPriChan 	=%d 
5093,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 365 ] PHYDEVLIB_PHY_INPUT homeCh		=%d 
5092,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 366 ] PHYDEVLIB_PHY_INPUT dtim 		=%d 
5091,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 367 ] PHYDEVLIB_PHY_INPUT extLNA 		=%d 
5090,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 368 ] PHYDEVLIB_PHY_INPUT extPA 		=%d 
5089,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 369 ] PHYDEVLIB_PHY_INPUT phyrf_init_GetPhyRfMode 		=%x 
5088,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 370 ] PHYDEVLIB_PHY_INPUT isSBSmode 	=%d 
5087,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 371 ] PHYDEVLIB_PHY_INPUT loType 		=%d 
5086,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 372 ] PHYDEVLIB_PHY_INPUT dpdMode 	=%d 
5085,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 373 ] PHYDEVLIB_PHY_INPUT loadIniMask 	=%d 
5084,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 374 ] PHYDEVLIB_PHY_INPUT calMask 	=%x 
5083,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 375 ] PHYDEVLIB_PHY_INPUT cal_mode_ctrl 	=%d 
5082,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 376 ] PHYDEVLIB_PHY_INPUT boardId 	=%d 
5081,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 377 ] PHYDEVLIB_PHY_INPUT phySscanEnMask 	=0x%x 
5080,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 378 ] PHYDEVLIB_PHY_INPUT phyDfsEnMask 	=0x%x 
5079,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 696 ] ITER2CMDIDX  iterIdx 		=%d 
5078,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 722 ] ITER2CMDIDX  cmdIdx 		=%d 
5077,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 269 ] MODE2CALID in  *calMode		=%d 
5076,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 270 ] MODE2CALID in  *calId		=%d 
5075,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 271 ] MODE2CALID in  retValue		=%d 
5074,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 491 ] FC_HANDLE  pHandle 		=%x 
5073,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 492 ] FC_HANDLE  phyInput 		=%x 
5072,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 493 ] FC_HANDLE  rxdcoInput 		=%x 
5071,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 495 ] FC_HANDLE  finalCase 		=%d 
5070,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 496 ] FC_HANDLE  rfChainMask 		=%x 
5069,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 497 ] FC_HANDLE  subMode80p80 		=%d 
5068,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 536 ] RXDCO ****** invokes rxdco RESTORE ***** 
5067,iii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 594 ] RXDCO ::: BF CAL_RESTORE bwCode=%d, chainIdx=%d homech=%d 
5066,ii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 597 ] RXDCO restore ::: pDcoLut chain 0: img:%d real:%d  
5065,ii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 600 ] RXDCO restore ::: pDcoLut chain 1: img:%d real:%d  
5064,ii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 603 ] RXDCO restore ::: pDcoLut chain 2: img:%d real:%d  
5063,ii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 607 ] RXDCO restore ::: pDcoLut chain 3: img:%d real:%d  
5062,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 629 ] FC_HANDLE  autoIterativeIdx 		=%d 
5061,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 630 ] FC_HANDLE  rxdcoInput->calCmdId 	=%d 
5060,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 631 ] FC_HANDLE  iterIdx 		=%d 
5059,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 632 ] RXDCO ****** invokes rxdco cal ***** 
5058,ii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 636 ] RXDCO ::: recipe : %d  , cal_mode : %d  
5057,iii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 651 ] RXDCO ::: BF CAL_SAVE bwCode=%d, chainIdx=%d homeCh=%d 
5056,ii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 654 ] RXDCO save ::: pDcoLut chain 0: img:%d real:%d  
5055,ii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 657 ] RXDCO save ::: pDcoLut chain 1: img:%d real:%d  
5054,ii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 660 ] RXDCO save ::: pDcoLut chain 2: img:%d real:%d  
5053,iii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 664 ] RXDCO save ::: pDcoLut chain 3: img:%d real:%d range:%d 
5052,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 669 ] RXDCO ::: AFTER:CAL_SAVE convertNewRxdcoLutfromCalDb failed
 
5051,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 467 ] OVERRIDE FINALCASE out finalCase 	=%d 
5050,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 732 ] UPDATE_RXDCO_TRACKING  pHandle 	=%x 
5049,iii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 733 ] UPDATE_RXDCO_TRACKING  calMode 	=%d (RXDCO_CAL_MODE_NORMAL=%d,RXDCO_CAL_MODE_DTIM=%d 
5048,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 734 ] UPDATE_RXDCO_TRACKING  rfChainMask 	=%x 
5047,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 735 ] UPDATE_RXDCO_TRACKING  subMode80p80 	=%d 
5046,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 740 ] UPDATE_RXDCO_TRACKING  	RXDCO_CAL_MODE_NORMAL 
5045,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 745 ] UPDATE_RXDCO_TRACKING  	RXDCO_CAL_MODE_NORMAL 
5044,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 291 ] COMPOSE RXDCO INPUT pIn 		=%x 
5043,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 292 ] COMPOSE RXDCO INPUT phyInput 	=%x 
5042,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 293 ] COMPOSE RXDCO INPUT rxdcoInput 	=%x 
5041,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 294 ] COMPOSE RXDCO INPUT pUnionDcoLut 	=%x 
5040,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 295 ] COMPOSE RXDCO INPUT in *calId 	=%x 
5039,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 313 ] COMPOSE RXDCO INPUT override bwCode 	=%x 
5038,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 337 ] COMPOSE RXDCO INPUT out *calId 	=%x 
5037,iI,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 803 ] RXDCO ::: save TablePtr chain:%d = %p 
5036,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 828 ] NEED_TO_DO_CAL:: cannot update rxdco caldb for chainIdx = %d! 
5035,iI,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 762 ] RXDCO ::: restore TablePtr chain:%d = %p 
5034,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 783 ] APPLICALBE_RESUBMISSION_ONLY:: failure on not getting pStart (= NULL) from caldb! 
5033,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 394 ] FINALCASE pHandle 		=%x 
5032,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 395 ] FINALCASE callingContext 		=%d 
5031,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 396 ] FINALCASE calMode 		=%x 
5030,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 397 ] FINALCASE calId 			=%d 
5029,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 398 ] FINALCASE rfChainMask 		=%x 
5028,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 399 ] FINALCASE in finalCase		=%x 
5027,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 400 ] FINALCASE statusChainMask 		=%x 
5026,I,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 401 ] FINALCASE subMode80p80 		=%x 
5025,Ii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 434 ] FINALCASE out finalCase 		=%x for calMode=%d 
5024,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 897 ] RXDCO SM COLDBOOT SUPPORT VERSION ************** 
5023,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 910 ] RXDCO SM FINAL VERSION bandw=%d>>>>>>>>>>>>>>>>>> 
5022,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 929 ] RXDCO callingContext = %d --> AFS_CAL_PROFILE 
5021,iiii,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 959 ] RXDCO SM::bwCode=%d, bandCode=%d, calCmdId=%d, cal_mode=%d 
5020,IiiiI,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 960 ] RXDCO SM::rxChainMask=%x, homech=%d, phyMode=%d, dtim=%d boardId=0x%x 
5019,iiIi,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 965 ] RXDCO SM SKIPPED:::finalCase = %d, doCalFlag = %d,  skipMask = %x, previousCalResultAtHomeCh=%d 
5018,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 970 ] RXDCO SM::FCS mode, so for home channel noCal 
5017,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 972 ] RXDCO SM::FCS calflag is wrong, should be doCal 
5016,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 996 ] RXDCO SM FINALCASE BASED 
5015,i,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 1001 ] RXDCO callingContext = %d  restore doCalFlag--> AFS_CAL_PROFILE 
5014,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 1011 ] :::: phyrf_turn_on is called 
5013,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 1013 ] :::: phyrf_turn_off is called 
5012,,[ hca_HwComponentTrxPine_calSmRxDco.cpp : 1016 ] RXDCO SM FINAL VERSION <<<<<<<<<<<<<<<<<< 
