From patchwork Thu May 28 06:16:45 2020
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
X-Patchwork-Submitter: Chuanjia Liu <chuanjia.liu@mediatek.com>
X-Patchwork-Id: 11574793
Return-Path: 
 <SRS0=ftSA=7K=lists.infradead.org=linux-mediatek-bounces+patchwork-linux-mediatek=patchwork.kernel.org@kernel.org>
Received: from mail.kernel.org (pdx-korg-mail-1.web.codeaurora.org
 [172.30.200.123])
	by pdx-korg-patchwork-2.web.codeaurora.org (Postfix) with ESMTP id 391201392
	for <patchwork-linux-mediatek@patchwork.kernel.org>;
 Thu, 28 May 2020 06:20:27 +0000 (UTC)
Received: from bombadil.infradead.org (bombadil.infradead.org
 [198.137.202.133])
	(using TLSv1.2 with cipher ECDHE-RSA-AES256-GCM-SHA384 (256/256 bits))
	(No client certificate requested)
	by mail.kernel.org (Postfix) with ESMTPS id 104F620657
	for <patchwork-linux-mediatek@patchwork.kernel.org>;
 Thu, 28 May 2020 06:20:27 +0000 (UTC)
Authentication-Results: mail.kernel.org;
	dkim=pass (2048-bit key) header.d=lists.infradead.org
 header.i=@lists.infradead.org header.b="raZHaWxs";
	dkim=fail reason="signature verification failed" (1024-bit key)
 header.d=mediatek.com header.i=@mediatek.com header.b="YztrByG/"
DMARC-Filter: OpenDMARC Filter v1.3.2 mail.kernel.org 104F620657
Authentication-Results: mail.kernel.org;
 dmarc=fail (p=none dis=none) header.from=mediatek.com
Authentication-Results: mail.kernel.org;
 spf=none
 smtp.mailfrom=linux-mediatek-bounces+patchwork-linux-mediatek=patchwork.kernel.org@lists.infradead.org
DKIM-Signature: v=1; a=rsa-sha256; q=dns/txt; c=relaxed/relaxed;
	d=lists.infradead.org; s=bombadil.20170209; h=Sender:
	Content-Transfer-Encoding:Content-Type:Cc:List-Subscribe:List-Help:List-Post:
	List-Archive:List-Unsubscribe:List-Id:MIME-Version:References:In-Reply-To:
	Message-ID:Date:Subject:To:From:Reply-To:Content-ID:Content-Description:
	Resent-Date:Resent-From:Resent-Sender:Resent-To:Resent-Cc:Resent-Message-ID:
	List-Owner; bh=aVtKU+Ey8KEM97+S66fz9ZMo+H8BP570jhAAvaRsNWc=; b=raZHaWxsfCxsrd
	Byn/w1oLN/J82ApnNdBBXixq9Qj0uXIU2tBVqkiQ9lG6QDk7uguxQSJLeTqrsI/uxQmCI/PGQtZdP
	sH0oboi2sbQSqJ/1ud4uL2pPaiLRJCxINF5oWjoZMsjn/b2fWvn52P6vTr/dxDTaabiVhY0HL0J+X
	7YGc1aYtO76HZHE2ke3puR42QkI8hE9E2cEhiLWeuUiLdUBegNM5MdYftu4nJTcCXnAeJjp/wIpYG
	7X737N9cmanDf6Bxr2bNPgaYzH+m7JK6eGxuAvWo0+PE9OX7MLrXY3KjixcjD/b0he0mfEM++gBAq
	KBYKl5wh1mnlR2WIWXew==;
Received: from localhost ([127.0.0.1] helo=bombadil.infradead.org)
	by bombadil.infradead.org with esmtp (Exim 4.92.3 #3 (Red Hat Linux))
	id 1jeBtx-0005JC-DJ; Thu, 28 May 2020 06:20:25 +0000
Received: from mailgw01.mediatek.com ([216.200.240.184])
 by bombadil.infradead.org with esmtps (Exim 4.92.3 #3 (Red Hat Linux))
 id 1jeBtW-0002f2-75; Thu, 28 May 2020 06:20:01 +0000
X-UUID: d5cb6d96c2a5421796c2f8a284ff3670-20200527
DKIM-Signature: v=1; a=rsa-sha256; q=dns/txt; c=relaxed/relaxed;
 d=mediatek.com;
 s=dk;
 h=Content-Transfer-Encoding:Content-Type:MIME-Version:References:In-Reply-To:Message-ID:Date:Subject:CC:To:From;
 bh=EqjC+5cHgv6eykN7FPf2mtwK9UivJ3XSCE0jEvb8h+8=;
 b=YztrByG/Ia304l9KDPBwoHFYkFCN6qBXPqwZgg56CA9VitadAg2+K1VgfEU+oHqsqcsGAMdZTRMQh17tpm4bJParw6MMzAQ28te2TcxvQMV8PZMkerJdZyyYblI7ybauPWuofAQgQMtuwSKVii8eTRJbf99OZ9vDGJP3zo2j1wU=;
X-UUID: d5cb6d96c2a5421796c2f8a284ff3670-20200527
Received: from mtkcas66.mediatek.inc [(172.29.193.44)] by
 mailgw01.mediatek.com
 (envelope-from <chuanjia.liu@mediatek.com>)
 (musrelay.mediatek.com ESMTP with TLS)
 with ESMTP id 681958707; Wed, 27 May 2020 22:20:16 -0800
Received: from MTKMBS07N2.mediatek.inc (172.21.101.141) by
 MTKMBS62N1.mediatek.inc (172.29.193.41) with Microsoft SMTP Server (TLS) id
 15.0.1497.2; Wed, 27 May 2020 23:18:52 -0700
Received: from mtkcas07.mediatek.inc (172.21.101.84) by
 mtkmbs07n2.mediatek.inc (172.21.101.141) with Microsoft SMTP Server (TLS) id
 15.0.1497.2; Thu, 28 May 2020 14:18:49 +0800
Received: from localhost.localdomain (10.17.3.153) by mtkcas07.mediatek.inc
 (172.21.101.73) with Microsoft SMTP Server id 15.0.1497.2 via Frontend
 Transport; Thu, 28 May 2020 14:18:47 +0800
From: <chuanjia.liu@mediatek.com>
To: <robh+dt@kernel.org>, <ryder.lee@mediatek.com>, <matthias.bgg@gmail.com>
Subject: [PATCH v2 1/4] dt-bindings: PCI: Mediatek: Update PCIe binding
Date: Thu, 28 May 2020 14:16:45 +0800
Message-ID: <20200528061648.32078-2-chuanjia.liu@mediatek.com>
X-Mailer: git-send-email 2.18.0
In-Reply-To: <20200528061648.32078-1-chuanjia.liu@mediatek.com>
References: <20200528061648.32078-1-chuanjia.liu@mediatek.com>
MIME-Version: 1.0
X-MTK: N
X-CRM114-Version: 20100106-BlameMichelson ( TRE 0.8.0 (BSD) ) MR-646709E3 
X-CRM114-CacheID: sfid-20200527_231958_261064_608CC03E 
X-CRM114-Status: GOOD (  13.95  )
X-Spam-Score: -0.2 (/)
X-Spam-Report: SpamAssassin version 3.4.4 on bombadil.infradead.org summary:
 Content analysis details:   (-0.2 points)
 pts rule name              description
 ---- ----------------------
 --------------------------------------------------
 -0.0 SPF_PASS               SPF: sender matches SPF record
 0.0 SPF_HELO_NONE          SPF: HELO does not publish an SPF Record
 0.0 MIME_BASE64_TEXT       RAW: Message text disguised using base64
 encoding
 -0.1 DKIM_VALID_AU          Message has a valid DKIM or DK signature from
 author's domain
 0.1 DKIM_SIGNED            Message has a DKIM or DK signature,
 not necessarily
 valid
 -0.1 DKIM_VALID Message has at least one valid DKIM or DK signature
 -0.1 DKIM_VALID_EF          Message has a valid DKIM or DK signature from
 envelope-from domain
 0.0 UNPARSEABLE_RELAY      Informational: message has unparseable relay
 lines
X-BeenThere: linux-mediatek@lists.infradead.org
X-Mailman-Version: 2.1.29
Precedence: list
List-Id: <linux-mediatek.lists.infradead.org>
List-Unsubscribe: <http://lists.infradead.org/mailman/options/linux-mediatek>,
 <mailto:linux-mediatek-request@lists.infradead.org?subject=unsubscribe>
List-Archive: <http://lists.infradead.org/pipermail/linux-mediatek/>
List-Post: <mailto:linux-mediatek@lists.infradead.org>
List-Help: <mailto:linux-mediatek-request@lists.infradead.org?subject=help>
List-Subscribe: <http://lists.infradead.org/mailman/listinfo/linux-mediatek>,
 <mailto:linux-mediatek-request@lists.infradead.org?subject=subscribe>
Cc: devicetree@vger.kernel.org, lorenzo.pieralisi@arm.com,
 srv_heupstream@mediatek.com, "chuanjia.liu" <Chuanjia.Liu@mediatek.com>,
 linux-pci@vger.kernel.org, linux-kernel@vger.kernel.org,
 jianjun.wang@mediatek.com, linux-mediatek@lists.infradead.org,
 yong.wu@mediatek.com, bhelgaas@google.com,
 linux-arm-kernel@lists.infradead.org, amurray@thegoodpenguin.co.uk
Sender: "Linux-mediatek" <linux-mediatek-bounces@lists.infradead.org>
Errors-To: 
 linux-mediatek-bounces+patchwork-linux-mediatek=patchwork.kernel.org@lists.infradead.org

From: "chuanjia.liu" <Chuanjia.Liu@mediatek.com>

There are two independent PCIe controllers in MT2712/MT7622 platform,
and each of them should contain an independent MSI domain.

In current architecture, MSI domain will be inherited from the root
bridge, and all of the devices will share the same MSI domain.
Hence that, the PCIe devices will not work properly if the irq number
which required is more than 32.

Split the PCIe node for MT2712/MT7622 platform to fix MSI issue and
comply with the hardware design.

Signed-off-by: chuanjia.liu <Chuanjia.Liu@mediatek.com>
---
 .../bindings/pci/mediatek-pcie-cfg.yaml       |  38 +++++
 .../devicetree/bindings/pci/mediatek-pcie.txt | 144 +++++++++++-------
 2 files changed, 129 insertions(+), 53 deletions(-)
 create mode 100644 Documentation/devicetree/bindings/pci/mediatek-pcie-cfg.yaml

--- /dev/null
+++ b/Documentation/devicetree/bindings/pci/mediatek-pcie-cfg.yaml
@@ -0,0 +1,38 @@
+# SPDX-License-Identifier: GPL-2.0-only OR BSD-2-Clause
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/pci/mediatek-pcie-cfg.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: Mediatek PCIECFG controller
+
+maintainers:
+  - Chuanjia Liu <chuanjia.liu@mediatek.com>
+  - Jianjun Wang <jianjun.wang@mediatek.com>
+
+description: |
+  The MediaTek PCIECFG controller controls some feature about
+  LTSSM, ASPM and so on.
+
+properties:
+  compatible:
+      items:
+        - enum:
+            - mediatek,mt7622-pciecfg
+            - mediatek,mt7629-pciecfg
+        - const: syscon
+
+  reg:
+    maxItems: 1
+
+required:
+  - compatible
+  - reg
+
+examples:
+  - |
+    pciecfg: pciecfg@1a140000 {
+        compatible = "mediatek,mt7622-pciecfg", "syscon";
+        reg = <0 0x1a140000 0 0x1000>;
+    };
+...
--- a/Documentation/devicetree/bindings/pci/mediatek-pcie.txt
+++ b/Documentation/devicetree/bindings/pci/mediatek-pcie.txt
@@ -8,7 +8,7 @@ Required properties:
 	"mediatek,mt7623-pcie"
 	"mediatek,mt7629-pcie"
 - device_type: Must be "pci"
-- reg: Base addresses and lengths of the PCIe subsys and root ports.
+- reg: Base addresses and lengths of the root ports.
 - reg-names: Names of the above areas to use during resource lookup.
 - #address-cells: Address representation for root ports (must be 3)
 - #size-cells: Size representation for root ports (must be 2)
@@ -19,10 +19,10 @@ Required properties:
    - sys_ckN :transaction layer and data link layer clock
   Required entries for MT2701/MT7623:
    - free_ck :for reference clock of PCIe subsys
-  Required entries for MT2712/MT7622:
+  Required entries for MT2712/MT7622/MT7629:
    - ahb_ckN :AHB slave interface operating clock for CSR access and RC
 	      initiated MMIO access
-  Required entries for MT7622:
+  Required entries for MT7622/MT7629:
    - axi_ckN :application layer MMIO channel operating clock
    - aux_ckN :pe2_mac_bridge and pe2_mac_core operating clock when
 	      pcie_mac_ck/pcie_pipe_ck is turned off
@@ -47,10 +47,13 @@ Required properties for MT7623/MT2701:
 - reset-names: Must be "pcie-rst0", "pcie-rst1", "pcie-rstN".. based on the
   number of root ports.
 
-Required properties for MT2712/MT7622:
+Required properties for MT2712/MT7622/MT7629:
 -interrupts: A list of interrupt outputs of the controller, must have one
 	     entry for each PCIe port
 
+Required properties for MT7622/MT7629:
+- mediatek,pcie-subsys: Should be a phandle of the pciecfg node.
+
 In addition, the device tree node must have sub-nodes describing each
 PCIe port interface, having the following mandatory properties:
 
@@ -143,56 +146,73 @@ Examples for MT7623:
 
 Examples for MT2712:
 
-	pcie: pcie@11700000 {
+	pcie1: pcie@112ff000 {
 		compatible = "mediatek,mt2712-pcie";
 		device_type = "pci";
-		reg = <0 0x11700000 0 0x1000>,
-		      <0 0x112ff000 0 0x1000>;
-		reg-names = "port0", "port1";
+		reg = <0 0x112ff000 0 0x1000>;
+		reg-names = "port1";
 		#address-cells = <3>;
 		#size-cells = <2>;
-		interrupts = <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>,
-			     <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
-		clocks = <&topckgen CLK_TOP_PE2_MAC_P0_SEL>,
-			 <&topckgen CLK_TOP_PE2_MAC_P1_SEL>,
-			 <&pericfg CLK_PERI_PCIE0>,
+		interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "pcie_irq";
+		clocks = <&topckgen CLK_TOP_PE2_MAC_P1_SEL>,
 			 <&pericfg CLK_PERI_PCIE1>;
-		clock-names = "sys_ck0", "sys_ck1", "ahb_ck0", "ahb_ck1";
-		phys = <&pcie0_phy PHY_TYPE_PCIE>, <&pcie1_phy PHY_TYPE_PCIE>;
-		phy-names = "pcie-phy0", "pcie-phy1";
+		clock-names = "sys_ck1", "ahb_ck1";
+		phys = <&u3port1 PHY_TYPE_PCIE>;
+		phy-names = "pcie-phy1";
 		bus-range = <0x00 0xff>;
-		ranges = <0x82000000 0 0x20000000  0x0 0x20000000  0 0x10000000>;
+		ranges = <0x82000000 0 0x11400000  0x0 0x11400000  0 0x300000>;
+		status = "disabled";
 
-		pcie0: pcie@0,0 {
-			reg = <0x0000 0 0 0 0>;
+		slot1: pcie@1,0 {
+			reg = <0x0800 0 0 0 0>;
 			#address-cells = <3>;
 			#size-cells = <2>;
 			#interrupt-cells = <1>;
 			ranges;
 			interrupt-map-mask = <0 0 0 7>;
-			interrupt-map = <0 0 0 1 &pcie_intc0 0>,
-					<0 0 0 2 &pcie_intc0 1>,
-					<0 0 0 3 &pcie_intc0 2>,
-					<0 0 0 4 &pcie_intc0 3>;
-			pcie_intc0: interrupt-controller {
+			interrupt-map = <0 0 0 1 &pcie_intc1 0>,
+					<0 0 0 2 &pcie_intc1 1>,
+					<0 0 0 3 &pcie_intc1 2>,
+					<0 0 0 4 &pcie_intc1 3>;
+			pcie_intc1: interrupt-controller {
 				interrupt-controller;
 				#address-cells = <0>;
 				#interrupt-cells = <1>;
 			};
 		};
+	};
 
-		pcie1: pcie@1,0 {
-			reg = <0x0800 0 0 0 0>;
+	pcie0: pcie@11700000 {
+		compatible = "mediatek,mt2712-pcie";
+		device_type = "pci";
+		reg = <0 0x11700000 0 0x1000>;
+		reg-names = "port0";
+		#address-cells = <3>;
+		#size-cells = <2>;
+		interrupts = <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "pcie_irq";
+		clocks = <&topckgen CLK_TOP_PE2_MAC_P0_SEL>,
+			 <&pericfg CLK_PERI_PCIE0>;
+		clock-names = "sys_ck0", "ahb_ck0";
+		phys = <&u3port0 PHY_TYPE_PCIE>;
+		phy-names = "pcie-phy0";
+		bus-range = <0x00 0xff>;
+		ranges = <0x82000000 0 0x20000000  0x0 0x20000000  0 0x10000000>;
+		status = "disabled";
+
+		slot0: pcie@0,0 {
+			reg = <0x0000 0 0 0 0>;
 			#address-cells = <3>;
 			#size-cells = <2>;
 			#interrupt-cells = <1>;
 			ranges;
 			interrupt-map-mask = <0 0 0 7>;
-			interrupt-map = <0 0 0 1 &pcie_intc1 0>,
-					<0 0 0 2 &pcie_intc1 1>,
-					<0 0 0 3 &pcie_intc1 2>,
-					<0 0 0 4 &pcie_intc1 3>;
-			pcie_intc1: interrupt-controller {
+			interrupt-map = <0 0 0 1 &pcie_intc0 0>,
+					<0 0 0 2 &pcie_intc0 1>,
+					<0 0 0 3 &pcie_intc0 2>,
+					<0 0 0 4 &pcie_intc0 3>;
+			pcie_intc0: interrupt-controller {
 				interrupt-controller;
 				#address-cells = <0>;
 				#interrupt-cells = <1>;
@@ -202,39 +222,31 @@ Examples for MT2712:
 
 Examples for MT7622:
 
-	pcie: pcie@1a140000 {
+	pcie0: pcie@1a143000 {
 		compatible = "mediatek,mt7622-pcie";
 		device_type = "pci";
-		reg = <0 0x1a140000 0 0x1000>,
-		      <0 0x1a143000 0 0x1000>,
-		      <0 0x1a145000 0 0x1000>;
-		reg-names = "subsys", "port0", "port1";
+		reg = <0 0x1a143000 0 0x1000>;
+		reg-names = "port0";
+		mediatek,pcie-cfg = <&pciecfg>;
 		#address-cells = <3>;
 		#size-cells = <2>;
-		interrupts = <GIC_SPI 228 IRQ_TYPE_LEVEL_LOW>,
-			     <GIC_SPI 229 IRQ_TYPE_LEVEL_LOW>;
+		interrupts = <GIC_SPI 228 IRQ_TYPE_LEVEL_LOW>;
+		interrupt-names = "pcie_irq";
 		clocks = <&pciesys CLK_PCIE_P0_MAC_EN>,
-			 <&pciesys CLK_PCIE_P1_MAC_EN>,
 			 <&pciesys CLK_PCIE_P0_AHB_EN>,
-			 <&pciesys CLK_PCIE_P1_AHB_EN>,
 			 <&pciesys CLK_PCIE_P0_AUX_EN>,
-			 <&pciesys CLK_PCIE_P1_AUX_EN>,
 			 <&pciesys CLK_PCIE_P0_AXI_EN>,
-			 <&pciesys CLK_PCIE_P1_AXI_EN>,
 			 <&pciesys CLK_PCIE_P0_OBFF_EN>,
-			 <&pciesys CLK_PCIE_P1_OBFF_EN>,
-			 <&pciesys CLK_PCIE_P0_PIPE_EN>,
-			 <&pciesys CLK_PCIE_P1_PIPE_EN>;
-		clock-names = "sys_ck0", "sys_ck1", "ahb_ck0", "ahb_ck1",
-			      "aux_ck0", "aux_ck1", "axi_ck0", "axi_ck1",
-			      "obff_ck0", "obff_ck1", "pipe_ck0", "pipe_ck1";
-		phys = <&pcie0_phy PHY_TYPE_PCIE>, <&pcie1_phy PHY_TYPE_PCIE>;
-		phy-names = "pcie-phy0", "pcie-phy1";
+			 <&pciesys CLK_PCIE_P0_PIPE_EN>;
+		clock-names = "sys_ck0", "ahb_ck0", "aux_ck0",
+			      "axi_ck0", "obff_ck0", "pipe_ck0";
+
 		power-domains = <&scpsys MT7622_POWER_DOMAIN_HIF0>;
 		bus-range = <0x00 0xff>;
-		ranges = <0x82000000 0 0x20000000  0x0 0x20000000  0 0x10000000>;
+		ranges = <0x82000000 0 0x20000000  0 0x20000000  0 0x8000000>;
+		status = "disabled";
 
-		pcie0: pcie@0,0 {
+		slot0: pcie@0,0 {
 			reg = <0x0000 0 0 0 0>;
 			#address-cells = <3>;
 			#size-cells = <2>;
@@ -251,8 +263,34 @@ Examples for MT7622:
 				#interrupt-cells = <1>;
 			};
 		};
+	};
+
+	pcie1: pcie@1a145000 {
+		compatible = "mediatek,mt7622-pcie";
+		device_type = "pci";
+		reg = <0 0x1a145000 0 0x1000>;
+		reg-names = "port1";
+		mediatek,pcie-cfg = <&pciecfg>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+		interrupts = <GIC_SPI 229 IRQ_TYPE_LEVEL_LOW>;
+		interrupt-names = "pcie_irq";
+		clocks = <&pciesys CLK_PCIE_P1_MAC_EN>,
+			 /* designer has connect RC1 with p0_ahb clock */
+			 <&pciesys CLK_PCIE_P0_AHB_EN>,
+			 <&pciesys CLK_PCIE_P1_AUX_EN>,
+			 <&pciesys CLK_PCIE_P1_AXI_EN>,
+			 <&pciesys CLK_PCIE_P1_OBFF_EN>,
+			 <&pciesys CLK_PCIE_P1_PIPE_EN>;
+		clock-names = "sys_ck1", "ahb_ck1", "aux_ck1",
+			      "axi_ck1", "obff_ck1", "pipe_ck1";
+
+		power-domains = <&scpsys MT7622_POWER_DOMAIN_HIF0>;
+		bus-range = <0x00 0xff>;
+		ranges = <0x82000000 0 0x28000000  0 0x28000000  0 0x8000000>;
+		status = "disabled";
 
-		pcie1: pcie@1,0 {
+		slot1: pcie@1,0 {
 			reg = <0x0800 0 0 0 0>;
 			#address-cells = <3>;
 			#size-cells = <2>;
