--- a/nl80211.h
+++ b/nl80211.h
@@ -2527,6 +2527,9 @@ enum nl80211_commands {
  *	override mask. Used with NL80211_ATTR_S1G_CAPABILITY in
  *	NL80211_CMD_ASSOCIATE or NL80211_CMD_CONNECT.
  *
+ * @NL80211_ATTR_WIPHY_ANTENNA_GAIN: Configured antenna gain. Used to reduce
+ *	transmit power to stay within regulatory limits. u32, dBi.
+ *
  * @NUM_NL80211_ATTR: total number of nl80211_attrs available
  * @NL80211_ATTR_MAX: highest attribute number currently defined
  * @__NL80211_ATTR_AFTER_LAST: internal use
@@ -3016,6 +3019,34 @@ enum nl80211_attrs {
 	NL80211_ATTR_S1G_CAPABILITY,
 	NL80211_ATTR_S1G_CAPABILITY_MASK,
 
+	NL80211_ATTR_SAE_PWE,
+
+	NL80211_ATTR_RECONNECT_REQUESTED,
+
+	NL80211_ATTR_SAR_SPEC,
+
+	NL80211_ATTR_DISABLE_HE,
+
+	NL80211_ATTR_HE_MUEDCA_PARAMS,
+
+	NL80211_ATTR_MULTIPLE_BSSID_PARENT,
+	NL80211_ATTR_MULTIPLE_BSSID_INDEX,
+	NL80211_ATTR_MULTIPLE_BSSID_COUNT,
+	NL80211_ATTR_MULTIPLE_BSSID_IES,
+	NL80211_ATTR_MULTIPLE_BSSID_EMA,
+
+	NL80211_ATTR_OBSS_COLOR_BITMAP,
+
+	NL80211_ATTR_COLOR_CHANGE_ANNOUNCEMENT_COUNT,
+	NL80211_ATTR_COLOR_CHANGE_ANNOUNCEMENT_COLOR,
+	NL80211_ATTR_COLOR_CHANGE_ANNOUNCEMENT_IES,
+
+	NL80211_ATTR_RNR_OFFSETS,
+
+	NL80211_ATTR_BEACON_TX_MODE,
+
+	NL80211_ATTR_WIPHY_ANTENNA_GAIN,
+
 	/* add attributes here, update the policy in nl80211.c */
 
 	__NL80211_ATTR_AFTER_LAST,
