#!/bin/sh

. /lib/functions.sh
. /lib/functions/uci-defaults.sh
. /lib/functions/system.sh

mediatek_setup_interfaces()
{
	local board="$1"

	case $board in
	bananapi,bpi-r2|\
	unielec,u7623-02-emmc-512m)
		ucidef_set_interfaces_lan_wan "lan0 lan1 lan2 lan3" "wan"
		;;
	esac
}

mediatek_setup_macs()
{
	local board="$1"

	case $board in
	unielec,u7623-02-emmc-512m)
		ucidef_set_interface_macaddr "wan" "$(cat /sys/class/net/wan/address)"
		;;
	esac
}

board_config_update
board=$(board_name)
mediatek_setup_interfaces $board
mediatek_setup_macs $board
board_config_flush

exit 0
