Changes to arch/powerpc/platforms/85xx/Makefile and Kconfig.

Keep these separate from the individual platform patches because all
platforms need to touch these two files.  By keeping these changes in
a separate patch allows the platform specific patchsets to sink/float
without conflicts in these two files.

diff --git a/arch/powerpc/platforms/85xx/Kconfig b/arch/powerpc/platforms/85xx/Kconfig
index b9a2559..2c1aa86 100644
--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -278,6 +278,19 @@ config CORENET_GENERIC
	  The following boards are supported for both 32bit and 64bit kernel:
	  P5020 DS, P5040 DS and T104xQDS

+config QUANTA_LB
+	bool "Quanta LBx"
+	select DEFAULT_UIMAGE
+	select HAS_RAPIDIO
+	help
+	  This option enables support for the Quanta LBx board
+
+config DELTA_7448
+	bool "Delta ET-7448BF"
+	select DEFAULT_UIMAGE
+	help
+	  This option enables support for the Delta ET-7448BF board
+
 endif # FSL_SOC_BOOKE

 config TQM85xx
diff --git a/arch/powerpc/platforms/85xx/Makefile b/arch/powerpc/platforms/85xx/Makefile
index bc5acb9..d04e66c 100644
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -30,3 +30,5 @@ obj-$(CONFIG_XES_MPC85xx) += xes_mpc85xx.o
 obj-$(CONFIG_GE_IMP3A)    += ge_imp3a.o
 obj-$(CONFIG_PPC_QEMU_E500) += qemu_e500.o
 obj-$(CONFIG_SGY_CTS1000) += sgy_cts1000.o
+obj-$(CONFIG_DELTA_7448)    += delta_7448.o
+obj-$(CONFIG_QUANTA_LB)   += quanta_lb.o
