--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/bcmendian.h
@@ -0,0 +1,324 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Byte order utilities
+ *
+ *  $Id: bcmendian.h 241182 2011-02-17 21:50:03Z $
+ *
+ * This file by default provides proper behavior on little-endian architectures.
+ * On big-endian architectures, IL_BIGENDIAN should be defined.
+ */
+
+#ifndef _BCMENDIAN_H_
+#define _BCMENDIAN_H_
+
+#include <typedefs.h>
+
+/* Reverse the bytes in a 16-bit value */
+#define BCMSWAP16(val) \
+	((uint16)((((uint16)(val) & (uint16)0x00ffU) << 8) | \
+		  (((uint16)(val) & (uint16)0xff00U) >> 8)))
+
+/* Reverse the bytes in a 32-bit value */
+#define BCMSWAP32(val) \
+	((uint32)((((uint32)(val) & (uint32)0x000000ffU) << 24) | \
+		  (((uint32)(val) & (uint32)0x0000ff00U) <<  8) | \
+		  (((uint32)(val) & (uint32)0x00ff0000U) >>  8) | \
+		  (((uint32)(val) & (uint32)0xff000000U) >> 24)))
+
+/* Reverse the two 16-bit halves of a 32-bit value */
+#define BCMSWAP32BY16(val) \
+	((uint32)((((uint32)(val) & (uint32)0x0000ffffU) << 16) | \
+		  (((uint32)(val) & (uint32)0xffff0000U) >> 16)))
+
+/* Byte swapping macros
+ *    Host <=> Network (Big Endian) for 16- and 32-bit values
+ *    Host <=> Little-Endian for 16- and 32-bit values
+ */
+#ifndef hton16
+#ifndef IL_BIGENDIAN
+#define HTON16(i) BCMSWAP16(i)
+#define	hton16(i) bcmswap16(i)
+#define	HTON32(i) BCMSWAP32(i)
+#define	hton32(i) bcmswap32(i)
+#define	NTOH16(i) BCMSWAP16(i)
+#define	ntoh16(i) bcmswap16(i)
+#define	NTOH32(i) BCMSWAP32(i)
+#define	ntoh32(i) bcmswap32(i)
+#define LTOH16(i) (i)
+#define ltoh16(i) (i)
+#define LTOH32(i) (i)
+#define ltoh32(i) (i)
+#define HTOL16(i) (i)
+#define htol16(i) (i)
+#define HTOL32(i) (i)
+#define htol32(i) (i)
+#else /* IL_BIGENDIAN */
+#define HTON16(i) (i)
+#define	hton16(i) (i)
+#define	HTON32(i) (i)
+#define	hton32(i) (i)
+#define	NTOH16(i) (i)
+#define	ntoh16(i) (i)
+#define	NTOH32(i) (i)
+#define	ntoh32(i) (i)
+#define	LTOH16(i) BCMSWAP16(i)
+#define	ltoh16(i) bcmswap16(i)
+#define	LTOH32(i) BCMSWAP32(i)
+#define	ltoh32(i) bcmswap32(i)
+#define HTOL16(i) BCMSWAP16(i)
+#define htol16(i) bcmswap16(i)
+#define HTOL32(i) BCMSWAP32(i)
+#define htol32(i) bcmswap32(i)
+#endif /* IL_BIGENDIAN */
+#endif /* hton16 */
+
+#ifndef IL_BIGENDIAN
+#define ltoh16_buf(buf, i)
+#define htol16_buf(buf, i)
+#else
+#define ltoh16_buf(buf, i) bcmswap16_buf((uint16 *)(buf), (i))
+#define htol16_buf(buf, i) bcmswap16_buf((uint16 *)(buf), (i))
+#endif /* IL_BIGENDIAN */
+
+/* Unaligned loads and stores in host byte order */
+#ifndef IL_BIGENDIAN
+#define load32_ua(a)		ltoh32_ua(a)
+#define store32_ua(a, v)	htol32_ua_store(v, a)
+#define load16_ua(a)		ltoh16_ua(a)
+#define store16_ua(a, v)	htol16_ua_store(v, a)
+#else
+#define load32_ua(a)		ntoh32_ua(a)
+#define store32_ua(a, v)	hton32_ua_store(v, a)
+#define load16_ua(a)		ntoh16_ua(a)
+#define store16_ua(a, v)	hton16_ua_store(v, a)
+#endif /* IL_BIGENDIAN */
+
+#define _LTOH16_UA(cp)	((cp)[0] | ((cp)[1] << 8))
+#define _LTOH32_UA(cp)	((cp)[0] | ((cp)[1] << 8) | ((cp)[2] << 16) | ((cp)[3] << 24))
+#define _NTOH16_UA(cp)	(((cp)[0] << 8) | (cp)[1])
+#define _NTOH32_UA(cp)	(((cp)[0] << 24) | ((cp)[1] << 16) | ((cp)[2] << 8) | (cp)[3])
+
+#define ltoh_ua(ptr) \
+	(sizeof(*(ptr)) == sizeof(uint8) ? *(const uint8 *)(ptr) : \
+	 sizeof(*(ptr)) == sizeof(uint16) ? _LTOH16_UA((const uint8 *)(ptr)) : \
+	 sizeof(*(ptr)) == sizeof(uint32) ? _LTOH32_UA((const uint8 *)(ptr)) : \
+	 *(uint8 *)0)
+
+#define ntoh_ua(ptr) \
+	(sizeof(*(ptr)) == sizeof(uint8) ? *(const uint8 *)(ptr) : \
+	 sizeof(*(ptr)) == sizeof(uint16) ? _NTOH16_UA((const uint8 *)(ptr)) : \
+	 sizeof(*(ptr)) == sizeof(uint32) ? _NTOH32_UA((const uint8 *)(ptr)) : \
+	 *(uint8 *)0)
+
+#ifdef __GNUC__
+
+/* GNU macro versions avoid referencing the argument multiple times, while also
+ * avoiding the -fno-inline used in ROM builds.
+ */
+
+#define bcmswap16(val) ({ \
+	uint16 _val = (val); \
+	BCMSWAP16(_val); \
+})
+
+#define bcmswap32(val) ({ \
+	uint32 _val = (val); \
+	BCMSWAP32(_val); \
+})
+
+#define bcmswap32by16(val) ({ \
+	uint32 _val = (val); \
+	BCMSWAP32BY16(_val); \
+})
+
+#define bcmswap16_buf(buf, len) ({ \
+	uint16 *_buf = (uint16 *)(buf); \
+	uint _wds = (len) / 2; \
+	while (_wds--) { \
+		*_buf = bcmswap16(*_buf); \
+		_buf++; \
+	} \
+})
+
+#define htol16_ua_store(val, bytes) ({ \
+	uint16 _val = (val); \
+	uint8 *_bytes = (uint8 *)(bytes); \
+	_bytes[0] = _val & 0xff; \
+	_bytes[1] = _val >> 8; \
+})
+
+#define htol32_ua_store(val, bytes) ({ \
+	uint32 _val = (val); \
+	uint8 *_bytes = (uint8 *)(bytes); \
+	_bytes[0] = _val & 0xff; \
+	_bytes[1] = (_val >> 8) & 0xff; \
+	_bytes[2] = (_val >> 16) & 0xff; \
+	_bytes[3] = _val >> 24; \
+})
+
+#define hton16_ua_store(val, bytes) ({ \
+	uint16 _val = (val); \
+	uint8 *_bytes = (uint8 *)(bytes); \
+	_bytes[0] = _val >> 8; \
+	_bytes[1] = _val & 0xff; \
+})
+
+#define hton32_ua_store(val, bytes) ({ \
+	uint32 _val = (val); \
+	uint8 *_bytes = (uint8 *)(bytes); \
+	_bytes[0] = _val >> 24; \
+	_bytes[1] = (_val >> 16) & 0xff; \
+	_bytes[2] = (_val >> 8) & 0xff; \
+	_bytes[3] = _val & 0xff; \
+})
+
+#define ltoh16_ua(bytes) ({ \
+	const uint8 *_bytes = (const uint8 *)(bytes); \
+	_LTOH16_UA(_bytes); \
+})
+
+#define ltoh32_ua(bytes) ({ \
+	const uint8 *_bytes = (const uint8 *)(bytes); \
+	_LTOH32_UA(_bytes); \
+})
+
+#define ntoh16_ua(bytes) ({ \
+	const uint8 *_bytes = (const uint8 *)(bytes); \
+	_NTOH16_UA(_bytes); \
+})
+
+#define ntoh32_ua(bytes) ({ \
+	const uint8 *_bytes = (const uint8 *)(bytes); \
+	_NTOH32_UA(_bytes); \
+})
+
+#else /* !__GNUC__ */
+
+/* Inline versions avoid referencing the argument multiple times */
+static INLINE uint16
+bcmswap16(uint16 val)
+{
+	return BCMSWAP16(val);
+}
+
+static INLINE uint32
+bcmswap32(uint32 val)
+{
+	return BCMSWAP32(val);
+}
+
+static INLINE uint32
+bcmswap32by16(uint32 val)
+{
+	return BCMSWAP32BY16(val);
+}
+
+/* Reverse pairs of bytes in a buffer (not for high-performance use) */
+/* buf	- start of buffer of shorts to swap */
+/* len  - byte length of buffer */
+static INLINE void
+bcmswap16_buf(uint16 *buf, uint len)
+{
+	len = len / 2;
+
+	while (len--) {
+		*buf = bcmswap16(*buf);
+		buf++;
+	}
+}
+
+/*
+ * Store 16-bit value to unaligned little-endian byte array.
+ */
+static INLINE void
+htol16_ua_store(uint16 val, uint8 *bytes)
+{
+	bytes[0] = val & 0xff;
+	bytes[1] = val >> 8;
+}
+
+/*
+ * Store 32-bit value to unaligned little-endian byte array.
+ */
+static INLINE void
+htol32_ua_store(uint32 val, uint8 *bytes)
+{
+	bytes[0] = val & 0xff;
+	bytes[1] = (val >> 8) & 0xff;
+	bytes[2] = (val >> 16) & 0xff;
+	bytes[3] = val >> 24;
+}
+
+/*
+ * Store 16-bit value to unaligned network-(big-)endian byte array.
+ */
+static INLINE void
+hton16_ua_store(uint16 val, uint8 *bytes)
+{
+	bytes[0] = val >> 8;
+	bytes[1] = val & 0xff;
+}
+
+/*
+ * Store 32-bit value to unaligned network-(big-)endian byte array.
+ */
+static INLINE void
+hton32_ua_store(uint32 val, uint8 *bytes)
+{
+	bytes[0] = val >> 24;
+	bytes[1] = (val >> 16) & 0xff;
+	bytes[2] = (val >> 8) & 0xff;
+	bytes[3] = val & 0xff;
+}
+
+/*
+ * Load 16-bit value from unaligned little-endian byte array.
+ */
+static INLINE uint16
+ltoh16_ua(const void *bytes)
+{
+	return _LTOH16_UA((const uint8 *)bytes);
+}
+
+/*
+ * Load 32-bit value from unaligned little-endian byte array.
+ */
+static INLINE uint32
+ltoh32_ua(const void *bytes)
+{
+	return _LTOH32_UA((const uint8 *)bytes);
+}
+
+/*
+ * Load 16-bit value from unaligned big-(network-)endian byte array.
+ */
+static INLINE uint16
+ntoh16_ua(const void *bytes)
+{
+	return _NTOH16_UA((const uint8 *)bytes);
+}
+
+/*
+ * Load 32-bit value from unaligned big-(network-)endian byte array.
+ */
+static INLINE uint32
+ntoh32_ua(const void *bytes)
+{
+	return _NTOH32_UA((const uint8 *)bytes);
+}
+
+#endif /* !__GNUC__ */
+#endif /* !_BCMENDIAN_H_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/bcmenetmib.h b/drivers/bcmdrivers/gmac/src/include/bcmenetmib.h
new file mode 100755
index 0000000..6f733fc
