--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/proto/vlan.h
@@ -0,0 +1,67 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * 802.1Q VLAN protocol definitions
+ *
+ * $Id: vlan.h 241182 2011-02-17 21:50:03Z $
+ */
+
+#ifndef _vlan_h_
+#define _vlan_h_
+
+#ifndef _TYPEDEFS_H_
+#include <typedefs.h>
+#endif
+
+/* This marks the start of a packed structure section. */
+#include <packed_section_start.h>
+
+#ifndef	VLAN_VID_MASK
+#define VLAN_VID_MASK		0xfff	/* low 12 bits are vlan id */
+#endif
+#define	VLAN_CFI_SHIFT		12	/* canonical format indicator bit */
+#define VLAN_PRI_SHIFT		13	/* user priority */
+
+#define VLAN_PRI_MASK		7	/* 3 bits of priority */
+
+#define	VLAN_TCI_OFFSET		14	/* offset of tag ctrl info field */
+
+#define	VLAN_TAG_LEN		4
+#define	VLAN_TAG_OFFSET		(2 * ETHER_ADDR_LEN)	/* offset in Ethernet II packet only */
+
+#define VLAN_TPID		0x8100	/* VLAN ethertype/Tag Protocol ID */
+
+struct ethervlan_header {
+	uint8	ether_dhost[ETHER_ADDR_LEN];
+	uint8	ether_shost[ETHER_ADDR_LEN];
+	uint16	vlan_type;		/* 0x8100 */
+	uint16	vlan_tag;		/* priority, cfi and vid */
+	uint16	ether_type;
+};
+
+#define	ETHERVLAN_HDR_LEN	(ETHER_HDR_LEN + VLAN_TAG_LEN)
+
+
+/* This marks the end of a packed structure section. */
+#include <packed_section_end.h>
+
+#define ETHERVLAN_MOVE_HDR(d, s) \
+do { \
+	struct ethervlan_header t; \
+	t = *(struct ethervlan_header *)(s); \
+	*(struct ethervlan_header *)(d) = t; \
+} while (0)
+
+#endif /* _vlan_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/proto/wpa.h b/drivers/bcmdrivers/gmac/src/include/proto/wpa.h
new file mode 100755
index 0000000..98b09a2
