--- /dev/null
+++ b/drivers/bcmdrivers/gmac/src/include/bcmsrom.h
@@ -0,0 +1,55 @@
+/*
+ * Copyright (C) 2013, Broadcom Corporation. All Rights Reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
+ * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
+ * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
+ * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ *
+ * Misc useful routines to access NIC local SROM/OTP .
+ *
+ * $Id: bcmsrom.h 280889 2011-08-31 18:39:27Z $
+ */
+
+#ifndef	_bcmsrom_h_
+#define	_bcmsrom_h_
+
+#include <bcmsrom_fmt.h>
+
+/* Prototypes */
+extern int srom_var_init(si_t *sih, uint bus, void *curmap, osl_t *osh,
+                         char **vars, uint *count);
+extern void srom_var_deinit(si_t *sih);
+
+extern int srom_read(si_t *sih, uint bus, void *curmap, osl_t *osh,
+                     uint byteoff, uint nbytes, uint16 *buf,
+                     bool check_crc);
+
+extern int srom_write(si_t *sih, uint bus, void *curmap, osl_t *osh,
+                      uint byteoff, uint nbytes, uint16 *buf);
+
+extern int srom_otp_cisrwvar(si_t *sih, osl_t *osh, char *vars, int *count);
+#if defined(WLTEST) || defined(BCMDBG)
+extern int srom_otp_write_region_crc(si_t *sih, uint nbytes, uint16* buf16, bool write);
+#endif
+
+/* parse standard PCMCIA cis, normally used by SB/PCMCIA/SDIO/SPI/OTP
+ *   and extract from it into name=value pairs
+ */
+extern int srom_probe_boardtype(uint8 *pcis[], uint ciscnt);
+extern int srom_parsecis(osl_t *osh, uint8 **pcis, uint ciscnt,
+                         char **vars, uint *count);
+
+#if defined(BCMUSBDEV)
+/* Return sprom size in 16-bit words */
+extern uint srom_size(si_t *sih, osl_t *osh);
+#endif
+
+#endif	/* _bcmsrom_h_ */
diff --git a/drivers/bcmdrivers/gmac/src/include/bcmsrom_fmt.h b/drivers/bcmdrivers/gmac/src/include/bcmsrom_fmt.h
new file mode 100755
index 0000000..9f90ed8
