From 5b08dd0d672b59fff16d02239ca6a36aaecdb1ca Mon Sep 17 00:00:00 2001
From: Roman Byshko <rbyshko@gmail.com>
Date: Fri, 7 Feb 2014 16:21:52 +0100
Subject: [PATCH] ARM: sun5i: dt: Add bindings for USB clocks

Signed-off-by: Roman Byshko <rbyshko@gmail.com>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun5i-a10s.dtsi | 9 +++++++++
 arch/arm/boot/dts/sun5i-a13.dtsi  | 9 +++++++++
 2 files changed, 18 insertions(+)

--- a/arch/arm/boot/dts/sun5i-a10s.dtsi
+++ b/arch/arm/boot/dts/sun5i-a10s.dtsi
@@ -272,6 +272,15 @@
 			clock-output-names = "ir0";
 		};
 
+		usb_clk: clk@01c200cc {
+			#clock-cells = <1>;
+		        #reset-cells = <1>;
+			compatible = "allwinner,sun5i-a13-usb-clk";
+			reg = <0x01c200cc 0x4>;
+			clocks = <&pll6 1>;
+			clock-output-names = "usb_ohci0", "usb_phy";
+		};
+
 		mbus_clk: clk@01c2015c {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-mod0-clk";
--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -274,6 +274,15 @@
 			clock-output-names = "ir0";
 		};
 
+		usb_clk: clk@01c200cc {
+			#clock-cells = <1>;
+		        #reset-cells = <1>;
+			compatible = "allwinner,sun5i-a13-usb-clk";
+			reg = <0x01c200cc 0x4>;
+			clocks = <&pll6 1>;
+			clock-output-names = "usb_ohci0", "usb_phy";
+		};
+
 		mbus_clk: clk@01c2015c {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-mod0-clk";
