From c2155e69578ea9f02c915960599bb5216ce860c1 Mon Sep 17 00:00:00 2001
From: Florian Meier <florian.meier@koalo.de>
Date: Fri, 22 Nov 2013 14:59:51 +0100
Subject: [PATCH 36/54] ASoC: Add support for PCM5102A codec

Some definitions to support the PCM5102A codec
by Texas Instruments.

Signed-off-by: Florian Meier <florian.meier@koalo.de>
---
 sound/soc/codecs/Kconfig    |  4 +++
 sound/soc/codecs/Makefile   |  2 ++
 sound/soc/codecs/pcm5102a.c | 63 +++++++++++++++++++++++++++++++++++++++++++++
 3 files changed, 69 insertions(+)
 create mode 100644 sound/soc/codecs/pcm5102a.c

diff --git a/sound/soc/codecs/Kconfig b/sound/soc/codecs/Kconfig
index 983d087a..f0d76ec 100644
--- a/sound/soc/codecs/Kconfig
+++ b/sound/soc/codecs/Kconfig
@@ -59,6 +59,7 @@ config SND_SOC_ALL_CODECS
 	select SND_SOC_PCM1681 if I2C
 	select SND_SOC_PCM1792A if SPI_MASTER
 	select SND_SOC_PCM3008
+	select SND_SOC_PCM5102A
 	select SND_SOC_RT5631 if I2C
 	select SND_SOC_RT5640 if I2C
 	select SND_SOC_SGTL5000 if I2C
@@ -313,6 +314,9 @@ config SND_SOC_PCM1792A
 config SND_SOC_PCM3008
        tristate
 
+config SND_SOC_PCM5102A
+	tristate
+
 config SND_SOC_RT5631
 	tristate
 
diff --git a/sound/soc/codecs/Makefile b/sound/soc/codecs/Makefile
index bc12676..612f414 100644
--- a/sound/soc/codecs/Makefile
+++ b/sound/soc/codecs/Makefile
@@ -46,6 +46,7 @@ snd-soc-hdmi-codec-objs := hdmi.o
 snd-soc-pcm1681-objs := pcm1681.o
 snd-soc-pcm1792a-codec-objs := pcm1792a.o
 snd-soc-pcm3008-objs := pcm3008.o
+snd-soc-pcm5102a-objs := pcm5102a.o
 snd-soc-rt5631-objs := rt5631.o
 snd-soc-rt5640-objs := rt5640.o
 snd-soc-sgtl5000-objs := sgtl5000.o
@@ -179,6 +180,7 @@ obj-$(CONFIG_SND_SOC_HDMI_CODEC) += snd-soc-hdmi-codec.o
 obj-$(CONFIG_SND_SOC_PCM1681)	+= snd-soc-pcm1681.o
 obj-$(CONFIG_SND_SOC_PCM1792A)	+= snd-soc-pcm1792a-codec.o
 obj-$(CONFIG_SND_SOC_PCM3008)	+= snd-soc-pcm3008.o
+obj-$(CONFIG_SND_SOC_PCM5102A)	+= snd-soc-pcm5102a.o
 obj-$(CONFIG_SND_SOC_RT5631)	+= snd-soc-rt5631.o
 obj-$(CONFIG_SND_SOC_RT5640)	+= snd-soc-rt5640.o
 obj-$(CONFIG_SND_SOC_SGTL5000)  += snd-soc-sgtl5000.o
diff --git a/sound/soc/codecs/pcm5102a.c b/sound/soc/codecs/pcm5102a.c
new file mode 100644
index 0000000..126f1e9
--- /dev/null
+++ b/sound/soc/codecs/pcm5102a.c
@@ -0,0 +1,63 @@
+/*
+ * Driver for the PCM5102A codec
+ *
+ * Author:	Florian Meier <florian.meier@koalo.de>
+ *		Copyright 2013
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ */
+
+
+#include <linux/init.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+
+#include <sound/soc.h>
+
+static struct snd_soc_dai_driver pcm5102a_dai = {
+	.name = "pcm5102a-hifi",
+	.playback = {
+		.channels_min = 2,
+		.channels_max = 2,
+		.rates = SNDRV_PCM_RATE_8000_192000,
+		.formats = SNDRV_PCM_FMTBIT_S16_LE |
+			   SNDRV_PCM_FMTBIT_S24_LE |
+			   SNDRV_PCM_FMTBIT_S32_LE
+	},
+};
+
+static struct snd_soc_codec_driver soc_codec_dev_pcm5102a;
+
+static int pcm5102a_probe(struct platform_device *pdev)
+{
+	return snd_soc_register_codec(&pdev->dev, &soc_codec_dev_pcm5102a,
+			&pcm5102a_dai, 1);
+}
+
+static int pcm5102a_remove(struct platform_device *pdev)
+{
+	snd_soc_unregister_codec(&pdev->dev);
+	return 0;
+}
+
+static struct platform_driver pcm5102a_codec_driver = {
+	.probe 		= pcm5102a_probe,
+	.remove 	= pcm5102a_remove,
+	.driver		= {
+		.name	= "pcm5102a-codec",
+		.owner	= THIS_MODULE,
+	},
+};
+
+module_platform_driver(pcm5102a_codec_driver);
+
+MODULE_DESCRIPTION("ASoC PCM5102A codec driver");
+MODULE_AUTHOR("Florian Meier <florian.meier@koalo.de>");
+MODULE_LICENSE("GPL v2");
-- 
1.9.1

