From 2fc6dcd5e7c76c203d2e174e70ef21393a231163 Mon Sep 17 00:00:00 2001
From: Zoltan HERPAI <wigyori@uid0.hu>
Date: Mon, 13 Jan 2014 14:15:01 +0100
Subject: [PATCH] ARM: sun4i: dt: Add basic board support for LinkSprite
 pcDuino

This patch will add a basic board support DT for the
LinkSprite pcDuino board.

Signed-off-by: Zoltan HERPAI <wigyori@uid0.hu>
Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/Makefile              |  1 +
 arch/arm/boot/dts/sun4i-a10-pcduino.dts | 48 +++++++++++++++++++++++++++++++++
 2 files changed, 49 insertions(+)
 create mode 100644 arch/arm/boot/dts/sun4i-a10-pcduino.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -284,6 +284,7 @@ dtb-$(CONFIG_ARCH_SUNXI) += \
 	sun4i-a10-cubieboard.dtb \
 	sun4i-a10-mini-xplus.dtb \
 	sun4i-a10-hackberry.dtb \
+	sun4i-a10-pcduino.dtb \
 	sun5i-a10s-olinuxino-micro.dtb \
 	sun5i-a13-olinuxino.dtb \
 	sun5i-a13-olinuxino-micro.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/sun4i-a10-pcduino.dts
@@ -0,0 +1,48 @@
+/*
+ * Copyright 2014 Zoltan HERPAI
+ * Zoltan HERPAI <wigyori@uid0.hu>
+ *
+ * The code contained herein is licensed under the GNU General Public
+ * License. You may obtain a copy of the GNU General Public License
+ * Version 2 or later at the following locations:
+ *
+ * http://www.opensource.org/licenses/gpl-license.html
+ * http://www.gnu.org/copyleft/gpl.html
+ */
+
+/dts-v1/;
+/include/ "sun4i-a10.dtsi"
+
+/ {
+	model = "LinkSprite pcDuino";
+	compatible = "linksprite,a10-pcduino", "allwinner,sun4i-a10";
+
+	soc@01c00000 {
+		emac: ethernet@01c0b000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&emac_pins_a>;
+			phy = <&phy1>;
+			status = "okay";
+		};
+
+		mdio@01c0b080 {
+			status = "okay";
+
+			phy1: ethernet-phy@1 {
+				reg = <1>;
+			};
+		};
+
+		uart0: serial@01c28000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart0_pins_a>;
+			status = "okay";
+		};
+
+		i2c0: i2c@01c2ac00 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c0_pins_a>;
+			status = "okay";
+		};
+	};
+};
