--- a/drivers/spi/Kconfig
+++ b/drivers/spi/Kconfig
@@ -229,6 +229,13 @@ config SPI_XILINX
 	  See the "OPB Serial Peripheral Interface (SPI) (v1.00e)"
 	  Product Specification document (DS464) for hardware details.
 
+config SPI_BCM63XX
+	tristate "Broadcom BCM63xx SPI controller"
+	depends on BCM63XX
+	select SPI_BITBANG
+	help
+	  SPI driver for the Broadcom BCM63xx SPI controller.
+
 #
 # Add new SPI master controllers in alphabetical order above this line
 #
--- a/drivers/spi/Makefile
+++ b/drivers/spi/Makefile
@@ -31,6 +31,7 @@ obj-$(CONFIG_SPI_S3C24XX)		+= spi_s3c24x
 obj-$(CONFIG_SPI_TXX9)			+= spi_txx9.o
 obj-$(CONFIG_SPI_XILINX)		+= xilinx_spi.o
 obj-$(CONFIG_SPI_SH_SCI)		+= spi_sh_sci.o
+obj-$(CONFIG_SPI_BCM63XX)		+= bcm63xx_spi.o
 # 	... add above this line ...
 
 # SPI protocol drivers (device/link on bus)
