[1;34;40mList of disjunctions[0m
[]
[1;34;40mAggregating similar requests[0m
[1;34;40mThe following services have been requested:[0m
[PathRequest 0
	source: 	trx Abilene
	destination:	trx Albany
	trx type:	Voyager
	trx mode:	mode 3
	baud_rate:	44.0 Gbaud
	bit_rate:	300.0 Gb/s
	spacing:	62.50000000000001 GHz
	power:  	0.0 dBm
	nb channels: 	76
	path_bandwidth: 	100.0 Gbit/s
	nodes-list:	[]
	loose-list:	[]
]
[1;34;40mComputing all paths with constraints[0m
[1;34;40mPropagating on selected path[0m
[1;34;40mResult summary[0m
req id   demand                       GSNR@bandwidth A-Z (Z-A)   GSNR@0.1nm A-Z (Z-A)        Receiver minOSNR               mode                    Gbit/s              nb of tsp pairs      N,M or blocking reason 
0       trx Abilene to trx Albany :             9.04                     14.5                      -                      mode 3                   100.0                      -                MODE_NOT_FEASIBLE    
[1;33;40mResult summary shows mean GSNR and OSNR (average over all channels)[0m
