From: Michal Kazior <michal.kazior@tieto.com>
Date: Thu, 21 Jan 2016 14:23:07 +0100
Subject: [PATCH] mac80211: fix txq queue related crashes

The driver can access the queue simultanously
while mac80211 tears down the interface. Without
spinlock protection this could lead to corrupting
sk_buff_head and subsequently to an invalid
pointer dereference.

Fixes: ba8c3d6f16a1 ("mac80211: add an intermediate software queue implementation")
Signed-off-by: Michal Kazior <michal.kazior@tieto.com>
---

--- a/net/mac80211/iface.c
+++ b/net/mac80211/iface.c
@@ -977,7 +977,10 @@ static void ieee80211_do_stop(struct iee
 	if (sdata->vif.txq) {
 		struct txq_info *txqi = to_txq_info(sdata->vif.txq);
 
+		spin_lock_bh(&txqi->queue.lock);
 		ieee80211_purge_tx_queue(&local->hw, &txqi->queue);
+		spin_unlock_bh(&txqi->queue.lock);
+
 		atomic_set(&sdata->txqs_len[txqi->txq.ac], 0);
 	}
 
